{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Cassini Master Schedule-c.csv"],"read":"whole","date_system":"1904"}

{"sheet":"Cassini Master Schedule-c.csv","index":0,"n_rows":43489,"n_cols":16,"rows_kept":4500,"cut":true,"bounds":{"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0}}
["Start time (UTC)","Duration","Date ","Team","SPASS Type","Target","Request Name","Library Definition","Title","Description"]
[]
["2004-135T18:40:00","000T01:00:00","2004-05-14","ADMIN","Prime","Saturn","TEST333",null,null,"Milestone."]
["2004-135T18:40:00","000T09:22:00","2004-05-14","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey"]
["2004-135T18:40:00","025T20:57:59","2004-05-14","CDA","Non-SPASS","DustRAM direction","SURVEY","Magnetospheric survey","dust exploration - saturn","for prograde dust (Saturn cent.): -z2E, -x 21;-18.6   AM=52"]
["2004-135T18:40:00","000T10:37:00","2004-05-14","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2004-135T18:40:00","027T09:21:59","2004-05-14","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SUR Campaign","Part of SUR MAPS Campaign.   Pointing: -X to sun, with either -Y to Saturn, or Saturn in S/C X, Z plane. This allows pick up ions to be measure, along with either Saturn ENA, or upstream ion events."]
["2004-135T18:40:00","002T23:52:00","2004-05-14","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-135T20:01:00","000T02:30:00","2004-05-14","ISS","Prime","rings(general)","DIFSATSRC","Diffuse ring satellite search","OBSERVATIONS OF DIFFUSE RINGS AND SATELLITES PRE-S","OBSERVATIONS OF DIFFUSE RINGS AND SATELLITES AT LOW PHASE BEFORE SOI; LAST CHANCE BEFORE FINAL SOI TRAJECTORY IS SET. THIS SET MAY HAVE 2 POINTINGS AT EACH ANSA, REPEAT L,R,L,R. EACH POINTING HAS 28 IMAGES AS: 2 SATELLITE EXP, 10 DIFFUSE RING EXP/POL/FILT, 2 SATELLITE EXP."]
["2004-135T20:01:00","000T02:30:00","2004-05-14","VIMS","SPASS Rider","rings(general)","DIFSATSRC","Diffuse ring satellite search","Early search for E Ring","Rider on ISS E Ring/satellite search. 1-sec exposures, IR + VIS.  Dimensions selected to fit ISS dwell times. Additional short exposures.  21 Mbits/hour.  Further details TBD."]
["2004-135T22:31:00","000T04:16:00","2004-05-14","UVIS","Prime","Saturn","MOS04PER","Linear mosaic","MOSAIC_09_PER_04","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. 1)  Align slit perpendicular to the Saturn Equator. 2) Slew about the Z-axis from Saturn Center to +MOS Orb. 3) Step 20 times using 1.75mrad increments about the Z-axis to -MOS Orb for 7200s. Stare for 360s during each step increment. 4) Step 14 times using 1.75mrad increments about the Z-axis toward +MOS Orb for 3600s. Stare for 360s during each step increment. 5) Slew back to Saturn Center and reset pointing. Stare for remaining observation time. MOS Orb (+/-Range): 16.88mrad."]
["2004-136T02:47:00","000T02:30:00","2004-05-15","ISS","Prime","rings(general)","DIFSATSRC","Diffuse ring satellite search","OBSERVATIONS OF DIFFUSE RINGS AND SATELLITES PRE-S","OBSERVATIONS OF DIFFUSE RINGS AND SATELLITES AT LOW PHASE BEFORE SOI; LAST CHANCE BEFORE FINAL SOI TRAJECTORY IS SET. THIS SET MAY HAVE 2 POINTINGS AT EACH ANSA, REPEAT L,R,L,R. EACH POINTING HAS 28 IMAGES AS: 2 SATELLITE EXP, 10 DIFFUSE RING EXP/POL/FILT, 2 SATELLITE EXP."]
["2004-136T02:47:00","000T02:30:00","2004-05-15","VIMS","SPASS Rider","rings(general)","DIFSATSRC","Diffuse ring satellite search","Early search for E Ring","Rider on ISS E Ring/satellite search. 1-sec exposures, IR + VIS.  Dimensions selected to fit ISS dwell times. Additional short exposures.  21 Mbits/hour.  Further details TBD."]
["2004-136T04:02:00","013T19:58:00","2004-05-15","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey"]
["2004-136T05:17:00","000T10:06:00","2004-05-15","CIRS","Prime","Saturn","TEMPSIT","Thermal map","CIRS_000SA_TEMPSIT","Early temperature map of Saturn, starting when  Saturn subtends ~5 mrad.  With a 2 mrad pointing uncertainty, 3 array positions covers the disk"]
["2004-136T05:17:00","000T10:06:00","2004-05-15","ISS","SPASS Rider","Saturn","TEMPSIT","Thermal map","Saturn Methane imaging","Methane Band Photometry"]
["2004-136T05:17:00","000T05:00:00","2004-05-15","MAG","Non-SPASS","InstrumentCalibration","SCAS","MAG SCAS instrument","MAG/SCAS_Cal","Boom alignment calibration using SCAS. If moved within scheduling window, KEEP OUTSIDE SCHEDULED MAPS CAMPAIGNS. Note: SCAS operations disturb RSS and RPWS. IF OpMode not ORS, unique sequence will be required. Includes 2 hours for IFC cal and range checks."]
["2004-136T10:17:00","006T15:30:00","2004-05-15","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2004-136T13:08:00","000T08:00:00","2004-05-15","RSS","SPASS Rider","Earth","USO","Ultra stable oscillator","RSS USO Characterization plus PIM","RSS USO characterization plus PIM. Pointing=XBAND to Earth. Last 4 hours required to be tracked at DSS-25 in 1-way mode. Last 4 hours are also desired to be tracked at DSS-14 in 1-way mode."]
["2004-136T15:23:00","000T00:30:00","2004-05-15","ISS","Prime","Other","RETARGETS","Retargetable observation","RETARGETABLES FOR SATELLITES DISCOVERED ON APPROAC","RETARGETABLES FOR SATELLITES DISCOVERED DURING APPROACH(START 0 TO PHOEBE ENCOUNTER)"]
["2004-136T17:08:00","000T09:00:00","2004-05-15","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-136T17:53:00","000T06:00:00","2004-05-15","CIRS","SPASS Rider","InstrumentCalibration","DSCAL0","Deep space calibration",null,"Deep space obervations for calibration."]
["2004-136T18:00:00","000T02:17:00","2004-05-15","CAPS","Non-SPASS","Saturn","BURST8K","8 kbps burst","Burst of 8kbps data","Burst of 8 kbps data (which gives uncollapsed ELS data). 32 B cycles duration. Data is in addition to 1000 bps from survey."]
["2004-137T03:00:00","000T02:17:00","2004-05-16","CAPS","Non-SPASS","Saturn","BURST8K","8 kbps burst","Burst of 8kbps data","Burst of 8 kbps data (which gives uncollapsed ELS data). 32 B cycles duration. Data is in addition to 1000 bps from survey."]
["2004-137T03:23:00","000T11:37:00","2004-05-16","UVIS","Prime","Saturn","MOS10PE","Linear mosaic","MOSAIC_10_PER_04","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. 1) Align slit parallel with Saturn Spin Axis. 2) Slew about the Z-axis from Saturn Center to +MOS Orb.  2) Step 77 times using 0.115 deg increments for 7200s to -MOS Orb. Stare for 94s during each step increment.  3) Step 77 times about the Z-axis using .115 deg increments for 7200s to +MOS Orb. Stare for 94s during each step increment. 4) Step 77 times about the Z-axis using .115 deg increments for 7200s to -MOS Orb. Stare for 94s during each step increment. 5) Step 77 times about the Z-axis using .115 deg increments for 7200s to +MOS Orb. Stare for 94s during each step increment.  6) Step 77 times about the Z-axis using .115 deg increments for 7200s to -MOS Orb. Stare for 94s during each step increment.  7) Slew back to Saturn Center. Return to WAYPOINT pointing. Stare for remaining observation time. MOS Orb (+/-range): 77.27mrad."]
["2004-137T15:00:00","000T00:20:00","2004-05-16","ISS","Prime","Other","RETARGETS","Retargetable observation","RETARGETABLES FOR SATELLITES DISCOVERED ON APPROAC","RETARGETABLES FOR SATELLITES DISCOVERED DURING APPROACH(START 0 TO PHOEBE ENCOUNTER)"]
["2004-137T15:20:00","000T00:30:00","2004-05-16","ISS","Prime","Other","SATELLORA","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 001 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [HY-DI-EN-HE-PA (602, 604, 607, 612, 617)]"]
["2004-137T17:05:00","000T09:00:00","2004-05-16","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-137T17:50:00","000T06:00:00","2004-05-16","CIRS","SPASS Rider","InstrumentCalibration","DSCAL0","Deep space calibration",null,"Deep space obervations for calibration."]
["2004-138T03:20:00","000T03:57:00","2004-05-17","UVIS","Prime","Saturn","MOS10PE","Linear mosaic","MOSAIC_10_PER_05","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on.  1) Align slit parallel with the Saturn Spin Axis. 2) Slew about the Z-axis from Saturn Center to +MOS Orb.   3) Step 77 times about the Z-axis using 0.115 deg increments for 7200s to -MOS Orb. Stare for 94s during each step increment.  4) Step 38 times about the Z-axis using .115 deg increments for 3600s to Saturn Center. 5) Reset pointing for the WAYPOINT. Stare for remaining observation time. MOS Orb (+/-Range): 77.27mrad."]
["2004-138T07:17:00","000T00:30:00","2004-05-17","ISS","Prime","Other","RETARGETS","Retargetable observation","RETARGETABLES FOR SATELLITES DISCOVERED ON APPROAC","RETARGETABLES FOR SATELLITES DISCOVERED DURING APPROACH(START 0 TO PHOEBE ENCOUNTER)"]
["2004-138T07:47:00","000T00:30:00","2004-05-17","ISS","Prime","Other","SATELLORA","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 002 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [DI-AT-CP-PM-JA (604, 610, 614, 615, 616)]"]
["2004-138T09:32:00","000T09:00:00","2004-05-17","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-138T10:17:00","000T06:00:00","2004-05-17","CIRS","SPASS Rider","InstrumentCalibration","DSCAL0","Deep space calibration",null,"Deep space obervations for calibration."]
["2004-138T18:32:00","004T07:15:00","2004-05-17","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-138T19:47:00","000T12:06:00","2004-05-17","CIRS","Prime","Saturn","TEMPSIT","Thermal map","CIRS_000SA_TEMPSIT","Early temperature map of Saturn, starting when  Saturn subtends ~5 mrad.  With a 2 mrad pointing uncertainty, 3 array positions covers the disk"]
["2004-138T19:47:00","000T12:06:00","2004-05-17","ISS","SPASS Rider","Saturn","TEMPSIT","Thermal map","Saturn polarimetry","NAC Polarimetery & Color"]
["2004-138T20:00:00","000T02:17:00","2004-05-17","CAPS","Non-SPASS","Saturn","BURST8K","8 kbps burst","Burst of 8kbps data","Burst of 8 kbps data (which gives uncollapsed ELS data). 32 B cycles duration. Data is in addition to 1000 bps from survey."]
["2004-139T07:53:00","000T07:50:00","2004-05-18","UVIS","Prime","Saturn","MOS10PE","Linear mosaic","MOSAIC_10_PER_06","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. 1) Align slit parallel with the Saturn Spin Axis. 2) Slew about the Z-axis from Saturn Center to +MOS Orb.  3) Step 77 times about the Z-axis using .115 deg step increments for 7200s to -MOS Orb. Stare for 94s during each step increment. 4) Step 77 times about the Z-axis for 7200s to +MOS Orb. Stare for 94s during each step increment. 5) Step 77 times about the Z-axis for 7200s to -MOS Orb. Stare for 94s during each step increment. 6) Step 38 times about the Z-axis for 3600s to Saturn Center. Stare for 94s during each step increment. 7) Reset pointing for the WAYPOINT. Stare for remaining observation time. MOS Orb (+/-Range): 77.27mrad."]
["2004-139T16:58:00","000T09:00:00","2004-05-18","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-139T18:00:00","000T02:17:00","2004-05-18","CAPS","Non-SPASS","Saturn","BURST8K","8 kbps burst","Burst of 8kbps data","Burst of 8 kbps data (which gives uncollapsed ELS data). 32 B cycles duration. Data is in addition to 1000 bps from survey."]
["2004-140T03:00:00","000T02:17:00","2004-05-19","CAPS","Non-SPASS","Saturn","BURST8K","8 kbps burst","Burst of 8kbps data","Burst of 8 kbps data (which gives uncollapsed ELS data). 32 B cycles duration. Data is in addition to 1000 bps from survey."]
["2004-140T03:13:00","000T11:26:00","2004-05-19","UVIS","Prime","Saturn","MOS10PE","Linear mosaic","MOSAIC_10_PER_07","UVIS mosaic. EUV and FUV low resolution slits on. 1) Align slit parallel with the Saturn Spin axis. 2) Slew about the Z-axis from Saturn Center to +MOS Orb. 3) Step 77 times about the Z-axis using .115 deg increments for 7200s to -MOS Orb. Stare for 94s during each step increment. 4) Step 77 times about the Z-axis using .115 deg increments for 7200s to +MOS Orb. Stare for 94s during each step increment. 5) Step 77 times about the Z-axis using .115 deg increments for 7200s to -MOS Orb. Stare for 94s during each step increment. 6) Step 77 times about the Z-axis using .115 deg increments for 7200s to +MOS Orb. Stare for 94s during each step increment. 7) Step 77 times about the Z-axis using .115 deg increments for 7200s to -MOS Orb. Stare for 94s during each step increment. 8) Slew back to Saturn Center and reset pointing for WAYPOINT. Stare for remaining observation time. MOS ORB (+/-Range): 77.27mrad."]
["2004-140T14:39:00","000T00:30:00","2004-05-19","ISS","Prime","Other","RETARGETS","Retargetable observation","RETARGETABLES FOR SATELLITES DISCOVERED ON APPROAC","RETARGETABLES FOR SATELLITES DISCOVERED DURING APPROACH(START 0 TO PHOEBE ENCOUNTER)"]
["2004-140T15:09:00","000T00:30:00","2004-05-19","ISS","Prime","Other","SATELLORA","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 003 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [EN-JA-PM-PA-EP (602, 610, 611, 616, 617)]"]
["2004-140T16:54:00","000T09:00:00","2004-05-19","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-141T03:09:00","000T03:57:00","2004-05-20","UVIS","Prime","Saturn","MOS11PA","Linear mosaic","MOSAIC_11_PAR_01","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on.  1) Align slit parallel with the Saturn Equator.  2) Slew about the Z-axis from Saturn Center to +MOS Orb. 3) Step 28 times about the Z-axis using .114 deg step increments for 7200s to -MOS Orb. Stare for 257s during each step increment. 4) Step 14 times about the Z-axis using .114 deg step increments for 3600s to Saturn Center. Stare for 257s during each step increment. 5) Reset pointing for Saturn Center and stare for remaining observation time. MOS Orb (+/-Range): 27.86mrad"]
["2004-141T07:06:00","000T00:30:00","2004-05-20","ISS","Prime","Other","RETARGETS","Retargetable observation","RETARGETABLES FOR SATELLITES DISCOVERED ON APPROAC","RETARGETABLES FOR SATELLITES DISCOVERED DURING APPROACH(START 0 TO PHOEBE ENCOUNTER)"]
["2004-141T07:36:00","000T00:30:00","2004-05-20","ISS","Prime","Other","SATELLORA","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 004 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [AT-TL-EN-PA-EP (602, 611, 613, 615, 617)]"]
["2004-141T09:21:00","000T09:00:00","2004-05-20","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-141T19:36:00","000T12:00:00","2004-05-20","CIRS","Prime","Saturn","TEMPSIT","Thermal map","CIRS_000SA_TEMPSIT","Early temperature map of Saturn, starting when  Saturn subtends ~5 mrad.  With a 2 mrad pointing uncertainty, 3 array positions covers the disk"]
["2004-141T19:36:00","000T12:00:00","2004-05-20","ISS","SPASS Rider","Saturn","TEMPSIT","Thermal map","Saturn Methane imaging","Methane Band Photometry"]
["2004-142T07:36:00","000T07:56:00","2004-05-21","UVIS","Prime","Saturn","MOS11PA","Linear mosaic","MOSAIC_11_PAR_02","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. 1) Align slit parallel with the Saturn Equator. 1) Slew about the Z-axis from Saturn Center to -MOS Orb. 2) Step 28 times about the Z-axis using .114 deg step increments for 7200s to -MOS Orb. Stare for 257s during each step increment. 3) Step 28 times about the Z-axis using .114 deg step increments for 7200s to +MOS Orb. Stare for 257s during each step increment. 4) Step 28 times about the Z-axis using .114 deg step increments for 7200s to -MOS Orb. Stare for 257s during each step increment. 5) Step 14 times about the Z-axis using .114 deg increments for 3600s to Saturn Center. Stare for 257s during each step increment. 6) Reset pointing for Saturn Center and stare for remaining observation time. MOS Orb (+/-Range): 27.86mrad."]
["2004-142T16:47:00","000T09:00:00","2004-05-21","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-142T17:32:00","000T06:00:00","2004-05-21","CIRS","SPASS Rider","InstrumentCalibration","DSCAL0","Deep space calibration",null,"Deep space obervations for calibration."]
["2004-143T01:47:00","001T16:24:00","2004-05-22","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2004-143T01:47:00","001T16:24:00","2004-05-22","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-143T03:00:00","000T04:34:00","2004-05-22","CAPS","Non-SPASS","Saturn","BURST8K","8 kbps burst","Burst of 8kbps data","Burst of 8 kbps data (which gives uncollapsed ELS data). 64 B cycles duration. Data is in addition to 1000 bps from survey."]
["2004-143T03:02:00","000T00:30:00","2004-05-22","ISS","Prime","Titan","MOVIEOP","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-143T03:02:00","000T00:30:00","2004-05-22","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve","Titan Light Curve, Observtion #1, ride along with ISS"]
["2004-143T03:32:00","000T01:51:00","2004-05-22","UVIS","Prime","Titan","MOS11PAA","Linear mosaic","MOSAIC_11_PAR_03a","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. 1) Slew about the Z-axis from Titan to +MOS Orb. Align slit parallel with the Saturn Equator. 2) Step 28 times about the Z-axis using 0.114 deg increments for 3600s to -MOS Orb. Stare for 129s during each step increment.  3) Slew back to Titan. Reset pointing and stare for remaining observation time. MOS Orb (Saturn+/-Range): 27.86mrad."]
["2004-143T05:23:00","000T00:30:00","2004-05-22","ISS","Prime","Titan","MOVIEPP","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-143T05:23:00","000T00:30:00","2004-05-22","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #2","Titan Light Curve, Observation #2, ride along with ISS"]
["2004-143T05:53:00","000T02:00:00","2004-05-22","UVIS","Prime","Titan","MOS11PAB","Linear mosaic","MOSAIC_11_PAR_03b","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. 1) Slew about the Z-axis from Titan to +MOS Orb. Align slit parallel with the Saturn Equator. 2) Step 28 times about the Z-axis using 0.114 deg increments for 3600s to -MOS Orb. Stare for 129s during each step increment. 3) Step 14 times about the Z-axis using .114deg increments for 1800s to Titan. Stare for 129s during each step increment. 4) Reset pointing and stare for remaining observation time. MOS Orb (Saturn+/-Range): 27.86mrad."]
["2004-143T07:53:00","000T00:30:00","2004-05-22","ISS","Prime","Titan","MOVIEPP","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-143T07:53:00","000T00:30:00","2004-05-22","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #3","Titan Light Curve, Observation #3, ride along with ISS"]
["2004-143T08:23:00","000T02:00:00","2004-05-22","UVIS","Prime","Titan","MOS11PAC","Linear mosaic","MOSAIC_11_PAR_03C","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. 1) Slew about the Z-axis from Titan to +MOS Orb. Align slit parallel with the Saturn Equator. 2) Step 28 times about the Z-axis using 0.114 deg increments for 3600s to -MOS Orb. Stare for 129s during each step increment. 3) Step 14 times about the Z-axis using .114 deg increments for 1800s to Titan. Stare for 129s during each step increment. 4) Reset pointing and stare for remaining observation time. MOS Orb (Saturn +/-Range): 27.86mrad."]
["2004-143T10:23:00","000T00:30:00","2004-05-22","ISS","Prime","Titan","MOVIEPP","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-143T10:23:00","000T00:30:00","2004-05-22","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #4","Titan Light Curve, Observation #4, ride along with ISS"]
["2004-143T10:53:00","000T02:00:00","2004-05-22","UVIS","Prime","Titan","MOS11PAD","Linear mosaic","MOSAIC_11_PAR_03d","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. 1) Slew about the Z-axis from Titan to +MOS Orb. Align slit parallel with the Saturn Equator. 2) Step 28 times about the Z-axis using 0.114 deg increments for 3600s to -MOS Orb. Stare for 129s during each step increment. 3) Step 14 times about the Z-axis using .114 deg increments for 1800s to Titan. Stare for 129s during each step increment. 4) Reset pointing and stare for remaining observation time. MOS Orb (Saturn+/-Range): 27.86mrad."]
["2004-143T12:00:00","000T04:34:00","2004-05-22","CAPS","Non-SPASS","Saturn","BURST8K","8 kbps burst","Burst of 8kbps data","Burst of 8 kbps data (which gives uncollapsed ELS data). 64 B cycles duration. Data is in addition to 1000 bps from survey."]
["2004-143T12:53:00","000T00:30:00","2004-05-22","ISS","Prime","Titan","MOVIEPP","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-143T12:53:00","000T00:30:00","2004-05-22","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #5","Titan Light Curve, Observation #5, ride along with ISS"]
["2004-143T13:23:00","000T01:05:00","2004-05-22","UVIS","Prime","Titan","MOS11PAE","Linear mosaic","MOSAIC_11_PAR_03E","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. 1) Stare at WAYPOINT for observation duration."]
["2004-143T14:28:00","000T00:30:00","2004-05-22","ISS","Prime","Other","RETARGETS","Retargetable observation","RETARGETABLES FOR SATELLITES DISCOVERED ON APPROAC","RETARGETABLES FOR SATELLITES DISCOVERED DURING APPROACH(START 0 TO PHOEBE ENCOUNTER)"]
["2004-143T14:58:00","000T00:30:00","2004-05-22","ISS","Prime","Other","SATELLORA","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 005 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [EP-EN-CP-PM-PA (602, 611, 614, 616, 617)]"]
["2004-143T16:43:00","000T09:00:00","2004-05-22","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-143T17:28:00","000T06:00:00","2004-05-22","CIRS","SPASS Rider","InstrumentCalibration","DSCAL0","Deep space calibration",null,"Deep space obervations for calibration."]
["2004-144T02:58:00","000T00:30:00","2004-05-23","ISS","Prime","Titan","MOVIEQQ","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-144T02:58:00","000T00:30:00","2004-05-23","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #6","Titan Light Curve, Observation #6, ride along with ISS"]
["2004-144T03:00:00","000T04:34:00","2004-05-23","CAPS","Non-SPASS","Saturn","BURST8K","8 kbps burst","Burst of 8kbps data","Burst of 8 kbps data (which gives uncollapsed ELS data). 64 B cycles duration. Data is in addition to 1000 bps from survey."]
["2004-144T03:28:00","000T02:00:00","2004-05-23","UVIS","Prime","Titan","MOS11PAA","Linear mosaic","MOSAIC_11_PAR_04A","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. 1) Slew about the Z-axis from Titan to -MOS Orb. Align slit parallel with the Saturn Equator. 2) Step 28 times about the Z-axis using 0.114 deg increments for 3600s to +MOS Orb. Stare for 129s during each step increment. 3) Step 14 times about the Z-axis using .114 deg increments for 1800s to Titan. Stare for 129s during each step increment. 4) Reset pointing and stare for remaining observation time. MOS Orb (Saturn+/-Range): 27.86mrad."]
["2004-144T05:28:00","000T00:30:00","2004-05-23","ISS","Prime","Titan","MOVIEQQ","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-144T05:28:00","000T00:30:00","2004-05-23","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #7","Titan Light Curve, Observation #7, ride along with ISS"]
["2004-144T05:58:00","000T00:58:00","2004-05-23","UVIS","Prime","Titan","MOS11PAB","Linear mosaic","MOSAIC_11_PAR_04b","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. Stare at waypoint for duration of observation."]
["2004-144T06:56:00","000T00:30:00","2004-05-23","ISS","Prime","Other","RETARGETS","Retargetable observation","RETARGETABLES FOR SATELLITES DISCOVERED ON APPROAC","RETARGETABLES FOR SATELLITES DISCOVERED DURING APPROACH(START 0 TO PHOEBE ENCOUNTER)"]
["2004-144T07:26:00","000T00:30:00","2004-05-23","ISS","Prime","Other","SATELLORA","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 006 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [TL-EP-AT-PM-JA (610, 611, 613, 615, 616)]"]
["2004-144T09:11:00","000T09:00:00","2004-05-23","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-144T09:56:00","000T06:00:00","2004-05-23","CIRS","SPASS Rider","InstrumentCalibration","DSCAL0","Deep space calibration",null,"Deep space obervations for calibration."]
["2004-144T10:00:00","000T06:51:00","2004-05-23","CAPS","Non-SPASS","Saturn","BURST8K","8 kbps burst","Burst of 8kbps data","Burst of 8 kbps data (which gives uncollapsed ELS data). 96 B cycles duration. Data is in addition to 1000 bps from survey."]
["2004-144T18:11:00","007T08:18:00","2004-05-23","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2004-144T18:11:00","005T23:37:00","2004-05-23","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-144T19:26:00","000T12:00:00","2004-05-23","CIRS","Prime","Saturn","TEMPSIT","Thermal map","CIRS_000SA_TEMPSIT","Early temperature map of Saturn, starting when  Saturn subtends ~5 mrad.  With a 2 mrad pointing uncertainty, 3 array positions covers the disk"]
["2004-144T19:26:00","000T12:00:00","2004-05-23","ISS","SPASS Rider","Saturn","TEMPSIT","Thermal map","Saturn polarimetry","NAC Polarimetery & Color"]
["2004-144T20:00:00","000T02:17:00","2004-05-23","CAPS","Non-SPASS","Saturn","BURST8K","8 kbps burst","Burst of 8kbps data","Burst of 8 kbps data (which gives uncollapsed ELS data). 32 B cycles duration. Data is in addition to 1000 bps from survey."]
["2004-145T07:26:00","000T00:30:00","2004-05-24","ISS","Prime","Titan","MOVIERR","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds. 6 images every 10 minutes"]
["2004-145T07:26:00","000T00:30:00","2004-05-24","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #8","Titan Light Curve, Observation #8, ride along with ISS"]
["2004-145T07:56:00","000T02:00:00","2004-05-24","UVIS","Prime","Titan","MOS11PAA","Linear mosaic","MOSAIC_11_PAR_05A","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. 1) Slew about the Z-axis from Titan to -MOS Orb. Align slit parallel with the Saturn Equator. 2) Step 28 times about the Z-axis using 0.114 deg increments for 3600s to +MOS Orb. Stare for 129s during each step increment. 3) Step 14 times about the Z-axis using .114 deg increments for 1800s to Titan. Stare for 129s during each step increment. 4) Reset pointing and stare for remaining observation time. MOS Orb (Saturn+/-Range): 27.86mrad."]
["2004-145T09:56:00","000T00:30:00","2004-05-24","ISS","Prime","Titan","MOVIERR","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds. 6 images every 10 minutes"]
["2004-145T09:56:00","000T00:30:00","2004-05-24","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #9","Titan Light Curve, Observation #9, ride along with ISS"]
["2004-145T10:26:00","000T02:00:00","2004-05-24","UVIS","Prime","Titan","MOS11PAB","Linear mosaic","MOSAIC_11_PAR_05b","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. 1) Slew about the Z-axis from Titan to -MOS Orb. Align slit parallel with the Saturn Equator. 2) Step 28 times about the Z-axis using 0.114 deg increments for 3600s to +MOS Orb. Stare for 129s during each step increment. 3) Step 14 times about the Z-axis using .114 deg increments for 1800s to Titan. Stare for 129s during each step increment. 4) Reset pointing and stare for remaining observation time. MOS Orb (Saturn+/-Range): 27.86mrad."]
["2004-145T12:26:00","000T00:30:00","2004-05-24","ISS","Prime","Titan","MOVIERR","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds. 6 images every 10 minutes"]
["2004-145T12:26:00","000T00:30:00","2004-05-24","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #10","Titan Light Curve, Observation #10, ride along with ISS"]
["2004-145T12:56:00","000T02:00:00","2004-05-24","UVIS","Prime","Titan","MOS11PAC","Linear mosaic","MOSAIC_11_PAR_05C","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. 1) Slew about the Z-axis from Titan to -MOS Orb. Align slit parallel with the Saturn Equator. 2) Step 28 times about the Z-axis using 0.114 deg increments for 3600s to +MOS Orb. Stare for 129s during each step increment. 3) Step 14 times about the Z-axis using .114 deg increments for 1800s to Titan. Stare for 129s during each step increment. 4) Reset pointing and stare for remaining observation time. MOS Orb (Saturn+/-Range): 27.86mrad."]
["2004-145T14:56:00","000T00:25:00","2004-05-24","ISS","Prime","Titan","MOVIERS","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds. 6 images every 10 minutes"]
["2004-145T14:56:00","000T00:25:00","2004-05-24","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #11","Titan Light Curve, Observation #11, ride along with ISS"]
["2004-145T16:36:00","000T09:00:00","2004-05-24","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-145T17:00:00","000T02:17:00","2004-05-24","CAPS","Non-SPASS","Saturn","BURST8K","8 kbps burst","Burst of 8kbps data","Burst of 8 kbps data (which gives uncollapsed ELS data). 32 B cycles duration. Data is in addition to 1000 bps from survey."]
["2004-145T17:21:00","000T06:00:00","2004-05-24","CIRS","SPASS Rider","InstrumentCalibration","DSCAL0","Deep space calibration",null,"Deep space obervations for calibration."]
["2004-146T02:51:00","000T00:30:00","2004-05-25","ISS","Prime","Titan","MOVIESS","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-146T02:51:00","000T00:30:00","2004-05-25","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #12","Titan Light Curve, Observation #12, ride along with ISS"]
["2004-146T03:21:00","000T02:00:00","2004-05-25","UVIS","Prime","Titan","MOS11PAA","Linear mosaic","MOSAIC_11_PAR_06a","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. 1) Align slit parallel with the Saturn Equator. 2) Step 28 times about the Z-axis using 0.114 deg increments for 3600s from Titan to +MOS Orb (increasing DEC angles). Stare for 129s during each step increment. 3) Step 14 times about the Z-axis using .114 deg increments for 1800s toward Titan. 4) Slew back to Titan and reset pointing. Stare for remaining observation time. MOS Orb (Saturn +/- Range): 27.86mrad."]
["2004-146T05:21:00","000T00:30:00","2004-05-25","ISS","Prime","Titan","MOVIESS","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-146T05:21:00","000T00:30:00","2004-05-25","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #13","Titan Light Curve, Observation #13, ride along with ISS"]
["2004-146T05:51:00","000T02:00:00","2004-05-25","UVIS","Prime","Titan","MOS11PAB","Linear mosaic","MOSAIC_11_PAR_06b","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. 1) Align slit parallel with the Saturn Equator. 2) Step 28 times about the Z-axis using 0.114 deg increments for 3600s from Titan to +MOS Orb (increasing DEC angles). Stare for 129s during each step increment. 3) Step 14 times about the Z-axis using .114deg increments for 1800s toward Titan. Stare for 129s during each step increment. 4) Slew back to Titan and reset pointing. Stare for remaining observation time. MOS Orb (Saturn +/- Range): 27.86mrad."]
["2004-146T07:51:00","000T00:30:00","2004-05-25","ISS","Prime","Titan","MOVIESS","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-146T07:51:00","000T00:30:00","2004-05-25","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #14","Titan Light Curve, Observation #14, ride along with ISS"]
["2004-146T08:21:00","000T02:00:00","2004-05-25","UVIS","Prime","Titan","MOS11PAC","Linear mosaic","MOSAIC_11_PAR_06c","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. 1) Align slit parallel with the Saturn Equator. 2) Step 28 times about the Z-axis using 0.114 deg increments for 3600s from Titan to +MOS Orb (increasing DEC angles). Stare for 129s during each step increment. 3) Step 14 times about the Z-axis using .114 deg increments for 1800s toward Titan 4) Slew back to Titan and reset pointing. Stare for remaining observation time. MOS Orb (Saturn +/- Range): 27.86mrad."]
["2004-146T10:21:00","000T00:30:00","2004-05-25","ISS","Prime","Titan","MOVIESS","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-146T10:21:00","000T00:30:00","2004-05-25","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #15","Titan Light Curve, Observation #15, ride along with ISS"]
["2004-146T10:51:00","000T02:00:00","2004-05-25","UVIS","Prime","Titan","MOS11PAD","Linear mosaic","MOSAIC_11_PAR_06D","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. 1) Align slit parallel with the Saturn Equator. 2) Step 28 times about the Z-axis using 0.114 deg increments for 3600s from Titan to +MOS Orb (increasing DEC angles). Stare for 129s during each step increment. 3) Step 14 times about the Z-axis using .114 deg increments for 1800s toward Titan. Stare for 129s during each step increment. 4) Slew back to Titan and reset pointing. Stare for remaining observation time. MOS Orb (Saturn +/- Range): 27.86mrad."]
["2004-146T12:51:00","000T00:30:00","2004-05-25","ISS","Prime","Titan","MOVIESS","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-146T12:51:00","000T00:30:00","2004-05-25","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #16","Titan Light Curve, Observation #16, ride along with ISS"]
["2004-146T13:21:00","000T00:57:00","2004-05-25","UVIS","Prime","Titan","MOS11PAE","Linear mosaic","MOSAIC_11_PAR_06E","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. Stare at waypoint for duration of observation"]
["2004-146T14:18:00","000T00:30:00","2004-05-25","ISS","Prime","Other","RETARGETS","Retargetable observation","RETARGETABLES FOR SATELLITES DISCOVERED ON APPROAC","RETARGETABLES FOR SATELLITES DISCOVERED DURING APPROACH(START 0 TO PHOEBE ENCOUNTER)"]
["2004-146T14:48:00","000T00:30:00","2004-05-25","ISS","Prime","Other","SATELLORA","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 007 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [PA-DI-PM-EN-JA (602, 604, 610, 616, 617)]"]
["2004-146T16:33:00","000T09:00:00","2004-05-25","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-147T02:48:00","000T00:30:00","2004-05-26","ISS","Prime","Titan","MOVIETT","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-147T02:48:00","000T00:30:00","2004-05-26","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #17","Titan Light Curve, Observation #17, ride along with ISS"]
["2004-147T03:18:00","000T02:00:00","2004-05-26","UVIS","Prime","Titan","MOS11PAA","Linear mosaic","MOSAIC_11_PAR_07A","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. 1) Align slit parallel with the Saturn Equator. 2) Step 28 times about the Z-axis using 0.114 deg increments for 3600s from Titan to +MOS Orb (increasing DEC angles). Stare for 129s during each step increment. 3) Step 14 times about the Z-axis using .114 deg increments for 1800s toward Titan. Stare for 129s during each step increment. 4) Slew back to Titan and reset pointing. Stare for remaining observation time. MOS Orb (Saturn+/-Range): 27.86mrad."]
["2004-147T05:18:00","000T00:30:00","2004-05-26","ISS","Prime","Titan","MOVIETT","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-147T05:18:00","000T00:30:00","2004-05-26","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #18","Titan Light Curve, Observation #18, ride along with ISS"]
["2004-147T05:48:00","000T00:57:00","2004-05-26","UVIS","Prime","Titan","MOS11PAB","Linear mosaic","MOSAIC_11_PAR_07b","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, parallel to the orbital plane.  1) Slew from Titan to START RA/DEC: 36.89/11.32 deg.  2) Step 28 times using 0.114 deg increments. Step in the direction of decreasing declination angles in the XY plane.  Stare during each step increment.  Total mosaic time 2700 seconds. 3) Slew back to Titan and reset pointing.  Stare for remaining observation time."]
["2004-147T06:45:00","000T00:30:00","2004-05-26","ISS","Prime","Other","RETARGETS","Retargetable observation","RETARGETABLES FOR SATELLITES DISCOVERED ON APPROAC","RETARGETABLES FOR SATELLITES DISCOVERED DURING APPROACH(START 0 TO PHOEBE ENCOUNTER)"]
["2004-147T07:15:00","000T00:30:00","2004-05-26","ISS","Prime","Other","SATELLORA","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 008 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [AT-HY-DI-MI-HE (601, 604, 607, 612, 615)]"]
["2004-147T09:00:00","000T09:00:00","2004-05-26","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-147T19:15:00","000T12:00:00","2004-05-26","ISS","Prime","rings(general)","SATSRCHBP","Ansa movie","ANSA MOVIE FOR SATELLITE SEARCHES, PRE PHOEBE IN R","ANSA MOVIE FOR SEARCHING FOR SATELLITES IN RING GAPS ON APPROACH. ONE NAC, ALTERNATE ANSAE, EVERY 12 MINUTES."]
["2004-148T07:15:00","000T00:30:00","2004-05-27","ISS","Prime","Titan","MOVIEUU","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-148T07:15:00","000T00:30:00","2004-05-27","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #19","Titan Light Curve, Observation #19, ride along with ISS"]
["2004-148T07:45:00","000T02:00:00","2004-05-27","UVIS","Prime","Titan","MOS11PEA","Linear mosaic","MOSAIC_11_PER_01A","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on.  1) Align slit parallel with the Saturn Spin Axis. 2) Step 96 times about the Z-axis using 0.119 deg increments for 3600s from Titan to -MOS Orb (decreasing RA angles). Stare for 37.5s during each step increment. 3) Step 48 times about the Z-axis using .119 deg increments for 1800s toward Titan. Stare for 37.5s during each step increment. 3) Slew back to Titan and reset pointing. Stare for remaining observation time.  MOS Orb (Saturn +/-Range): 99.69mrad."]
["2004-148T09:45:00","000T00:30:00","2004-05-27","ISS","Prime","Titan","MOVIEUU","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-148T09:45:00","000T00:30:00","2004-05-27","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #20","Titan Light Curve, Observation #20, ride along with ISS"]
["2004-148T10:15:00","000T02:00:00","2004-05-27","UVIS","Prime","Titan","MOS11PEB","Linear mosaic","MOSAIC_11_PER_01b","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on.  1) Align slit parallel with the Saturn Spin Axis. 2) Step 96 times about the Z-axis using 0.119 deg increments for 3600s from Titan  to -MOS ORB. Stare for 37.5s during each step increment. 3) Step 48 times about the Z-axis using .119 deg increments for 1800s toward Titan. Stare for 37.5s during each step increment. 3) Slew back to Titan and reset pointing. Stare for remaining observation time.  MOS Orb (Saturn +/-Range): 99.69mrad."]
["2004-148T12:15:00","000T00:30:00","2004-05-27","ISS","Prime","Titan","MOVIEUU","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-148T12:15:00","000T00:30:00","2004-05-27","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #21","Titan Light Curve, Observation #21, ride along with ISS"]
["2004-148T12:45:00","000T02:00:00","2004-05-27","UVIS","Prime","Titan","MOS11PEC","Linear mosaic","MOSAIC_11_PER_01c","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on.  1) Align slit parallel with the Saturn Spin Axis. 2) Step 96 times about the Z-axis using 0.119 deg increments for 3600s from Titan  to -MOS ORB. Stare for 37.5s during each step increment. 3) Step 48 times about the Z-axis using .119deg increments for 1800s toward Titan. Stare for 37.5s during each step increment. 4) Slew back to Titan and reset pointing. Stare for remaining observation time.  MOS Orb (Saturn+/-Range): 99.69mrad."]
["2004-148T14:45:00","000T00:26:00","2004-05-27","ISS","Prime","Titan","MOVIEUV","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-148T14:45:00","000T00:26:00","2004-05-27","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #22","Titan Light Curve, Observation #22, ride along with ISS"]
["2004-148T16:26:00","000T10:47:00","2004-05-27","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-149T03:13:00","000T03:40:00","2004-05-28","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-149T11:41:00","000T00:30:00","2004-05-28","ISS","Prime","Titan","MOVIEVV","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-149T12:11:00","000T01:55:00","2004-05-28","UVIS","Prime","Titan","MOS11PEE","Linear mosaic","MOSAIC_11_PER_02e","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. Stare at waypoint for duration of observation"]
["2004-149T14:06:00","000T00:30:00","2004-05-28","ISS","Prime","Other","RETARGETS","Retargetable observation","RETARGETABLES FOR SATELLITES DISCOVERED ON APPROAC","RETARGETABLES FOR SATELLITES DISCOVERED DURING APPROACH(START 0 TO PHOEBE ENCOUNTER)"]
["2004-149T14:36:00","000T00:30:00","2004-05-28","ISS","Prime","Other","SATELLORA","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 009 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [JA-HY-HE-CP-PA (607, 610, 612, 614, 617)]"]
["2004-149T16:21:00","000T09:00:00","2004-05-28","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-150T00:00:00","013T04:02:00","2004-05-29","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey"]
["2004-150T02:00:00","013T02:02:00","2004-05-29","INMS","Non-SPASS","Saturn","OPSTEST",null,"MAPS Survey","Ride with prime instrument"]
["2004-150T02:36:00","000T00:30:00","2004-05-29","ISS","Prime","Titan","MOVIEWW","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-150T02:36:00","000T00:30:00","2004-05-29","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #28","Titan Light Curve, Observation #28, ride along with ISS"]
["2004-150T03:06:00","000T02:00:00","2004-05-29","UVIS","Prime","Titan","MOS11PEA","Linear mosaic","MOSAIC_11_PER_03A","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. 1) Align slit parallel with the Saturn Spin Axis. 2) Step 96 times about the Z-axis using 0.119 deg increments for 3600s from Titan  (decreasing RA angles) to -MOS Orb. Stare for 37.5s during each step increment. 3) Step 48 times about the Z-axis using .119 deg increments for 1800s toward Titan. Stare for 37.5s during each step increment. 4) Slew back to Titan and reset pointing. Stare for remaining observation time.  MOS Orb (+/-Range): 99.69mrad"]
["2004-150T05:06:00","000T00:30:00","2004-05-29","ISS","Prime","Titan","MOVIEWW","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-150T05:06:00","000T00:30:00","2004-05-29","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #29","Titan Light Curve, Observation #29, ride along with ISS"]
["2004-150T05:36:00","000T00:57:00","2004-05-29","UVIS","Prime","Titan","MOS11PEB","Linear mosaic","MOSAIC_11_PER_03b","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. Stare at waypoint for duration of observation"]
["2004-150T06:33:00","000T00:30:00","2004-05-29","ISS","Prime","Other","RETARGETS","Retargetable observation","RETARGETABLES FOR SATELLITES DISCOVERED ON APPROAC","RETARGETABLES FOR SATELLITES DISCOVERED DURING APPROACH(START 0 TO PHOEBE ENCOUNTER)"]
["2004-150T07:03:00","000T00:30:00","2004-05-29","ISS","Prime","Other","SATELLORA","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 010 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [AT-EN-TL-JA-PM (602, 610, 613, 615, 616)]"]
["2004-150T07:33:00","000T00:23:00","2004-05-29","UVIS","Non-SPASS","SpacecraftActivity","PIM","Periodic Instrument maintenance","UVIS PIM in S01","This is an engineering activity.  Start time should be around doy 150, but can be moved by several days (30) if needed. Any orientation is Ok.  Does not require  SSR allocation."]
["2004-150T08:48:00","000T09:00:00","2004-05-29","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-150T17:48:00","001T08:41:00","2004-05-29","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-150T19:03:00","000T00:30:00","2004-05-29","ISS","Prime","Saturn","2X1CH4NAC","Photometry","Saturn Methane imaging","Methane Band Photometry"]
["2004-150T19:33:00","000T00:30:00","2004-05-29","ISS","Prime","Saturn","2X1CH4NAC","Photometry","Saturn Methane imaging","Methane Band Photometry"]
["2004-150T20:03:00","000T00:30:00","2004-05-29","ISS","Prime","Saturn","2X1CH4NAC","Photometry","Saturn Methane imaging","Methane Band Photometry"]
["2004-150T20:33:00","000T00:30:00","2004-05-29","ISS","Prime","Saturn","2X1CH4NAC","Photometry","Saturn Methane imaging","Methane Band Photometry"]
["2004-150T21:03:00","000T00:30:00","2004-05-29","ISS","Prime","Saturn","2X1CH4NAC","Photometry","Saturn Methane imaging","Methane Band Photometry"]
["2004-150T21:33:00","000T00:30:00","2004-05-29","ISS","Prime","Saturn","2X1CH4NAC","Photometry","Saturn Methane imaging","Methane Band Photometry"]
["2004-150T22:03:00","000T00:30:00","2004-05-29","ISS","Prime","Saturn","2X1CH4NAC","Photometry","Saturn Methane imaging","Methane Band Photometry"]
["2004-150T22:33:00","000T00:30:00","2004-05-29","ISS","Prime","Saturn","2X1CH4NAC","Photometry","Saturn Methane imaging","Methane Band Photometry"]
["2004-150T23:03:00","000T00:30:00","2004-05-29","ISS","Prime","Saturn","2X1CH4NAC","Photometry","Saturn Methane imaging","Methane Band Photometry"]
["2004-150T23:33:00","000T00:30:00","2004-05-29","ISS","Prime","Saturn","2X1CH4NAC","Photometry","Saturn Methane imaging","Methane Band Photometry"]
["2004-151T00:03:00","000T00:30:00","2004-05-30","ISS","Prime","Saturn","2X1CH4NAC","Photometry","Saturn Methane imaging","Methane Band Photometry"]
["2004-151T00:33:00","000T00:30:00","2004-05-30","ISS","Prime","Saturn","2X1CH4NAC","Photometry","Saturn Methane imaging","Methane Band Photometry"]
["2004-151T01:03:00","000T00:30:00","2004-05-30","ISS","Prime","Saturn","2X1CH4NAC","Photometry","Saturn Methane imaging","Methane Band Photometry"]
["2004-151T01:33:00","000T00:30:00","2004-05-30","ISS","Prime","Saturn","2X1CH4NAC","Photometry","Saturn Methane imaging","Methane Band Photometry"]
["2004-151T02:03:00","000T00:30:00","2004-05-30","ISS","Prime","Saturn","2X1CH4NAC","Photometry","Saturn Methane imaging","Methane Band Photometry"]
["2004-151T02:33:00","000T00:30:00","2004-05-30","ISS","Prime","Saturn","2X1CH4NAC","Photometry","Saturn Methane imaging","Methane Band Photometry"]
["2004-151T03:03:00","000T00:30:00","2004-05-30","ISS","Prime","Saturn","2X1CH4NAC","Photometry","Saturn Methane imaging","Methane Band Photometry"]
["2004-151T03:33:00","000T00:30:00","2004-05-30","ISS","Prime","Saturn","2X1CH4NAC","Photometry","Saturn Methane imaging","Methane Band Photometry"]
["2004-151T04:03:00","000T00:30:00","2004-05-30","ISS","Prime","Saturn","2X1CH4NAC","Photometry","Saturn Methane imaging","Methane Band Photometry"]
["2004-151T04:33:00","000T00:30:00","2004-05-30","ISS","Prime","Saturn","2X1CH4NAC","Photometry","Saturn Methane imaging","Methane Band Photometry"]
["2004-151T05:03:00","000T00:29:48","2004-05-30","ISS","Prime","Saturn","2X1PLRNCC","Polarimetry","Saturn polarimetry","NAC Polarimetery & Color"]
["2004-151T05:32:48","000T00:29:48","2004-05-30","ISS","Prime","Saturn","2X1PLRNCC","Polarimetry","Saturn polarimetry","NAC Polarimetery & Color"]
["2004-151T06:02:36","000T00:29:48","2004-05-30","ISS","Prime","Saturn","2X1PLRNCC","Polarimetry","Saturn polarimetry","NAC Polarimetery & Color"]
["2004-151T06:32:24","000T00:29:48","2004-05-30","ISS","Prime","Saturn","2X1PLRNCC","Polarimetry","Saturn polarimetry","NAC Polarimetery & Color"]
["2004-151T07:02:12","000T00:29:48","2004-05-30","ISS","Prime","Saturn","2X1PLRNCC","Polarimetry","Saturn polarimetry","NAC Polarimetery & Color"]
["2004-151T07:32:00","000T00:29:48","2004-05-30","ISS","Prime","Saturn","2X1PLRNCC","Polarimetry","Saturn polarimetry","NAC Polarimetery & Color"]
["2004-151T08:01:48","000T00:29:48","2004-05-30","ISS","Prime","Saturn","2X1PLRNCC","Polarimetry","Saturn polarimetry","NAC Polarimetery & Color"]
["2004-151T08:31:36","000T00:29:48","2004-05-30","ISS","Prime","Saturn","2X1PLRNCC","Polarimetry","Saturn polarimetry","NAC Polarimetery & Color"]
["2004-151T09:01:24","000T00:29:48","2004-05-30","ISS","Prime","Saturn","2X1PLRNCC","Polarimetry","Saturn polarimetry","NAC Polarimetery & Color"]
["2004-151T09:31:12","000T00:29:48","2004-05-30","ISS","Prime","Saturn","2X1PLRNCC","Polarimetry","Saturn polarimetry","NAC Polarimetery & Color"]
["2004-151T10:01:00","000T00:29:48","2004-05-30","ISS","Prime","Saturn","2X1PLRNCC","Polarimetry","Saturn polarimetry","NAC Polarimetery & Color"]
["2004-151T10:30:48","000T00:29:48","2004-05-30","ISS","Prime","Saturn","2X1PLRNCC","Polarimetry","Saturn polarimetry","NAC Polarimetery & Color"]
["2004-151T11:00:36","000T00:29:48","2004-05-30","ISS","Prime","Saturn","2X1PLRNCC","Polarimetry","Saturn polarimetry","NAC Polarimetery & Color"]
["2004-151T11:30:24","000T00:29:48","2004-05-30","ISS","Prime","Saturn","2X1PLRNCC","Polarimetry","Saturn polarimetry","NAC Polarimetery & Color"]
["2004-151T12:00:12","000T00:29:48","2004-05-30","ISS","Prime","Saturn","2X1PLRNCC","Polarimetry","Saturn polarimetry","NAC Polarimetery & Color"]
["2004-151T12:30:00","000T00:29:48","2004-05-30","ISS","Prime","Saturn","2X1PLRNCC","Polarimetry","Saturn polarimetry","NAC Polarimetery & Color"]
["2004-151T12:59:48","000T00:29:48","2004-05-30","ISS","Prime","Saturn","2X1PLRNCC","Polarimetry","Saturn polarimetry","NAC Polarimetery & Color"]
["2004-151T13:29:36","000T00:29:48","2004-05-30","ISS","Prime","Saturn","2X1PLRNCC","Polarimetry","Saturn polarimetry","NAC Polarimetery & Color"]
["2004-151T13:59:24","000T00:29:48","2004-05-30","ISS","Prime","Saturn","2X1PLRNCC","Polarimetry","Saturn polarimetry","NAC Polarimetery & Color"]
["2004-151T14:29:12","000T00:29:48","2004-05-30","ISS","Prime","Saturn","2X1PLRNCC","Polarimetry","Saturn polarimetry","NAC Polarimetery & Color"]
["2004-151T16:14:00","000T09:00:00","2004-05-30","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-151T17:00:00","000T02:17:00","2004-05-30","CAPS","Non-SPASS","Saturn","BURST8K","8 kbps burst","Burst of 8kbps data","Burst of 8 kbps data (which gives uncollapsed ELS data). 32 B cycles duration. Data is in addition to 1000 bps from survey."]
["2004-152T02:29:00","000T11:27:00","2004-05-31","RPWS","Prime","Saturn","ANTCAL","Antenna calibration","RPWS Post-Probe Release Antenna Cal.","Repeat of portion of Jupiter RPWS antenna calibration.  Require two eleven hour periods during the approach phase.  Attitude, rotate about offset axis of spacecraft in such a way that the RPWS antenna directions sweep through Saturn once per turn."]
["2004-152T02:29:00","000T11:27:00","2004-05-31","MAG","Non-SPASS","Saturn","ANTCAL","Antenna calibration","Offset Calibration using RPWS rolls","Use RPWS rolls to perform an offset calibration of the MAG sensors"]
["2004-152T13:56:00","000T00:30:00","2004-05-31","ISS","Prime","Other","RETARGETS","Retargetable observation","RETARGETABLES FOR SATELLITES DISCOVERED ON APPROAC","RETARGETABLES FOR SATELLITES DISCOVERED DURING APPROACH(START 0 TO PHOEBE ENCOUNTER)"]
["2004-152T13:56:00","001T12:22:00","2004-05-31","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2004-152T13:56:00","001T12:22:00","2004-05-31","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-152T14:26:00","000T00:30:00","2004-05-31","ISS","Prime","Other","SATELLORA","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 011 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [PA-EN-AT-EP-DI (602, 604, 611, 615, 617)]"]
["2004-152T16:11:00","000T09:00:00","2004-05-31","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-152T16:56:00","000T06:00:00","2004-05-31","CIRS","SPASS Rider","InstrumentCalibration","DSCAL1","Deep space calibration",null,"Deep space obervations for calibration."]
["2004-153T02:26:00","000T10:37:00","2004-06-01","ISS","Prime","rings(general)","SATSRCHBP","Ansa movie","ANSA MOVIE FOR SATELLITE SEARCHES, PRE PHOEBE IN R","ANSA MOVIE FOR SEARCHING FOR SATELLITES IN RING GAPS ON APPROACH(PRE PHOEBE ENCOUNTER)"]
["2004-153T14:18:00","000T12:00:00","2004-06-01","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-154T02:18:00","002T16:24:00","2004-06-02","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2004-154T02:18:00","002T15:09:00","2004-06-02","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-154T02:18:00","000T01:00:00","2004-06-02","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-154T04:00:00","000T02:17:00","2004-06-02","CAPS","Non-SPASS","Saturn","BURST8K","8 kbps burst","Burst of 8kbps data","Burst of 8 kbps data (which gives uncollapsed ELS data). 32 B cycles duration. Data is in addition to 1000 bps from survey."]
["2004-154T04:33:00","000T00:30:00","2004-06-02","ISS","Prime","Titan","MOVIEZZ","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-154T04:33:00","000T00:30:00","2004-06-02","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #30","Titan Light Curve, Observation #30, ride along with ISS"]
["2004-154T05:03:00","000T02:00:00","2004-06-02","CIRS","Prime","Saturn","MIRCMPSTA","Sit and stare to derive composition","CIRS_000SA_MIRCMPSITA","Measure oxygen compounds (CO2) in stratosphere as a function of latitude to determine whether rings are the source. Search for new stratospheric hydrocarbons (C3H4, C4H2). Determine isotopic ratios (CH3D/CH4, 12C/13C).  FP3/4 to Saturn. Z parallel to Saturn pole direction."]
["2004-154T07:03:00","000T00:30:00","2004-06-02","ISS","Prime","Titan","MOVIEZZ","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-154T07:03:00","000T00:30:00","2004-06-02","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #31","Titan Light Curve, Observation #31, ride along with ISS"]
["2004-154T07:33:00","000T02:00:00","2004-06-02","CIRS","Prime","Saturn","MIRCMPSTB","Sit and stare to derive composition","CIRS_000SA_MIRCMPSITA","Measure oxygen compounds (CO2) in stratosphere as a function of latitude to determine whether rings are the source. Search for new stratospheric hydrocarbons (C3H4, C4H2). Determine isotopic ratios (CH3D/CH4, 12C/13C).  FP3/4 to Saturn. Z parallel to Saturn pole direction."]
["2004-154T09:33:00","000T00:30:00","2004-06-02","ISS","Prime","Titan","MOVIEZZ","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-154T09:33:00","000T00:30:00","2004-06-02","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #32","Titan Light Curve, Observation #32, ride along with ISS"]
["2004-154T10:03:00","000T02:00:00","2004-06-02","CIRS","Prime","Saturn","MIRCMPSTC","Sit and stare to derive composition","CIRS_000SA_MIRCMPSITC","Measure oxygen compounds (CO2) in stratosphere as a function of latitude to determine whether rings are the source. Search for new stratospheric hydrocarbons (C3H4, C4H2). Determine isotopic ratios (CH3D/CH4, 12C/13C).  FP3/4 to Saturn. Z parallel to Saturn pole direction."]
["2004-154T12:03:00","000T00:30:00","2004-06-02","ISS","Prime","Other","RETARGETS","Retargetable observation","RETARGETABLES FOR SATELLITES DISCOVERED ON APPROAC","RETARGETABLES FOR SATELLITES DISCOVERED DURING APPROACH(START 0 TO PHOEBE ENCOUNTER)"]
["2004-154T12:33:00","000T00:30:00","2004-06-02","ISS","Prime","Other","SATELLORA","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 012 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [PA-EP-DI-PM-JA (604, 610, 611, 616, 617)]"]
["2004-154T14:18:00","000T13:00:00","2004-06-02","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-154T15:00:00","000T02:17:00","2004-06-02","CAPS","Non-SPASS","Saturn","BURST8K","8 kbps burst","Burst of 8kbps data","Burst of 8 kbps data (which gives uncollapsed ELS data). 32 B cycles duration. Data is in addition to 1000 bps from survey."]
["2004-155T04:00:00","000T02:17:00","2004-06-03","CAPS","Non-SPASS","Saturn","BURST8K","8 kbps burst","Burst of 8kbps data","Burst of 8 kbps data (which gives uncollapsed ELS data). 32 B cycles duration. Data is in addition to 1000 bps from survey."]
["2004-155T04:33:00","000T01:56:00","2004-06-03","UVIS","Prime","Titan","MOS12PAA","Linear mosaic","MOSAIC_12_PAR_01A","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. 1) Align slit parallel with the Saturn Equator 2) Step 41 times about the Z-axis using 0.114 deg increments for 3600s from Titan  to -MOS Orb (decreasing DEC angles). Stare for 88s during each step increment. 3) Step 20 times about the Z-axis using .114 deg increments for 1800s towards Titan. Stare for 88s during each step increment.  4) Slew back to Titan and reset pointing. Stare for remaining observation time.  MOS Orb (Saturn +/-Range): 40.79mrad"]
["2004-155T06:29:00","000T00:30:00","2004-06-03","ISS","Prime","Titan","MOVIEAAA","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-155T06:29:00","000T00:30:00","2004-06-03","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #33","Titan Light Curve, Observation #33, ride along with ISS"]
["2004-155T06:59:00","000T02:00:00","2004-06-03","UVIS","Prime","Titan","MOS12PAB","Linear mosaic","MOSAIC_12_PAR_01b","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. 1) Align slit parallel with the Saturn Equator 2) Step 41 times about the Z-axis using 0.114 deg increments for 3600s from Titan  to -MOS Orb (decreasing DEC angles). Stare for 88s during each step increment. 3) Step 20 times about the Z-axis using .114 deg increments for 1800s toward Titan. Stare for 88s during each step increment. 3) Slew back to Titan and reset pointing. Stare for remaining observation time.  MOS Orb (Saturn +/- Range): 40.79mrad"]
["2004-155T08:59:00","000T00:30:00","2004-06-03","ISS","Prime","Titan","MOVIEAAA","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-155T08:59:00","000T00:30:00","2004-06-03","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #34","Titan Light Curve, Observation #34, ride along with ISS"]
["2004-155T09:29:00","000T02:00:00","2004-06-03","UVIS","Prime","Titan","MOS12PAC","Linear mosaic","MOSAIC_12_PAR_01C","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. 1) Align slit parallel with the Saturn Equator 2) Step 41 times about the Z-axis using 0.114 deg increments for 3600s from Titan  to -MOS Orb (decreasing DEC angles). Stare for 88s during each step increment. 3) Step 20 times about the Z-axis using .114 deg increments for 1800s toward Titan. Stare for 88s during each step increment. 4) Slew back to Titan and reset pointing. Stare for remaining observation time.  MOS Orb (Saturn+/-Range): 40.79mrad"]
["2004-155T11:29:00","000T00:30:00","2004-06-03","ISS","Prime","Titan","MOVIEAAA","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-155T11:29:00","000T00:30:00","2004-06-03","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #35","Titan Light Curve, Observation #35, ride along with ISS"]
["2004-155T11:59:00","000T01:46:00","2004-06-03","UVIS","Prime","Titan","MOS12PAD","Linear mosaic","MOSAIC_12_PAR_01d","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. 1) Align slit parallel with the Saturn Equator 2) Step 41 times about the Z-axis using 0.114 deg increments for 3600s from Titan  to -MOS Orb (decreasing DEC angles). Stare for 88s during each step increment. 3) Slew back to Titan and reset pointing. Stare for remaining observation time.  MOS Orb (Saturn+/-Range): 40.79mrad"]
["2004-155T13:45:00","000T00:30:00","2004-06-03","ISS","Prime","Other","RETARGETS","Retargetable observation","RETARGETABLES FOR SATELLITES DISCOVERED ON APPROAC","RETARGETABLES FOR SATELLITES DISCOVERED DURING APPROACH(START 0 TO PHOEBE ENCOUNTER)"]
["2004-155T14:15:00","000T00:30:00","2004-06-03","ISS","Prime","Other","SATELLORA","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 013 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [PA-EP-EN-AT-PM (602, 611, 615, 616, 617)]"]
["2004-155T16:00:00","000T09:00:00","2004-06-03","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-155T16:45:00","000T06:00:00","2004-06-03","CIRS","SPASS Rider","InstrumentCalibration","DSCAL1","Deep space calibration",null,"Deep space obervations for calibration."]
["2004-155T17:00:00","000T04:34:00","2004-06-03","CAPS","Non-SPASS","Saturn","BURST8K","8 kbps burst","Burst of 8kbps data","Burst of 8 kbps data (which gives uncollapsed ELS data). 64 B cycles duration. Data is in addition to 1000 bps from survey."]
["2004-156T02:00:00","000T04:34:00","2004-06-04","CAPS","Non-SPASS","Saturn","BURST8K","8 kbps burst","Burst of 8kbps data","Burst of 8 kbps data (which gives uncollapsed ELS data). 64 B cycles duration. Data is in addition to 1000 bps from survey."]
["2004-156T02:15:00","000T00:30:00","2004-06-04","ISS","Prime","Titan","MOVIEBBB","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-156T02:15:00","000T00:30:00","2004-06-04","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #36","Titan Light Curve, Observation #36, ride along with ISS"]
["2004-156T02:45:00","000T02:00:00","2004-06-04","CIRS","Prime","Saturn","MIRCMPSTA","Sit and stare to derive composition","CIRS_000SA_MIRCMPSITA","Measure oxygen compounds (CO2) in stratosphere as a function of latitude to determine whether rings are the source. Search for new stratospheric hydrocarbons (C3H4, C4H2). Determine isotopic ratios (CH3D/CH4, 12C/13C).  FP3/4 to Saturn. Z parallel to Saturn pole direction."]
["2004-156T04:45:00","000T00:30:00","2004-06-04","ISS","Prime","Titan","MOVIEBBB","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-156T04:45:00","000T00:30:00","2004-06-04","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #37","Titan Light Curve, Observation #37, ride along with ISS"]
["2004-156T05:15:00","000T01:00:00","2004-06-04","CIRS","Prime","Saturn","MIRCMPSTB","Sit and stare to derive composition","CIRS_000SA_MIRCMPSITB","Measure oxygen compounds (CO2) in stratosphere as a function of latitude to determine whether rings are the source. Search for new stratospheric hydrocarbons (C3H4, C4H2). Determine isotopic ratios (CH3D/CH4, 12C/13C).  FP3/4 to Saturn. Z parallel to Saturn pole direction."]
["2004-156T06:15:00","000T00:27:00","2004-06-04","ISS","Prime","Other","RETARGETS","Retargetable observation","RETARGETABLES FOR SATELLITES DISCOVERED ON APPROAC","RETARGETABLES FOR SATELLITES DISCOVERED DURING APPROACH(START 0 TO PHOEBE ENCOUNTER)"]
["2004-156T06:42:00","000T00:30:00","2004-06-04","ISS","Prime","Other","SATELLORA","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 014 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [DI-HE-JA-CP-TL (604, 610, 612, 613, 614)]"]
["2004-156T08:27:00","000T09:00:00","2004-06-04","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-156T09:00:00","000T04:34:00","2004-06-04","CAPS","Non-SPASS","Saturn","BURST8K","8 kbps burst","Burst of 8kbps data","Burst of 8 kbps data (which gives uncollapsed ELS data). 64 B cycles duration. Data is in addition to 1000 bps from survey."]
["2004-156T09:12:00","000T06:00:00","2004-06-04","CIRS","SPASS Rider","InstrumentCalibration","DSCAL1","Deep space calibration",null,"Deep space obervations for calibration."]
["2004-156T17:27:00","000T01:15:00","2004-06-04","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-156T18:00:00","000T02:17:00","2004-06-04","CAPS","Non-SPASS","Saturn","BURST8K","8 kbps burst","Burst of 8kbps data","Burst of 8 kbps data (which gives uncollapsed ELS data). 32 B cycles duration. Data is in addition to 1000 bps from survey."]
["2004-156T18:42:00","000T11:30:00","2004-06-04","RPWS","Prime","Saturn","ANTCAL","Antenna calibration","RPWS Post-Probe Release Antenna Cal.","Repeat of portion of Jupiter RPWS antenna calibration. Require two eleven hour periods during approach.  Attitude, rotate about x-axis of spacecraft in such a way that the RPWS antenna directions sweep through Saturn once per turn."]
["2004-156T18:42:00","000T11:30:00","2004-06-04","MAG","Non-SPASS","Saturn","ANTCAL","Antenna calibration","Offset Calibration using RPWS rolls","Use RPWS rolls to perform an offset calibration of the MAG sensors"]
["2004-157T06:12:00","000T00:30:00","2004-06-05","ISS","Prime","Titan","MOVIECCC","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-157T06:12:00","000T00:30:00","2004-06-05","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #38","Titan Light Curve, Observation #38, ride along with ISS"]
["2004-157T06:12:00","004T09:26:00","2004-06-05","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2004-157T06:12:00","002T11:05:00","2004-06-05","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-157T06:42:00","000T02:00:00","2004-06-05","CIRS","Prime","Saturn","FIRCMPSTA","Sit and stare to derive composition","CIRS_000SA_FIRCMPSIT001_PRIME","Measure oxygen compounds (H2O) in stratosphere. Search for new tropospheric species (HCP, H2S, H2Se, Halides). Measure  hydrogen dimers and PH3. Determine HD/H2. FP1 to Saturn."]
["2004-157T08:42:00","000T00:30:00","2004-06-05","ISS","Prime","Titan","MOVIECCC","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-157T08:42:00","000T00:30:00","2004-06-05","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #39","Titan Light Curve, Observation #39, ride along with ISS"]
["2004-157T09:12:00","000T02:00:00","2004-06-05","CIRS","Prime","Saturn","FIRCMPSTB","Sit and stare to derive composition","CIRS_000SA_FIRCMPSIT001_PRIME","Measure oxygen compounds (H2O) in stratosphere. Search for new tropospheric species (HCP, H2S, H2Se, Halides). Measure  hydrogen dimers and PH3. Determine HD/H2. FP1 to Saturn."]
["2004-157T11:12:00","000T00:30:00","2004-06-05","ISS","Prime","Titan","MOVIECCC","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-157T11:12:00","000T00:30:00","2004-06-05","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #40","Titan Light Curve, Observation #40, ride along with ISS"]
["2004-157T11:42:00","000T02:26:00","2004-06-05","CIRS","Prime","Saturn","FIRCMPSTC","Sit and stare to derive composition","CIRS_000SA_FIRCMPSIT001_PRIME","Measure oxygen compounds (H2O) in stratosphere. Search for new tropospheric species (HCP, H2S, H2Se, Halides). Measure  hydrogen dimers and PH3. Determine HD/H2. FP1 to Saturn."]
["2004-157T14:08:00","000T00:30:00","2004-06-05","ISS","Prime","Titan","MOVIECCD","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-157T14:08:00","000T00:30:00","2004-06-05","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #41","Titan Light Curve, Observation #41, ride along with ISS"]
["2004-157T15:53:00","000T09:00:00","2004-06-05","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-157T16:38:00","000T06:00:00","2004-06-05","CIRS","SPASS Rider","InstrumentCalibration","DSCAL2","Deep space calibration",null,"Deep space obervations for calibration."]
["2004-157T17:00:00","000T02:17:00","2004-06-05","CAPS","Non-SPASS","Saturn","BURST8K","8 kbps burst","Burst of 8kbps data","Burst of 8 kbps data (which gives uncollapsed ELS data). 32 B cycles duration. Data is in addition to 1000 bps from survey."]
["2004-158T02:00:00","000T02:17:00","2004-06-06","CAPS","Non-SPASS","Saturn","BURST8K","8 kbps burst","Burst of 8kbps data","Burst of 8 kbps data (which gives uncollapsed ELS data). 32 B cycles duration. Data is in addition to 1000 bps from survey."]
["2004-158T02:08:00","000T00:40:00","2004-06-06","ISS","Prime","Titan","MOVIECDD","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-158T02:08:00","000T00:40:00","2004-06-06","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #42","Titan Light Curve, Observation #42, ride along with ISS"]
["2004-158T02:48:00","000T02:00:00","2004-06-06","CIRS","Prime","Saturn","MIRCMPSTA","Sit and stare to derive composition","CIRS_000SA_MIRCMPSITA","Measure oxygen compounds (CO2) in stratosphere as a function of latitude to determine whether rings are the source. Search for new stratospheric hydrocarbons (C3H4, C4H2). Determine isotopic ratios (CH3D/CH4, 12C/13C).  FP3/4 to Saturn. Z parallel to Saturn pole direction."]
["2004-158T04:48:00","000T00:30:00","2004-06-06","ISS","Prime","Titan","MOVIEDDD","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-158T04:48:00","000T00:30:00","2004-06-06","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #43","Titan Light Curve, Observation #43, ride along with ISS"]
["2004-158T05:18:00","000T02:00:00","2004-06-06","CIRS","Prime","Saturn","MIRCMPSTB","Sit and stare to derive composition","CIRS_000SA_MIRCMPSITB","Measure oxygen compounds (CO2) in stratosphere as a function of latitude to determine whether rings are the source. Search for new stratospheric hydrocarbons (C3H4, C4H2). Determine isotopic ratios (CH3D/CH4, 12C/13C).  FP3/4 to Saturn. Z parallel to Saturn pole direction."]
["2004-158T07:18:00","000T00:30:00","2004-06-06","ISS","Prime","Titan","MOVIEDDD","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-158T07:18:00","000T00:30:00","2004-06-06","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #44","Titan Light Curve, Observation #44, ride along with ISS"]
["2004-158T07:48:00","000T02:00:00","2004-06-06","CIRS","Prime","Saturn","MIRCMPSTC","Sit and stare to derive composition","CIRS_000SA_MIRCMPSITC","Measure oxygen compounds (CO2) in stratosphere as a function of latitude to determine whether rings are the source. Search for new stratospheric hydrocarbons (C3H4, C4H2). Determine isotopic ratios (CH3D/CH4, 12C/13C).  FP3/4 to Saturn. Z parallel to Saturn pole direction."]
["2004-158T09:48:00","000T00:30:00","2004-06-06","ISS","Prime","Titan","MOVIEDDD","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-158T09:48:00","000T00:30:00","2004-06-06","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #45","Titan Light Curve, Observation #45, ride along with ISS"]
["2004-158T10:18:00","000T02:47:00","2004-06-06","CIRS","Prime","Saturn","MIRCMPSTD","Sit and stare to derive composition","CIRS_000SA_MIRCMPSITD","Measure oxygen compounds (CO2) in stratosphere as a function of latitude to determine whether rings are the source. Search for new stratospheric hydrocarbons (C3H4, C4H2). Determine isotopic ratios (CH3D/CH4, 12C/13C).  FP3/4 to Saturn. Z parallel to Saturn pole direction."]
["2004-158T11:50:00","000T08:00:00","2004-06-06","RSS","SPASS Rider","Earth","PIM","Periodic Instrument maintenance","RSS PIM (Ka-TWTA Maintenance)","RSS PIM. Pointing=Not Applicable.  DSN Tracking=None."]
["2004-158T13:05:00","000T00:30:00","2004-06-06","ISS","Prime","Titan","MOVIEDDE","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-158T13:05:00","000T00:30:00","2004-06-06","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #46","Titan Light Curve, Observation #46, ride along with ISS Changed start time to match TOL 4/8/03, DPC"]
["2004-158T13:35:00","000T00:30:00","2004-06-06","ISS","Prime","Other","RETARGETS","Retargetable observation","RETARGETABLES FOR SATELLITES DISCOVERED ON APPROAC","RETARGETABLES FOR SATELLITES DISCOVERED DURING APPROACH(START 0 TO PHOEBE ENCOUNTER)"]
["2004-158T14:05:00","000T00:30:00","2004-06-06","ISS","Prime","Other","SATELLORA","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 015 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [EP-PM-AT-JA-PA (610, 611, 615, 616, 617)]"]
["2004-158T15:50:00","000T09:00:00","2004-06-06","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-158T16:35:00","000T03:00:00","2004-06-06","CIRS","SPASS Rider","InstrumentCalibration","DSCAL1","Deep space calibration",null,"Deep space obervations for calibration."]
["2004-158T17:00:00","000T02:17:00","2004-06-06","CAPS","Non-SPASS","Saturn","BURST8K","8 kbps burst","Burst of 8kbps data","Burst of 8 kbps data (which gives uncollapsed ELS data). 32 B cycles duration. Data is in addition to 1000 bps from survey."]
["2004-159T02:00:00","000T02:17:00","2004-06-07","CAPS","Non-SPASS","Saturn","BURST8K","8 kbps burst","Burst of 8kbps data","Burst of 8 kbps data (which gives uncollapsed ELS data). 32 B cycles duration. Data is in addition to 1000 bps from survey."]
["2004-159T02:05:00","000T00:30:00","2004-06-07","ISS","Prime","Titan","MOVIEEEE","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-159T02:05:00","000T00:30:00","2004-06-07","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #47","Titan Light Curve, Observation #47, ride along with ISS"]
["2004-159T02:35:00","000T02:00:00","2004-06-07","UVIS","Prime","Titan","MOS12PAA","Linear mosaic","MOSAIC_12_PAR_05a","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. 1) Slew about the Z-axis from Titan to +MOS Orb. Align slit parallel with the Saturn Equator 2) Step 41 times about the Z-axis using 0.114 deg increments for 3600s to -MOS Orb.  Stare for 88s during each step increment. 3) Step 20 times about the Z-axis using .114 deg increments for 1800s to Titan. Stare for 88s during each step increment. 4)Reset pointing and stare for remaining observation time.  MOS Orb (Saturn +/- Range): 40.79mrad"]
["2004-159T04:35:00","000T00:30:00","2004-06-07","ISS","Prime","Titan","MOVIEEEE","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-159T04:35:00","000T00:30:00","2004-06-07","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #48","Titan Light Curve, Observation #48, ride along with ISS"]
["2004-159T05:05:00","000T00:57:00","2004-06-07","UVIS","Prime","Titan","MOS12PAB","Linear mosaic","MOSAIC_12_PAR_05b","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on.  Stare at waypoint for observation duration"]
["2004-159T06:02:00","000T00:30:00","2004-06-07","ISS","Prime","Other","RETARGETS","Retargetable observation","RETARGETABLES FOR SATELLITES DISCOVERED ON APPROAC","RETARGETABLES FOR SATELLITES DISCOVERED DURING APPROACH(START 0 TO PHOEBE ENCOUNTER)"]
["2004-159T06:32:00","000T00:30:00","2004-06-07","ISS","Prime","Other","SATELLORA","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 016 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [CP-EN-DI-HY-HE (602, 604, 607, 612, 614)]"]
["2004-159T08:17:00","000T09:00:00","2004-06-07","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-159T09:00:00","000T02:17:00","2004-06-07","CAPS","Non-SPASS","Saturn","BURST8K","8 kbps burst","Burst of 8kbps data","Burst of 8 kbps data (which gives uncollapsed ELS data). 32 B cycles duration. Data is in addition to 1000 bps from survey."]
["2004-159T09:02:00","000T03:00:00","2004-06-07","CIRS","SPASS Rider","InstrumentCalibration","DSCAL2","Deep space calibration",null,"Deep space obervations for calibration."]
["2004-159T17:17:00","001T22:21:00","2004-06-07","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-159T18:00:00","000T02:17:00","2004-06-07","CAPS","Non-SPASS","Saturn","BURST8K","8 kbps burst","Burst of 8kbps data","Burst of 8 kbps data (which gives uncollapsed ELS data). 32 B cycles duration. Data is in addition to 1000 bps from survey."]
["2004-159T18:32:00","000T00:30:00","2004-06-07","ISS","Prime","Titan","MOVIEEEB","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-159T18:32:00","000T00:30:00","2004-06-07","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #49","Titan Light Curve, Observation #49, ride along with ISS"]
["2004-159T19:02:00","000T02:00:00","2004-06-07","UVIS","Prime","Titan","MOS12PAA","Linear mosaic","MOSAIC_12_PAR_06A","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. 1) Slew about the Z-axis from Titan to +MOS Orb. Align slit parallel with the Saturn Equator 2) Step 41 times about the Z-axis using 0.114 deg increments for 3600s to -MOS Orb.  Stare for 88s during each step increment. 3) Step 20 times about the Z-axis using .114 deg increments for 1800s toward Titan. Stare for 88s during each step increment. 4) Slew back to Titan and reset pointing. Stare for remaining observation time.  MOS Orb (Saturn+/-Range): 40.79mrad"]
["2004-159T21:02:00","000T00:30:00","2004-06-07","ISS","Prime","Titan","MOVIEEEB","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-159T21:02:00","000T00:30:00","2004-06-07","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #50","Titan Light Curve, Observation #50, ride along with ISS"]
["2004-159T21:32:00","000T02:00:00","2004-06-07","UVIS","Prime","Titan","MOS12PAB","Linear mosaic","MOSAIC_12_PAR_06b","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. 1) Slew about the Z-axis from Titan to +MOS Orb. Align slit parallel with the Saturn Equator 2) Step 41 times about the Z-axis using 0.114 deg increments for 3600s to -MOS Orb.  Stare for 88s during each step increment. 3) Step 20 times about the Z-axis using .114 deg increments for 1800s toward Titan. Stare for 88s during each step increment. 3) Slew back to Titan and reset pointing. Stare for remaining observation time.  MOS Orb (Saturn +/- Range): 40.79mrad"]
["2004-159T23:32:00","000T00:30:00","2004-06-07","ISS","Prime","Titan","MOVIEEEB","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-159T23:32:00","000T00:30:00","2004-06-07","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #51","Titan Light Curve, Observation #51, ride along with ISS"]
["2004-160T00:02:00","000T02:56:00","2004-06-08","UVIS","Prime","Titan","MOS12PAC","Linear mosaic","MOSAIC_12_PAR_06C","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. 1) Slew about the Z-axis from Titan to +MOS Orb. Align slit parallel with the Saturn Equator 2) Step 41 times about the Z-axis using 0.114 deg increments for 3600s to -MOS Orb.  Stare for 88s during each step increment. 3) Step 21 times about the Z-axis for 1800s to Titan. 4) Reset pointing for waypoint. Stare for remaining observation time.  MOS Orb (Saturn +/- Range): 40.79mrad"]
["2004-160T02:58:00","000T00:30:00","2004-06-08","ISS","Prime","Titan","MOVIEFFF","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-160T02:58:00","000T00:30:00","2004-06-08","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #52","Titan Light Curve, Observation #52, ride along with ISS"]
["2004-160T03:28:00","000T02:00:00","2004-06-08","CIRS","Prime","Saturn","MIRCMPSTA","Sit and stare to derive composition","CIRS_000SA_MIRCMPSIT","Measure oxygen compounds (CO2) in stratosphere as a function of latitude to determine whether rings are the source. Search for new stratospheric hydrocarbons (C3H4, C4H2). Determine isotopic ratios (CH3D/CH4, 12C/13C).  FP3/4 to Saturn. Z parallel to Saturn pole direction."]
["2004-160T05:28:00","000T00:30:00","2004-06-08","ISS","Prime","Titan","MOVIEFFF","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-160T05:28:00","000T00:30:00","2004-06-08","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #53","Titan Light Curve, Observation #53, ride along with ISS"]
["2004-160T05:58:00","000T02:00:00","2004-06-08","CIRS","Prime","Saturn","MIRCMPSTB","Sit and stare to derive composition","CIRS_000SA_MIRCMPSIT","Measure oxygen compounds (CO2) in stratosphere as a function of latitude to determine whether rings are the source. Search for new stratospheric hydrocarbons (C3H4, C4H2). Determine isotopic ratios (CH3D/CH4, 12C/13C).  FP3/4 to Saturn. Z parallel to Saturn pole direction."]
["2004-160T07:58:00","000T00:30:00","2004-06-08","ISS","Prime","Titan","MOVIEFFF","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-160T07:58:00","000T00:30:00","2004-06-08","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #54","Titan Light Curve, Observation #54, ride along with ISS"]
["2004-160T08:28:00","000T02:00:00","2004-06-08","CIRS","Prime","Saturn","MIRCMPSTC","Sit and stare to derive composition","CIRS_000SA_MIRCMPSIT","Measure oxygen compounds (CO2) in stratosphere as a function of latitude to determine whether rings are the source. Search for new stratospheric hydrocarbons (C3H4, C4H2). Determine isotopic ratios (CH3D/CH4, 12C/13C).  FP3/4 to Saturn. Z parallel to Saturn pole direction."]
["2004-160T10:28:00","000T00:30:00","2004-06-08","ISS","Prime","Titan","MOVIEFFF","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-160T10:28:00","000T00:30:00","2004-06-08","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #55","Titan Light Curve, Observation #55, ride along with ISS"]
["2004-160T10:58:00","000T02:00:00","2004-06-08","CIRS","Prime","Saturn","MIRCMPSTD","Sit and stare to derive composition","CIRS_000SA_MIRCMPSIT","Measure oxygen compounds (CO2) in stratosphere as a function of latitude to determine whether rings are the source. Search for new stratospheric hydrocarbons (C3H4, C4H2). Determine isotopic ratios (CH3D/CH4, 12C/13C).  FP3/4 to Saturn. Z parallel to Saturn pole direction."]
["2004-160T12:58:00","000T00:30:00","2004-06-08","ISS","Prime","Titan","MOVIEFFF","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-160T12:58:00","000T00:30:00","2004-06-08","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #56","Titan Light Curve, Observation #56, ride along with ISS"]
["2004-160T13:28:00","000T01:00:00","2004-06-08","CIRS","Prime","Saturn","MIRCMPSTE","Sit and stare to derive composition","CIRS_000SA_MIRCMPSIT","Measure oxygen compounds (CO2) in stratosphere as a function of latitude to determine whether rings are the source. Search for new stratospheric hydrocarbons (C3H4, C4H2). Determine isotopic ratios (CH3D/CH4, 12C/13C).  FP3/4 to Saturn. Z parallel to Saturn pole direction."]
["2004-160T15:43:00","000T09:00:00","2004-06-08","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-160T16:28:00","000T06:00:00","2004-06-08","CIRS","SPASS Rider","InstrumentCalibration","DSCAL1","Deep space calibration",null,"Deep space obervations for calibration."]
["2004-160T17:00:00","000T04:34:00","2004-06-08","CAPS","Non-SPASS","Saturn","BURST8K","8 kbps burst","Burst of 8kbps data","Burst of 8 kbps data (which gives uncollapsed ELS data). 64 B cycles duration. Data is in addition to 1000 bps from survey."]
["2004-161T01:58:00","000T00:30:00","2004-06-09","ISS","Prime","Titan","MOVIEGGG","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-161T01:58:00","000T00:30:00","2004-06-09","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #57","Titan Light Curve, Observation #57, ride along with ISS"]
["2004-161T02:00:00","000T04:34:00","2004-06-09","CAPS","Non-SPASS","Saturn","BURST8K","8 kbps burst","Burst of 8kbps data","Burst of 8 kbps data (which gives uncollapsed ELS data). 64 B cycles duration. Data is in addition to 1000 bps from survey."]
["2004-161T02:28:00","000T02:00:00","2004-06-09","CIRS","Prime","Saturn","FIRCMPSTA","Sit and stare to derive composition","CIRS_000SA_FIRCMPSIT001_PRIME","Measure oxygen compounds (H2O) in stratosphere. Search for new tropospheric species (HCP, H2S, H2Se, Halides). Measure  hydrogen dimers and PH3. Determine HD/H2. FP1 to Saturn."]
["2004-161T04:28:00","000T00:30:00","2004-06-09","ISS","Prime","Titan","MOVIEGGG","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-161T04:28:00","000T00:30:00","2004-06-09","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #58","Titan Light Curve, Observation #58, ride along with ISS"]
["2004-161T04:58:00","000T02:00:00","2004-06-09","CIRS","Prime","Saturn","FIRCMPSTB","Sit and stare to derive composition","CIRS_000SA_FIRCMPSIT001_PRIME","Measure oxygen compounds (H2O) in stratosphere. Search for new tropospheric species (HCP, H2S, H2Se, Halides). Measure  hydrogen dimers and PH3. Determine HD/H2. FP1 to Saturn."]
["2004-161T06:58:00","000T00:30:00","2004-06-09","ISS","Prime","Titan","MOVIEGGG","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-161T06:58:00","000T00:30:00","2004-06-09","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #59","Titan Light Curve, Observation #59, ride along with ISS"]
["2004-161T07:28:00","000T02:00:00","2004-06-09","CIRS","Prime","Saturn","FIRCMPSTC","Sit and stare to derive composition","CIRS_000SA_FIRCMPSIT001_PRIME","Measure oxygen compounds (H2O) in stratosphere. Search for new tropospheric species (HCP, H2S, H2Se, Halides). Measure  hydrogen dimers and PH3. Determine HD/H2. FP1 to Saturn."]
["2004-161T09:28:00","000T00:30:00","2004-06-09","ISS","Prime","Titan","MOVIEGGG","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-161T09:28:00","000T00:30:00","2004-06-09","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #60 (DPC)","Titan Light Curve, Observation #60 (DPC), ride along with ISS"]
["2004-161T09:58:00","000T02:55:00","2004-06-09","CIRS","Prime","Saturn","FIRCMPSTD","Sit and stare to derive composition","CIRS_000SA_FIRCMPSIT001_PRIME","Measure oxygen compounds (H2O) in stratosphere. Search for new tropospheric species (HCP, H2S, H2Se, Halides). Measure  hydrogen dimers and PH3. Determine HD/H2. FP1 to Saturn."]
["2004-161T12:53:00","000T00:30:00","2004-06-09","ISS","Prime","Titan","MOVIEGGH","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-161T12:53:00","000T00:30:00","2004-06-09","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #61 (DPC)","Titan Light Curve, Observation #61 (DPC), ride along with ISS"]
["2004-161T13:23:00","000T00:30:00","2004-06-09","ISS","Prime","Other","RETARGETS","Retargetable observation","RETARGETABLES FOR SATELLITES DISCOVERED ON APPROAC","RETARGETABLES FOR SATELLITES DISCOVERED DURING APPROACH(START 0 TO PHOEBE ENCOUNTER)"]
["2004-161T13:53:00","000T00:30:00","2004-06-09","ISS","Prime","Other","SATELLORA","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 017 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [TL-EN-JA-PM-AT (602, 610, 613, 615, 616)]"]
["2004-161T15:38:00","001T12:24:00","2004-06-09","CDA","Non-SPASS","DustRAM direction","SURVEY","Magnetospheric survey","dust exploration","for prograde dust (Saturn cent.): -z2E, -x 21;-18.6   AM=52"]
["2004-161T15:38:00","001T12:24:00","2004-06-09","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps).  End was tied to Phoebe-2hrs = 163T17:33:37. Removed epoch for SOPU/SSUP."]
["2004-161T15:38:00","001T12:24:00","2004-06-09","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-161T15:38:00","000T09:00:00","2004-06-09","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-161T16:23:00","000T03:00:00","2004-06-09","CIRS","SPASS Rider","InstrumentCalibration","DSCAL2","Deep space calibration",null,"Deep space obervations for calibration."]
["2004-162T01:53:00","000T11:44:00","2004-06-10","ISS","Prime","Phoebe","FULROTIN",null,"Phoebe pre-encounter global mapping","Turn -Y to Phoebe; shift back-and-forth between CIRS FP3, FP1, and UVIS FUV about every hour (about 20 min dwell for each position) (total of 34 positions). Do clr and color filter during FP3, clr filter observations during FUV pointings. Turn back to WP."]
["2004-162T01:53:00","000T11:44:00","2004-06-10","CIRS","SPASS Rider","Phoebe","FULROTIN",null,null,"CIRS rider on ISS distant full rotation observation (AD typ 0.2 mrad).  CIRS: center detectors, coadd, FP1 and FP3 only, 38 RTI, shutter closed occasionally during periods where FP1 is on Phoebe, to calibrate FP3.  Lego table #790.  Timings (UT) are: --------------------- > The detailed timeline for pointing is (absolute SCET): > > 01:53 UTC: Request start, turn to CIRS FP3 > 02:00 UTC (approx.): CIRS FP3 (only 11m instead of 20m) > 02:11 UTC: CIRS FP1 - shutter closed > 02:31 UTC: UVIS FUV > 02:53 UTC: CIRS FP3 > 03:13 UTC: CIRS FP1 > 03:33 UTC: UVIS FUV > 03:55 UTC: CIRS FP3 (includes first ISS) > 04:15 UTC: CIRS FP1 > 04:35 UTC: UVIS FUV > 04:57 UTC: CIRS FP3 > 05:17 UTC: CIRS FP1 - shutter closed > 05:37 UTC: UVIS FUV > 05:59 UTC: CIRS FP3 > 06:19 UTC: CIRS FP1 > 06:39 UTC: UVIS FUV > 07:01 UTC: CIRS FP3 > 07:21 UTC: CIRS FP1 > 07:41 UTC: UVIS FUV > 08:03 UTC: CIRS FP3 > 08:23 UTC: CIRS FP1 - shutter closed > 08:43 UTC: UVIS FUV > 09:05 UTC: CIRS FP3 > 09:25 UTC: CIRS FP1 > 09:45 UTC: UVIS FUV > 10:07 UTC: CIRS FP3 > 10:27 UTC: CIRS FP1 > 10:47 UTC: UVIS FUV > 11:09 UTC: CIRS FP3 > 11:29 UTC: CIRS FP1 - shutter closed > 11:49 UTC: UVIS FUV > 12:11 UTC: CIRS FP3 > 12:31 UTC: CIRS FP1 > 13:51 UTC: UVIS FUV > 13:13 UTC: CIRS FP3 (only ~17m instead of 20m) > 13:30 UTC (approx.): turn to WP > 13:37 UTC: Request end > --------------------"]
["2004-162T01:53:00","000T11:44:00","2004-06-10","UVIS","SPASS Rider","Phoebe","FULROTIN",null,"ICYLON full Phoebe rotation","RIDER TO ISS REQUEST"]
["2004-162T01:53:00","000T11:44:00","2004-06-10","VIMS","SPASS Rider","Phoebe","FULROTIN",null,"Phoebe","Multiple VIMS cubes over one complete Phoebe rotation"]
["2004-162T13:37:00","000T00:30:00","2004-06-10","ISS","Prime","Titan","APPROACH","Aproach imaging","Titan Approach Imaging","Point to Titan, run through sequence of filters most likely to be of use, determine which are best."]
["2004-162T13:37:00","000T00:30:00","2004-06-10","CIRS","SPASS Rider","Titan","APPROACH","Aproach imaging",null,"Titan observation"]
["2004-162T13:37:00","000T00:30:00","2004-06-10","VIMS","SPASS Rider","Titan","LIGHTC","Titan light curve","Lightcurve (DPC)","Titan Light Curve, Observation #62 (DPC), ride along with ISS Added 4/8/03, DPC"]
["2004-162T15:22:00","000T11:00:00","2004-06-10","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-162T16:07:00","000T03:00:00","2004-06-10","CIRS","SPASS Rider","InstrumentCalibration","DSCAL1","Deep space calibration",null,"Deep space obervations for calibration."]
["2004-163T02:22:00","000T01:40:00","2004-06-11","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-163T04:02:00","000T15:01:37","2004-06-11","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey"]
["2004-163T04:02:00","000T15:16:37","2004-06-11","CDA","Non-SPASS","Phoebe","SURVEY","Magnetospheric survey","Phoebe dust survey","dust survey data rate = 100 bps power = 12 W"]
["2004-163T04:02:00","000T14:31:37","2004-06-11","INMS","Non-SPASS","Saturn","OPSTEST",null,"INMS Ops. Test","Ride with prime instrument"]
["2004-163T04:02:00","000T13:31:37","2004-06-11","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps).  End was tied to Phoebe-2hrs = 163T17:33:37. Removed epoch for SOPU/SSUP."]
["2004-163T04:02:00","000T14:21:03","2004-06-11","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SUR Campaign","Part of SUR MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2004-163T04:02:00","000T15:04:37","2004-06-11","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-163T04:40:00","000T00:43:00","2004-06-11","CIRS","Prime","Phoebe","FP13LTCRV","CIRS FP13 light curve","Group #2 CIRS PRIME requests","AD=0.68 mrad; phase=87; LT=6.5; (-22, 87); duration 00:43. CIRS: 38 RTI (4.75 sec, 15.5 cm-1 res.),center detectors."]
["2004-163T04:40:00","000T08:38:00","2004-06-11","UVIS","SPASS Rider","Phoebe","ICYMAP","Icy satellite surface map","ICYMAP:  Phoebe UV Map","UV albedo of Phoebe's surface"]
["2004-163T05:23:00","000T00:16:00","2004-06-11","ISS","Prime","Phoebe","LOWRES0","Low resolution imaging","Phoebe Approach Global Color Mapping","Do 1x1 mosaic (3 NAC clr, 6 NAC color, 3 NAC polarizer filters)"]
["2004-163T05:23:00","000T00:16:00","2004-06-11","CIRS","SPASS Rider","Phoebe","LOWRES0","Low resolution imaging","Rider on ISS low resolution longitude coverage.","ISS rider; duration 00:16. CIRS: center detectors, shutter closed.  Calibration only:  ca. 5 min. 38 RTI, 10 min 96 RTI."]
["2004-163T05:39:00","000T02:52:00","2004-06-11","CIRS","Prime","Phoebe","FP13LTCRV","CIRS FP13 light curve","FP13 Light Curve","AD=0.72 mrad; phase=87; LT=6.5; (-22, 126); duration 02:52. CIRS: 38 RTI (4.75 sec, 15.5 cm-1 res.),center detectors."]
["2004-163T08:31:00","000T00:16:00","2004-06-11","ISS","Prime","Phoebe","LOWRES1A","Low resolution imaging","Phoebe Approach Global Mapping","Do 1x1 mosaic (3 NAC clr filters)"]
["2004-163T08:31:00","000T00:16:00","2004-06-11","CIRS","SPASS Rider","Phoebe","LOWRES1A","Low resolution imaging","Rider on ISS low resolution longitude coverage.","ISS rider; duration 00:16. CIRS: center detectors, 96 RTI."]
["2004-163T08:47:00","000T00:31:00","2004-06-11","CIRS","Prime","Phoebe","FP13LTCRV","CIRS FP13 light curve","FP13 Light Curve","AD=0.93 mrad; phase=87; LT=6.5; (-22, 247); duration 00:31. CIRS: 38 RTI (4.75 sec, 15.5 cm-1 res.),center detectors."]
["2004-163T08:47:00","000T00:31:00","2004-06-11","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis hi-res and ir hi-res, 12x12, 640ms, 160 ms, 10 of each cube"]
["2004-163T09:18:00","000T00:16:00","2004-06-11","ISS","Prime","Phoebe","LOWRES1B","Low resolution imaging","Phoebe Approach Global Color Mapping","Do 1x1 mosaic (3 NAC clr, 12 NAC color, 6 NAC polarizer filters)"]
["2004-163T09:18:00","000T00:16:00","2004-06-11","CIRS","SPASS Rider","Phoebe","LOWRES1B","Low resolution imaging","Rider on ISS low resolution longitude coverage.","ISS rider; duration 00:16. CIRS: center detectors, 96 RTI."]
["2004-163T09:18:00","000T00:16:00","2004-06-11","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis hi-res and ir hi-res, 12x12, 320ms"]
["2004-163T09:34:00","000T00:31:00","2004-06-11","CIRS","Prime","Phoebe","FP13LTCRV","CIRS FP13 light curve","FP13 Light Curve","AD=1.01 mrad; phase=87; LT=6.5; (-22, 277); duration 00:31. CIRS: 38 RTI (4.75 sec, 15.5 cm-1 res.),center detectors."]
["2004-163T09:34:00","000T00:31:00","2004-06-11","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis hi-res and ir hi-res, 12x12, 640ms, 160 ms, 10 of each cube"]
["2004-163T10:05:00","000T00:16:00","2004-06-11","ISS","Prime","Phoebe","LOWRES1C","Low resolution imaging","Phoebe Approach Global Mapping","Do 1x1 mosaic (3 NAC clr filters)"]
["2004-163T10:05:00","000T00:16:00","2004-06-11","CIRS","SPASS Rider","Phoebe","LOWRES1C","Low resolution imaging","Rider on ISS low resolution longitude coverage.","ISS rider; duration 00:16. CIRS: center detectors, 96 RTI."]
["2004-163T10:05:00","000T00:16:00","2004-06-11","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis hi-res and ir hi-res, 12x12, 320ms"]
["2004-163T10:21:00","000T00:31:00","2004-06-11","CIRS","Prime","Phoebe","FP13LTCRV","CIRS FP13 light curve","FP13 Light Curve","AD=1.09 mrad; phase=87; LT=6.5; (-22, 308); duration 00:31. CIRS: 38 RTI (4.75 sec, 15.5 cm-1 res.),center detectors."]
["2004-163T10:21:00","000T00:31:00","2004-06-11","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis hi-res and ir hi-res, 24x12, 640ms, 160 ms, 6 cubes of each"]
["2004-163T10:52:00","000T00:16:00","2004-06-11","ISS","Prime","Phoebe","LOWRES1D","Low resolution imaging","Phoebe Approach Global Color Mapping","Do 1x1 mosaic (3 NAC clr, 12 NAC color, 6 NAC polarizer filters)"]
["2004-163T10:52:00","000T00:16:00","2004-06-11","CIRS","SPASS Rider","Phoebe","LOWRES1D","Low resolution imaging","Rider on ISS low resolution longitude coverage.","ISS rider; duration 00:16. CIRS: center detectors, 96 RTI."]
["2004-163T10:52:00","000T00:16:00","2004-06-11","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis hi-res and ir hi-res, 12x12, 320ms"]
["2004-163T11:03:37","000T03:00:00","2004-06-11","RADAR","SPASS Rider","Phoebe","WARMDAT","RADAR warmup","Warmup, with bits","Warmup the instrument in an opmode that allows RADAR operation as well as collects RADAR data."]
["2004-163T11:03:37","000T04:31:00","2004-06-11","RADAR","Non-SPASS","Phoebe","REUBITS","Data volume adjustment","REU bits request","REU bits"]
["2004-163T11:08:00","000T00:31:00","2004-06-11","CIRS","Prime","Phoebe","FP13LTCRV","CIRS FP13 light curve","FP13 Light Curve","AD=1.19 mrad; phase=87; LT=6.5; (-22, 338); duration 00:31. CIRS: 38 RTI (4.75 sec, 15.5 cm-1 res.),center detectors."]
["2004-163T11:08:00","000T00:31:00","2004-06-11","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis hi-res and ir hi-res, 24x12, 160ms and 640ms 6 cubes of each"]
["2004-163T11:39:00","000T00:16:00","2004-06-11","ISS","Prime","Phoebe","LOWRES1E","Low resolution imaging","Phoebe Approach Global Mapping","Do 1x1 mosaic (3 NAC clr filters)"]
["2004-163T11:39:00","000T00:16:00","2004-06-11","CIRS","SPASS Rider","Phoebe","LOWRES1E","Low resolution imaging","Rider on ISS low resolution longitude coverage.","ISS rider; duration 00:16. CIRS: center detectors, 96 RTI."]
["2004-163T11:39:00","000T00:16:00","2004-06-11","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis low-res and ir hi-res, 12x12, 320ms"]
["2004-163T11:55:00","000T00:31:00","2004-06-11","CIRS","Prime","Phoebe","FP13LTCRV","CIRS FP13 light curve","FP13 Light Curve","AD=1.32 mrad; phase=87; LT=6.5; (-22, 8); duration 00:31. CIRS: 38 RTI (4.75 sec, 15.5 cm-1 res.),center detectors."]
["2004-163T11:55:00","000T00:31:00","2004-06-11","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis hi-res and ir hi-res, 24x12, 160ms and 640ms 6 cubes of each"]
["2004-163T12:26:00","000T00:16:00","2004-06-11","ISS","Prime","Phoebe","LOWRES1F","Low resolution imaging","Phoebe Approach Global Color Mapping","Do 1x1 mosaic (3 NAC clr, 12 NAC color, 6 NAC polarizer filters)"]
["2004-163T12:26:00","000T00:16:00","2004-06-11","CIRS","SPASS Rider","Phoebe","LOWRES1F","Low resolution imaging","Rider on ISS low resolution longitude coverage.","ISS rider; duration 00:16. CIRS: center detectors, shutter closed.  Calibration only:  ca. 5 min. 38 RTI, 10 min 96 RTI."]
["2004-163T12:26:00","000T00:16:00","2004-06-11","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis low-res and ir hi-res, 12x12, 320ms"]
["2004-163T12:42:00","000T00:31:00","2004-06-11","CIRS","Prime","Phoebe","FP13LTCRV","CIRS FP13 light curve","FP13 Light Curve","AD=1.47 mrad; phase=87; LT=6.5; (-22, 39); duration 00:31. CIRS: 38 RTI (4.75 sec, 15.5 cm-1 res.),center detectors."]
["2004-163T12:42:00","000T00:31:00","2004-06-11","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis hi-res and ir hi-res, 24x12, 160ms and 640ms 6 cubes of each"]
["2004-163T13:13:00","000T00:05:00","2004-06-11","ISS","Prime","Phoebe","LOWRES1G","Low resolution imaging","Phoebe Approach Global Mapping","Do 1x1 mosaic (3 NAC clr filters)"]
["2004-163T13:13:00","000T00:05:00","2004-06-11","CIRS","SPASS Rider","Phoebe","LOWRES1G","Low resolution imaging","Rider on ISS low resolution longitude coverage.","ISS rider; duration 00:05. CIRS: center detectors, 96 RTI."]
["2004-163T13:13:00","000T00:05:00","2004-06-11","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis hi-res and ir hi-res, 12x12, 320ms"]
["2004-163T14:03:37","000T01:31:00","2004-06-11","RADAR","Prime","Phoebe","SCATTRAD","RADAR Scatterometry / Radiometry","Scatterometry/Radiometry of Phoebe.","Point -Z axis at target and execute raster scan(s) centered on target. Obtain simultaneous scatterometry and radiometry."]
["2004-163T15:34:37","000T00:36:00","2004-06-11","ISS","Prime","Phoebe","LOWRES1J","Low resolution imaging","Phoebe Approach Global Color Mapping","Turn -Y to Phoebe; Do 1x1 mosaic (3 NAC clr, 12 NAC color, 6 NAC polarizer filters)"]
["2004-163T15:34:37","000T00:36:00","2004-06-11","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis and ir hi res, 12 x12 320ms"]
["2004-163T15:54:37","000T00:47:00","2004-06-11","UVIS","SPASS Rider","Phoebe","ICYMAP","Icy satellite surface map","ICYMAP:  Phoebe UV Map","UV albedo of Phoebe's surface"]
["2004-163T16:10:37","000T00:31:00","2004-06-11","CIRS","Prime","Phoebe","FP3REGION","CIRS FP3 regional map","FP3 map","AD=2.96 mrad; phase=86; LT=6.6; (-22, 172); duration 00:31. CIRS: 38 RTI (4.75 sec, 15.5 cm-1 res.), blink."]
["2004-163T16:10:37","000T00:31:00","2004-06-11","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","36 x36 hi res vis and ir, one each of 640 and 160ms"]
["2004-163T16:41:37","000T00:16:00","2004-06-11","ISS","Prime","Phoebe","LOWRES1K","Low resolution imaging","Phoebe Approach Global Mapping","Do 1x1 mosaic (3 NAC clr) filters; do 9 dark frames (for HIRESC inbound color data)"]
["2004-163T16:41:37","000T00:16:00","2004-06-11","CIRS","SPASS Rider","Phoebe","LOWRES1K","Low resolution imaging","Rider on ISS low resolution 30 degree longitude co","ISS rider; duration 00:16. CIRS: blink, shutter closed.  Calibration only:  ca. 5 min. 38 RTI, 10 min 96 RTI."]
["2004-163T16:41:37","000T00:47:00","2004-06-11","UVIS","SPASS Rider","Phoebe","ICYMAP","Icy satellite surface map","ICYMAP:  Phoebe UV Map","UV albedo of Phoebe's surface"]
["2004-163T16:41:37","000T00:16:00","2004-06-11","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis and ir hi res, 12x12, 320 ms"]
["2004-163T16:57:37","000T00:31:00","2004-06-11","CIRS","Prime","Phoebe","FP3REGION","CIRS FP3 regional map","FP3 map","AD=3.85 mrad; phase=85; LT=6.6; (-22, 202); duration 00:31. CIRS: 38 RTI (4.75 sec, 15.5 cm-1 res.), blink."]
["2004-163T16:57:37","000T00:31:00","2004-06-11","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis and ir hi res, 36x36,640 ms, and 160ms 1 cube each"]
["2004-163T17:28:37","000T00:15:00","2004-06-11","ISS","Prime","Phoebe","LOWRES1L","Low resolution imaging","Phoebe Approach Global Color Mapping","Do 1x1 mosaic (3 NAC clr, 12 NAC color, 6 NAC polarizer filters)"]
["2004-163T17:28:37","000T00:15:00","2004-06-11","CIRS","SPASS Rider","Phoebe","LOWRES1L","Low resolution imaging","Rider on ISS low resolution 30 degree longitude co","ISS rider; duration 00:15. CIRS: blink, 38 RTI."]
["2004-163T17:28:37","000T00:35:00","2004-06-11","UVIS","SPASS Rider","Phoebe","ICYMAP","Icy satellite surface map","ICYMAP:  Phoebe UV Map","UV albedo of Phoebe's surface"]
["2004-163T17:28:37","000T00:16:00","2004-06-11","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis hi and ir hi res, 12x12, 320ms"]
["2004-163T17:33:37","000T04:00:00","2004-06-11","MAG","Non-SPASS","Phoebe","PHTAR","Phoebe targeted flyby","Phoebe targeted flyby","Monitor the interaction of Phoebe with the Saturnian magnetospheric plasma and determine whether it generates an internal magnetic field.  Starttime was tied to Phoebe LMB epoch - 2 hours (163T17:33:37). This has been removed for SOPU/SSUP."]
["2004-163T17:43:37","000T00:20:00","2004-06-11","CIRS","Prime","Phoebe","FP3REGION","CIRS FP3 regional map","FP3 map","AD=5.45 mrad; phase=85; LT=6.6; (-21, 231); duration 00:20. CIRS: 38 RTI (4.75 sec, 15.5 cm-1 res.), blink."]
["2004-163T17:43:37","000T00:20:00","2004-06-11","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis and ir hi-res, 48 x 48 320 ms"]
["2004-163T18:03:37","000T00:08:00","2004-06-11","ISS","Prime","Phoebe","MEDRESA","Medium resolution global mapping","Phoebe Approach Mapping and Color","Do 2x1 NAC mosaic (clear filters)"]
["2004-163T18:03:37","000T00:08:00","2004-06-11","CIRS","SPASS Rider","Phoebe","MEDRESA","Medium resolution global mapping","ISS rider","ISS rider; duration 00:08. CIRS: blink, 38 RTI."]
["2004-163T18:03:37","000T00:08:00","2004-06-11","UVIS","SPASS Rider","Phoebe","ICYMAP","Icy satellite surface map","ICYMAP:  Phoebe UV Map","UV albedo of Phoebe's surface"]
["2004-163T18:03:37","000T00:08:00","2004-06-11","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis and ir hi res, 12 x 12, 320ms"]
["2004-163T18:11:37","000T00:13:00","2004-06-11","CIRS","Prime","Phoebe","FP3EWMAPN",null,"FP3 EW map (north)","AD=7.29 mrad; phase=84; LT=6.6; (-21, 248); duration 00:13. CIRS: 38 RTI (4.75 sec, 15.5 cm-1 res.), blink."]
["2004-163T18:11:37","000T00:13:00","2004-06-11","UVIS","SPASS Rider","Phoebe","ICYMAP","Icy satellite surface map","ICYMAP:  Phoebe UV Map","UV albedo of Phoebe's surface"]
["2004-163T18:11:37","000T00:13:00","2004-06-11","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis and ir hi-res, 36x36, 320ms and 160ms, 1 of each"]
["2004-163T18:24:37","000T00:14:00","2004-06-11","ISS","Prime","Phoebe","MEDRESB","Medium resolution global mapping","Phoebe Approach Mapping","Do 3x2 NAC clear mosaic + 3-color WAC context"]
["2004-163T18:24:37","000T00:14:00","2004-06-11","CIRS","SPASS Rider","Phoebe","MEDRESB","Medium resolution global mapping","ISS rider","ISS rider; duration 00:14. CIRS: blink, 38 RTI."]
["2004-163T18:24:37","000T00:14:00","2004-06-11","UVIS","SPASS Rider","Phoebe","ICYMAP","Icy satellite surface map","ICYMAP:  Phoebe UV Map","UV albedo of Phoebe's surface"]
["2004-163T18:24:37","000T00:14:00","2004-06-11","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis and ir hi res, 12x12, 320ms"]
["2004-163T18:33:37","000T02:00:00","2004-06-11","MIMI","SPASS Rider","Phoebe","ENCOUNTER","MAPS Campaign","MAPS RS Campaign","Part of RS MAPS Campaign.  Icy moon encounter in solar wind. Pointing: -X to sun."]
["2004-163T18:33:37","000T03:00:00","2004-06-11","RADAR","SPASS Rider","Phoebe","WARMNODAT","RADAR warmup","Warmup, no bits.","Warmup the instrument in an opmode that allows RADAR operation.  But in a telemetry mode that does not allow collection of RADAR data."]
["2004-163T18:33:37","000T02:00:00","2004-06-11","INMS","Non-SPASS","Phoebe","ENCOUNTER","MAPS Campaign","MAPS Survey","MAPS magnetospheric survey."]
["2004-163T18:38:37","000T00:12:00","2004-06-11","CIRS","Prime","Phoebe","FP3NITMAP","CIRS FP3 nighttime map","FP3 nighttime map","AD=11.00 mrad; phase=82; LT=6.7; (-21, 264); duration 00:12. CIRS: 38 RTI (4.75 sec, 15.5 cm-1 res.), blink."]
["2004-163T18:38:37","000T00:12:00","2004-06-11","UVIS","SPASS Rider","Phoebe","ICYMAP","Icy satellite surface map","ICYMAP:  Phoebe UV Map","UV albedo of Phoebe's surface"]
["2004-163T18:38:37","000T00:12:00","2004-06-11","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis and ir hi-res, 36x36, 320ms and 80ms, 1 of each"]
["2004-163T18:50:37","000T00:21:00","2004-06-11","ISS","Prime","Phoebe","HIRESA","High resolution image","Phoebe High Resolution Mosaics and High-res color","Do high-res NAC mosaics (3x2 and 6-frame), 4 WAC filter 1x1 context for both; 3-color NAC at last footprint"]
["2004-163T18:50:37","000T00:21:00","2004-06-11","CIRS","SPASS Rider","Phoebe","HIRESA","High resolution image","ISS rider","ISS rider; duration 00:21. CIRS: blink, 38 RTI."]
["2004-163T18:50:37","000T00:21:00","2004-06-11","UVIS","SPASS Rider","Phoebe","ICYMAP","Icy satellite surface map","ICYMAP:  Phoebe UV Map","UV albedo of Phoebe's surface"]
["2004-163T18:50:37","000T00:21:00","2004-06-11","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis and ir hi res, 12x12, 320ms,"]
["2004-163T19:03:37","000T01:00:00","2004-06-11","CAPS","SPASS Rider","Phoebe","ENCOUNTER","MAPS Campaign","MAPS 000PH Campaign","Part of 000PH MAPS Campaign.  Observe interaction between Phoebe and the solar wind"]
["2004-163T19:06:37","000T00:54:00","2004-06-11","RPWS","Non-SPASS","Phoebe","PHCA","Phoebe closest approach","Phoebe closest approach observations","RPWS observations in the immediate vicinity of Phoebe, including the characterization of the plasma wave spectrum and search for evidence of pickup ions.  No pointing requirement."]
["2004-163T19:11:37","000T00:10:00","2004-06-11","CIRS","Prime","Phoebe","FP1NITMAP","CIRS FP1 dark side map","FP3 nighttime map","AD=25.92 mrad; phase=75; LT=7.0; (-19, 277); duration 00:10. CIRS: 38 RTI (4.75 sec, 15.5 cm-1 res.), blink, shutter closed."]
["2004-163T19:11:37","000T00:10:00","2004-06-11","UVIS","SPASS Rider","Phoebe","ICYMAP","Icy satellite surface map","ICYMAP:  Phoebe UV Map","UV albedo of Phoebe's surface"]
["2004-163T19:11:37","000T00:10:00","2004-06-11","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis and ir hi-res, 36x36, 320ms"]
["2004-163T19:18:37","000T00:30:00","2004-06-11","CDA","Non-SPASS","Phoebe","PHODUST","Phoebe dust observation","Dust envelope around Phoebe","Study dust envelope around Phoebe.  CDA boresight must be  orientated toward the Phobe dust RAM (see CDA TOST white paper for definition). Our pointing requirements are met by various orientations. It seems to be inpossible to share the observation with the ORS instruments. Estimated data volume: 7.5 Mbits, data rate: 4192 bps, power: 19.5 W (with articulation), 11 W (without articulation)"]
["2004-163T19:21:37","000T01:07:00","2004-06-11","ISS","Prime","Phoebe","HIRESC","High resolution image","Phoebe High Resolution Mosaics and Color","Do highest-res NAC mosaics (8 footprints inbound, 9 outbound) plus WAC context; outbound also 19 color + 6 polarizer highres NAC."]
["2004-163T19:21:37","000T01:07:00","2004-06-11","CIRS","SPASS Rider","Phoebe","HIRESC","High resolution image","ISS rider","INCLUDES CLOSEST APPROACH (from DIGIT this is at 19:33:37).    At start of observation: AD=43.8, phase=66, LT=8.0, (-15, 273);    at C/A: AD=109.0, phase=24, LT=11.0, (11, 220);    at end of observation: AD=11.0, phase=88, LT=18.0, (23, 167).     Duration 01:07.  CIRS: 38 RTI (15.5 cm-1, 4.75 sec), blink; shutter closed last 00:07."]
["2004-163T19:21:37","000T01:07:00","2004-06-11","UVIS","SPASS Rider","Phoebe","ICYMAP","Icy satellite surface map","ICYMAP:  Phoebe UV Map","UV albedo of Phoebe's surface"]
["2004-163T19:21:37","000T01:07:00","2004-06-11","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis and ir hi res, 12x12, 320ms"]
["2004-163T19:49:00","000T01:48:21","2004-06-11","CDA","Non-SPASS","Phoebe","SURVEY","Magnetospheric survey","Phoebe dust survey","dust survey data rate = 100 bps power = 12 W"]
["2004-163T20:00:37","001T02:31:23","2004-06-11","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-163T20:03:37","001T02:29:39","2004-06-11","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey"]
["2004-163T20:22:03","001T02:09:57","2004-06-11","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SUR Campaign","Part of SUR MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2004-163T20:28:37","000T00:15:00","2004-06-11","CIRS","Prime","Phoebe","FP3DAYMAP","CIRS FP3 daytime map","FP3 daytime map","AD=11.04 mrad; phase=88; LT=18.1; (23, 167); duration 00:15. CIRS: 38 RTI (4.75 sec, 15.5 cm-1 res.), blink."]
["2004-163T20:28:37","000T00:15:00","2004-06-11","UVIS","SPASS Rider","Phoebe","ICYMAP","Icy satellite surface map","ICYMAP:  Phoebe UV Map","UV albedo of Phoebe's surface"]
["2004-163T20:28:37","000T00:15:00","2004-06-11","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis and ir hi-res, 48x48, 320ms"]
["2004-163T20:33:37","005T03:33:23","2004-06-11","INMS","Non-SPASS","Saturn","OPSTEST",null,"MAPS Survey","Ride with prime instrument"]
["2004-163T20:43:37","000T00:10:00","2004-06-11","ISS","Prime","Phoebe","MEDRESD","Medium resolution global mapping","Phoebe Departure Mapping and regional color","Do 2x1 NAC mosaic, then 1x1 regional short wavelength color (12 NACs from UV1 to GRN)"]
["2004-163T20:43:37","000T00:10:00","2004-06-11","CIRS","SPASS Rider","Phoebe","MEDRESD","Medium resolution global mapping","ISS rider","ISS rider; duration 00:10. CIRS: blink, 38 RTI."]
["2004-163T20:43:37","000T00:10:00","2004-06-11","UVIS","SPASS Rider","Phoebe","ICYMAP","Icy satellite surface map","ICYMAP:  Phoebe UV Map","UV albedo of Phoebe's surface"]
["2004-163T20:43:37","000T00:10:00","2004-06-11","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis and ir hi res, 12x12, 320ms"]
["2004-163T20:53:37","000T00:39:00","2004-06-11","CIRS","Prime","Phoebe","FP3NITMAP","CIRS FP3 nighttime map","FP3 nighttime map","AD=7.59 mrad; phase=89; LT=18.0; (23, 181); duration 00:39. CIRS: 38 RTI (4.75 sec, 15.5 cm-1 res.), blink."]
["2004-163T20:53:37","000T00:39:00","2004-06-11","UVIS","SPASS Rider","Phoebe","ICYMAP","Icy satellite surface map","ICYMAP:  Phoebe UV Map","UV albedo of Phoebe's surface"]
["2004-163T20:53:37","000T00:39:00","2004-06-11","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis and ir hi-res, 36x36, 640, 160ms 2 of each"]
["2004-163T21:33:37","000T04:15:00","2004-06-11","RADAR","Prime","Phoebe","2SCATTRAD","RADAR Scatterometry / Radiometry","Scatterometry/Radiometry of Phoebe. #2","Point -Z axis at target and execute raster scan(s) centered on target. Obtain simultaneous scatterometry and radiometry."]
["2004-163T21:33:37","001T00:58:23","2004-06-11","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps).  Starttime was tied to Phoebe LMB + 4hrs (163T21:33:37). Has been removed for SOPU/SSUP."]
["2004-163T21:33:37","000T04:15:00","2004-06-11","RADAR","Non-SPASS","Phoebe","REUBITS","Data volume adjustment","REU bits request","REU bits"]
["2004-163T21:38:37","000T04:15:00","2004-06-11","CDA","Non-SPASS","Phoebe","PHODUST","Phoebe dust observation","study of Phoebe dust environment","Study dust in the vincinity of Phoebe. Ride along with RADAR. Secondary axis: -x =  (ra: 283.6, dec:  50.6) @ 21:35, -x = (ra: 284.9, dec: 51.7) @ 23:00  Power: 11 W.  Data rate: 200 bps."]
["2004-164T01:54:00","003T22:12:59","2004-06-12","CDA","Non-SPASS","DustRAM direction","RETRO","MAPS retrograde campaign","retrograd dust exploration","dust anti-RAM:  -z2E and a) -x 18 ; -5    AM=97 b) -x 120 ; -67  AM=261"]
["2004-164T02:33:00","000T00:16:00","2004-06-12","ISS","Prime","Phoebe","LOWRES2A","Low resolution imaging","Phoebe Departure Global Color Mapping","Turn -Y to Phoebe; do 1x1 mosaic (3 NAC clr, 12 NAC color, 6 NAC polarizer filters)"]
["2004-164T02:33:00","000T00:16:00","2004-06-12","CIRS","SPASS Rider","Phoebe","LOWRES2A","Low resolution imaging","Rider on ISS low resolution longitude coverage.","ISS rider; duration 00:16. CIRS: center detectors, 96 RTI."]
["2004-164T02:33:00","000T09:37:00","2004-06-12","UVIS","SPASS Rider","Phoebe","ICYMAP","Icy satellite surface map","ICYMAP:  Phoebe UV Map","UV albedo of Phoebe's surface"]
["2004-164T02:33:00","000T00:16:00","2004-06-12","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis and ir hi res, 12x12, 320ms"]
["2004-164T02:49:00","000T00:31:00","2004-06-12","CIRS","Prime","Phoebe","FP13LTCRV","CIRS FP13 light curve","FP13 Light Curve","AD=1.39 mrad; phase=92; LT=18.0; (22, 48); duration 00:31. CIRS: 38 RTI (4.75 sec, 15.5 cm-1 res.), center detectors."]
["2004-164T02:49:00","000T00:31:00","2004-06-12","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis low res and ir hi res, 12x12, 640ms and  160ms.  Do 12 of each time"]
["2004-164T03:20:00","000T00:16:00","2004-06-12","ISS","Prime","Phoebe","LOWRES2B","Low resolution imaging","Phoebe Departure Global Mapping","Do 1x1 mosaic (3 NAC clr filters)"]
["2004-164T03:20:00","000T00:16:00","2004-06-12","CIRS","SPASS Rider","Phoebe","LOWRES2B","Low resolution imaging","Rider on ISS low resolution longitude coverage.","ISS rider; duration 00:16. CIRS: cnter detectors, shutter closed.  Calibration only:  ca. 5 min. 38 RTI, 10 min 96 RTI."]
["2004-164T03:20:00","000T00:16:00","2004-06-12","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis and ir hi res, 12x12, 320ms"]
["2004-164T03:36:00","000T00:31:00","2004-06-12","CIRS","Prime","Phoebe","FP13LTCRV","CIRS FP13 light curve","FP13 Light Curve","AD=1.25 mrad; phase=92; LT=18.0; (22, 78); duration 00:31. CIRS: 38 RTI (4.75 sec, 15.5 cm-1 res.), center detectors."]
["2004-164T03:36:00","000T00:31:00","2004-06-12","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis low res and ir hi res, 12x12, 640ms and  160ms.  Do 12 of each time"]
["2004-164T04:07:00","000T00:16:00","2004-06-12","ISS","Prime","Phoebe","LOWRES2C","Low resolution imaging","Phoebe Departure Global Color Mapping","Do 1x1 mosaic (3 NAC clr, 12 NAC color, 6 NAC polarizer filters)"]
["2004-164T04:07:00","000T00:16:00","2004-06-12","CIRS","SPASS Rider","Phoebe","LOWRES2C","Low resolution imaging","Rider on ISS low resolution longitude coverage.","ISS rider; duration 00:16. CIRS: center detectors, 96 RTI."]
["2004-164T04:07:00","000T00:16:00","2004-06-12","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis and ir hi res, 12x12, 320ms"]
["2004-164T04:23:00","000T00:31:00","2004-06-12","CIRS","Prime","Phoebe","FP13LTCRV","CIRS FP13 light curve","FP13 Light Curve","AD=1.14 mrad; phase=92; LT=18.0; (22, 108); duration 00:31. CIRS: 38 RTI (4.75 sec, 15.5 cm-1 res.), center detectors."]
["2004-164T04:23:00","000T00:31:00","2004-06-12","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis low res and ir hi res, 12x12, 640ms and  160ms.  Do 12 of each time"]
["2004-164T04:54:00","000T00:16:00","2004-06-12","ISS","Prime","Phoebe","LOWRES2D","Low resolution imaging","Phoebe Departure Global Mapping","Do 1x1 mosaic (3 NAC clr filters)"]
["2004-164T04:54:00","000T00:16:00","2004-06-12","CIRS","SPASS Rider","Phoebe","LOWRES2D","Low resolution imaging","Rider on ISS low resolution longitude coverage.","ISS rider; duration 00:16. CIRS: center detectors, 96 RTI."]
["2004-164T04:54:00","000T00:16:00","2004-06-12","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis and ir hi res, 12x12, 320ms"]
["2004-164T05:10:00","000T00:31:00","2004-06-12","CIRS","Prime","Phoebe","FP13LTCRV","CIRS FP13 light curve","FP13 Light Curve","AD=1.05 mrad; phase=92; LT=18.0; (22, 139); duration 00:31. CIRS: 38 RTI (4.75 sec, 15.5 cm-1 res.), center detectors."]
["2004-164T05:10:00","000T00:31:00","2004-06-12","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis low res and ir hi res, 12x12, 640ms and  160ms.  Do 12 of each time"]
["2004-164T05:41:00","000T00:16:00","2004-06-12","ISS","Prime","Phoebe","LOWRES2E","Low resolution imaging","Phoebe Departure Global Color Mapping","Do 1x1 mosaic (3 NAC clr, 12 NAC color, 6 NAC polarizer filters)"]
["2004-164T05:41:00","000T00:16:00","2004-06-12","CIRS","SPASS Rider","Phoebe","LOWRES2E","Low resolution imaging","Rider on ISS low resolution longitude coverage.","ISS rider; duration 00:16. CIRS: center detectors, 96 RTI."]
["2004-164T05:41:00","000T00:16:00","2004-06-12","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis and ir hi res, 12x12, 320ms"]
["2004-164T05:57:00","000T00:31:00","2004-06-12","CIRS","Prime","Phoebe","FP13LTCRV","CIRS FP13 light curve","FP13 Light Curve","AD=0.97mrad; phase=92; LT=18.0; (22, 169); duration 00:31. CIRS: 38 RTI (4.75 sec, 15.5 cm-1 res.), center detectors."]
["2004-164T05:57:00","000T00:31:00","2004-06-12","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis low res and ir hi res, 12x12, 640ms and  160ms.  Do 12 of each time"]
["2004-164T06:28:00","000T00:16:00","2004-06-12","ISS","Prime","Phoebe","LOWRES2F","Low resolution imaging","Phoebe Departure Global Mapping","Do 1x1 mosaic (3 NAC clr filters)"]
["2004-164T06:28:00","000T00:16:00","2004-06-12","CIRS","SPASS Rider","Phoebe","LOWRES2F","Low resolution imaging","Rider on ISS low resolution longitude coverage.","ISS rider; duration 00:16. CIRS: center detectors, 96 RTI."]
["2004-164T06:28:00","000T00:16:00","2004-06-12","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis and ir hi res, 12x12, 320ms"]
["2004-164T06:44:00","000T00:31:00","2004-06-12","CIRS","Prime","Phoebe","FP13LTCRV","CIRS FP13 light curve","FP13 Light Curve","AD=0.90mrad; phase=92; LT=18.0; (22, 199); duration 00:31. CIRS: 38 RTI (4.75 sec, 15.5 cm-1 res.), center detectors."]
["2004-164T06:44:00","000T00:31:00","2004-06-12","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis low res and ir hi res, 12x12, 640ms and  160ms.  Do 12 of each time"]
["2004-164T07:15:00","000T00:16:00","2004-06-12","ISS","Prime","Phoebe","LOWRES2G","Low resolution imaging","Phoebe Departure Global Color Mapping","Do 1x1 mosaic (3 NAC clr, 12 NAC color, 6 NAC polarizer filters)"]
["2004-164T07:15:00","000T00:16:00","2004-06-12","CIRS","SPASS Rider","Phoebe","LOWRES2G","Low resolution imaging","Rider on ISS low resolution longitude coverage.","ISS rider; duration 00:16. CIRS: center detectors, 96 RTI."]
["2004-164T07:15:00","000T00:16:00","2004-06-12","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis and ir hi res, 12x12, 320ms"]
["2004-164T07:31:00","000T00:31:00","2004-06-12","CIRS","Prime","Phoebe","FP13LTCRV","CIRS FP13 light curve","FP13 Light Curve","AD=0.84mrad; phase=92; LT=18.0; (22, 230); duration 00:31. CIRS: 38 RTI (4.75 sec, 15.5 cm-1 res.), center detectors."]
["2004-164T07:31:00","000T00:31:00","2004-06-12","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis low res and ir hi res, 12x12, 640ms and  160ms.  Do 12 of each time"]
["2004-164T08:02:00","000T00:16:00","2004-06-12","ISS","Prime","Phoebe","LOWRES2H","Low resolution imaging","Phoebe Departure Global Mapping","Do 1x1 mosaic (3 NAC clr filters)"]
["2004-164T08:02:00","000T00:16:00","2004-06-12","CIRS","SPASS Rider","Phoebe","LOWRES2H","Low resolution imaging","Rider on ISS low resolution longitude coverage.","ISS rider; duration 00:16. CIRS: center detectors, 96 RTI."]
["2004-164T08:02:00","000T00:16:00","2004-06-12","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis and ir hi res, 12x12, 320ms"]
["2004-164T08:18:00","000T00:31:00","2004-06-12","CIRS","Prime","Phoebe","FP13LTCRV","CIRS FP13 light curve","FP13 Light Curve","AD=0.79mrad; phase=92; LT=18.0; (22, 260); duration 00:31. CIRS: 38 RTI (4.75 sec, 15.5 cm-1 res.), center detectors."]
["2004-164T08:18:00","000T00:31:00","2004-06-12","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis low res and ir hi res, 12x12, 640ms and  160ms.  Do 12 of each time"]
["2004-164T08:49:00","000T00:16:00","2004-06-12","ISS","Prime","Phoebe","LOWRES2I","Low resolution imaging","Phoebe Departure Global Color Mapping","Do 1x1 mosaic (3 NAC clr, 12 NAC color, 6 NAC polarizer filters)"]
["2004-164T08:49:00","000T00:16:00","2004-06-12","CIRS","SPASS Rider","Phoebe","LOWRES2I","Low resolution imaging","Rider on ISS low resolution longitude coverage.","ISS rider; duration 00:16. CIRS: center detectors, 96 RTI."]
["2004-164T08:49:00","000T00:16:00","2004-06-12","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis and ir hi res, 12x12, 320ms"]
["2004-164T09:05:00","000T00:31:00","2004-06-12","CIRS","Prime","Phoebe","FP13LTCRV","CIRS FP13 light curve","FP13 Light Curve","AD=0.74mrad; phase=92; LT=18.0; (22, 290); duration 00:31. CIRS: 38 RTI (4.75 sec, 15.5 cm-1 res.), center detectors."]
["2004-164T09:05:00","000T00:31:00","2004-06-12","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis low res and ir hi res, 12x12, 640ms and  160ms.  Do 12 of each time"]
["2004-164T09:36:00","000T00:16:00","2004-06-12","ISS","Prime","Phoebe","LOWRES2J","Low resolution imaging","Phoebe Departure Global Mapping","Do 1x1 mosaic (3 NAC clr filters)"]
["2004-164T09:36:00","000T00:16:00","2004-06-12","CIRS","SPASS Rider","Phoebe","LOWRES2J","Low resolution imaging","Rider on ISS low resolution longitude coverage.","ISS rider; duration 00:16. CIRS: center detectors, 96 RTI."]
["2004-164T09:36:00","000T00:16:00","2004-06-12","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis and ir hi res, 12x12, 320ms"]
["2004-164T09:52:00","000T00:31:00","2004-06-12","CIRS","Prime","Phoebe","FP13LTCRV","CIRS FP13 light curve","FP13 Light Curve","AD=0.70mrad; phase=93; LT=17.9; (22, 321); duration 00:31. CIRS: 38 RTI (4.75 sec, 15.5 cm-1 res.), center detectors."]
["2004-164T09:52:00","000T00:31:00","2004-06-12","VIMS","SPASS Rider","Phoebe","PHOEBE","Phoebe observation","Phoebe","vis low res and ir hi res, 12x12, 640ms and  160ms.  Do 12 of each time"]
["2004-164T10:23:00","000T00:16:00","2004-06-12","ISS","Prime","Phoebe","LOWRES2K","Low resolution imaging","Phoebe Departure Global Color Mapping","Do 1x1 mosaic (3 NAC clr, 12 NAC color, 6 NAC polarizer filters). Do 6 dark frames for LOWRES color observations."]
["2004-164T10:23:00","000T00:16:00","2004-06-12","CIRS","SPASS Rider","Phoebe","LOWRES2K","Low resolution imaging","Rider on ISS low resolution longitude coverage.","ISS rider; duration 00:16. CIRS: center detectors, 96 RTI."]
["2004-164T10:39:00","000T00:31:00","2004-06-12","CIRS","Prime","Phoebe","FP13LTCRV","CIRS FP13 light curve","FP13 Light Curve","AD=0.67mrad; phase=93; LT=17.9; (22, 351); duration 00:31. CIRS: 38 RTI (4.75 sec, 15.5 cm-1 res.), center detectors."]
["2004-164T11:10:00","000T00:16:00","2004-06-12","ISS","Prime","Phoebe","LOWRES2L","Low resolution imaging","Phoebe Departure Global Mapping","Do 1x1 mosaic (up to 3 NAC clr filters). Do up to 21 dark frames for LOWRES color observations."]
["2004-164T11:10:00","000T00:16:00","2004-06-12","CIRS","SPASS Rider","Phoebe","LOWRES2L","Low resolution imaging","Rider on ISS low resolution longitude coverage.","ISS rider; duration 00:16. CIRS: center detectors, shutter closed.  Calibration only:  ca. 5 min. 38 RTI, 10 min 96 RTI."]
["2004-164T11:26:00","000T00:44:00","2004-06-12","CIRS","Prime","Phoebe","FP13LTCRV","CIRS FP13 light curve","FP13 Light Curve","AD=0.63mrad; phase=93; LT=17.9; (22,  21); duration 00:44. CIRS: 38 RTI (4.75 sec, 15.5 cm-1 res.), center detectors."]
["2004-164T13:32:00","000T02:28:00","2004-06-12","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-164T16:30:00","000T02:30:00","2004-06-12","CIRS","SPASS Rider","InstrumentCalibration","DSCAL2","Deep space calibration",null,"Deep space obervations for calibration."]
["2004-164T22:32:00","006T23:20:00","2004-06-12","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey"]
["2004-164T22:32:00","003T01:35:00","2004-06-12","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2004-164T22:32:00","003T01:35:00","2004-06-12","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-164T22:33:00","004T01:34:00","2004-06-12","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SUR Campaign","Part of SUR MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2004-164T23:50:00","000T00:30:00","2004-06-12","ISS","Prime","Other","SATELLORA","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 087 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [EN-DI-HY-HE-EP (602, 604, 607, 611, 612)]"]
["2004-165T00:20:00","000T00:30:00","2004-06-13","ISS","Prime","Titan","MOVIEHHH","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-165T00:50:00","000T02:00:00","2004-06-13","UVIS","Prime","Titan","MOS12PEA","Linear mosaic","MOSAIC_12_PER_04a","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. 1) Align slit parallel with the Saturn Spin Axis. 2) Step 160 times about the Z-axis using 0.114 deg increments for 3600s from Titan to -MOS Orb (decreasing RA angles). Stare for 22.5s during each step increment. 3) Step 80 times about the Z-axis using .114 deg increments for 1800s toward Titan. Stare for 22.5s during each step increment. 4) Slew back to Titan and reset pointing. Stare for remaining observation time. MOS Orb (Saturn+/-Range): 159.17mrad."]
["2004-165T02:50:00","000T00:30:00","2004-06-13","ISS","Prime","Titan","MOVIEHHH","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-165T03:20:00","000T02:00:00","2004-06-13","UVIS","Prime","Titan","MOS12PEB","Linear mosaic","MOSAIC_12_PER_04b",".  Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. 1) Align slit parallel with the Saturn Spin Axis. 2) Step 160 times about the Z-axis using 0.114 deg increments for 3600s from Titan to -MOS Orb (decreasing RA angles). Stare for 22.5s during each step increment. 3) Step 80 times about the Z-axis using .114 deg increments for 1800s toward Titan. Stare for 22.5s during each step increment. 4) Slew back to Titan and reset pointing. Stare for remaining observation time. MOS Orb (Saturn +/- Range): 159.17mrad."]
["2004-165T05:20:00","000T00:30:00","2004-06-13","ISS","Prime","Titan","MOVIEHHH","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-165T05:50:00","000T00:40:00","2004-06-13","UVIS","Prime","Titan","MOS12PEC","Linear mosaic","MOSAIC_12_PER_04c","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. Stare at waypoint for duration of observation."]
["2004-165T07:52:00","000T09:00:00","2004-06-13","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-165T08:37:00","000T03:00:00","2004-06-13","CIRS","SPASS Rider","InstrumentCalibration","DSCAL1","Deep space calibration",null,"Deep space obervations for calibration."]
["2004-165T18:07:00","000T00:30:00","2004-06-13","ISS","Prime","Other","SATELLORA","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 090 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [PA-CP-DI-PM-JA (604, 610, 614, 616, 617)]"]
["2004-165T18:37:00","000T00:30:00","2004-06-13","ISS","Prime","Titan","MOVIEIII","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-165T19:07:00","000T02:00:00","2004-06-13","UVIS","Prime","Titan","MOS12PEA","Linear mosaic","MOSAIC_12_PER_05a","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. 1) Align slit parallel with the Saturn Spin Axis. 2) Step 160 times about the Z-axis using 0.114 deg increments for 3600s from Titan to -MOS Orb (decreasing RA angles). Stare for 22.5s during each step increment. 3) Step 80 times about the Z-axis using .114 deg increments for 1800s toward Titan. Stare for 22.5s during each step increment. 4) Slew back to Titan and reset pointing. Stare for remaining observation time. MOS Orb (Saturn+/-Range): 159.17mrad."]
["2004-165T21:07:00","000T00:30:00","2004-06-13","ISS","Prime","Titan","MOVIEIII","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-165T21:37:00","000T02:00:00","2004-06-13","UVIS","Prime","Titan","MOS12PEB","Linear mosaic","MOSAIC_12_PER_05b","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. 1) Align slit parallel with the Saturn Spin Axis. 2) Step 160 times about the Z-axis using 0.114 deg increments for 3600s from Titan to -MOS Orb (decreasing RA angles). Stare for 22.5s during each step increment. 3) Step 80 times about the Z-axis using .114 deg increments for 1800s toward Titan. Stare for 22.5s during each step increment. 4) Slew back to Titan and reset pointing. Stare for remaining observation time. MOS Orb (Saturn+/-Range): 159.17mrad."]
["2004-165T23:37:00","000T00:30:00","2004-06-13","ISS","Prime","Titan","MOVIEIII","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-166T00:07:00","000T02:00:00","2004-06-14","UVIS","Prime","Titan","MOS12PEC","Linear mosaic","MOSAIC_12_PER_05c",".Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. 1) Align slit parallel with the Saturn Spin Axis. 2) Step 160 times about the Z-axis using 0.114 deg increments for 3600s from Titan to -MOS Orb (decreasing RA angles). Stare for 22.5s during each step increment. 3) Step 80 times about the Z-axis using .114 deg increments for 1800s toward Titan. Stare for 22.5s during each step increment. 4) Slew back to Titan and reset pointing. Stare for remaining observation time. MOS Orb (Saturn+/-Range): 159.17mrad."]
["2004-166T02:07:00","000T00:30:00","2004-06-14","ISS","Prime","Titan","MOVIEIII","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-166T02:37:00","000T02:00:00","2004-06-14","UVIS","Prime","Titan","MOS12PED","Linear mosaic","MOSAIC_12_PER_05d","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. 1) Align slit parallel with the Saturn Spin Axis. 2) Step 160 times about the Z-axis using 0.114 deg increments for 3600s from Titan to -MOS Orb (decreasing RA angles). Stare for 22.5s during each step increment. 3) Step 80 times about the Z-axis using .114 deg increments for 1800s toward Titan. Stare for 22.5s during each step increment. 4) Slew back to Titan and reset pointing. Stare for remaining observation time. MOS Orb (Saturn+/-Range): 159.17mrad."]
["2004-166T04:37:00","000T00:30:00","2004-06-14","ISS","Prime","Titan","MOVIEIII","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-166T05:07:00","000T02:00:00","2004-06-14","UVIS","Prime","Titan","MOS12PEE","Linear mosaic","MOSAIC_12_PER_05e","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. 1) Align slit parallel with the Saturn Spin Axis. 2) Step 160 times about the Z-axis using 0.114 deg increments for 3600s from Titan to -MOS Orb (decreasing RA angles). Stare for 22.5s during each step increment. 3) Step 80 times about the Z-axis using .114 deg increments for 1800s toward Titan. Stare for 22.5s during each step increment. 4) Slew back to Titan and reset pointing. Stare for remaining observation time. MOS Orb (Saturn +/-Range): 159.17mrad."]
["2004-166T07:07:00","000T00:30:00","2004-06-14","ISS","Prime","Titan","MOVIEIII","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-166T07:37:00","000T02:00:00","2004-06-14","UVIS","Prime","Titan","MOS12PEF","Linear mosaic","MOSAIC_12_PER_05f","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. 1) Align slit parallel with the Saturn Spin Axis. 2) Step 160 times about the Z-axis using 0.114 deg increments for 3600s from Titan to -MOS Orb (decreasing RA angles). Stare for 22.5s during each step increment. 3) Step 80 times about the Z-axis using .114 deg increments for 1800s toward Titan. Stare for 22.5s during each step increment. 4) Slew back to Titan and reset pointing. Stare for remaining observation time. MOS Orb (Saturn+/-Range): 159.17mrad."]
["2004-166T09:37:00","000T04:15:00","2004-06-14","VIMS","Prime","rings(general)","RINGMOS","Ring mosaic","Ring Mosaic during rev 0","Cube Size (X,Z) = 64*64, Time per SC pointing (mins) = 30, Number of SC pointings = 2. Time of observation (hours) = 3.75. Volume (Mbits) = 61.9.   Mosaic of entire ring system near apoapse. Sunlit face. Mosaic size 1x2. Also 8 radial scans 64x12 across lit ring ansa in high-res mode. Exposures 80 msec and 320 msec."]
["2004-166T09:37:00","000T04:15:00","2004-06-14","CIRS","SPASS Rider","rings(general)","RINGMOS","Ring mosaic","Rider on VIMS ring mosaic","FP1 integrations on main rings during VIMS ring mosaics"]
["2004-166T15:07:00","000T09:00:00","2004-06-14","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-167T00:00:00","001T00:00:00","2004-06-15","RPWS","Non-SPASS","InstrumentCalibration","PIM","Periodic Instrument maintenance","RPWS PIM","Perform RPWS PIM, Bias the Langmuir Probe to remove any contamination Data rate set to near zero -- overlaps normal science data observations, so produces no additional data volume."]
["2004-167T01:22:00","000T00:30:00","2004-06-15","ISS","Prime","Other","SATELLORA","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 094 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [EP-AT-TL-EN-JA (602, 610, 611, 613, 615)]"]
["2004-167T01:52:00","000T00:30:00","2004-06-15","ISS","Prime","Titan","MOVIEJJJ","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-167T02:22:00","000T02:00:00","2004-06-15","UVIS","Prime","Titan","MOS12PEA","Linear mosaic","MOSAIC_12_PER_06a","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. 1) Align slit parallel with the Saturn Spin Axis. 2) Step 160 times about the Z-axis using 0.114 deg increments for 3600s from Titan to -MOS Orb (decreasing RA angles). Stare for 22.5s during each step increment. 3) Step 80 times about the Z-axis using .114 deg increments for 1800s toward Titan. Stare for 22.5s during each step increment. 4) Slew back to Titan and reset pointing. Stare for remaining observation time. MOS Orb (Saturn+/-Range): 159.17mrad."]
["2004-167T04:22:00","000T00:30:00","2004-06-15","ISS","Prime","Titan","MOVIEJJJ","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-167T04:52:00","000T02:00:00","2004-06-15","UVIS","Prime","Titan","MOS12PEB","Linear mosaic","MOSAIC_12_PER_06b","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. 1) Align slit parallel with the Saturn Spin Axis. 2) Step 160 times about the Z-axis using 0.114 deg increments for 3600s from Titan to -MOS Orb (decreasing RA angles). Stare for 22.5s during each step increment. 3) Step 80 times about the Z-axis using .114 deg increments for 1800s toward Titan. Stare for 22.5s during each step increment. 4) Slew back to Titan and reset pointing. Stare for remaining observation time. MOS Orb (Saturn+/-Range): 159.17mrad."]
["2004-167T06:52:00","000T00:30:00","2004-06-15","ISS","Prime","Titan","MOVIEJJJ","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-167T07:22:00","000T02:00:00","2004-06-15","UVIS","Prime","Titan","MOS12PEC","Linear mosaic","MOSAIC_12_PER_06c","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. 1) Align slit parallel with the Saturn Spin Axis. 2) Step 160 times about the Z-axis using 0.114 deg increments for 3600s from Titan to -MOS Orb (decreasing RA angles). Stare for 22.5s during each step increment. 3) Step 80 times about the Z-axis using .114 deg increments for 1800s toward Titan. Stare for 22.5s during each step increment. 4) Slew back to Titan and reset pointing. Stare for remaining observation time. MOS Orb (Saturn +/-Range): 159.17mrad."]
["2004-167T09:22:00","000T00:30:00","2004-06-15","ISS","Prime","Titan","MOVIEJJJ","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-167T09:52:00","000T02:00:00","2004-06-15","UVIS","Prime","Titan","MOS12PED","Linear mosaic","MOSAIC_12_PER_06d","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. 1) Align slit parallel with the Saturn Spin Axis. 2) Step 160 times about the Z-axis using 0.114 deg increments for 3600s from Titan to -MOS Orb (decreasing RA angles). Stare for 22.5s during each step increment. 3) Step 80 times about the Z-axis using .114 deg increments for 1800s toward Titan. Stare for 22.5s during each step increment. 4) Slew back to Titan and reset pointing. Stare for remaining observation time. MOS Orb (Saturn+/-Range): 159.17mrad."]
["2004-167T11:52:00","000T00:30:00","2004-06-15","ISS","Prime","Titan","MOVIEJJJ","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-167T12:22:00","000T01:30:00","2004-06-15","UVIS","Prime","Titan","MOS12PEE","Linear mosaic","MOSAIC_12_PER_06e","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. Stare at waypoint for duration of observation."]
["2004-167T15:07:00","000T09:00:00","2004-06-15","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-168T00:07:00","003T15:44:59","2004-06-16","CDA","Non-SPASS","DustRAM direction","RETRO","MAPS retrograde campaign","retrograd dust exploration","dust anti-RAM:  -z2E and a) -x 18 ; -5    AM=97 b) -x 120 ; -67  AM=261"]
["2004-168T00:07:00","002T23:45:00","2004-06-16","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2004-168T00:07:00","002T23:45:00","2004-06-16","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-168T01:22:00","000T00:30:00","2004-06-16","ISS","Prime","Other","SATELLORA","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 097 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [AT-EN-PM-PA-EP (602, 611, 615, 616, 617)]"]
["2004-168T01:52:00","000T00:30:00","2004-06-16","ISS","Prime","Titan","MOVIEKKK","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-168T02:00:00","000T02:17:00","2004-06-16","CAPS","Non-SPASS","Saturn","BURST8K","8 kbps burst","Burst of 8kbps data","Burst of 8 kbps data (which gives uncollapsed ELS data). 32 B cycles duration. Data is in addition to 1000 bps from survey."]
["2004-168T02:22:00","000T02:00:00","2004-06-16","UVIS","Prime","Titan","MOS12PEA","Linear mosaic","MOSAIC_12_PER_07a","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. 1) Align slit parallel with the Saturn Spin Axis. 2) Step 160 times about the Z-axis using 0.114 deg increments for 3600s from Titan to -MOS Orb (decreasing RA angles). Stare for 22.5s during each step increment. 3) Step 80 times about the Z-axis for 1800s toward Titan. Stare for 22.5s during each step increment. 4) Slew back to Titan and reset pointing. Stare for remaining observation time. MOS Orb (Saturn+/-Range): 159.17mrad."]
["2004-168T04:22:00","000T00:30:00","2004-06-16","ISS","Prime","Titan","MOVIEKKK","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-168T04:52:00","000T02:00:00","2004-06-16","UVIS","Prime","Titan","MOS12PEB","Linear mosaic","MOSAIC_12_PER_07b","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. 1) Align slit parallel with the Saturn Spin Axis. 2) Step 160 times about the Z-axis using 0.114 deg increments for 3600s from Titan to -MOS Orb (decreasing RA angles). Stare for 22.5s during each step increment. 3) Step 80 times about the Z-axis using .114 deg increments for 1800s toward Titan. Stare for 22.5s during each step increment. 4) Slew back to Titan and reset pointing. Stare for remaining observation time. MOS Orb (Saturn+/-Range): 159.17mrad."]
["2004-168T06:52:00","000T00:30:00","2004-06-16","ISS","Prime","Titan","MOVIEKKK","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-168T07:22:00","000T02:00:00","2004-06-16","UVIS","Prime","Titan","MOS12PEC","Linear mosaic","MOSAIC_12_PER_07c","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. 1) Align slit parallel with the Saturn Spin Axis. 2) Step 160 times about the Z-axis using 0.114 deg increments for 3600s from Titan to -MOS Orb (decreasing RA angles). Stare for 22.5s during each step increment. 3) Step 80 times about the Z-axis using .114 deg increments for 1800s toward Titan. Stare for 22.5s during each step increment. 4) Slew back to Titan and reset pointing. Stare for remaining observation time. MOS Orb (Saturn+/-Range): 159.17mrad."]
["2004-168T09:22:00","000T00:30:00","2004-06-16","ISS","Prime","Titan","MOVIEKKK","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds"]
["2004-168T09:52:00","000T01:30:00","2004-06-16","UVIS","Prime","Titan","MOS12PED","Linear mosaic","MOSAIC_12_PER_07d","Linear mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on. Stare at waypoint for duration of observation."]
["2004-168T11:22:00","000T02:30:00","2004-06-16","VIMS","Prime","rings(general)","RINGMOS","Ring mosaic","Ring Mosaic during rev 0","Cube Size (X,Z) = 64*64, Time per SC pointing (mins) = 30, Number of SC pointings = 2, Time of observation (hours) = 2.0, Volume (Mbits) = 45  Mosaic of entire ring system near apoapse. Sunlit face. Mosaic size 1x2. Also 3 radial scans 64x12 across lit ring ansa in high-res mode, exposures 80 msec and 320 msec."]
["2004-168T11:22:00","000T02:30:00","2004-06-16","CIRS","SPASS Rider","rings(general)","RINGMOS","Ring mosaic","Rider on VIMS ring mosaic","FP1 integrations on main rings during VIMS ring mosaics"]
["2004-168T15:07:00","000T09:00:00","2004-06-16","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-168T16:00:00","000T02:17:00","2004-06-16","CAPS","Non-SPASS","Saturn","BURST8K","8 kbps burst","Burst of 8kbps data","Burst of 8 kbps data (which gives uncollapsed ELS data). 32 B cycles duration. Data is in addition to 1000 bps from survey."]
["2004-169T00:07:00","000T15:00:00","2004-06-17","INMS","Non-SPASS","Saturn","OPSTEST",null,"MAPS Survey","Ride with prime instrument"]
["2004-169T00:07:00","002T15:45:00","2004-06-17","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SUR Campaign","Part of SUR MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2004-169T01:22:00","000T00:30:00","2004-06-17","ISS","Prime","Titan","APPROACH","Aproach imaging","Titan Approach Imaging","Point to Titan, run through sequence of filters most likely to be of use, determine which are best."]
["2004-169T01:22:00","000T00:30:00","2004-06-17","CIRS","SPASS Rider","Titan","APPROACH","Aproach imaging","Titan rider","Titan rider"]
["2004-169T01:52:00","000T03:00:00","2004-06-17","CIRS","Prime","Saturn","FIRCMPSIT","Sit and stare to derive composition","CIRS_000SA_FIRCMPSIT006_PRIME","Measure oxygen compounds (H2O) in stratosphere. Search for new tropospheric species (HCP, H2S, H2Se, Halides). Measure  hydrogen dimers and PH3. Determine HD/H2. FP1 to Saturn."]
["2004-169T06:07:00","000T09:00:00","2004-06-17","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-169T15:07:00","002T06:45:00","2004-06-17","INMS","Non-SPASS","Saturn","OPSTEST",null,"MAPS Survey","Ride with prime instrument"]
["2004-169T16:22:00","000T00:30:00","2004-06-17","ISS","Prime","Saturn","2X2PLRNC","Polarimetry","Saturn polarimetry","NAC Polarimetery & Color & methane imaging"]
["2004-169T16:52:00","000T00:30:00","2004-06-17","ISS","Prime","Saturn","2X2PLRNC","Polarimetry","Saturn polarimetry","NAC Polarimetery & Color & methane imaging"]
["2004-169T17:22:00","000T00:30:00","2004-06-17","ISS","Prime","Saturn","2X2PLRNC","Polarimetry","Saturn polarimetry","NAC Polarimetery & Color & methane imaging"]
["2004-169T17:52:00","000T00:30:00","2004-06-17","ISS","Prime","Saturn","2X2PLRNC","Polarimetry","Saturn polarimetry","NAC Polarimetery & Color & methane imaging"]
["2004-169T18:22:00","000T00:30:00","2004-06-17","ISS","Prime","Saturn","2X2PLRNC","Polarimetry","Saturn polarimetry","NAC Polarimetery & Color & methane imaging"]
["2004-169T18:52:00","000T00:30:00","2004-06-17","ISS","Prime","Saturn","2X2PLRNC","Polarimetry","Saturn polarimetry","NAC Polarimetery & Color & methane imaging"]
["2004-169T19:22:00","000T00:30:00","2004-06-17","ISS","Prime","Saturn","2X2PLRNC","Polarimetry","Saturn polarimetry","NAC Polarimetery & Color & methane imaging"]
["2004-169T19:52:00","000T00:30:00","2004-06-17","ISS","Prime","Saturn","2X2PLRNC","Polarimetry","Saturn polarimetry","NAC Polarimetery & Color & methane imaging"]
["2004-169T20:22:00","000T00:30:00","2004-06-17","ISS","Prime","Saturn","2X2PLRNC","Polarimetry","Saturn polarimetry","NAC Polarimetery & Color & methane imaging"]
["2004-169T20:52:00","000T00:30:00","2004-06-17","ISS","Prime","Saturn","2X2PLRNC","Polarimetry","Saturn polarimetry","NAC Polarimetery & Color & methane imaging"]
["2004-169T21:22:00","000T00:30:00","2004-06-17","ISS","Prime","Saturn","2X2PLRNC","Polarimetry","Saturn polarimetry","NAC Polarimetery & Color & methane imaging"]
["2004-169T21:52:00","000T00:30:00","2004-06-17","ISS","Prime","Saturn","2X2PLRNC","Polarimetry","Saturn polarimetry","NAC Polarimetery & Color & methane imaging"]
["2004-169T22:22:00","000T00:30:00","2004-06-17","ISS","Prime","Saturn","2X2PLRNC","Polarimetry","Saturn polarimetry","NAC Polarimetery & Color & methane imaging"]
["2004-169T22:52:00","000T00:30:00","2004-06-17","ISS","Prime","Saturn","2X2PLRNC","Polarimetry","Saturn polarimetry","NAC Polarimetery & Color & methane imaging"]
["2004-169T23:22:00","000T00:30:00","2004-06-17","ISS","Prime","Saturn","2X2PLRNC","Polarimetry","Saturn polarimetry","NAC Polarimetery & Color & methane imaging"]
["2004-169T23:52:00","000T00:30:00","2004-06-17","ISS","Prime","Saturn","2X2PLRNC","Polarimetry","Saturn polarimetry","NAC Polarimetery & Color & methane imaging"]
["2004-170T00:22:00","000T00:30:00","2004-06-18","ISS","Prime","Saturn","2X2PLRNC","Polarimetry","Saturn polarimetry","NAC Polarimetery & Color & methane imaging"]
["2004-170T00:52:00","000T00:30:00","2004-06-18","ISS","Prime","Saturn","2X2PLRNC","Polarimetry","Saturn polarimetry","NAC Polarimetery & Color & methane imaging"]
["2004-170T01:00:00","000T11:23:00","2004-06-18","CAPS","Non-SPASS","Saturn","BURST8K","8 kbps burst","Burst of 8kbps data","Burst of 8 kbps data (which gives uncollapsed ELS data). 160 B cycles duration. Data is in addition to 1000 bps from survey."]
["2004-170T01:22:00","000T00:30:00","2004-06-18","ISS","Prime","Saturn","2X2PLRNC","Polarimetry","Saturn polarimetry","NAC Polarimetery & Color & methane imaging"]
["2004-170T01:52:00","000T00:30:00","2004-06-18","ISS","Prime","Saturn","2X2PLRNC","Polarimetry","Saturn polarimetry","NAC Polarimetery & Color & methane imaging"]
["2004-170T02:22:00","000T01:15:00","2004-06-18","ISS","Prime","Saturn","2X2PLRNC","Polarimetry","Saturn polarimetry","NAC Polarimetery & Color & methane imaging"]
["2004-170T03:37:00","000T10:00:00","2004-06-18","CIRS","Prime","Saturn","MIRCMPSIT","Sit and stare to derive composition","CIRS_000SA_MIRCMPSIT","Composition study at 0.5cm-1. Make sure FP1, FP3, & FP4 are on Saturn. After other requests were cut we need more pre-SOI integration time on FP1. If all FP's do not fit on the portion of Saturn unobscured by rings, then divide the time between FP1 on Saturn (5 hours) and FP3/4 on Saturn (5 hours)."]
["2004-170T14:52:00","000T09:00:00","2004-06-18","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-170T15:45:00","000T06:00:00","2004-06-18","CIRS","SPASS Rider","InstrumentCalibration","DSCAL2","Deep space calibration",null,"Deep space obervations for calibration."]
["2004-170T23:52:00","000T16:00:00","2004-06-18","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2004-170T23:52:00","000T16:00:00","2004-06-18","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-171T01:07:00","000T00:30:00","2004-06-19","ISS","Prime","Rhea","PRESOIA","Pre-SOI imaging","Rhea pre-SOI observation (leading side)","Turn -Y to Rhea; do 1x1 mosaic 2 NAC clear plus multiple NAC color and polarizer filters; do dark frames; turn to WP."]
["2004-171T01:07:00","000T00:30:00","2004-06-19","CIRS","SPASS Rider","Rhea","PRESOIA","Pre-SOI imaging","Rhea rider","Rhea rider on ISS.  AD=0.21, phase=63, (-17, 121).   Duration 00:30.  CIRS:  38 RTI, center detectors.  No data 00:00 to 00:17 (data rate multiplier 0.42); data, shutter open 00:17 to 00:29; shutter closed 00:20 to 00:30."]
["2004-171T01:37:00","000T10:30:00","2004-06-19","CIRS","Prime","Saturn","FIRCMPSIT","Sit and stare to derive composition","CIRS_000SA_FIRCMPSIT001_PRIME","Measure oxygen compounds (H2O) in stratosphere. Search for new tropospheric species (HCP, H2S, H2Se, Halides). Measure  hydrogen dimers and PH3. Determine HD/H2. FP1 to Saturn."]
["2004-171T12:07:00","000T00:30:00","2004-06-19","ISS","Prime","Titan","APPROACH","Aproach imaging","Titan Approach Imaging","Point to Titan, run through sequence of filters most likely to be of use, determine which are best."]
["2004-171T12:07:00","000T00:30:00","2004-06-19","CIRS","SPASS Rider","Titan","APPROACH","Aproach imaging","Titan rider","Titan rider"]
["2004-171T12:37:00","000T02:00:00","2004-06-19","VIMS","Prime","rings(general)","RINGMOS","Ring mosaic","Ring Mosaic during rev 0","Cube Size (X,Z) = 64*64, Time per SC pointing (mins) = 30, Number of SC pointings = 2, Time of observation (hours) = 2.0, Volume (Mbits) = 45  Mosaic of entire ring system near apoapse. Sunlit face. Mosaic size 1x2. Also 3 radial scans 64x12 across lit ring ansa in high-res mode, exposures 80 msec and 320 msec."]
["2004-171T12:37:00","000T02:00:00","2004-06-19","CIRS","SPASS Rider","rings(general)","RINGMOS","Ring mosaic","Rider on VIMS ring mosaic","FP1 integrations on main rings during VIMS ring mosaics"]
["2004-171T14:37:00","000T01:15:00","2004-06-19","CIRS","SPASS Rider","InstrumentCalibration","DEEPSPACE","Deep space calibration","OPNAV rider for deep space","Any pointing O.K.  Deep space during OPNAV turns"]
["2004-171T15:52:00","000T06:00:00","2004-06-19","CIRS","SPASS Rider","InstrumentCalibration","DSCAL1","Deep space calibration",null,"Deep space obervations for calibration."]
["2004-171T15:52:00","000T05:59:59","2004-06-19","CDA","Non-SPASS","DustRAM direction","RETRO","MAPS retrograde campaign","retrograd dust exploration","dust anti-RAM:  -z2E and a) -x 18 ; -5    AM=97 b) -x 120 ; -67  AM=261"]
["2004-171T15:52:00","000T06:00:00","2004-06-19","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2004-171T15:52:00","000T06:00:00","2004-06-19","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SUR Campaign","Part of SUR MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2004-171T15:52:00","000T06:00:00","2004-06-19","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-171T15:52:00","000T06:00:00","2004-06-19","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-171T21:52:00","002T20:40:00","2004-06-19","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey"]
["2004-171T21:52:00","002T20:40:00","2004-06-19","CDA","Non-SPASS","DustRAM direction","SURVEY","Magnetospheric survey","dust survey","prograde dust, day 174: -z2E and  -x 26.9; -24.6      AM=42 (60deg from +x2NEP) geometry changes fast, -x pointing only valid at beginning in the first days."]
["2004-171T21:52:00","000T00:23:00","2004-06-19","INMS","Non-SPASS","Saturn","MRO","Instrument memory readout","Memory Dump","Ride with prime instrument"]
["2004-171T21:52:00","002T02:20:00","2004-06-19","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2004-171T21:52:00","002T20:40:00","2004-06-19","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SUR Campaign","Part of SUR MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2004-171T21:52:00","002T20:40:00","2004-06-19","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-171T22:15:00","002T01:37:00","2004-06-19","INMS","Non-SPASS","Saturn","OPSTEST",null,"MAPS Survey","Ride with prime instrument"]
["2004-171T23:07:00","000T00:30:00","2004-06-19","ISS","Prime","Dione","PRESOIB","Pre-SOI imaging","Dione pre-SOI observation","Turn -Y to Dione; do 1x1 NAC mosaic 1 clear + 12 color + 6 polarizer filters; turn to WP"]
["2004-171T23:07:00","000T00:30:00","2004-06-19","CIRS","SPASS Rider","Dione","PRESOIB","Pre-SOI imaging","Dione rider","Dione rider"]
["2004-171T23:07:00","000T00:30:00","2004-06-19","UVIS","SPASS Rider","Dione","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2004-171T23:37:00","000T05:30:00","2004-06-19","CIRS","Prime","Saturn","FIRCMPSIT","Sit and stare to derive composition","CIRS_000SA_FIRCMPSIT001_PRIME","Measure oxygen compounds (H2O) in stratosphere. Search for new tropospheric species (HCP, H2S, H2Se, Halides). Measure  hydrogen dimers and PH3. Determine HD/H2. FP1 to Saturn."]
["2004-172T05:07:00","000T02:00:00","2004-06-20","VIMS","Prime","rings(general)","RINGMOS","Ring mosaic","Ring Mosaic during rev 0","Cube Size (X,Z) = 64*64, Time per SC pointing (mins) = 30, Number of SC pointings = 2, Time of observation (hours) = 2.0, Volume (Mbits) = 45  Mosaic of entire ring system near apoapse. Sunlit face. Mosaic size 1x2. Also 3 radial scans 64x12 across lit ring ansa in high-res mode, exposures 80 msec and 320 msec."]
["2004-172T05:07:00","000T02:00:00","2004-06-20","CIRS","SPASS Rider","rings(general)","RINGMOS","Ring mosaic","Rider on VIMS ring mosaic","FP1 integrations on main rings during VIMS ring mosaics"]
["2004-172T07:07:00","000T01:15:00","2004-06-20","CIRS","SPASS Rider","InstrumentCalibration","DEEPSPACE","Deep space calibration","OPNAV rider for deep space","Any pointing O.K.  Deep space during OPNAV turns"]
["2004-172T08:22:00","000T06:00:00","2004-06-20","CIRS","SPASS Rider","InstrumentCalibration","DSCAL2","Deep space calibration",null,"Deep space obervations for calibration."]
["2004-172T08:22:00","000T06:00:00","2004-06-20","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-172T15:37:00","000T02:00:00","2004-06-20","VIMS","Prime","rings(general)","RINGMOS","Ring mosaic","Ring Mosaic during rev 0","Cube Size (X,Z) = 64*64, Time per SC pointing (mins) = 30, Number of SC pointings = 2, Time of observation (hours) = 2.0, Volume (Mbits) = 45  Mosaic of entire ring system near apoapse. Sunlit face. Mosaic size 1x2. Also 3 radial scans 64x12 across lit ring ansa in high-res mode, exposures 80 msec and 320 msec."]
["2004-172T15:37:00","000T02:00:00","2004-06-20","CIRS","SPASS Rider","rings(general)","RINGMOS","Ring mosaic","Rider on VIMS ring mosaic","FP1 integrations on main rings during VIMS ring mosaics"]
["2004-172T17:37:00","000T00:20:00","2004-06-20","ISS","Prime","Tethys","PRESOIC","Pre-SOI imaging","Tethys pre-SOI observation","Turn to Tethys; 2x NAC clear + 23 NAC color/polarization filters; turn to WP"]
["2004-172T17:37:00","000T00:20:00","2004-06-20","CIRS","SPASS Rider","Tethys","PRESOIA","Pre-SOI imaging","Tethys rider","Tethys rider"]
["2004-172T17:37:00","000T00:20:00","2004-06-20","UVIS","SPASS Rider","Tethys","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2004-172T17:57:00","000T16:30:00","2004-06-20","ISS","Prime","rings(general)","SATSRCHAP","Ansa movie","ANSA MOVIE FOR SATELLITE SEARCHES, POST PHOEBE IN","ANSA MOVIE,1 X 2,C RING AND A RING REGION, FOR SEARCHING FOR SATELLITES IN RING GAPS ON APPROACH(POST PHOEBE ENCOUNTER)"]
["2004-172T17:57:00","000T16:30:00","2004-06-20","CIRS","SPASS Rider","rings(general)","SATSRCHAP","Ansa movie","CIRS_000_SATSRCHAP rider","Ride with ISS during SATSRCH"]
["2004-173T10:27:00","000T00:40:00","2004-06-21","ISS","Prime","Other","DIONERHEA",null,"Dione (leading) and Rhea (trailing side) pre-SOI c","Turn -Y to Dione; do 1x1 mosaic 2 NAC clear plus 23 NAC color/ polarizer filters. Turn -Y to Rhea; do 1x1 mosaic 2 NAC clear plus 23 NAC color and polarizer filters. Turn to WP"]
["2004-173T10:27:00","000T00:20:00","2004-06-21","CIRS","SPASS Rider","Dione","PRESOIA","Pre-SOI imaging","Dione rider","Dione rider"]
["2004-173T10:27:00","000T00:40:00","2004-06-21","UVIS","SPASS Rider","Dione","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2004-173T10:47:00","000T00:20:00","2004-06-21","CIRS","SPASS Rider","Rhea","PRESOIB","Pre-SOI imaging","Rhea rider","rhea rider"]
["2004-173T11:07:00","000T01:30:00","2004-06-21","ISS","Prime","rings(general)","RINGPHOTM","Ring photometry","RING PHOTOMETRY ON APPROACH","RING PHOTOMETRY DURING LATE APPROACH BETWEEN PHOEBE AND SOI"]
["2004-173T11:07:00","000T01:30:00","2004-06-21","CIRS","SPASS Rider","rings(general)","RINGPHOTM","Ring photometry","Rider on ISS ring photometry","FP3 and FP4 integrations on main rings during ISS ring mosaics"]
["2004-173T11:07:00","000T01:30:00","2004-06-21","VIMS","SPASS Rider","rings(general)","RINGMOS","Ring mosaic","Ring Mosaic during rev 0","ISS Rider. Cube Size (X,Z) = 12*12, Time per SC pointing (mins) = 2.5, Number of SC pointings = 16,  Time of observation (hours) = 1.5, Volume (Mbits) = 10.   Mosaic of entire ring system near apoapse. Sunlit face. Mosaic size 4x4. Exposures 80 msec and 320 msec. Data vol is enough for an extra 16 cubes."]
["2004-173T12:37:00","000T01:00:00","2004-06-21","ISS","Prime","Other","ENHYTE",null,"Enceladus, Hyperion, and Tethys pre-SOI  color obs","Turn to satellite; do 2x NAC clear + 23 NAC color/polarization filters for each of the three satellites, then return to WP. Each satellite gets same amount of dwell time."]
["2004-173T12:37:00","000T00:20:00","2004-06-21","CIRS","SPASS Rider","Enceladus","PRESOI","Pre-SOI imaging","Enceladus rider","Enceladus rider"]
["2004-173T12:37:00","000T01:00:00","2004-06-21","UVIS","SPASS Rider","Enceladus","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2004-173T12:57:00","000T00:20:00","2004-06-21","CIRS","SPASS Rider","Hyperion","PRESOI","Pre-SOI imaging","Hyperion rider","Hyperion rider"]
["2004-173T13:17:00","000T00:20:00","2004-06-21","CIRS","SPASS Rider","Tethys","PRESOIB","Pre-SOI imaging","Tethys rider","Tethys rider"]
["2004-173T13:37:00","000T01:15:00","2004-06-21","CIRS","SPASS Rider","InstrumentCalibration","DEEPSPACE","Deep space calibration","OPNAV rider for deep space","Any pointing O.K.  Deep space during OPNAV turns"]
["2004-173T23:52:00","000T18:40:00","2004-06-21","INMS","Non-SPASS","Saturn","OPSTEST",null,"MAPS Survey","Ride with prime instrument"]
["2004-174T00:12:00","000T07:30:00","2004-06-22","CIRS","Prime","RingB","COMP","Sit and stare to derive composition","CIRS_000RB_COMP","B ring composition:  Stare at West ansa, 90 deg phase, lit face -Y to ring, +Z perpendicular to ring radius"]
["2004-174T00:12:00","000T07:30:00","2004-06-22","CIRS","SPASS Rider","RingB","COMP","Sit and stare to derive composition","CIRS_000RB_COMP_SI","Support imaging for long integration on A ring and C rings"]
["2004-174T00:12:00","000T07:30:00","2004-06-22","VIMS","SPASS Rider","rings(general)","RINGMOS","Ring mosaic","Ring Mosaic during rev 0","Cube Size (X,Z) = 64*64, Time per SC pointing (mins) = 30, Number of SC pointings = 1.   FP1 stares at B ring near apoapse. Sunlit face.  Also 10 radial cubes 64x12 across lit ring ansa in high-res mode. Volume (Mbits) = 34 . Exposures 80 msec and 320 msec."]
["2004-174T00:12:00","000T05:00:00","2004-06-22","MAG","Non-SPASS","InstrumentCalibration","SCAS","MAG SCAS instrument","MAG/SCAS_Cal","Boom alignment calibration using SCAS. If moved within scheduling window, KEEP OUTSIDE SCHEDULED MAPS CAMPAIGNS. Note: SCAS operations disturb RSS and RPWS. IF OpMode not ORS, unique sequence will be required. Includes 2 hours for IFC cal and range checks. Final calibration before SOI."]
["2004-174T05:12:00","000T13:20:00","2004-06-22","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2004-174T07:42:00","000T01:22:00","2004-06-22","ISS","Prime","Other","TIMIIA",null,"Titan, Mimas, and Iapetus pre-SOI (approach) color","Turn NAC to Titan; do 26 NAC images for filter testing; turn NAC to Mimas; do 1 clear + 13 color + 6 polarizer filters (all NAC 1x1); turn NAC to Iapetus, do 19 color + 6 polarizer + 2 clear filters (all NAC 1x1); turn to WP."]
["2004-174T07:42:00","000T00:30:00","2004-06-22","CIRS","SPASS Rider","Titan","APPROACH","Aproach imaging","Titan rider","Titan rider"]
["2004-174T07:42:00","000T00:13:00","2004-06-22","VIMS","SPASS Rider","InstrumentCalibration","FSW20MST","Flight software test","VIMS FSW 20ms Anonoly Test","Flight software test."]
["2004-174T07:55:00","000T00:13:00","2004-06-22","VIMS","SPASS Rider","InstrumentCalibration","FSW20MST","Flight software test","VIMS FSW 20ms Anonoly Test","Flight software test."]
["2004-174T08:08:00","000T00:13:00","2004-06-22","VIMS","SPASS Rider","InstrumentCalibration","FSW20MST","Flight software test","VIMS FSW 20ms Anonoly Test","Flight software test."]
["2004-174T08:12:00","000T00:30:00","2004-06-22","CIRS","SPASS Rider","Mimas","PRESOI","Pre-SOI imaging","Mimas rider","Mimas rider"]
["2004-174T08:21:00","000T00:13:00","2004-06-22","VIMS","SPASS Rider","InstrumentCalibration","FSW20MST","Flight software test","VIMS FSW 20ms Anonoly Test","Flight software test."]
["2004-174T08:34:00","000T00:13:00","2004-06-22","VIMS","SPASS Rider","InstrumentCalibration","FSW20MST","Flight software test","VIMS FSW 20ms Anonoly Test","Flight software test."]
["2004-174T08:42:00","000T00:22:00","2004-06-22","CIRS","SPASS Rider","Iapetus","PRESOI","Pre-SOI imaging","Iapetus rider","Iapetus rider"]
["2004-174T08:47:00","000T00:13:00","2004-06-22","VIMS","SPASS Rider","InstrumentCalibration","FSW20MST","Flight software test","VIMS FSW 20ms Anonoly Test","Flight software test."]
["2004-174T18:32:00","000T11:05:00","2004-06-22","CAPS","SPASS Rider","Saturn","PRESOIOBS","Pre-SOI imaging","Observations during SOI & SOI quiet period","Observe Saturn's magnetosphere during first pass through the system (i.e. pre-SOI quiet period) Rate changes during this period are all done inside an IEB; multiple requests are necessary to model data volume. Rate left unchanged from original request based on May 24, 2002 email from Bill Kurth. This assumes high activity days will be allowed."]
["2004-174T18:32:00","005T10:50:00","2004-06-22","CDA","Non-SPASS","DustRAM direction","SURVEY","Magnetospheric survey","dust survey","prograde dust, day 174: -z2E and  -x 26.9; -24.6      AM=42 (60deg from +x2NEP) geometry changes fast, -x pointing only valid at beginning in the first days."]
["2004-174T18:32:00","000T00:23:00","2004-06-22","INMS","Non-SPASS","Saturn","MRO","Instrument memory readout","Memory Dump","Ride with prime instrument"]
["2004-174T18:32:00","000T04:28:00","2004-06-22","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2004-174T18:32:00","000T05:28:00","2004-06-22","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SUR Campaign","Part of SUR MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2004-174T18:32:00","000T05:05:00","2004-06-22","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-174T18:55:00","000T05:05:00","2004-06-22","INMS","Non-SPASS","Saturn","OPSTEST",null,"MAPS Survey","Ride with prime instrument"]
["2004-174T23:00:00","008T04:02:00","2004-06-22","MAG","SPASS Rider","Other","SOINTFLD","MAG internal field measurements","MAG_Internal_Field_Measurements","This request will yield unique observations of Saturns internal magnetic field during SOI. It is timed to start just before the beginning of the SOI critical sequence. Note pointing constraints only apply with 4Rs."]
["2004-174T23:00:00","000T01:00:00","2004-06-22","MIMI","SPASS Rider","Other","CONFIGURE","Huygens probe support","Configure for SOI Quiet","Configure MIMI for SOI Quiet (data and power carried in another request)"]
["2004-174T23:37:00","000T00:23:00","2004-06-22","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-174T23:40:00","000T00:01:00","2004-06-22","UVIS","Non-SPASS","Saturn","SOISLEEP","Huygens probe support","UVIS TO SLEEP PRIOR TO SOI CRITICAL SEQUENCE","UVIS to go to sleep prior to SOI critical sequence"]
["2004-174T23:45:00","000T00:09:50","2004-06-22","ISS","Non-SPASS","Other","SOIQUIET","Huygens probe support","put ISS to sleep for SOI activity","placeholder activity put into CIMS to remenind ISS to go into sleep for SOI"]
["2004-174T23:52:00","000T00:02:00","2004-06-22","VIMS","Non-SPASS","SpacecraftActivity","SLEEP","Instrument to sleep mode","VIMS to SLEEP for SOI","VIMS to SLEEP for SOI"]
["2004-174T23:59:15","000T00:00:00","2004-06-22","CIRS","Non-SPASS","Other","SOISLEEP","Huygens probe support","sleep/mute placeholder for post-SOI","Go to sleep pre-SOI"]
["2004-175T00:00:00","005T05:22:00","2004-06-23","MIMI","SPASS Rider","co-rotation","SOIQUIET","Huygens probe support","Pre-SOI QUIET Campaign","Part of MAGDYN MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2004-175T00:00:00","008T03:15:00","2004-06-23","INMS","Non-SPASS","Saturn","SLEEP","Instrument to sleep mode","SLEEP between Instr test and SOI","SLEEP/MUTE for PCO14"]
["2004-175T00:00:00","006T19:00:00","2004-06-23","RPWS","Non-SPASS","Saturn","PRESOI","Pre-SOI imaging","RPWS SOI Critical Sequence Observations","RPWS Observations during the SOI  critical sequence, including the periapsis period.  By requirement, this request covers the full 8-day quiet period."]
["2004-175T05:37:00","001T02:23:00","2004-06-23","CAPS","SPASS Rider","Saturn","PRESOIOBS","Pre-SOI imaging","Observations during SOI & SOI quiet period","Observe Saturn's magnetosphere during first pass through the system (i.e. pre-SOI quiet period) Rate changes during this period are all done inside an IEB; multiple requests are necessary to model data volume. Rate left unchanged from original request based on May 24, 2002 email from Bill Kurth. This assumes high activity days will be allowed."]
["2004-176T08:00:00","001T15:37:00","2004-06-24","CAPS","SPASS Rider","Saturn","PRESOIOBS","Pre-SOI imaging","Observations during SOI & SOI quiet period","Observe Saturn's magnetosphere during first pass through the system (i.e. pre-SOI quiet period) Rate changes during this period are all done inside an IEB; multiple requests are necessary to model data volume. Rate left unchanged from original request based on May 24, 2002 email from Bill Kurth. This assumes high activity days will be allowed."]
["2004-177T23:37:00","001T18:23:00","2004-06-25","CAPS","SPASS Rider","Saturn","PRESOIOBS","Pre-SOI imaging","Observations during SOI & SOI quiet period","Observe Saturn's magnetosphere during first pass through the system (i.e. pre-SOI quiet period) Rate changes during this period are all done inside an IEB; multiple requests are necessary to model data volume. Rate left unchanged from original request based on May 24, 2002 email from Bill Kurth. This assumes high activity days will be allowed."]
["2004-179T18:00:00","000T11:22:00","2004-06-27","CAPS","SPASS Rider","Saturn","PRESOIOBS","Pre-SOI imaging","Observations during SOI & SOI quiet period","Observe Saturn's magnetosphere during first pass through the system (i.e. pre-SOI quiet period) Rate changes during this period are all done inside an IEB; multiple requests are necessary to model data volume. Rate left unchanged from original request based on May 24, 2002 email from Bill Kurth. This assumes high activity days will be allowed."]
["2004-180T05:22:00","001T13:38:00","2004-06-28","CAPS","SPASS Rider","Saturn","PRESOIOBS","Pre-SOI imaging","Observations during SOI & SOI quiet period","Observe Saturn's magnetosphere during first pass through the system (i.e. pre-SOI quiet period) Rate changes during this period are all done inside an IEB; multiple requests are necessary to model data volume. Rate left unchanged from original request based on May 24, 2002 email from Bill Kurth. This assumes high activity days will be allowed."]
["2004-180T05:22:00","001T13:38:00","2004-06-28","MIMI","SPASS Rider","co-rotation","SOIQUIET","Huygens probe support","Pre-SOI QUIET Campaign","Part of MAGDYN MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2004-180T05:22:00","001T04:38:00","2004-06-28","CDA","Non-SPASS","DustRAM direction","SURVEY","Magnetospheric survey","dust survey","prograde dust, day 174: -z2E and  -x 26.9; -24.6      AM=42 (60deg from +x2NEP) geometry changes fast, -x pointing only valid at beginning in the first days."]
["2004-181T10:00:00","003T00:00:00","2004-06-29","CDA","Non-SPASS","DustRAM direction","SOI","Saturn orbit insertion","SOI","prograde dust,HRD measurements around SOI"]
["2004-181T19:00:00","000T20:40:00","2004-06-29","MIMI","SPASS Rider","co-rotation","SOIQUIET","Huygens probe support","Pre-SOI QUIET Campaign","Part of MAGDYN MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2004-181T19:00:00","000T20:12:00","2004-06-29","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey"]
["2004-181T19:00:00","001T05:42:00","2004-06-29","RPWS","Non-SPASS","Saturn","SOINBOUND",null,"RPWS inbound to SOI","RPWS comprehensive observations during SOI-29 hours inbound to ARPC."]
["2004-182T15:12:00","000T09:05:00","2004-06-30","CAPS","SPASS Rider","Saturn","RNGSAT","Ring / Satellite","Rings and Satellites Campaign","Observe the plasma interaction with the E ring and icy satellites. NOTE: This change in data rate must be inside a long-running IEB, not in the background sequence (SOI critical sequence requirement.)"]
["2004-182T15:40:00","000T11:26:40","2004-06-30","MIMI","SPASS Rider","co-rotation","SOIQUIET","Huygens probe support","Pre-SOI QUIET Campaign","Part of MAGDYN MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2004-183T00:17:00","000T02:49:40","2004-07-01","CAPS","SPASS Rider","Saturn","SOIOBS",null,"Observations during SOI","Monitor instrument status SOI burn, with all high voltages down. NOTE: This mode change must be inside a long-running IEB, not in the background sequence (SOI critical sequence requirement.)"]
["2004-183T00:42:00","000T00:10:00","2004-07-01","RPWS","Non-SPASS","Saturn","SOIARPC","Ascending ring plane crossing","RPWS SOI ARPC","Acquire high resolution waveforms during SOI ARPC for use in dust impact counts (and crude mass determination)."]
["2004-183T00:52:00","000T00:20:00","2004-07-01","RPWS","Non-SPASS","Saturn","SOIINNER",null,"RPWS Inbound Inner SOI measurements","Comprehensive measurements above rings after SOI APRC and before the SOI burn."]
["2004-183T01:12:00","000T01:40:00","2004-07-01","RPWS","Non-SPASS","Saturn","SOIBURN","Saturn orbit insertion burn","RPWS observations during SOI burn","Provides continuing coverage over the rings during SOI ME burn. Concentrates on direction-finding of SED  which should be unaffected by the burn.  Includes comprehensive measurements of full spectrum, as well"]
["2004-183T02:52:00","000T00:14:40","2004-07-01","RPWS","Non-SPASS","Saturn","SOIINNER",null,"RPWS observation over rings","Continues comprehensive observations over rings after the SOI ME burn and before the end of the critical sequence."]
["2004-183T03:02:00","000T07:49:00","2004-07-01","MAG","SPASS Rider","Other","SOINTFLD","MAG internal field measurements","MAG_Internal_Field_Measurements","This request will yield unique observations of Saturns internal magnetic field during SOI. It is timed to start just before the beginning of the SOI critical sequence. Note pointing constraints only apply with 4Rs."]
["2004-183T03:06:40","000T00:49:50","2004-07-01","CAPS","SPASS Rider","rings(general)","RINGS","Ring observation","Observations of ring ionosphere","Observe the ring ionosphere from the end of SOI (over the B ring), through ring plane crossing, and out to post-SOI downlink (~3 RS)"]
["2004-183T03:06:40","000T01:01:35","2004-07-01","ISS","SPASS Rider","rings(general)","SOISPTURN",null,"RING OBS'S DURING SOI - G POINTING (RINGSCAN001)","IMAGING OF RINGS DURING SOI G POINTING."]
["2004-183T03:06:40","000T00:17:30","2004-07-01","VIMS","SPASS Rider","rings(general)","RINGSCANG","Ring radial scan","Ring radial scan during SOI","Stellar_occ mode, star_finding OFF, IR_only. tau_IR = 160 msec, time per cube = 11.4 min. Time of observation (after turn) = 13:25 min. Observe throughout turn & science period, to minimize loss of SOI  data. Data vol incl VIS data in case design is reworked later."]
["2004-183T03:06:40","000T00:47:35","2004-07-01","RPWS","Non-SPASS","Saturn","SACA","Saturn closest approach","RPWS POST SOI Saturn Periapsis","RPWS post-SOI periapsis observations to study lightning, ring, and the inner magnetosphere phenomena."]
["2004-183T03:06:41","000T01:44:19","2004-07-01","MIMI","SPASS Rider","DustRAM direction","POSTBURN",null,"MIMI Ring Interaction Science","Part of RS MAPS Campaign.   Spacecraft must be pointed such that the dust ram is not entering the INCA FOV. Required to satisfy FR76C3. This means INCA boresight (in S/C X, Y plane, 9.5 deg toward +X from -Y) >70 deg from dust ram."]
["2004-183T03:06:55","000T00:15:00","2004-07-01","CAPS","Non-SPASS","SpacecraftActivity","CONFIGCHG","Huygens probe support","Config after SOI critical sequence","Change instrument state placeholder for a change after the SOI critical sequence"]
["2004-183T03:07:10","000T00:16:50","2004-07-01","UVIS","SPASS Rider","rings(general)","RINGSCANG","Ring radial scan",null,"Highest spatial resolution UV spectral mapping of Saturn's rings. Spatial variation of UV albedo and water absorption edge indicative of scattering center size scale."]
["2004-183T03:07:25","000T00:03:20","2004-07-01","CIRS","Non-SPASS","Other","SOIWAKE","Huygens probe support","wake/unmute placeholder for post-SOI","Wake and un-mute post-SOI. Note power transients!"]
["2004-183T03:07:40","000T00:01:00","2004-07-01","ISS","Non-SPASS","Other","POSTSOI","Huygens Probe support","put ISS to sleep for SOI activity","ISS wake after SOI"]
["2004-183T03:07:50","000T02:17:10","2004-07-01","CIRS","SPASS Rider","rings(general)","SOIRINGS",null,"CIRS_000RI_SOIRINGS","Radial scan of main rings during SOI,  deep space time during turns included also."]
["2004-183T03:09:10","000T00:02:00","2004-07-01","VIMS","Non-SPASS","SpacecraftActivity","WAKEUP","Wakeup instrument from sleep mode","VIMS to Active Mode after SOI","VIMS to Active after SOI"]
["2004-183T03:15:00","000T00:03:00","2004-07-01","INMS","Non-SPASS","Saturn","CVRJET","Instrument cover jettison","INMS Cover Jettison","The protective cover for INMS shall be released upon Cassini SOI."]
["2004-183T03:18:00","000T00:03:00","2004-07-01","INMS","Non-SPASS","Saturn","CVRJET","Instrument cover jettison","INMS Cover Jettison","The protective cover for INMS shall be released upon Cassini SOI."]
["2004-183T03:21:00","000T00:33:30","2004-07-01","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","Ride with prime instrument"]
["2004-183T03:24:00","000T00:30:30","2004-07-01","UVIS","SPASS Rider","rings(general)","RINGSCANA","Ring radial scan",null,"Highest spatial resolution UV spectral mapping of Saturn's rings. Spatial variation of UV albedo and water absorption edge indicative of scattering center size scale."]
["2004-183T03:24:10","000T00:30:20","2004-07-01","VIMS","SPASS Rider","rings(general)","RINGSCANA","Ring radial scan","Ring radial scan of A ring during SOI","Cube Size (X,Z) = 64*1, Tau_IR = 160 ms, Tau_VIS = 10.2 s, Time per SC pointing (sec) = 10.7, Number of SC pointings = 170 Time of observation (min) = 30.3."]
["2004-183T03:54:15","000T00:06:31","2004-07-01","RPWS","Non-SPASS","rings(general)","RPXING","Measurements of dust flux, scale height and plasma waves at the magnetic equator during ring plane crossing","RPWS Ring Plane Crossing","Determine the equatorial dust flux and scale height as a function of radial distance.  Obtain high resolution of plasma waves at the magnetic equator."]
["2004-183T03:54:30","000T00:09:00","2004-07-01","INMS","SPASS Rider","Saturn","RINGCOMP","Ring composition","INMS Ring Compostion","This request looks 'down' the magnetic field lines (compensating for the velocity of the SC and the particles we're looking for)."]
["2004-183T03:54:30","000T00:13:45","2004-07-01","VIMS","SPASS Rider","rings(general)","WAKE",null,"A Ring wake observation during SOI","Stellar_occ mode, star_finding OFF, IR_only. tau_IR = 160 msec, time per cube = 11.4 min. Time of observation (between turns) = 3:40. Observe throughout turn & science periods, to minimize loss of SOI  data. Data vol incl VIS data in case design is reworked later."]
["2004-183T03:56:30","000T00:08:32","2004-07-01","CAPS","SPASS Rider","rings(general)","RINGS","Ring observation","Observations of ring ionosphere","Observe the ring ionosphere from the end of SOI (over the B ring), through ring plane crossing, and out to post-SOI downlink (~3 RS)"]
["2004-183T03:56:30","000T00:01:00","2004-07-01","CAPS","SPASS Rider","SpacecraftActivity","RATE4K","Data volume adjustment","Change logical telemetry rate to 4 kbps","Change logical telemetry rate to 4 kbps. Explicitly in CIMS to make sure timing works with S&ER-5a TLM change and keep automatic command generation from exploding."]
["2004-183T04:00:46","000T00:08:29","2004-07-01","RPWS","Non-SPASS","rings(general)","RPXING","Measurements of dust flux, scale height and plasma waves at the magnetic equator during ring plane crossing","RPWS Ring Plane Crossing","Determine the equatorial dust flux and scale height as a function of radial distance.  Obtain high resolution of plasma waves at the magnetic equator."]
["2004-183T04:03:30","000T00:04:45","2004-07-01","INMS","SPASS Rider","Saturn","RINGCOMP","Ring composition","INMS Ring Compostion","This request looks into Dust Ram (for Neutral Particles)"]
["2004-183T04:05:02","000T00:45:58","2004-07-01","CAPS","SPASS Rider","rings(general)","RINGS","Ring observation","Observations of ring ionosphere","Observe the ring ionosphere from the end of SOI (over the B ring), through ring plane crossing, and out to post-SOI downlink (~3 RS)"]
["2004-183T04:05:02","000T00:01:00","2004-07-01","CAPS","SPASS Rider","SpacecraftActivity","RATE16K","Data volume adjustment","Change logical telemetry rate to 16 kbps","Change logical telemetry rate to 16 kbps. Explicitly in CIMS to make sure timing works with S&ER-5a TLM change and keep automatic command generation from exploding."]
["2004-183T04:08:15","000T10:31:45","2004-07-01","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","Ride with prime instrument"]
["2004-183T04:09:15","000T00:44:45","2004-07-01","RPWS","Non-SPASS","rings(general)","RPXING","Measurements of dust flux, scale height and plasma waves at the magnetic equator during ring plane crossing","RPWS Ring Plane Crossing","Determine the equatorial dust flux and scale height as a function of radial distance.  Obtain high resolution of plasma waves at the magnetic equator."]
["2004-183T04:51:00","000T00:30:00","2004-07-01","CAPS","SPASS Rider","Saturn","RNGSAT","Ring / Satellite","Rings and Satellites Campaign","Observe the plasma interaction with the E ring and icy satellites."]
["2004-183T04:51:00","000T01:34:00","2004-07-01","MIMI","SPASS Rider","DustRAM direction","POSTBURN",null,"MIMI Ring Interaction Science","Part of RS MAPS Campaign.   Spacecraft must be pointed such that the dust ram is not entering the INCA FOV. Required to satisfy FR76C3. This means INCA boresight (in S/C X, Y plane, 9.5 deg toward +X from -Y) >70 deg from dust ram."]
["2004-183T04:54:00","000T00:22:00","2004-07-01","ISS","Prime","rings(general)","ARINGLIT","A ring observation","POST-SOI POST-RPLXING HI RES A RING OBSERVATION","HI RES OUTER A RING IMAGING POST SOI,POST RING PLANE CROSSING.  MOSAIC (1x9) FROM F RING TO MIMAS 5:3 IVR AT 131,900 KM, SKIPPING REGION BETW/ F RING AND  A RING.  ALL POSITIONS ARE BOTSIMS"]
["2004-183T04:54:00","000T00:22:00","2004-07-01","UVIS","SPASS Rider","rings(general)","RANSASCN",null,null,"Highest spatial resolution UV spectral mapping of Saturn's rings. Spatial variation of UV albedo and water absorption edge indicative of scattering center size scale."]
["2004-183T04:54:00","000T00:22:00","2004-07-01","VIMS","SPASS Rider","rings(general)","ARINGLIT","A ring observation","SOI radial scan, high phase, lit face after DRPX","32*32 cubes, tau_IR=80 msec, tau_VIS=2.5 sec, time per cube = 95 sec (?),  up to 10 ISS pointings. Data vol allows for continuous imaging."]
["2004-183T04:54:00","000T00:12:00","2004-07-01","RPWS","Non-SPASS","Saturn","INNERMAG","Observing neutral molecules in the inner magnetosphere","RPWS INNER MAGNETOSPHERE","Outbound inner magnetosphere observations following desending ring plane crossing."]
["2004-183T05:06:00","000T01:19:00","2004-07-01","RPWS","Non-SPASS","Saturn","INSURVEY","Inner magnetosphere survey","RPWS Inner Survey","Set up RPWS for inner magnetosphere survey, attitude N/A, any OPMODE and science TLM mode including RPWS."]
["2004-183T05:21:00","000T20:00:00","2004-07-01","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey"]
["2004-183T05:26:00","000T09:50:00","2004-07-01","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-183T06:25:00","000T19:00:00","2004-07-01","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SUR Campaign","Part of SUR MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2004-183T06:25:00","000T17:45:00","2004-07-01","RPWS","Non-SPASS","Saturn","INSURVEY","Inner magnetosphere survey","RPWS Inner Survey","Set up RPWS for inner magnetosphere survey, attitude N/A, any OPMODE and science TLM mode including RPWS."]
["2004-183T10:51:00","000T14:30:00","2004-07-01","MAG","SPASS Rider","Other","SOINTFLD","MAG internal field measurements","MAG_Internal_Field_Measurements","This request will yield unique observations of Saturns internal magnetic field during SOI. The whole request is timed to start just before the beginning of the SOI critical sequence, this is the TOST portion. Note pointing constraints only apply with 4Rs."]
["2004-183T14:40:00","000T10:45:00","2004-07-01","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","Ride with prime instrument"]
["2004-183T15:16:00","000T09:50:00","2004-07-01","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-184T00:10:00","000T01:11:00","2004-07-02","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-184T01:21:00","000T04:09:21","2004-07-02","MAG","SPASS Rider","Other","SOINTFLD","MAG internal field measurements","MAG_Internal_Field_Measurements","This request will yield unique observations of Saturns internal magnetic field during SOI. The whole request is timed to start just before the beginning of the SOI critical sequence, this is the TOST portion. NOTE: pointing constraints only apply within 4Rs. NOTE: This is the T0min request."]
["2004-184T01:21:00","000T18:56:00","2004-07-02","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey"]
["2004-184T01:21:00","000T18:56:00","2004-07-02","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-184T01:25:00","000T16:35:00","2004-07-02","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","Ride with prime instrument"]
["2004-184T01:25:01","000T06:07:10","2004-07-02","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SUR Campaign","Part of SUR MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2004-184T01:56:21","000T01:34:00","2004-07-02","ISS","Prime","Titan","2X2WIND","Wind observation","Titan T0 imaging","Surface/winds/clouds"]
["2004-184T01:56:21","000T01:34:00","2004-07-02","CIRS","SPASS Rider","Titan","FIRNADCMP","Far infrared nadir composition map","CIRS_000TI_FIRNADCMP_01","Ride-along with ISS. Obtain information on CO, HCN, CH4.  Integrate on disk.  POINTING: -y to Titan, -x to sun."]
["2004-184T01:56:21","000T01:34:00","2004-07-02","VIMS","SPASS Rider","Titan","SPOLEA","South pole campaign","Titan global mapping","IR:32x64 double res, vis 32x32 single res; Titan global mapping of surface (south-polar area at 220 km/pxl)"]
["2004-184T03:30:21","000T01:22:00","2004-07-02","CIRS","Prime","Titan","TEMPMAP","Thermal map","CIRS_000TI_TEMPMAP038","obtain information on the thermal structure of Titan's stratosphere.  Slew across disk at 4 microrad/s.  POINTING: -y to Titan, -x aligned E/W toward sun (E-W slews)"]
["2004-184T03:30:21","000T01:22:00","2004-07-02","CIRS","SPASS Rider","Titan","TEMPMAP","Thermal map","CIRS_000_TI_TEMPMAP101","ISS NAC support imaging, 2 images per integration (~2 integrations total = 4 frames, 0.5 Mb/frame)"]
["2004-184T04:52:21","000T00:24:00","2004-07-02","ISS","Prime","Titan","2X2WIND","Wind observation","Titan T0 imaging","Surface/winds/clouds"]
["2004-184T04:52:21","000T00:24:00","2004-07-02","CIRS","SPASS Rider","Titan","FIRNADCMP","Far infrared nadir composition map","CIRS_000TI_FIRNADCMP_011","Obtain information on CO, HCN, CH4.  Integrate on disk.  POINTING: -y to Titan, x away from sun."]
["2004-184T04:52:21","000T00:24:00","2004-07-02","VIMS","SPASS Rider","Titan","SPOLEA","South pole campaign","Titan global mapping","Titan global mapping as a ridealong with ISS. 48 square double res images. If ISS is mosaicing, do 12 square."]
["2004-184T05:16:21","000T01:24:00","2004-07-02","CIRS","Prime","Titan","TEMPMAP","Thermal map","CIRS_000TI_TEMPMAP042","obtain information on the thermal structure of Titan's stratosphere.  Slew across disk at 4 microrad/s.  POINTING: -y to Titan, -x aligned E/W toward sun (E-W slews)"]
["2004-184T05:16:21","000T01:24:00","2004-07-02","CIRS","SPASS Rider","Titan","TEMPMAP","Thermal map","CIRS_000_TI_TEMPMAP102","ISS NAC support imaging, 2 images per integration (~2 integrations total = 4 frames, 0.5 Mb/frame)"]
["2004-184T05:30:21","000T08:00:00","2004-07-02","MAG","Non-SPASS","Titan","MAGTITAN","MAG Titan observation","T0 Flyby","T0 is formally the first Titan encounter of the mission although the closest approach is at a very large distance of 338082 km. Because of the large flyby distance the emphasis is not on Titan science but on the exploration of the region around Titan's orbit. This is important in connection with an accurate definition of the external field contributions to the magnetic field measurements around Saturn closest approach, the prime objective of which is the determination od Saturn's internal magnetic field.  NOTE: Data rate is composed of continuous 494 bps (8 vps) plus bursts of 1976 bps (32 vps). NOTE: This is the T0min request."]
["2004-184T06:40:21","000T00:24:00","2004-07-02","ISS","Prime","Titan","2X2WIND","Wind observation","Titan T0 imaging","Surface/winds/clouds"]
["2004-184T06:40:21","000T00:24:00","2004-07-02","CIRS","SPASS Rider","Titan","FIRNADCMP","Far infrared nadir composition map","CIRS_000TI_FIRNADCMP_010","Obtain information on CO, HCN, CH4.  Integrate on disk.  POINTING: -y to Titan, x away from sun."]
["2004-184T06:40:21","000T00:24:00","2004-07-02","VIMS","SPASS Rider","Titan","SPOLEA","South pole campaign","Titan global mapping","Titan global mapping as a ridealong with ISS. 48 square double res images. If ISS is mosaicing, do 12 square."]
["2004-184T07:04:21","000T01:26:00","2004-07-02","CIRS","Prime","Titan","TEMPMAP","Thermal map","CIRS_000TI_TEMPMAP044","obtain information on the thermal structure of Titan's stratosphere.  Slew across disk at 4 microrad/s.  POINTING: -y to Titan, -x E/W toward sun (E-W slews)"]
["2004-184T07:04:21","000T01:26:00","2004-07-02","CIRS","SPASS Rider","Titan","TEMPMAP","Thermal map","CIRS_000_TI_TEMPMAP103","ISS NAC support imaging, 2 images per integration (~2 integrations total = 4 frames, 0.5 Mb/frame)"]
["2004-184T07:04:21","000T01:26:00","2004-07-02","UVIS","SPASS Rider","Titan","TEMPMAP","Thermal map","UVIS Rider to CIRS TEMPMAP","UVIS Rider to CIRS  TEMP Map"]
["2004-184T07:32:10","000T00:58:11","2004-07-02","MIMI","SPASS Rider","Titan","T0INBND",null,"MAPS 000TI(T0) Campaign","Part of 000TI(T0) MAPS Campaign.   Investigate micro-scale and near aspects of the Titan interaction by observing during about one hour period around an encounter. With -Y pointed toward Titan, when within 30 minutes of the targeted flyby, optimize secondary axis for corotation flow as close to the S/C -X, +/- Z plane as works with the other constraints on pointing. Also, measure Titan exosphere/magnetosphere interaction by imaging in ENA with INCA (when sun is not in INCA FOV)."]
["2004-184T08:30:21","000T00:09:00","2004-07-02","ISS","Prime","Titan","2X2WIND","Wind observation","Titan T0 imaging","Surface/winds/clouds"]
["2004-184T08:30:21","000T00:09:00","2004-07-02","CIRS","SPASS Rider","Titan","FIRNADCMP","Far infrared nadir composition map","CIRS_000TI_FIRNADCMP_004","Obtain information on CO, HCN, CH4.  Integrate on disk.  POINTING: -y to Titan, x away from sun."]
["2004-184T08:30:21","000T02:00:00","2004-07-02","MIMI","SPASS Rider","Titan","T0CLOSE",null,"MAPS 000TI(T0) Campaign","Part of 000TI(T0) MAPS Campaign.   Investigate micro-scale and near aspects of the Titan interaction by observing during about one hour period around an encounter. With -Y pointed toward Titan, when within 30 minutes of the targeted flyby, optimize secondary axis for corotation flow as close to the S/C -X, +/- Z plane as works with the other constraints on pointing. Also, measure Titan exosphere/magnetosphere interaction by imaging in ENA with INCA (when sun is not in INCA FOV)."]
["2004-184T08:30:21","000T00:09:00","2004-07-02","VIMS","SPASS Rider","Titan","SPOLEA","South pole campaign","Titan global mapping","Titan global mapping as a ridealong with ISS. 48 square double res images. If ISS is mosaicing, do 12 square."]
["2004-184T08:39:21","000T00:51:00","2004-07-02","VIMS","Prime","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #63","Titan Light Curve, Observation #63.Changes  made 5/19/02 by Buratti as per TOST and  ISS agreements."]
["2004-184T08:39:21","000T00:51:00","2004-07-02","CIRS","SPASS Rider","Titan","FIRNADCMP","Far infrared nadir composition map","CIRS_000TI_FIRNADCMP_01","Obtain information on CO, HCN, CH4.  Integrate on disk.  POINTING: -y to Titan, x away from sun."]
["2004-184T08:39:21","000T00:51:00","2004-07-02","ISS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan T0 imaging","Photometry/polarimetry"]
["2004-184T09:30:21","000T01:00:00","2004-07-02","ISS","Prime","Titan","SPOLEB","South pole campaign","Titan T0 2x3 mosaic, S pole","Turn -Y to Titan; do 2X3 mosaic with multiple NAC filters at each footprint"]
["2004-184T09:30:21","000T01:00:00","2004-07-02","CIRS","SPASS Rider","Titan","FIRNADCMP","Far infrared nadir composition map","CIRS_000TI_FIRNADCMP_01","Obtain information on CO, HCN, CH4.  Integrate on disk.  POINTING: -y to Titan, x away from sun."]
["2004-184T09:30:21","000T01:00:00","2004-07-02","VIMS","SPASS Rider","Titan","SPOLEB","South pole campaign","Titan global mapping","IR:32x64 double res, vis 32x32 single res; Titan global mapping of surface (south-polar area at 170 km/pxl)"]
["2004-184T10:00:00","012T02:55:00","2004-07-02","CDA","Non-SPASS","DustRAM direction","SURVEY","Magnetospheric survey","dust survey","prograde dust, day 174: -z2E and  -x 26.9; -24.6      AM=42 (60deg from +x2NEP) geometry changes fast, -x pointing only valid at beginning in the first days."]
["2004-184T10:30:21","000T04:00:00","2004-07-02","CIRS","Prime","Titan","TEMPMAP","Thermal map","CIRS_000TI_TEMPMAP01","obtain information on the thermal structure of Titan's stratosphere.  Slew across disk at 4 microrad/s.  POINTING: -y to Titan, -X aligned E/W toward sun (E/W slews)"]
["2004-184T10:30:21","000T04:00:00","2004-07-02","CIRS","SPASS Rider","Titan","TEMPMAP","Thermal map","CIRS_000_TI_TEMPMAP104","ISS NAC support imaging, 2 images per integration (~4 integrations total = 8 frames, 0.5 Mb/frame)"]
["2004-184T10:30:21","000T04:00:00","2004-07-02","ISS","SPASS Rider","Titan","TEMPMAP","Thermal map","Titan T0 imaging","Photometry/polarimetry"]
["2004-184T10:30:21","000T01:01:49","2004-07-02","MIMI","SPASS Rider","Titan","T0OUTBND",null,"MAPS 000TI(T0) Campaign","Part of 000TI(T0) MAPS Campaign.   Investigate micro-scale and near aspects of the Titan interaction by observing during about one hour period around an encounter. With -Y pointed toward Titan, when within 30 minutes of the targeted flyby, optimize secondary axis for corotation flow as close to the S/C -X, +/- Z plane as works with the other constraints on pointing. Also, measure Titan exosphere/magnetosphere interaction by imaging in ENA with INCA (when sun is not in INCA FOV)."]
["2004-184T10:30:21","000T04:00:00","2004-07-02","UVIS","SPASS Rider","Titan","TEMPMAP","Thermal map","UVIS Rider to CIRS TEMPMAP","UVIS Rider to CIRS  TEMP Map"]
["2004-184T10:30:21","000T04:00:00","2004-07-02","VIMS","SPASS Rider","Titan","TEMPMAP","Thermal map","CIRS Temp Map","Titan global mapping as a ridealong with CIRS There will be pauses in mosaic for ISS/VIMS"]
["2004-184T11:32:21","000T08:44:39","2004-07-02","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SUR Campaign","Part of SUR MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2004-184T13:30:21","000T06:50:39","2004-07-02","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps). NOTE: This is the T0min request."]
["2004-184T14:30:21","000T00:45:00","2004-07-02","VIMS","Prime","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #62","Titan Light Curve, Observation #62. Changes made by Buratti as per TOST agreements."]
["2004-184T14:30:21","000T00:45:00","2004-07-02","CIRS","SPASS Rider","Titan","FIRNADCMP","Far infrared nadir composition map","CIRS_000TI_FIRNADCMP_01","Obtain information on CO, HCN, CH4.  Integrate on disk.  POINTING: -y to Titan, x away from sun."]
["2004-184T14:30:21","000T00:45:00","2004-07-02","ISS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan T0 imaging","Photometry/polarimetry"]
["2004-184T15:15:21","000T01:45:00","2004-07-02","CIRS","Prime","Titan","TEMPMAP","Thermal map","CIRS_000TI_TEMPMAP01","obtain information on the thermal structure of Titan's stratosphere.  Slew across disk at 4 microrad/s.  POINTING: -y to Titan, -x aligned E/W toward sun (slews e/w)"]
["2004-184T15:15:21","000T01:45:00","2004-07-02","CIRS","SPASS Rider","Titan","TEMPMAP","Thermal map","CIRS_000_TI_TEMPMAP105","ISS NAC support imaging, 2 images per integration (~2 integrations total = 4 frames, 0.5 Mb/frame)"]
["2004-184T17:51:00","000T02:45:00","2004-07-02","CIRS","SPASS Rider","InstrumentCalibration","DSCAL","Deep space calibration",null,"Deep space obervations for calibration."]
["2004-184T17:51:00","000T02:45:00","2004-07-02","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-184T18:00:00","000T00:23:00","2004-07-02","INMS","Non-SPASS","Saturn","MRO","Instrument memory readout","Memory Dump","Ride with prime instrument"]
["2004-184T18:23:00","001T04:43:00","2004-07-02","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","Ride with prime instrument"]
["2004-184T20:17:00","001T05:02:00","2004-07-02","MIMI","SPASS Rider","co-rotation","MAGDYN","MAPS magnetosphere dynamics campaign","MAPS MAGDYN Campaign","Part of MAGDYN MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2004-184T20:17:00","002T02:49:00","2004-07-02","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey"]
["2004-184T20:17:00","001T02:49:00","2004-07-02","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-184T20:21:00","001T02:45:00","2004-07-02","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2004-184T20:36:00","000T01:24:00","2004-07-02","CIRS","SPASS Rider","InstrumentCalibration","DEEPSPACE","Deep space calibration","OPNAV rider for deep space","Any pointing O.K.  Deep space during OPNAV turns"]
["2004-184T22:00:00","000T02:45:00","2004-07-02","CIRS","Prime","rings(general)","SHADLMP","Saturn ring shadow observation","CIRS_000RB_ShadLMP","Longitudinal scan of  ring in the early mission (highest temperature contrasts), in and around shadow, Low Phase, dawn side. -Y to ring, +Z perpendicular to rings (if not possible, +Z parallel to pole)"]
["2004-184T22:00:00","000T02:45:00","2004-07-02","CIRS","SPASS Rider","rings(general)","SHADLMP","Saturn ring shadow observation","CIRS_000RI_SHADLMP_SI","Support imaging for ring shadow observation, multiple scans"]
["2004-185T01:00:00","000T02:15:00","2004-07-03","CIRS","Prime","Titan","FIRNADCMP","Far infrared nadir composition map","CIRS_000TI_FIRNADIRCOMPINT_01","Obtain information on CO, HCN, CH4.  Integrate on disk at airmass 0.0.  POINTING: -y to Titan, x away from sun PIC"]
["2004-185T01:00:00","000T02:15:00","2004-07-03","CIRS","SPASS Rider","Titan","FIRNADCMP","Far infrared nadir composition map","CIRS_000_TI_FIRNADCMP017","ISS NAC support imaging, 2 images per integration (~2 integrations total = 4 frames, 0.5 Mb/frame)"]
["2004-185T01:00:00","000T02:15:00","2004-07-03","ISS","SPASS Rider","Titan","FIRNADCMP","Far infrared nadir composition map","RCI (Ridealong Context Imaging/Titan imaging)","ISS on, max data rate = 182.784 kbps, number of frames and bits/frame are input parameters, data volume = number of frames x bits/frame, average data rate = data volume/duration."]
["2004-185T03:15:00","000T00:45:00","2004-07-03","VIMS","Prime","Titan","LIGHTC","Titan light curve","Titan Light Curve, Obs #65","Titan Light Curve, Observation #65. Added 5/19/02 by Buratti as per TOST agreement."]
["2004-185T03:15:00","000T00:45:00","2004-07-03","CIRS","SPASS Rider","Titan","FIRNADCMP","Far infrared nadir composition map","CIRS_000TI_FIRNADCMP_01","Obtain information on CO, HCN, CH4.  Integrate on disk.  POINTING: -y to Titan, x away from sun."]
["2004-185T03:15:00","000T00:45:00","2004-07-03","ISS","SPASS Rider","Titan","LIGHTC","Titan light curve","Titan T0 imaging","Photometry/polarimetry"]
["2004-185T04:00:00","000T06:00:00","2004-07-03","CIRS","Prime","Titan","FIRNADCMP","Far infrared nadir composition map","CIRS_000TI_FIRNADIRCOMPINT_01","Obtain information on CO, HCN, CH4.  Integrate on disk at airmass 0.0.  POINTING: FP1 to Titan, x away from sun, PIC."]
["2004-185T04:00:00","000T06:00:00","2004-07-03","CIRS","SPASS Rider","Titan","FIRNADCMP","Far infrared nadir composition map","CIRS_000_TI_FIRNADCMP001","ISS NAC support imaging, 2 images per integration (~4 integrations total = 8 frames, 0.5 Mb/frame)"]
["2004-185T04:00:00","000T06:00:00","2004-07-03","ISS","SPASS Rider","Titan","FIRNADCMP","Far infrared nadir composition map","RCI (Ridealong Context Imaging/Titan T0 imaging)","Photometry/polarimetry"]
["2004-185T04:00:00","000T06:00:00","2004-07-03","UVIS","SPASS Rider","Titan","FIRNADCMP","Far infrared nadir composition map","UVIS Rider to CIRS Far Nadir Comp","UVIS Rider to CIRS Far-IR Nadir Comp"]
["2004-185T04:00:00","000T06:00:00","2004-07-03","VIMS","SPASS Rider","Titan","FARIRMAP","Far Infrared map","CIRS Far IR Map","Titan global mapping as a ridealong with CIRS There will be pauses in mosaic for ISS/VIMS"]
["2004-185T10:00:00","000T01:00:00","2004-07-03","ISS","Prime","Titan","1X2WIND","Wind observation","Titan T0 imaging","Surface/winds/clouds"]
["2004-185T10:00:00","000T01:00:00","2004-07-03","CIRS","SPASS Rider","Titan","MIDIRTMAP","Mid infrared thermal map","CIRS_013TI_MIDIRTMAP07","obtain information on the thermal structure of Titan's stratosphere.  Slew across disk at 4 microrad/s.  POINTING: -y to Titan, x to pole"]
["2004-185T10:00:00","000T01:00:00","2004-07-03","VIMS","SPASS Rider","Titan","MAP",null,"Titan Light Curve, Obs #65","Ridealong with ISS Map. If they are doing NAC, take 12 X 12 high res., If WAC do 38 square high res."]
["2004-185T11:00:00","000T01:30:00","2004-07-03","CIRS","SPASS Rider","Iapetus","MIDIRTMAP","Mid infrared thermal map","CIRS_013TI_MIDIRTMAP07","obtain information on the thermal structure of Titan's stratosphere.  Slew across disk at 4 microrad/s.  POINTING: -y to Titan, x to pole"]
["2004-185T11:20:00","000T01:10:00","2004-07-03","ISS","Prime","Iapetus","TERRAINCA","Terra incognita observation","Iapetus terra incognita (south hem) low phase obs","Turn -Y to Iapetus; Do 1x1 mosaic 2 NAC clear + 4 NAC color + 3 NAC polarizer filters; custom handoff to NAV at -Y to Iapetus"]
["2004-185T14:06:00","000T09:00:00","2004-07-03","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-185T15:00:00","000T06:00:00","2004-07-03","CIRS","SPASS Rider","InstrumentCalibration","DSCAL2","Deep space calibration",null,"Deep space obervations for calibration."]
["2004-185T23:06:00","000T01:25:00","2004-07-03","CIRS","SPASS Rider","InstrumentCalibration","DEEPSPACE","Deep space calibration","OPNAV rider for deep space","Any pointing O.K.  Deep space during OPNAV turns"]
["2004-185T23:06:00","001T00:00:00","2004-07-03","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","Ride with prime instrument"]
["2004-185T23:06:00","000T03:25:00","2004-07-03","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2004-185T23:06:00","001T23:45:00","2004-07-03","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-186T00:31:00","000T02:00:00","2004-07-04","UVIS","Prime","rings(general)","IMPACT",null,null,"Use UVIS HSP and FUV to detect flashes from meter-sized interplanetary impactors on rings to constrain flux of important impact population for ring origin/evolution."]
["2004-186T00:31:00","000T02:00:00","2004-07-04","CIRS","SPASS Rider","rings(general)","URIMPACT",null,"CIRS_000RI_URIMPACT_SI","Support imaging for long integration on A ring and C rings"]
["2004-186T00:31:00","000T02:00:00","2004-07-04","CIRS","SPASS Rider","rings(general)","URIMPACT",null,"CIRS_000_RI_URIMPACT rider with UVIS","Ride with URIMPACT, staring at B ring shadow"]
["2004-186T00:31:00","000T02:00:00","2004-07-04","ISS","SPASS Rider","rings(general)","IMPACT",null,"URIMPACT spoke and F ring images day 186","WACs for F ring at beginning (R ansa), and during UVIS shadow stare (L ansa), and at end (R ansa) to catch emerging spokes. Added one dark current."]
["2004-186T00:31:00","000T02:00:00","2004-07-04","VIMS","SPASS Rider","rings(general)","IMPACT",null,"F Ring during UVIS impact observations","F Ring observations during UVIS searches for ring impacts."]
["2004-186T01:19:01","004T10:41:00","2004-07-04","MIMI","SPASS Rider","co-rotation","MAGDYN","MAPS magnetosphere dynamics campaign","MAPS MAGDYN Campaign","Part of MAGDYN MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2004-186T02:31:00","000T10:10:00","2004-07-04","CIRS","Prime","rings(general)","COMP","Sit and stare to derive composition","CIRS_000RI_COMP","Stare at West ansa, low phase, lit face, 5 hrs on C ring, 5 hrs on A ring -Y to ring, +Z perpendicular to ring radius"]
["2004-186T02:31:00","000T10:10:00","2004-07-04","CIRS","SPASS Rider","rings(general)","COMP","Sit and stare to derive composition","CIRS_000RI_COMP_SI","Support imaging for long integration on A ring and C rings"]
["2004-186T02:31:00","000T05:00:00","2004-07-04","MAG","Non-SPASS","InstrumentCalibration","SCAS","MAG SCAS instrument","MAG/SCAS_Cal","Boom alignment calibration using SCAS. If moved within scheduling window, KEEP OUTSIDE SCHEDULED MAPS CAMPAIGNS. Note: SCAS operations disturb RSS and RPWS. IF OpMode not ORS, unique sequence will be required. Includes 2 hours for IFC cal and range checks. First calibration after SOI."]
["2004-186T07:31:00","008T05:29:00","2004-07-04","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2004-186T12:41:00","000T01:25:00","2004-07-04","CIRS","SPASS Rider","InstrumentCalibration","DEEPSPACE","Deep space calibration","OPNAV rider for deep space","Any pointing O.K.  Deep space during OPNAV turns"]
["2004-186T14:06:00","000T09:00:00","2004-07-04","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-186T23:06:00","006T23:30:00","2004-07-04","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey"]
["2004-186T23:06:00","000T00:23:00","2004-07-04","INMS","Non-SPASS","Saturn","MRO","Instrument memory readout","Memory Dump","Ride with prime instrument"]
["2004-186T23:29:00","002T00:31:00","2004-07-04","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","Ride with prime instrument"]
["2004-186T23:36:00","000T04:14:00","2004-07-04","ISS","Prime","Iapetus","TERRAINCC","Terra incognita observation","Iapetus terra incognita (south hem) low phase obs","Turn -Y to Iapetus; do 1x1 NAC mosaic 20 clear + 66 color + 18 polarizer + 15 WAC color filters; turn to WP"]
["2004-186T23:36:00","000T04:14:00","2004-07-04","UVIS","SPASS Rider","Iapetus","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2004-186T23:36:00","000T01:00:00","2004-07-04","VIMS","SPASS Rider","Iapetus","TERRAINCC","Terra incognita observation","Iapetus southern hemisphere","Multiple 640ms 12x12 cubes"]
["2004-187T13:51:00","000T09:00:00","2004-07-05","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-187T14:45:00","000T06:00:00","2004-07-05","CIRS","SPASS Rider","InstrumentCalibration","DSCAL2","Deep space calibration",null,"Deep space obervations for calibration."]
["2004-187T22:51:00","005T14:45:00","2004-07-05","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-188T14:00:00","000T06:00:00","2004-07-06","CIRS","SPASS Rider","InstrumentCalibration","DSCAL1","Deep space calibration",null,"Deep space obervations for calibration."]
["2004-189T00:00:00","000T00:23:00","2004-07-07","INMS","Non-SPASS","Saturn","MRO","Instrument memory readout","Memory Dump","Ride with prime instrument"]
["2004-189T00:23:00","001T23:37:00","2004-07-07","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","Ride with prime instrument"]
["2004-189T09:00:00","000T06:00:00","2004-07-07","CIRS","SPASS Rider","InstrumentCalibration","DSCAL2","Deep space calibration",null,"Deep space obervations for calibration."]
["2004-190T12:00:00","004T01:00:00","2004-07-08","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SUR Campaign","Part of SUR MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2004-191T00:00:00","000T00:23:00","2004-07-09","INMS","Non-SPASS","Saturn","MRO","Instrument memory readout","Memory Dump","Ride with prime instrument"]
["2004-191T00:23:00","001T23:37:00","2004-07-09","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","Ride with prime instrument"]
["2004-193T00:00:00","000T00:23:00","2004-07-11","INMS","Non-SPASS","Saturn","MRO","Instrument memory readout","Memory Dump","Ride with prime instrument"]
["2004-193T00:23:00","001T23:37:00","2004-07-11","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","Ride with prime instrument"]
["2004-193T13:36:00","000T23:24:00","2004-07-11","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-193T13:36:00","000T09:00:00","2004-07-11","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-193T14:45:00","000T06:00:00","2004-07-11","CIRS","SPASS Rider","InstrumentCalibration","DSCAL2","Deep space calibration",null,"Deep space obervations for calibration."]
["2004-193T22:36:00","000T14:24:00","2004-07-11","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey"]
["2004-194T13:00:00","002T00:08:00","2004-07-12","CAPS","SPASS Rider","Saturn","SWAURORA","Solar wind campaign","MAPS SW1 Campaign","Part of SW1 MAPS Campaign.  Observe solar wind while ORS instruments simultaneously observer Saturn's aurora"]
["2004-194T13:00:00","002T00:00:00","2004-07-12","MIMI","SPASS Rider","Saturn","SWAURORA","Solar wind campaign","MAPS SW1 Campaign","Part of SW1 MAPS Campaign.   Image the magnetosphere and observe solar wind and pickup ions while ORS instruments make simultaneous observations of Saturns aurora, CAPS observes the solar wind, and RPWS observes SKR. -Y to Saturn (auroral region) and -X ~ to sun."]
["2004-194T13:00:00","002T00:07:00","2004-07-12","MAG","Non-SPASS","Other","SWAURORA","Solar wind campaign","MAPS SW Aurora Campaign","SW observations in conjunction with ISS auroral observations"]
["2004-194T13:00:00","002T00:02:00","2004-07-12","RPWS","Non-SPASS","Saturn","SWAURORA","Solar wind campaign","MAPS SW1 Campaign","Part of SW1 MAPS Campaign.  Observe solar wind plasma waves and Saturn radio emissions while ORS instruments simultaneously observe Saturn's aurora and other MAPS observe solar wind conditions."]
["2004-194T13:36:00","000T09:00:00","2004-07-12","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-194T14:45:00","000T06:00:00","2004-07-12","CIRS","SPASS Rider","InstrumentCalibration","DSCAL1","Deep space calibration",null,"Deep space obervations for calibration."]
["2004-195T00:00:00","000T00:23:00","2004-07-13","INMS","Non-SPASS","Saturn","MRO","Instrument memory readout","Memory Dump","Ride with prime instrument"]
["2004-195T00:06:00","000T01:00:00","2004-07-13","ISS","Prime","Iapetus","SOUTHHEMB","Southern hemisphere imaging","Iapetus terra incognita (south hem) obs.","Turn -Y to Iapetus; Do 1x1 mosaic 2 NAC clear + 4 NAC color + 3 NAC polarizer filters; turn to WP."]
["2004-195T00:06:00","000T01:00:00","2004-07-13","UVIS","SPASS Rider","Iapetus","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2004-195T00:06:00","000T01:00:00","2004-07-13","VIMS","SPASS Rider","Iapetus","SOUTHHEMB","Southern hemisphere imaging","Iapetus southern hemisphere","Multiple 640ms 12x12 cubes"]
["2004-195T00:23:00","001T12:34:00","2004-07-13","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","Ride with prime instrument"]
["2004-195T01:06:00","000T04:25:00","2004-07-13","UVIS","Prime","Saturn","MOS00WA","Apoapsis mosaic","MOSAIC_APO_01_21b","Mosaic of Saturn inner magnetosphere.  EUV and FUV low resolution slits on, aligned parallel to Saturn spin axis.  1) Slew about the Z-axis from Saturn center to +MOS orb.  2)  Drift at a rate of .0156  mrad/sec about the Z-axis toward -MOS orb for 14000s. 3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS orb (+/- range from Saturn Center): 123.77 mrad."]
["2004-195T06:06:00","000T09:00:00","2004-07-13","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-195T16:31:00","000T10:30:00","2004-07-13","UVIS","Prime","Saturn","AURORAA","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 10.5 hours.  A similar request (auroralB) is identical except it repeats for 5.0 hours."]
["2004-195T16:31:00","000T10:30:00","2004-07-13","CIRS","SPASS Rider","Saturn","SPTEMPL10","South pole imaging","Saturn South Pole Template","Saturn south pole"]
["2004-195T16:31:00","000T10:30:00","2004-07-13","ISS","SPASS Rider","Saturn","AURORAA","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-196T03:01:00","000T03:25:00","2004-07-14","UVIS","Prime","Saturn","MOS00WA","Apoapsis mosaic","MOSAIC_APO_01_21c","Mosaic of Saturn inner magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with Saturn spin axis.  1) Slew about the Z-axis from Saturn Center to -MOS orb. 2)  Drift at a rate of .0148 mrad/sec about the Z-axis towards +MOS orb for 11700s.  3) Slew Back to Saturn center and reset pointing.  Stare for remaining observation time. MOS ORB (+/-range from Saturn Center): 117.92 mrad."]
["2004-196T06:26:00","000T05:00:00","2004-07-14","UVIS","Prime","Saturn","AURORAB","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 5 hours.  A similar request (auroralA) is identical except it repeats for 10.5 hours."]
["2004-196T06:26:00","000T05:00:00","2004-07-14","CIRS","SPASS Rider","Saturn","SPTEMPL05","South pole imaging","Saturn South Pole Template","Saturn south pole"]
["2004-196T06:26:00","000T05:00:00","2004-07-14","ISS","SPASS Rider","Saturn","AURORAB","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-196T12:54:00","000T00:06:00","2004-07-14","CAPS","SPASS Rider","SpacecraftActivity","SLEEP","Instrument to sleep mode","Sleep for Probe activity","sleep instrument"]
["2004-196T12:55:00","000T09:49:00","2004-07-14","CDA","SPASS Rider","Other","PCOMUTE","Mute instrument for Probe Checkout","Probe Checkout Mute","Sleep/Mute Unmute/Active for PCO"]
["2004-196T12:56:00","000T00:17:00","2004-07-14","CIRS","Non-SPASS","Other","PROBEMUTE","Huygens Probe support","Sleep/mute placeholder for PCO14","Put CIRS to sleep/mute for PCO#14 CIRS to sleep at epoch - 00:17, mute by  epoch -00:06"]
["2004-196T12:57:00","000T00:10:00","2004-07-14","INMS","Non-SPASS","SpacecraftActivity","SLEEP","Instrument to sleep mode","PCO 14 SLEEP","SLEEP/MUTE for PCO14"]
["2004-196T12:58:00","000T00:09:50","2004-07-14","ISS","Non-SPASS","Earth","SLEEPMUTE","Huygens probe support","put ISS to sleep for probe activity","placeholder activity put into CIMS to remenind ISS to go into sleep for probe activity at request of MAG TWT"]
["2004-196T13:00:00","000T09:42:00","2004-07-14","MIMI","SPASS Rider","co-rotation","PCOMUTE","Mute instrument for Probe Checkout","Probe Checkout Mute","SLEEP/MUTE for PCO"]
["2004-196T13:02:00","000T09:49:00","2004-07-14","RPWS","Non-SPASS","SpacecraftActivity","SLEEPMUTE","Huygens probe support","RPWS Sleep and Mute for Probe activity","RPWS sleep/mute for Probe activity, followed by unmute/sleep."]
["2004-196T13:04:00","000T00:03:00","2004-07-14","UVIS","Non-SPASS","Saturn","SLEEPMUTE","Huygens probe support","UVIS TO SLEEP/MUTE (PCO 14)","UVIS to go to sleep/mute for PCO 14 (MGTWT request)"]
["2004-196T13:05:00","000T00:08:00","2004-07-14","VIMS","Non-SPASS","SpacecraftActivity","SLEEPMUTE","Huygens probe support","VIMS to SLEEP / MUTE","VIMS to SLEEP/ MUTE for PCO14_PSAON"]
["2004-196T13:07:00","000T00:01:00","2004-07-14","CAPS","SPASS Rider","SpacecraftActivity","MUTE","Instrument to sleep mode","Mute for Probe activity","mute biu"]
["2004-196T13:07:00","000T09:35:00","2004-07-14","INMS","Non-SPASS","SpacecraftActivity","MUTE","Instrument to sleep mode","PCO 14 MUTE","SLEEP/MUTE for PCO14"]
["2004-196T13:07:00","000T09:35:00","2004-07-14","MAG","Non-SPASS","SpacecraftActivity","PROBEMUTE","Huygens Probe support","Mute/Unmute for PCO14","Mute instrument for probe patch load, unmute at end. NOTE: MAG does not go to sleep for probe activities, other instruments do"]
["2004-196T13:13:00","000T09:23:00","2004-07-14","PROBE","Non-SPASS","Earth","PCO14","Probe Checkout","Post-SOI Probe Checkout","Regular Probe Checkout. X-band downlink required. The following Orbiter instruments will be ON, in sleep mode, and muted prior to PSA ON: CDA, CAPS, ISS, MIMI, RPWS, MAG, UVIS, and VIMS; other orbiter instruments OFF."]
["2004-196T22:42:00","001T01:34:00","2004-07-14","CAPS","SPASS Rider","Saturn","SWAURORA","Solar wind campaign","MAPS SW1 Campaign","Part of SW1 MAPS Campaign.  Observe solar wind while ORS instruments simultaneously observer Saturn's aurora"]
["2004-196T22:42:00","000T00:01:00","2004-07-14","CAPS","SPASS Rider","SpacecraftActivity","UNMUTE","Huygens probe support","UnMute at Probe activity","unmute biu"]
["2004-196T22:42:00","000T00:07:00","2004-07-14","MIMI","SPASS Rider","co-rotation","PCOUNMUTE","Huygens probe support","Probe Checkout Mute","UNMUTE/ACTIVE after PCO  UNMUTE at request start. Active 7 minutes later"]
["2004-196T22:42:00","000T00:04:00","2004-07-14","CIRS","Non-SPASS","Other","PROUNMUTE","Huygens Probe support","wake/unmute placeholder for PCO14","UNMUTE.  Note power transients! unmute at 00:06, wake at epoch+00:09"]
["2004-196T22:42:00","000T00:04:00","2004-07-14","INMS","Non-SPASS","SpacecraftActivity","UNMUTE","Huygens probe support","PCO 14 UNMUTE","SLEEP/MUTE for PCO14"]
["2004-196T22:42:00","000T00:07:00","2004-07-14","ISS","Non-SPASS","Earth","WAKESLEEP","Wakeup instrument from sleep mode","wake up  ISS after probe activity","placeholder activity put into CIMS to remind ISS to wake up after probe activity at request of MAG TWT"]
["2004-196T22:42:00","001T16:09:00","2004-07-14","MAG","Non-SPASS","Other","SWAURORA","Solar wind campaign","MAPS SW Aurora Campaign","SW observations in conjunction with ISS auroral observations"]
["2004-196T22:42:00","000T00:11:00","2004-07-14","UVIS","Non-SPASS","Saturn","UNMUTEWAK","Huygens probe support","UVIS to unmute and wake up after PCO 14","Unmute/go to active after PCO 14 (MAGTWT request)"]
["2004-196T22:42:00","000T00:15:00","2004-07-14","VIMS","Non-SPASS","SpacecraftActivity","WAKEUP","Wakeup instrument from sleep mode","VIMS to Active Mode","VIMS to UnMute and Active at PCO14_PSAOFF"]
["2004-196T22:43:00","000T02:16:00","2004-07-14","CAPS","SPASS Rider","SpacecraftActivity","WAKEUP","Wakeup instrument from sleep mode","WakeUp at Probe activity","wake up"]
["2004-196T22:43:00","000T02:16:00","2004-07-14","CAPS","SPASS Rider","SpacecraftActivity","WAKEUP","Wakeup instrument from sleep mode","WakeUp at Probe activity","wake up"]
["2004-196T22:44:00","001T16:07:00","2004-07-14","CDA","Non-SPASS","DustRAM direction","SURVEY","Magnetospheric survey","dust survey","prograde dust, day 174: -z2E and  -x 26.9; -24.6      AM=42 (60deg from +x2NEP) geometry changes fast, -x pointing only valid at beginning in the first days."]
["2004-196T22:46:00","000T00:23:00","2004-07-14","INMS","Non-SPASS","Saturn","MRO","Instrument memory readout","MAPS Survey","Ride with prime instrument"]
["2004-196T22:49:00","001T16:02:00","2004-07-14","MIMI","SPASS Rider","Saturn","SWAURORA","Solar wind campaign","MAPS SW1 Campaign","Part of SW1 MAPS Campaign.   Image the magnetosphere and observe solar wind and pickup ions while ORS instruments make simultaneous observations of Saturns aurora, CAPS observes the solar wind, and RPWS observes SKR. -Y to Saturn (auroral region) and -X ~ to sun."]
["2004-196T22:51:00","001T16:00:00","2004-07-14","RPWS","Non-SPASS","Saturn","SWAURORA","Solar wind campaign","MAPS SW1 Campaign","Part of SW1 MAPS Campaign.  Observe solar wind plasma waves and Saturn radio emissions while ORS instruments simultaneously observe Saturn's aurora and other MAPS observe solar wind conditions."]
["2004-196T23:09:00","001T23:51:00","2004-07-14","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","Ride with prime instrument"]
["2004-197T01:26:00","000T00:55:00","2004-07-15","UVIS","Prime","Saturn","MOS00WA","Apoapsis mosaic","MOSAIC_APO_01_05","Mosaic of Saturn inner magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with the Saturn spin axis. 1) Slew from Saturn Center about the Z-axis to +MOS orb.  2) Drift at a rate of .0143 mrad/sec about the Z-axis towards -MOS orb for 3000S.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time.  MOS ORB (+/- range from Saturn Center): 113.77 mrad."]
["2004-197T02:21:00","000T10:30:00","2004-07-15","UVIS","Prime","Saturn","AURORAA","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It uses the GENMOS_P module. It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 10.5 hours.  A similar request (auroralB) is identical except it repeats for 5.0 hours."]
["2004-197T02:21:00","000T10:30:00","2004-07-15","ISS","SPASS Rider","Saturn","AURORAA","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-197T13:21:00","000T09:00:00","2004-07-15","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-197T23:51:00","000T01:00:00","2004-07-15","ISS","Prime","Iapetus","SOUTHHEME","Southern hemisphere imaging","Iapetus terra incognita (south hem) obs.","Turn -Y to Iapetus; Do 1x1 mosaic 2 NAC clear + 4 NAC color + 3 NAC polarizer filters"]
["2004-197T23:51:00","000T01:00:00","2004-07-15","UVIS","SPASS Rider","Iapetus","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2004-197T23:51:00","000T01:00:00","2004-07-15","VIMS","SPASS Rider","Iapetus","SOUTHHEME","Southern hemisphere imaging","Iapetus southern hemisphere","Multiple 640ms 12x12 cubes"]
["2004-198T00:06:00","004T21:26:00","2004-07-16","CAPS","SPASS Rider","Saturn","SWAURORA","Solar wind campaign","MAPS SW1 Campaign","Part of SW1 MAPS Campaign.  Observe solar wind while ORS instruments simultaneously observer Saturn's aurora"]
["2004-198T00:51:00","000T04:25:00","2004-07-16","UVIS","Prime","Saturn","MOS00WB","Apoapsis mosaic","MOSAIC_APO_01_05a","Mosaic of Saturn inner magnetosphere.  EUV and FUV low resolution slits on, aligned parallel to the Saturn spin axis.  1) Slew about the Z-axis from Saturn center to +MOS orb and rotate +64 mrad in the YZ plane. 2) Drift at a rate of .0424 mrad/sec about the Z-axis toward -MOS orb for 13900s. 3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS ORB (+/- range): 318.29 mrad"]
["2004-198T05:51:00","000T09:00:00","2004-07-16","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-198T14:51:00","008T23:31:00","2004-07-16","MIMI","SPASS Rider","Saturn","SWAURORA","Solar wind campaign","MAPS SW1 Campaign","Part of SW1 MAPS Campaign.   Image the magnetosphere and observe solar wind and pickup ions while ORS instruments make simultaneous observations of Saturns aurora, CAPS observes the solar wind, and RPWS observes SKR. -Y to Saturn (auroral region) and -X ~ to sun."]
["2004-198T14:51:00","008T23:31:00","2004-07-16","CDA","Non-SPASS","DustRAM direction","SURVEY","Magnetospheric survey","dust survey","prograde dust, day 174: -z2E and  -x 26.9; -24.6      AM=42 (60deg from +x2NEP) geometry changes fast, -x pointing only valid at beginning in the first days."]
["2004-198T14:51:00","003T00:00:00","2004-07-16","MAG","Non-SPASS","Other","SWAURORA","Solar wind campaign","MAPS SW Aurora Campaign","SW observations in conjunction with ISS auroral observations"]
["2004-198T14:51:00","003T00:00:00","2004-07-16","RPWS","Non-SPASS","Saturn","SWAURORA","Solar wind campaign","MAPS SW1 Campaign","Part of SW1 MAPS Campaign.  Observe solar wind plasma waves and Saturn radio emissions while ORS instruments simultaneously observe Saturn's aurora and other MAPS observe solar wind conditions."]
["2004-198T16:16:00","000T10:30:00","2004-07-16","UVIS","Prime","Saturn","AURORAA","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 10.5 hours.  A similar request (auroralB) is identical except it repeats for 5.0 hours."]
["2004-198T16:16:00","000T10:30:00","2004-07-16","CIRS","SPASS Rider","Saturn","SPTEMPL10","South pole imaging","Saturn South Pole Template","Saturn south pole"]
["2004-198T16:16:00","000T10:30:00","2004-07-16","ISS","SPASS Rider","Saturn","AURORAA","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-198T16:30:00","000T04:33:30","2004-07-16","CAPS","Non-SPASS","Saturn","BURST8K","8 kbps burst","Burst of 8kbps data","Burst of 8 kbps data (which gives uncollapsed ELS data). 64 B cycles duration. Data is in addition to 2000 bps from SWSKR."]
["2004-198T23:00:00","000T00:23:00","2004-07-16","INMS","Non-SPASS","Saturn","MRO","Instrument memory readout","Memory Dump","Ride with prime instrument"]
["2004-198T23:23:00","000T22:58:00","2004-07-16","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","Ride with prime instrument"]
["2004-199T02:46:00","000T04:55:00","2004-07-17","UVIS","Prime","Saturn","MOS00WB","Apoapsis mosaic","MOSAIC_APO_01_05b","Mosaic of Saturn inner magnetosphere.  EUV and FUV low resolution slits on, aligned parallel to the Saturn spin axis.  1) Slew about the Z-axis from Saturn Center to +MOS orb. 2) Drift at a rate of .0410 mrad/sec about the Z-axis toward -MOS orb for 15000s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS ORB (+/- RANGE): 307.25 mrad."]
["2004-199T07:41:00","000T05:00:00","2004-07-17","UVIS","Prime","Saturn","AURORAB","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 5 hours.  A similar request (auroralA) is identical except it repeats for 10.5 hours."]
["2004-199T07:41:00","000T05:00:00","2004-07-17","CIRS","SPASS Rider","Saturn","SPTEMPL05","South pole imaging","Saturn South Pole Template","Saturn south pole"]
["2004-199T07:41:00","000T05:00:00","2004-07-17","ISS","SPASS Rider","Saturn","AURORAB","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-199T13:21:00","000T09:00:00","2004-07-17","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-199T22:21:00","001T00:00:00","2004-07-17","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","Ride with prime instrument"]
["2004-199T23:41:00","000T02:25:00","2004-07-17","UVIS","Prime","Saturn","MOS00WB","Apoapsis mosaic","MOSAIC_APO_01_05c","Mosaic of Saturn inner magnetosphere.  EUV and FUV low resolution slits on, aligned parallel to the Saturn spin axis.  1) Slew about the Z-axis from Saturn Center to +MOS orb and rotate -64mrad in the YZ plane. 2) Drift at a rate of .0399 mrad/sec about the Z-axis in the direction toward -MOS orb for 6700s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time.  MOS orb (+/- range): 299.22 mrad"]
["2004-200T02:06:00","000T10:30:00","2004-07-18","UVIS","Prime","Saturn","AURORAA","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 10.5 hours.  A similar request (auroralB) is identical except it repeats for 5.0 hours."]
["2004-200T02:06:00","000T10:30:00","2004-07-18","ISS","SPASS Rider","Saturn","AURORAA","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-200T13:21:00","000T09:00:00","2004-07-18","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-200T22:21:00","000T00:23:00","2004-07-18","INMS","Non-SPASS","Saturn","MRO","Instrument memory readout","Memory Dump","Ride with prime instrument"]
["2004-200T22:44:00","001T23:37:00","2004-07-18","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","Ride with prime instrument"]
["2004-200T23:51:00","000T01:00:00","2004-07-18","ISS","Prime","Iapetus","SOUTHHEMH","Southern hemisphere imaging","Iapetus terra incognita (south hem) obs.","Turn -Y to Iapetus; Do 1x1 mosaic 8 NAC clear + 9 NAC color + 6 NAC polarizer + 15 WAC color filters"]
["2004-200T23:51:00","000T01:00:00","2004-07-18","UVIS","SPASS Rider","Iapetus","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2004-200T23:51:00","000T01:00:00","2004-07-18","VIMS","SPASS Rider","Iapetus","SOUTHHEMH","Southern hemisphere imaging","Iapetus southern hemisphere","Multiple 640ms 12x12 cubes"]
["2004-201T00:51:00","000T04:25:00","2004-07-19","UVIS","Prime","Saturn","MOS00WC","Apoapsis mosaic","MOSAIC_APO_01_05d","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel to the Saturn spin axis. 1) Slew about the Z-axis from Saturn Center to -MOS orb and rotate +64mrad in the YZ plane. 2) Drift at a rate of .0387 mrad/sec about the Z-axis toward +MOS orb for 13900s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS orb (+/- range): 290.44 mrad."]
["2004-201T05:51:00","000T09:00:00","2004-07-19","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-201T14:51:00","002T23:45:00","2004-07-19","MAG","Non-SPASS","Other","SWAURORA","Solar wind campaign","MAPS SW Aurora Campaign","SW observations in conjunction with ISS auroral observations"]
["2004-201T14:51:00","002T23:45:00","2004-07-19","RPWS","Non-SPASS","Saturn","SWAURORA","Solar wind campaign","MAPS SW1 Campaign","Part of SW1 MAPS Campaign.  Observe solar wind plasma waves and Saturn radio emissions while ORS instruments simultaneously observe Saturn's aurora and other MAPS observe solar wind conditions."]
["2004-201T16:16:00","000T10:30:00","2004-07-19","UVIS","Prime","Saturn","AURORAA","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It uses the GENMOS_P module. It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 10.5 hours.  A similar request (auroralB) is identical except it repeats for 5.0 hours."]
["2004-201T16:16:00","000T10:30:00","2004-07-19","CIRS","SPASS Rider","Saturn","SPTEMPL10","South pole imaging","Saturn South Pole Template","Saturn south pole"]
["2004-201T16:16:00","000T10:30:00","2004-07-19","ISS","SPASS Rider","Saturn","AURORAA","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-201T16:30:00","000T04:33:30","2004-07-19","CAPS","Non-SPASS","Saturn","BURST8K","8 kbps burst","Burst of 8kbps data","Burst of 8 kbps data (which gives uncollapsed ELS data). 64 B cycles duration. Data is in addition to 2000 bps from SWSKR."]
["2004-202T02:46:00","000T04:55:00","2004-07-20","UVIS","Prime","Saturn","MOS00WC","Apoapsis mosaic","MOSAIC_APO_01_06","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel to the Saturn spin axis. 1) Slew about the Z-axis from Saturn center to -MOS orb. 2) Drift at a rate of .0376 mrad/sec about the Z-axis to +MOS orb for 15000s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS orb (+/- range): 282.29 mrad."]
["2004-202T02:46:00","000T09:55:00","2004-07-20","VIMS","SPASS Rider","Saturn","SATURN","Saturn global map",null,"Saturn Global"]
["2004-202T07:41:00","000T05:00:00","2004-07-20","UVIS","Prime","Saturn","AURORAB","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It uses the GENMOS_P module. It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 5 hours.  A similar request (auroralA) is identical except it repeats for 10.5 hours."]
["2004-202T07:41:00","000T05:00:00","2004-07-20","CIRS","SPASS Rider","Saturn","SPTEMPL05","South pole imaging","Saturn South Pole Template","Saturn south pole"]
["2004-202T07:41:00","000T05:00:00","2004-07-20","ISS","SPASS Rider","Saturn","AURORAB","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-202T13:06:00","000T09:00:00","2004-07-20","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-202T14:41:00","000T06:00:00","2004-07-20","CIRS","SPASS Rider","InstrumentCalibration","DSCALTMP","Deep space calibration","Deep space cal","Saturn south pole"]
["2004-202T21:32:00","004T16:50:00","2004-07-20","CAPS","SPASS Rider","Saturn","SWAURORA","Solar wind campaign","MAPS SW1 Campaign","Part of SW1 MAPS Campaign.  Observe solar wind while ORS instruments simultaneously observer Saturn's aurora"]
["2004-202T22:21:00","000T00:23:00","2004-07-20","INMS","Non-SPASS","Saturn","MRO","Instrument memory readout","Memory Dump","Ride with prime instrument"]
["2004-202T22:44:00","001T23:37:00","2004-07-20","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","Ride with prime instrument"]
["2004-202T23:41:00","000T02:25:00","2004-07-20","UVIS","Prime","Saturn","MOS00WC","Apoapsis mosaic","MOSAIC_APO_01_06a","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel to the Saturn spin axis. 1) Slew about the Z-axis from Saturn Center to -MOS orb and rotate -64mrad in the YZ plane. 2) Drift at a rate of .0368 mrad/sec about the Z-axis toward +MOS orb for 6700s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS ORB (+/- range): 276.28 mrad."]
["2004-203T02:06:00","000T10:30:00","2004-07-21","UVIS","Prime","Saturn","AURORAA","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 10.5 hours.  A similar request (auroralB) is identical except it repeats for 5.0 hours."]
["2004-203T02:06:00","000T10:30:00","2004-07-21","ISS","SPASS Rider","Saturn","AURORAA","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-203T13:06:00","000T09:00:00","2004-07-21","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-203T23:36:00","000T01:00:00","2004-07-21","ISS","Prime","Iapetus","SOUTHHEMK","Southern hemisphere imaging","Iapetus terra incognita (south hem) obs.","Turn -Y to Iapetus; Do 1x1 mosaic NAC clear + 4 NAC color + NAC polarizer filters."]
["2004-203T23:36:00","000T01:00:00","2004-07-21","UVIS","SPASS Rider","Iapetus","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2004-204T00:36:00","000T04:25:00","2004-07-22","UVIS","Prime","Saturn","MOS00WD","Apoapsis mosaic","MOSAIC_APO_01_06b","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel to the Saturn spin axis. 1) Slew about the Z-axis from Saturn center to +MOS orb.  2) Drift at a rate of .0360 mrad/sec about the Z-axis toward -MOS orb for 13900s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS orb (+/- range): 269.70."]
["2004-204T05:36:00","000T09:00:00","2004-07-22","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-204T14:36:00","002T23:46:00","2004-07-22","MAG","Non-SPASS","Other","SWAURORA","Solar wind campaign","MAPS SW Aurora Campaign","SW observations in conjunction with ISS auroral observations"]
["2004-204T14:36:00","002T23:46:00","2004-07-22","RPWS","Non-SPASS","Saturn","SWAURORA","Solar wind campaign","MAPS SW1 Campaign","Part of SW1 MAPS Campaign.  Observe solar wind plasma waves and Saturn radio emissions while ORS instruments simultaneously observe Saturn's aurora and other MAPS observe solar wind conditions."]
["2004-204T16:01:00","000T10:30:00","2004-07-22","UVIS","Prime","Saturn","AURORAA","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It uses the GENMOS_P module. It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 10.5 hours.  A similar request (auroralB) is identical except it repeats for 5.0 hours."]
["2004-204T16:01:00","000T10:30:00","2004-07-22","CIRS","SPASS Rider","Saturn","SPTEMPL10","South pole imaging","Saturn South Pole Template","Saturn south pole"]
["2004-204T16:01:00","000T10:30:00","2004-07-22","ISS","SPASS Rider","Saturn","AURORAA","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-204T16:30:00","000T06:51:00","2004-07-22","CAPS","Non-SPASS","Saturn","BURST8K","8 kbps burst","Burst of 8kbps data","Burst of 8 kbps data (which gives uncollapsed ELS data). 96 B cycles duration. Data is in addition to 2000 bps from SWSKR."]
["2004-204T22:21:00","000T00:23:00","2004-07-22","INMS","Non-SPASS","Saturn","MRO","Instrument memory readout","Memory Dump","Ride with prime instrument"]
["2004-204T22:44:00","001T23:37:00","2004-07-22","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","Ride with prime instrument"]
["2004-205T02:31:00","000T04:55:00","2004-07-23","UVIS","Prime","Saturn","MOS00WD","Apoapsis mosaic","MOSAIC_APO_01_06c","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel to the Saturn spin axis. 1) Slew about the Z axis to +MOS orb and rotate -64mrad in the YZ plane from Saturn Center. 2) Drift at a rate of .0351 mrad/sec about the Z-axis toward -MOS orb for 15000s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS orb (+/- range): 263.45 mrad."]
["2004-205T02:31:00","000T09:55:00","2004-07-23","VIMS","SPASS Rider","Saturn","SATURN","Saturn global map",null,"Saturn Far Encounter Global Mosaic #5"]
["2004-205T07:26:00","000T05:00:00","2004-07-23","UVIS","Prime","Saturn","AURORAB","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It uses the GENMOS_P module. It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 5 hours.  A similar request (auroralA) is identical except it repeats for 10.5 hours."]
["2004-205T07:26:00","000T05:00:00","2004-07-23","CIRS","SPASS Rider","Saturn","SPTEMPL05","South pole imaging","Saturn South Pole Template","Saturn south pole"]
["2004-205T07:26:00","000T05:00:00","2004-07-23","ISS","SPASS Rider","Saturn","AURORAB","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-205T12:52:00","000T09:00:00","2004-07-23","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-205T14:26:00","000T06:00:00","2004-07-23","CIRS","SPASS Rider","InstrumentCalibration","DSCALTMP","Deep space calibration","Deep space cal","Saturn south pole"]
["2004-205T23:26:00","000T02:25:00","2004-07-23","UVIS","Prime","Saturn","MOS00WD","Apoapsis mosaic","MOSAIC_APO_01_06d","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel to the Saturn spin axis. 1) Slew about Z to +MOS ORB and rotate +64 mrad in the YZ plane from Saturn Center 2) Drift at a rate of .0345 mrad/sec about the Z-axis in the direction of -MOS Orb for 6700s. 3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time.  MOS Orb (+/-Range): 258.81 mrad"]
["2004-206T01:51:00","000T10:30:00","2004-07-24","UVIS","Prime","Saturn","AURORAA","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It uses the GENMOS_P module. It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 10.5 hours.  A similar request (auroralB) is identical except it repeats for 5.0 hours."]
["2004-206T01:51:00","000T10:30:00","2004-07-24","ISS","SPASS Rider","Saturn","AURORAA","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-206T12:52:00","000T09:00:00","2004-07-24","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-206T22:21:00","000T00:23:00","2004-07-24","INMS","Non-SPASS","Saturn","MRO","Instrument memory readout","Memory Dump","Ride with prime instrument"]
["2004-206T22:44:00","001T23:37:00","2004-07-24","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","Ride with prime instrument"]
["2004-206T23:22:00","000T01:00:00","2004-07-24","ISS","Prime","Iapetus","SOUTHHEMN","Southern hemisphere imaging","Iapetus terra incognita (south hem) obs.","Turn -Y to Iapetus; Do 1x1 mosaic NAC clear + NAC color + NAC polarizer filters"]
["2004-206T23:22:00","000T01:00:00","2004-07-24","UVIS","SPASS Rider","Iapetus","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2004-207T00:22:00","000T04:25:00","2004-07-25","UVIS","Prime","Saturn","MOS00WE","Apoapsis mosaic","MOSAIC_APO_01_06e","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned with Saturn spin axis. 1) Slew about Z to -MOS Orb from Saturn Center 2) Drift at a rate of .0338 mrad/sec about the Z-axis in the direction of +MOS orb for 13900s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time.  MOS Orb (+/- Range): 253.67 mrad"]
["2004-207T05:22:00","000T09:00:00","2004-07-25","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-207T14:22:00","004T13:10:00","2004-07-25","CAPS","SPASS Rider","Saturn","SWAURORA","Solar wind campaign","MAPS SW1 Campaign","Part of SW1 MAPS Campaign.  Observe solar wind while ORS instruments simultaneously observer Saturn's aurora"]
["2004-207T14:22:00","002T23:45:00","2004-07-25","MIMI","SPASS Rider","Saturn","SWAURORA","Solar wind campaign","MAPS SW1 Campaign","Part of SW1 MAPS Campaign.   Image the magnetosphere and observe solar wind and pickup ions while ORS instruments make simultaneous observations of Saturns aurora, CAPS observes the solar wind, and RPWS observes SKR. -Y to Saturn (auroral region) and -X ~ to sun."]
["2004-207T14:22:00","005T07:09:59","2004-07-25","CDA","Non-SPASS","DustRAM direction","SURVEY","Magnetospheric survey","new (sponge bits)","prograde dust, day 174: -z2E and  -x 26.9; -24.6      AM=42 (60deg from +x2NEP) geometry changes fast, -x pointing only valid at beginning in the first days."]
["2004-207T14:22:00","004T13:10:00","2004-07-25","MAG","Non-SPASS","Other","SWAURORA","Solar wind campaign","MAPS SW Aurora Campaign","SW observations in conjunction with ISS auroral observations"]
["2004-207T14:22:00","004T13:10:00","2004-07-25","RPWS","Non-SPASS","Saturn","SWAURORA","Solar wind campaign","MAPS SW1 Campaign","Part of SW1 MAPS Campaign.  Observe solar wind plasma waves and Saturn radio emissions while ORS instruments simultaneously observe Saturn's aurora and other MAPS observe solar wind conditions."]
["2004-207T15:47:00","000T10:30:00","2004-07-25","UVIS","Prime","Saturn","AURORAA","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It uses the GENMOS_P module. It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 10.5 hours.  A similar request (auroralB) is identical except it repeats for 5.0 hours."]
["2004-207T15:47:00","000T10:30:00","2004-07-25","CIRS","SPASS Rider","Saturn","SPTEMPL10","South pole imaging","Saturn South Pole Template","Saturn south pole"]
["2004-207T15:47:00","000T10:30:00","2004-07-25","ISS","SPASS Rider","Saturn","AURORAA","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-208T02:17:00","000T04:55:00","2004-07-26","UVIS","Prime","Saturn","MOS00WE","Apoapsis mosaic","MOSAIC_APO_01_06f","Mosaic of Saturn inner magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with the Saturn spin axis. 1) Slew about Z to -MOS Orb   and -64 mrad in the YZ plane from Saturn Center.  2) Drift at a rate of .0332 mrad/sec about the Z-axis toward +MOS Orb for 15000s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 248.77 mrad."]
["2004-208T07:12:00","000T05:00:00","2004-07-26","UVIS","Prime","Saturn","AURORAB","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It uses the GENMOS_P module. It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 5 hours.  A similar request (auroralA) is identical except it repeats for 10.5 hours."]
["2004-208T07:12:00","000T05:00:00","2004-07-26","CIRS","SPASS Rider","Saturn","SPTEMPL05","South pole imaging","Saturn South Pole Template","Saturn south pole"]
["2004-208T07:12:00","000T05:00:00","2004-07-26","ISS","SPASS Rider","Saturn","AURORAB","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-208T12:52:00","000T09:00:00","2004-07-26","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-208T14:12:00","000T06:00:00","2004-07-26","CIRS","SPASS Rider","InstrumentCalibration","DSCALTMP","Deep space calibration","Deep space cal","Saturn south pole"]
["2004-208T22:21:00","000T00:23:00","2004-07-26","INMS","Non-SPASS","Saturn","MRO","Instrument memory readout","Memory Dump","Ride with prime instrument"]
["2004-208T22:44:00","001T23:37:00","2004-07-26","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","Ride with prime instrument"]
["2004-208T23:12:00","000T02:25:00","2004-07-26","UVIS","Prime","Saturn","MOS00WE","Apoapsis mosaic","MOSAIC_APO_01_06g","Mosaic of Saturn inner magnetosphere.  EUV and FUV low resolution slits on, aligned parallel to Saturn spin axis.  1) Slew about Z to -MOS Orb and rotate +64mrad in the YZ plane from Saturn Center.  2) Drift at a rate of .0327 mrad/sec about the Z-axis toward +MOS orb for 6700s. 3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time.  MOS Orb (+/-Range): 245.09 mrad."]
["2004-209T01:37:00","000T10:30:00","2004-07-27","UVIS","Prime","Saturn","AURORAA","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It uses the GENMOS_P module. It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 10.5 hours.  A similar request (auroralB) is identical except it repeats for 5.0 hours."]
["2004-209T01:37:00","000T10:30:00","2004-07-27","ISS","SPASS Rider","Saturn","AURORAA","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-209T12:52:00","000T09:00:00","2004-07-27","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-209T23:22:00","000T01:00:00","2004-07-27","ISS","Prime","Iapetus","TRAILSIDA","Satellite trail side imaging","Iapetus early trailing side obs.","Turn -Y to Iapetus; Do 1x1 mosaic 2 NAC clear filters; Turn to WP."]
["2004-209T23:22:00","000T01:00:00","2004-07-27","UVIS","SPASS Rider","Iapetus","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2004-210T00:22:00","000T04:25:00","2004-07-28","UVIS","Prime","Saturn","MOS00WF","Apoapsis mosaic","MOSAIC_APO_01_06h","Mosaic of Saturn inner magnetosphere.  EUV and FUV low resolution slits on, aligned parallel to the Saturn spin axis.  1) Slew about Z to +MOS Orb and rotate -64mrad in the YZ plane from Saturn Center.  2) Drift at a rate of .0321 mrad/sec about the Z-axis toward -MOS Orb for 13900s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/- Range): 240.97 mrad"]
["2004-210T05:07:00","000T09:00:00","2004-07-28","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-210T14:07:00","001T13:25:00","2004-07-28","MIMI","SPASS Rider","Saturn","SWAURORA","Solar wind campaign","MAPS SW1 Campaign","Part of SW1 MAPS Campaign.   Image the magnetosphere and observe solar wind and pickup ions while ORS instruments make simultaneous observations of Saturns aurora, CAPS observes the solar wind, and RPWS observes SKR. -Y to Saturn (auroral region) and -X ~ to sun."]
["2004-210T15:47:00","000T10:30:00","2004-07-28","UVIS","Prime","Saturn","AURORAA","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It uses the GENMOS_P module. It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 10.5 hours.  A similar request (auroralB) is identical except it repeats for 5.0 hours."]
["2004-210T15:47:00","000T10:30:00","2004-07-28","CIRS","SPASS Rider","Saturn","SPTEMPL10","South pole imaging","Saturn South Pole Template","Saturn south pole"]
["2004-210T15:47:00","000T10:30:00","2004-07-28","ISS","SPASS Rider","Saturn","AURORAA","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-210T22:21:00","000T00:23:00","2004-07-28","INMS","Non-SPASS","Saturn","MRO","Instrument memory readout","Memory Dump","Ride with prime instrument"]
["2004-210T22:44:00","001T22:25:00","2004-07-28","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","Ride with prime instrument"]
["2004-211T02:17:00","000T04:55:00","2004-07-29","UVIS","Prime","Saturn","MOS00WF","Apoapsis mosaic","MOSAIC_APO_01_06i","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel to the Saturn spin axis.  1) Slew about Z to +MOS Orb from Saturn Center. 2) Drift at a rate of .0316 mrad/sec about the Z-axis toward -MOS Orb for 15000s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time.  MOS Orb (+/- Range): 237.05mrad"]
["2004-211T07:12:00","000T05:00:00","2004-07-29","UVIS","Prime","Saturn","AURORAB","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It uses the GENMOS_P module. It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 5 hours.  A similar request (auroralA) is identical except it repeats for 10.5 hours."]
["2004-211T07:12:00","000T05:00:00","2004-07-29","CIRS","SPASS Rider","Saturn","SPTEMPL05","South pole imaging","Saturn South Pole Template","Saturn south pole"]
["2004-211T07:12:00","000T05:00:00","2004-07-29","ISS","SPASS Rider","Saturn","AURORAB","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-211T12:12:00","000T02:25:00","2004-07-29","UVIS","Prime","Saturn","MOS00WF","Apoapsis mosaic","MOSAIC_APO_01_06l","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with the Saturn spin axis.  1) Slew about Z to +MOS Orb and rotate +64mrad in the YZ plane from Saturn Center. 2) Drift at a rate of .0312 mrad/sec about the Z-axis toward -MOS Orb for 6700s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 234.10mrad"]
["2004-211T14:37:00","000T10:30:00","2004-07-29","UVIS","Prime","Saturn","AURORAA","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It uses the GENMOS_P module. It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 10.5 hours.  A similar request (auroralB) is identical except it repeats for 5.0 hours."]
["2004-211T14:37:00","000T10:30:00","2004-07-29","ISS","SPASS Rider","Saturn","AURORAA","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-212T03:32:00","000T18:00:00","2004-07-30","CAPS","SPASS Rider","Saturn","SWAURORA","Solar wind campaign","MAPS SW1 Campaign","Part of SW1 MAPS Campaign.  Observe solar wind while ORS instruments simultaneously observer Saturn's aurora"]
["2004-212T03:32:00","000T18:00:00","2004-07-30","MIMI","SPASS Rider","Saturn","SWAURORA","Solar wind campaign","MAPS SW1 Campaign","Part of SW1 MAPS Campaign.   Image the magnetosphere and observe solar wind and pickup ions while ORS instruments make simultaneous observations of Saturns aurora, CAPS observes the solar wind, and RPWS observes SKR. -Y to Saturn (auroral region) and -X ~ to sun."]
["2004-212T03:32:00","000T18:00:00","2004-07-30","MAG","Non-SPASS","Other","SWAURORA","Solar wind campaign","MAPS SW Aurora Campaign","SW observations in conjunction with ISS auroral observations"]
["2004-212T03:32:00","000T18:00:00","2004-07-30","RPWS","Non-SPASS","Saturn","SWAURORA","Solar wind campaign","MAPS SW1 Campaign","Part of SW1 MAPS Campaign.  Observe solar wind plasma waves and Saturn radio emissions while ORS instruments simultaneously observe Saturn's aurora and other MAPS observe solar wind conditions."]
["2004-212T03:32:00","000T09:00:00","2004-07-30","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-212T05:32:00","000T06:00:00","2004-07-30","CIRS","SPASS Rider","InstrumentCalibration","DSCALTMP","Deep space calibration","Deep space cal","Saturn south pole"]
["2004-212T12:32:00","000T09:00:00","2004-07-30","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-212T21:09:00","000T00:23:00","2004-07-30","INMS","Non-SPASS","Saturn","MRO","Instrument memory readout","Memory Dump","Ride with prime instrument"]
["2004-212T21:32:00","005T14:01:00","2004-07-30","CAPS","SPASS Rider","Saturn","SWAURORA","Solar wind campaign","MAPS SW1 Campaign","Part of SW1 MAPS Campaign.  Observe solar wind while ORS instruments simultaneously observer Saturn's aurora"]
["2004-212T21:32:00","001T13:20:00","2004-07-30","MIMI","SPASS Rider","Saturn","SWAURORA","Solar wind campaign","MAPS SW1 Campaign","Part of SW1 MAPS Campaign.   Image the magnetosphere and observe solar wind and pickup ions while ORS instruments make simultaneous observations of Saturns aurora, CAPS observes the solar wind, and RPWS observes SKR. -Y to Saturn (auroral region) and -X ~ to sun."]
["2004-212T21:32:00","027T18:41:00","2004-07-30","CDA","Non-SPASS","DustRAM direction","SURVEY","Magnetospheric survey","dust survey","prograde dust, day 174: -z2E and  -x 26.9; -24.6      AM=42 (60deg from +x2NEP) geometry changes fast, -x pointing only valid at beginning in the first days."]
["2004-212T21:32:00","000T01:22:00","2004-07-30","INMS","Non-SPASS","Saturn","STARTUP","Sequence startup activity","STARTUP","Startup sequence.  Load FSW, MRO, Load IEB from SSR's, MRO"]
["2004-212T21:32:00","001T13:20:00","2004-07-30","MAG","Non-SPASS","Other","SWAURORA","Solar wind campaign","MAPS SW Aurora Campaign","SW observations in conjunction with ISS auroral observations"]
["2004-212T21:32:00","001T13:20:00","2004-07-30","RPWS","Non-SPASS","Saturn","SWAURORA","Solar wind campaign","MAPS SW1 Campaign","Part of SW1 MAPS Campaign.  Observe solar wind plasma waves and Saturn radio emissions while ORS instruments simultaneously observe Saturn's aurora and other MAPS observe solar wind conditions."]
["2004-212T22:54:00","005T00:06:00","2004-07-30","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","Ride with prime instrument"]
["2004-212T23:07:00","000T01:00:00","2004-07-30","ISS","Prime","Iapetus","TRAILSIDB","Satellite trail side imaging","Iapetus early trailing side obs.","Turn -Y to Iapetus; Do 1x1 mosaic 3 NAC clear filters"]
["2004-212T23:07:00","000T01:00:00","2004-07-30","UVIS","SPASS Rider","Iapetus","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2004-213T00:07:00","000T04:25:00","2004-07-31","UVIS","Prime","Saturn","MOS00WG","Apoapsis mosaic","MOSAIC_APO_01_06M","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with the Saturn spin axis. 1) Slew about Z to -MOS Orb and rotate -64mrad in the YZ plane from Saturn Center. 2) Drift at a rate of .0308 mrad/sec about the Z-axis toward +MOS Orb for 13900s. 3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time.  MOS Orb (+/-range): 230.81mrad."]
["2004-213T05:07:00","000T09:00:00","2004-07-31","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-213T15:32:00","000T10:30:00","2004-07-31","UVIS","Prime","Saturn","AURORAA","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It uses the GENMOS_P module. It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 10.5 hours.  A similar request (auroralB) is identical except it repeats for 5.0 hours."]
["2004-213T15:32:00","000T10:30:00","2004-07-31","CIRS","SPASS Rider","Saturn","SPTEMPL10","South pole imaging","Saturn South Pole Template","Saturn south pole"]
["2004-213T15:32:00","000T10:30:00","2004-07-31","ISS","SPASS Rider","Saturn","AURORAA","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-214T02:02:00","000T04:55:00","2004-08-01","UVIS","Prime","Saturn","MOS00WG","Apoapsis mosaic","MOSAIC_APO_01_06n","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel to the Saturn spin axis. 1) Slew about Z to -MOS Orb from Saturn Center. 2) Drift at a rate of .0304 mrad/sec about the Z-axis toward +MOS Orb for 15000s. 3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time.  MOS Orb (+/-Range): 227.64mrad."]
["2004-214T06:57:00","000T03:25:00","2004-08-01","UVIS","Prime","Saturn","AURORAB","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It uses the GENMOS_P module. It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 5 hours.  A similar request (auroralA) is identical except it repeats for 10.5 hours."]
["2004-214T06:57:00","000T03:25:00","2004-08-01","CIRS","SPASS Rider","Saturn","SPTEMPL05","South pole imaging","Saturn South Pole Template","Saturn south pole"]
["2004-214T06:57:00","000T03:25:00","2004-08-01","ISS","SPASS Rider","Saturn","AURORAB","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-214T10:52:00","004T17:45:00","2004-08-01","MIMI","SPASS Rider","Saturn","SWAURORA","Solar wind campaign","MAPS SW1 Campaign","Part of SW1 MAPS Campaign.   Image the magnetosphere and observe solar wind and pickup ions while ORS instruments make simultaneous observations of Saturns aurora, CAPS observes the solar wind, and RPWS observes SKR. -Y to Saturn (auroral region) and -X ~ to sun."]
["2004-214T10:52:00","004T17:45:00","2004-08-01","MAG","Non-SPASS","Other","SWAURORA","Solar wind campaign","MAPS SW Aurora Campaign","SW observations in conjunction with ISS auroral observations"]
["2004-214T10:52:00","004T17:45:00","2004-08-01","RPWS","Non-SPASS","Saturn","SWAURORA","Solar wind campaign","MAPS SW1 Campaign","Part of SW1 MAPS Campaign.  Observe solar wind plasma waves and Saturn radio emissions while ORS instruments simultaneously observe Saturn's aurora and other MAPS observe solar wind conditions."]
["2004-214T10:52:00","000T12:00:00","2004-08-01","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-214T13:57:00","000T06:00:00","2004-08-01","CIRS","SPASS Rider","InstrumentCalibration","DSCALTMP","Deep space calibration","Deep space cal","Saturn south pole"]
["2004-214T22:52:00","000T02:00:00","2004-08-01","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-215T01:22:00","000T09:00:00","2004-08-02","UVIS","Prime","Saturn","AURORAB","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It uses the GENMOS_P module. It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 5 hours.  A similar request (auroralA) is identical except it repeats for 10.5 hours."]
["2004-215T01:22:00","000T09:00:00","2004-08-02","CIRS","SPASS Rider","Saturn","SPTEMPL05","South pole imaging","Saturn South Pole Template","Saturn south pole"]
["2004-215T01:22:00","000T09:00:00","2004-08-02","ISS","SPASS Rider","Saturn","AURORAB","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-215T10:52:00","000T06:00:00","2004-08-02","CIRS","SPASS Rider","InstrumentCalibration","DSCALTMP","Deep space calibration","Deep space cal","Saturn south pole"]
["2004-215T10:52:00","000T06:00:00","2004-08-02","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-216T00:22:00","000T01:00:00","2004-08-03","ISS","Prime","Iapetus","TRAILSIDC","Satellite trail side imaging","Iapetus early trailing side obs.","Turn -Y to Iapetus; Do 1x1 mosaic 3 NAC clear filters; turn to WP"]
["2004-216T00:22:00","000T01:00:00","2004-08-03","UVIS","SPASS Rider","Iapetus","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2004-216T01:22:00","000T01:30:00","2004-08-03","ISS","Prime","rings(general)","DIFFUSRNG","Diffuse ring observation","DIFFUSE RINGS, GO WEST TEMPLATE, 006 TH OBSERVATIO","DIFFUSE RINGS IN REV 000, GO WEST TEMPLATE DOY 215-218"]
["2004-216T03:22:00","000T12:00:00","2004-08-03","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-216T16:52:00","000T09:30:00","2004-08-03","UVIS","Prime","Saturn","AURORAA","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It uses the GENMOS_P module. It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 10.5 hours.  A similar request (auroralB) is identical except it repeats for 5.0 hours."]
["2004-216T16:52:00","000T09:30:00","2004-08-03","CIRS","SPASS Rider","Saturn","SPTEMPL05","South pole imaging","Saturn South Pole Template","Saturn south pole"]
["2004-216T16:52:00","000T09:30:00","2004-08-03","ISS","SPASS Rider","Saturn","AURORAA","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-217T02:22:00","000T08:42:00","2004-08-04","UVIS","Prime","Saturn","MOS00WH","Apoapsis mosaic","MOSAIC_APO_01_06q","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with the Saturn spin axis. 1) Slew about Z to +MOS Orb and rotate +64mrad in the YZ plane from Saturn Center. 2) Drift at a rate of .0293 mrad/sec about the Z-axis toward -MOS Orb for 15000s. 3) Rotate -64mrad in the YZ Plane.  Drift at the indicated rate about Z for 15000s toward +MOS Orb.  4) Slew back to Saturn center and reset pointing.  Stare for remaining observation time.  MOS Orb (+/-Range): 220.02mrad"]
["2004-217T11:52:00","000T11:30:00","2004-08-04","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-217T13:42:00","000T06:00:00","2004-08-04","CIRS","SPASS Rider","InstrumentCalibration","DSCALTMP","Deep space calibration","Deep space cal","Saturn south pole"]
["2004-217T23:00:00","000T00:33:00","2004-08-04","INMS","Non-SPASS","Saturn","MRO","Instrument memory readout","MAPS Survey","MAPS magnetospheric survey."]
["2004-217T23:33:00","001T15:34:00","2004-08-04","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","Ride with prime instrument"]
["2004-218T00:52:00","000T09:30:00","2004-08-05","ISS","Prime","Star","CALSTARA","Stellar Calibration","ISS Photometric Calibration Star 1","Photometric Calibration Star 1 (Vega)"]
["2004-218T00:52:00","000T09:10:00","2004-08-05","CAPS","SPASS Rider","InstrumentCalibration","CALIBRATE","Calibration","CAPS Calibration","CAPS periodic gain test and calibration. The specified rate and data volume are the delta above the CAPS solar wind campaign rate (2000 bps), and the rate is the average over the entire request (current plans are to conduct the test in two different rates.)"]
["2004-218T10:52:00","000T12:00:00","2004-08-05","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-218T11:33:00","000T17:04:00","2004-08-05","CAPS","SPASS Rider","Saturn","SWAURORA","Solar wind campaign","MAPS SW1 Campaign","Part of SW1 MAPS Campaign.  Observe solar wind while ORS instruments simultaneously observer Saturn's aurora"]
["2004-219T00:22:00","000T03:45:00","2004-08-06","ISS","Prime","Phoebe","040PHO","Spectrophotometry","Phoebe Spectrophotometry and Multi-Color","Do during 0.4 Phoebe rotations 5 1x1 mosaics (109 images)"]
["2004-219T00:22:00","000T03:45:00","2004-08-06","UVIS","SPASS Rider","Phoebe","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2004-219T04:37:00","000T09:00:00","2004-08-06","CAPS","SPASS Rider","Saturn","SWAURORA","Solar wind campaign","MAPS SW1 Campaign","Part of SW1 MAPS Campaign.  Observe solar wind while ORS instruments simultaneously observer Saturn's aurora"]
["2004-219T04:37:00","000T09:00:00","2004-08-06","MIMI","SPASS Rider","Saturn","SWAURORA","Solar wind campaign","MAPS SW1 Campaign","Part of SW1 MAPS Campaign.   Image the magnetosphere and observe solar wind and pickup ions while ORS instruments make simultaneous observations of Saturns aurora, CAPS observes the solar wind, and RPWS observes SKR. -Y to Saturn (auroral region) and -X ~ to sun."]
["2004-219T04:37:00","000T09:00:00","2004-08-06","MAG","Non-SPASS","Other","SWAURORA","Solar wind campaign","MAPS SW Aurora Campaign","SW observations in conjunction with ISS auroral observations"]
["2004-219T04:37:00","000T09:00:00","2004-08-06","RPWS","Non-SPASS","Saturn","SWAURORA","Solar wind campaign","MAPS SW1 Campaign","Part of SW1 MAPS Campaign.  Observe solar wind plasma waves and Saturn radio emissions while ORS instruments simultaneously observe Saturn's aurora and other MAPS observe solar wind conditions."]
["2004-219T04:37:00","000T09:00:00","2004-08-06","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-219T13:37:00","021T02:39:00","2004-08-06","CAPS","Non-SPASS","Saturn","SWAURORA","Solar wind campaign","MAPS solar wind/aurora campaign","MAPS magnetospheric survey"]
["2004-219T13:37:00","000T01:30:00","2004-08-06","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2004-219T13:37:00","000T09:47:00","2004-08-06","RPWS","Non-SPASS","Saturn","SWAURORA","Solar wind campaign","MAPS SW1 Campaign","Part of SW1 MAPS Campaign.  Observe solar wind plasma waves and Saturn radio emissions while ORS instruments simultaneously observe Saturn's aurora and other MAPS observe solar wind conditions."]
["2004-219T13:37:01","000T09:47:00","2004-08-06","MIMI","SPASS Rider","Saturn","SWAURORA","Solar wind campaign","MAPS SW1 Campaign","Part of SW1 MAPS Campaign.   Image the magnetosphere and observe solar wind and pickup ions while ORS instruments make simultaneous observations of Saturns aurora, CAPS observes the solar wind, and RPWS observes SKR. -Y to Saturn (auroral region) and -X ~ to sun."]
["2004-219T15:07:00","000T02:00:00","2004-08-06","UVIS","Prime","Star","ALPVIR","Alpha Virginis occultation","USTRCAL02","INSTANCE OF USTRCAL02. Stellar Calibration: alpha Virginis"]
["2004-219T15:07:00","000T02:00:00","2004-08-06","ISS","SPASS Rider","Star","ALPVIR","Alpha Virginis occultation","ISS Sensitivity monitor","Periodic standard star image to monitor ISS sensitivity"]
["2004-219T15:07:00","003T07:53:00","2004-08-06","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","Ride with prime instrument"]
["2004-219T15:07:00","000T07:53:00","2004-08-06","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2004-219T15:30:00","000T09:06:08","2004-08-06","CAPS","Non-SPASS","Saturn","BURST16K","16 kbps burst","Burst of 16kbps data","Burst of 16 kbps data (which gives uncollapsed ELS data). 128 B cycles duration. Data is in addition to 1000 bps from SWSKR."]
["2004-219T17:07:00","000T10:55:00","2004-08-06","CIRS","Prime","Saturn","MIRCMPSIT","Sit and stare to derive composition","CIRS_000SA_MIRCMPSIT","Measure oxygen compounds (CO2) in stratosphere as a function of latitude to determine whether rings are the source. Search for new stratospheric hydrocarbons (C3H4, C4H2). Determine isotopic ratios (CH3D/CH4, 12C/13C).  FP3/4 to Saturn. Z parallel to Saturn pole direction."]
["2004-219T17:07:00","000T10:55:00","2004-08-06","VIMS","SPASS Rider","Saturn","FRGLOB","Saturn far encounter global mosaic","Saturn Far Global Mosaic Early Start","Saturn Far Encounter Global Mosaic. Ride-along with CIRS."]
["2004-219T23:00:00","000T05:00:00","2004-08-06","MAG","Non-SPASS","InstrumentCalibration","SCAS","MAG SCAS instrument","MAG/SCAS_Cal","Boom alignment calibration using SCAS. If moved within scheduling window, KEEP OUTSIDE SCHEDULED MAPS CAMPAIGNS. Note: SCAS operations disturb RSS and RPWS. IF OpMode not ORS, unique sequence will be required. Includes 2 hours for IFC cal and range checks."]
["2004-219T23:24:00","020T16:51:00","2004-08-06","MIMI","SPASS Rider","Saturn","SWAURORA","Solar wind campaign","MAPS SW1 Campaign","Part of SW1 MAPS Campaign.   Image the magnetosphere and observe solar wind and pickup ions while ORS instruments make simultaneous observations of Saturns aurora, CAPS observes the solar wind, and RPWS observes SKR. -Y to Saturn (auroral region) and -X ~ to sun."]
["2004-219T23:24:00","000T14:13:00","2004-08-06","RPWS","Non-SPASS","Saturn","SWAURORA","Solar wind campaign","MAPS SW1 Campaign","Part of SW1 MAPS Campaign.  Observe solar wind plasma waves and Saturn radio emissions while ORS instruments simultaneously observe Saturn's aurora and other MAPS observe solar wind conditions."]
["2004-220T04:00:00","000T09:37:00","2004-08-07","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2004-220T04:37:00","000T09:00:00","2004-08-07","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-220T06:07:00","000T06:00:00","2004-08-07","CIRS","SPASS Rider","InstrumentCalibration","DSCALTMP","Deep space calibration","Deep space cal","Saturn south pole"]
["2004-220T13:37:00","008T07:01:00","2004-08-07","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2004-220T13:37:00","008T07:01:00","2004-08-07","RPWS","Non-SPASS","Saturn","SWAURORA","Solar wind campaign","MAPS SW1 Campaign","Part of SW1 MAPS Campaign.  Observe solar wind plasma waves and Saturn radio emissions while ORS instruments simultaneously observe Saturn's aurora and other MAPS observe solar wind conditions."]
["2004-220T15:17:00","000T10:30:00","2004-08-07","UVIS","Prime","Saturn","AURORAA","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It uses the GENMOS_P module. It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 10.5 hours.  A similar request (auroralB) is identical except it repeats for 5.0 hours."]
["2004-220T15:17:00","000T10:30:00","2004-08-07","CIRS","SPASS Rider","Saturn","SPTEMPL10","South pole imaging","Saturn South Pole Template","Saturn south pole"]
["2004-220T15:17:00","000T10:30:00","2004-08-07","ISS","SPASS Rider","Saturn","AURORAA","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-220T15:17:00","000T10:30:00","2004-08-07","VIMS","SPASS Rider","Saturn","FARGLO","Saturn far encounter global mosaic","Saturn Far Global Mosaic #16","Saturn Far Encounter Global Mosaic #7"]
["2004-221T01:47:00","000T04:55:00","2004-08-08","UVIS","Prime","Saturn","MOS00SWAA","Apoapsis mosaic","MOSAIC_APO_01_07","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with the Saturn spin axis. 1) Slew about Z to +MOS Orb from Saturn Center. 2) Drift at a rate of .0283 mrad/sec about the Z-axis toward -MOS Orb for 15000s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time.  MOS Orb (+/-Range): 212.03mrad"]
["2004-221T06:42:00","000T05:00:00","2004-08-08","UVIS","Prime","Saturn","AURORAB","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 5 hours.  A similar request (auroralA) is identical except it repeats for 10.5 hours."]
["2004-221T06:42:00","000T05:00:00","2004-08-08","CIRS","SPASS Rider","Saturn","SPTEMPL05","South pole imaging","Saturn South Pole Template","Saturn south pole"]
["2004-221T06:42:00","000T05:00:00","2004-08-08","ISS","SPASS Rider","Saturn","AURORAB","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-221T06:42:00","000T05:00:00","2004-08-08","VIMS","SPASS Rider","Saturn","FARGLO","Saturn far encounter global mosaic","Saturn Far Global Mosaic #8","Saturn Far Encounter Global Mosaic #8"]
["2004-221T12:12:00","000T08:55:00","2004-08-08","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-221T13:42:00","000T06:00:00","2004-08-08","CIRS","SPASS Rider","InstrumentCalibration","DSCALTMP","Deep space calibration","Saturn South Pole Template","Deep Space Cal"]
["2004-221T22:42:00","000T02:25:00","2004-08-08","UVIS","Prime","Saturn","MOS00SWAA","Apoapsis mosaic","MOSAIC_APO_01_07a","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with the Saturn spin axis. 1) Slew about Z to +MOS Orb from Saturn Center and rotate -64mrad in the YZ plane. 2) Drift at a rate of .0281 mrad/sec about the Z-axis toward -MOS Orb for 6700s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 210.57mrad"]
["2004-222T01:07:00","000T10:30:00","2004-08-09","UVIS","Prime","Saturn","AURORAA","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It uses the GENMOS_P module. It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 10.5 hours.  A similar request (auroralB) is identical except it repeats for 5.0 hours."]
["2004-222T01:07:00","000T10:30:00","2004-08-09","ISS","SPASS Rider","Saturn","AURORAA","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-222T01:07:00","000T10:30:00","2004-08-09","VIMS","SPASS Rider","Saturn","FARGLO","Saturn far encounter global mosaic","Saturn Far Global Mosaic #9","Saturn Far Encounter Global Mosaic #9"]
["2004-222T12:07:00","000T09:00:00","2004-08-09","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-222T22:37:00","000T01:00:00","2004-08-09","ISS","Prime","Iapetus","TRAILSIDE","Satellite trail side imaging","Iapetus early trailing side obs.","Turn -Y to Iapetus; Do 1x1 mosaic 3 NAC clear filters"]
["2004-222T22:37:00","000T01:00:00","2004-08-09","UVIS","SPASS Rider","Iapetus","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2004-222T23:00:00","000T00:33:00","2004-08-09","INMS","Non-SPASS","Saturn","MRO","Instrument memory readout","MAPS Survey","MAPS magnetospheric survey."]
["2004-222T23:33:00","004T23:27:00","2004-08-09","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","Ride with prime instrument"]
["2004-222T23:37:00","000T04:25:00","2004-08-09","UVIS","Prime","Saturn","MOS00SWAB","Apoapsis mosaic","MOSAIC_APO_01_07b","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel to the Saturn spin axis. 1) Slew about Z to -MOS Orb from Saturn Center and rotate +64mrad in the YZ plane.  2) Drift at a rate of .0279 mrad/sec about the Z-axis toward +MOS Orb for 13900s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 208.94mrad"]
["2004-222T23:37:00","000T04:25:00","2004-08-09","ISS","SPASS Rider","Saturn","MOS00SWAB","Apoapsis mosaic","UVIS Ride-along for dark images","Ride along during system scans take 5 dark images"]
["2004-223T04:32:00","000T08:50:00","2004-08-10","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-223T15:02:00","000T10:30:00","2004-08-10","UVIS","Prime","Saturn","AURORAA","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It uses the GENMOS_P module. It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 10.5 hours.  A similar request (auroralB) is identical except it repeats for 5.0 hours."]
["2004-223T15:02:00","000T10:30:00","2004-08-10","CIRS","SPASS Rider","Saturn","SPTEMPL10","South pole imaging","Saturn South Pole Template","Saturn south pole"]
["2004-223T15:02:00","000T10:30:00","2004-08-10","ISS","SPASS Rider","Saturn","AURORAA","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-223T15:02:00","000T10:30:00","2004-08-10","VIMS","SPASS Rider","Saturn","FARGLO","Saturn far encounter global mosaic","Saturn Far Global Mosaic #10","Saturn Far Encounter Global Mosaic #10"]
["2004-224T01:32:00","000T04:55:00","2004-08-11","UVIS","Prime","Saturn","MOS00SWAB","Apoapsis mosaic","MOSAIC_APO_01_07c","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with the Saturn spin axis. 1) Slew about Z to -MOS Orb from Saturn Center.  2) Drift at a rate of .0277 mrad/sec about the Z-axis toward +MOS Orb for 15000s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time.  MOS Orb(+/-Range): 207.39mrad."]
["2004-224T01:32:00","000T04:55:00","2004-08-11","ISS","SPASS Rider","Saturn","MOS00SWAB","Apoapsis mosaic","UVIS Ride-along for dark images","Ride along during system scans take 5 dark images"]
["2004-224T06:27:00","000T05:00:00","2004-08-11","UVIS","Prime","Saturn","AURORAB","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 5 hours.  A similar request (auroralA) is identical except it repeats for 10.5 hours."]
["2004-224T06:27:00","000T05:00:00","2004-08-11","CIRS","SPASS Rider","Saturn","SPTEMPL05","South pole imaging","Saturn South Pole Template","Saturn south pole"]
["2004-224T06:27:00","000T05:00:00","2004-08-11","ISS","SPASS Rider","Saturn","AURORAB","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-224T06:27:00","000T05:00:00","2004-08-11","VIMS","SPASS Rider","Saturn","FARGLO","Saturn far encounter global mosaic","Saturn Far Global Mosaic #11","Saturn Far Encounter Global Mosaic #11"]
["2004-224T11:57:00","000T08:55:00","2004-08-11","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-224T13:27:00","000T06:00:00","2004-08-11","CIRS","SPASS Rider","InstrumentCalibration","DSCALTMP","Deep space calibration","Saturn South Pole Template","Deep Space Cal"]
["2004-224T22:27:00","000T02:25:00","2004-08-11","UVIS","Prime","Saturn","MOS00SWAB","Apoapsis mosaic","MOSAIC_APO_01_07d","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with the Saturn spin axis. 1) Slew about Z to -MOS Orb from Saturn Center and rotate -64mrad in the YZ plane. 2) Drift at a rate of .0277 mrad/sec about the Z-axis toward +MOS Orb for 6700s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 204.93mrad"]
["2004-225T00:52:00","000T10:30:00","2004-08-12","UVIS","Prime","Saturn","AURORAA","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It uses the GENMOS_P module. It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 10.5 hours.  A similar request (auroralB) is identical except it repeats for 5.0 hours."]
["2004-225T00:52:00","000T10:30:00","2004-08-12","ISS","SPASS Rider","Saturn","AURORAA","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-225T00:52:00","000T10:30:00","2004-08-12","VIMS","SPASS Rider","Saturn","FARGLO","Saturn far encounter global mosaic","Saturn Far Global Mosaic #12","Saturn Far Encounter Global Mosaic #12"]
["2004-225T11:52:00","000T09:00:00","2004-08-12","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-225T22:22:00","000T01:00:00","2004-08-12","ISS","Prime","rings(general)","DIFFUSRNG","Diffuse ring observation","DIFFUSE RINGS, GO WEST TEMPLATE, 001 TH OBSERVATIO","DIFFUSE RINGS IN REV 000, GO WEST TEMPLATE"]
["2004-225T22:22:00","000T01:00:00","2004-08-12","CIRS","SPASS Rider","rings(general)","DIFFUSRNG","Diffuse ring observation","Diffuse Rings, Go West Template Ridealong","Ridealong on ISS diffuse rings, Go West Template"]
["2004-225T23:22:00","000T04:25:00","2004-08-12","UVIS","Prime","Saturn","MOS00SWAC","Apoapsis mosaic","MOSAIC_APO_01_07e","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel to the Saturn spin axis.  1) Slew about Z to +MOS Orb from Saturn Center. 2) Drift at a rate of .0273 mrad/sec about the Z-axis towarad -MOS Orb for 13900s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 204.93mrad"]
["2004-225T23:22:00","000T04:25:00","2004-08-12","ISS","SPASS Rider","Saturn","MOS00SWAC","Apoapsis mosaic","UVIS Ride-along for dark images","Ride along during system scans take 5 dark images"]
["2004-226T04:17:00","000T09:00:00","2004-08-13","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-226T14:47:00","000T10:30:00","2004-08-13","UVIS","Prime","Saturn","AURORAA","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It uses the GENMOS_P module. It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 10.5 hours.  A similar request (auroralB) is identical except it repeats for 5.0 hours."]
["2004-226T14:47:00","000T10:30:00","2004-08-13","CIRS","SPASS Rider","Saturn","SPTEMPL10","South pole imaging","Saturn South Pole Template","Saturn south pole"]
["2004-226T14:47:00","000T10:30:00","2004-08-13","ISS","SPASS Rider","Saturn","AURORAA","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-226T14:47:00","000T10:30:00","2004-08-13","VIMS","SPASS Rider","Saturn","FARGLO","Saturn far encounter global mosaic","Saturn Far Global Mosaic #13","Saturn Far Encounter Global Mosaic #13"]
["2004-227T01:17:00","000T04:55:00","2004-08-14","UVIS","Prime","Saturn","MOS00SWAC","Apoapsis mosaic","MOSAIC_APO_01_07f","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel to the Saturn spin axis.  1) Slew about Z to +MOS Orb from Saturn Center and rotate +64mrad in the YZ plane. 2) Drift at a rate of .0271 mrad/sec about the Z-axis toward -MOS Orb for 15000s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 203.70mrad."]
["2004-227T01:17:00","000T04:55:00","2004-08-14","ISS","SPASS Rider","Saturn","MOS00SWAC","Apoapsis mosaic","UVIS Ride-along for dark images","Ride along during system scans take 5 dark images"]
["2004-227T06:12:00","000T05:00:00","2004-08-14","UVIS","Prime","Saturn","AURORAB","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 5 hours.  A similar request (auroralA) is identical except it repeats for 10.5 hours."]
["2004-227T06:12:00","000T05:00:00","2004-08-14","CIRS","SPASS Rider","Saturn","SPTEMPL05","South pole imaging","Saturn South Pole Template","Saturn south pole"]
["2004-227T06:12:00","000T05:00:00","2004-08-14","ISS","SPASS Rider","Saturn","AURORAB","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-227T06:12:00","000T05:00:00","2004-08-14","VIMS","SPASS Rider","Saturn","FARGLO","Saturn far encounter global mosaic","Saturn Far Global Mosaic #14","Saturn Far Encounter Global Mosaic #14"]
["2004-227T11:42:00","000T09:00:00","2004-08-14","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-227T13:12:00","000T06:00:00","2004-08-14","CIRS","SPASS Rider","InstrumentCalibration","DSCALTMP","Deep space calibration","Saturn South Pole Template","Deep Space Cal"]
["2004-227T22:12:00","000T02:25:00","2004-08-14","UVIS","Prime","Saturn","MOS00SWAC","Apoapsis mosaic","MOSAIC_APO_01_07g","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel to the Saturn spin axis. 1) Slew about Z to +MOS Orb from Saturn Center and rotate -64mrad in the YZ plane. 2) Drift at a rate of .0270 mrad/sec about the Z-axis toward -MOS Orb for 6700s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 202.79mrad."]
["2004-227T23:00:00","000T00:33:00","2004-08-14","INMS","Non-SPASS","Saturn","MRO","Instrument memory readout","MAPS Survey","MAPS magnetospheric survey."]
["2004-227T23:33:00","004T23:27:00","2004-08-14","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","Ride with prime instrument"]
["2004-228T00:37:00","000T10:30:00","2004-08-15","UVIS","Prime","Saturn","AURORAA","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It uses the GENMOS_P module. It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 10.5 hours.  A similar request (auroralB) is identical except it repeats for 5.0 hours."]
["2004-228T00:37:00","000T10:30:00","2004-08-15","ISS","SPASS Rider","Saturn","AURORAA","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-228T00:37:00","000T10:30:00","2004-08-15","VIMS","SPASS Rider","Saturn","FARGLO","Saturn far encounter global mosaic","Saturn Far Global Mosaic #15","Saturn Far Encounter Global Mosaic #15"]
["2004-228T11:38:00","000T09:00:00","2004-08-15","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-228T20:38:00","000T16:25:00","2004-08-15","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2004-228T20:38:00","000T16:25:00","2004-08-15","RPWS","Non-SPASS","Saturn","SWAURORA","Solar wind campaign","MAPS SW1 Campaign","Part of SW1 MAPS Campaign.  Observe solar wind plasma waves and Saturn radio emissions while ORS instruments simultaneously observe Saturn's aurora and other MAPS observe solar wind conditions."]
["2004-228T22:08:00","000T01:00:00","2004-08-15","ISS","Prime","rings(general)","DIFFUSRNG","Diffuse ring observation","DIFFUSE RINGS, GO WEST TEMPLATE, 002 TH OBSERVATIO","DIFFUSE RINGS IN REV 000, GO WEST TEMPLATE"]
["2004-228T22:08:00","000T01:00:00","2004-08-15","CIRS","SPASS Rider","rings(general)","DIFFUSRNG","Diffuse ring observation","Diffuse Rings, Go West Template Ridealong","Ridealong on ISS diffuse rings, Go West Template"]
["2004-228T22:30:00","000T06:49:36","2004-08-15","CAPS","Non-SPASS","Saturn","BURST16K","16 kbps burst","Burst of 16kbps data","Burst of 16 kbps data (which gives uncollapsed ELS data). 96 B cycles duration. Data is in addition to 1000 bps from SWSKR."]
["2004-228T23:08:00","000T04:25:00","2004-08-15","UVIS","Prime","Saturn","MOS00SWAD","Apoapsis mosaic","MOSAIC_APO_01_07h","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with the Saturn spin axis. 1) Slew about Z to -MOS Orb from Saturn Center. 2) Drift at a rate of .0269 mrad/sec about the Z-axis toward +MOS Orb for 13900s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 201.79mrad."]
["2004-228T23:08:00","000T04:25:00","2004-08-15","ISS","SPASS Rider","Saturn","MOS00SWAD","Apoapsis mosaic","UVIS Ride-along for dark images","Ride along during system scans take 5 dark images"]
["2004-229T04:03:00","000T09:00:00","2004-08-16","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-229T05:33:00","000T06:00:00","2004-08-16","CIRS","SPASS Rider","InstrumentCalibration","DSCALTMP","Deep space calibration","Deep Space Calibration","Deep Space Cal"]
["2004-229T13:03:00","005T07:20:00","2004-08-16","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2004-229T13:03:00","005T07:20:00","2004-08-16","RPWS","Non-SPASS","Saturn","SWAURORA","Solar wind campaign","MAPS SW1 Campaign","Part of SW1 MAPS Campaign.  Observe solar wind plasma waves and Saturn radio emissions while ORS instruments simultaneously observe Saturn's aurora and other MAPS observe solar wind conditions."]
["2004-229T14:33:00","000T10:30:00","2004-08-16","UVIS","Prime","Saturn","AURORAA","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It uses the GENMOS_P module. It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 10.5 hours.  A similar request (auroralB) is identical except it repeats for 5.0 hours."]
["2004-229T14:33:00","000T10:30:00","2004-08-16","CIRS","SPASS Rider","Saturn","SPTEMPL10","South pole imaging","Saturn South Pole Template","Saturn south pole"]
["2004-229T14:33:00","000T10:30:00","2004-08-16","ISS","SPASS Rider","Saturn","AURORAA","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-229T14:33:00","000T10:30:00","2004-08-16","VIMS","SPASS Rider","Saturn","FARGLO","Saturn far encounter global mosaic","Saturn Far Global Mosaic #16","Saturn Far Encounter Global Mosaic #16"]
["2004-230T01:03:00","000T04:55:00","2004-08-17","UVIS","Prime","Saturn","MOS00SWAD","Apoapsis mosaic","MOSAIC_APO_01_07i","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel to the Saturn spin axis. 1) Slew about Z to -MOS Orb from Saturn center and rotate -64mrad in YZ plane.  2) Drift at a rate of .0268 mrad/sec about the Z-axis toward +MOS Orb for 15000s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb(+/-Range): 200.85mrad."]
["2004-230T01:03:00","000T04:55:00","2004-08-17","ISS","SPASS Rider","Saturn","MOS00SWAD","Apoapsis mosaic","UVIS Ride-along for dark images","Ride along during system scans take 5 dark images"]
["2004-230T05:58:00","000T05:00:00","2004-08-17","UVIS","Prime","Saturn","AURORAB","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 5 hours.  A similar request (auroralA) is identical except it repeats for 10.5 hours."]
["2004-230T05:58:00","000T05:00:00","2004-08-17","CIRS","SPASS Rider","Saturn","SPTEMPL05","South pole imaging","Saturn South Pole Template","Saturn south pole"]
["2004-230T05:58:00","000T05:00:00","2004-08-17","ISS","SPASS Rider","Saturn","AURORAB","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-230T05:58:00","000T05:00:00","2004-08-17","VIMS","SPASS Rider","Saturn","FARGLO","Saturn far encounter global mosaic","Saturn Far Global Mosaic #17","Saturn Far Encounter Global Mosaic #17"]
["2004-230T11:28:00","000T09:00:00","2004-08-17","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-230T12:58:00","000T06:00:00","2004-08-17","CIRS","SPASS Rider","InstrumentCalibration","DSCALTMP","Deep space calibration","Saturn South Pole Template","Deep Space Cal"]
["2004-230T21:58:00","000T02:25:00","2004-08-17","UVIS","Prime","Saturn","MOS00SWAD","Apoapsis mosaic","MOSAIC_APO_01_07j","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel to the Saturn spin axis. 1) Slew about Z to -MOS Orb from Saturn Center and rotate +64mrad in the YZ plane. 2) Drift at a rate of .0268 mrad/sec about the Z-axis toward +MOS Orb for 6700s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-range): 200.16mrad."]
["2004-231T00:23:00","000T10:30:00","2004-08-18","UVIS","Prime","Saturn","AURORAA","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It uses the GENMOS_P module. It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 10.5 hours.  A similar request (auroralB) is identical except it repeats for 5.0 hours."]
["2004-231T00:23:00","000T10:30:00","2004-08-18","ISS","SPASS Rider","Saturn","AURORAA","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-231T00:23:00","000T10:30:00","2004-08-18","VIMS","SPASS Rider","Saturn","FARGLO","Saturn far encounter global mosaic","Saturn Far Global Mosaic #18","Saturn Far Encounter Global Mosaic #18"]
["2004-231T11:38:00","000T09:00:00","2004-08-18","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-231T22:08:00","000T01:00:00","2004-08-18","ISS","Prime","rings(general)","DIFFUSRNG","Diffuse ring observation","DIFFUSE RINGS, GO WEST TEMPLATE, 003 TH OBSERVATIO","DIFFUSE RINGS IN REV 000, GO WEST TEMPLATE"]
["2004-231T22:08:00","000T01:00:00","2004-08-18","CIRS","SPASS Rider","rings(general)","DIFFUSRNG","Diffuse ring observation","Diffuse Rings, Go West Template Ridealong","Ridealong on ISS diffuse rings, Go West Template"]
["2004-231T23:08:00","000T04:25:00","2004-08-18","UVIS","Prime","Saturn","MOS00SWAE","Apoapsis mosaic","MOSAIC_APO_01","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel to the Saturn spin axis. 1) Slew about Z to +MOS Orb from Saturn Center and rotate +64mrad in the YZ plane. 2) Drift at a rate of .027 mrad/sec about the Z-axis toward -MOS Orb for 13900s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 199.43mrad"]
["2004-231T23:08:00","000T04:25:00","2004-08-18","ISS","SPASS Rider","Saturn","MOS00SWAE","Apoapsis mosaic","UVIS Ride-along for dark images","Ride along during system scans take 5 dark images"]
["2004-232T04:03:00","000T08:50:00","2004-08-19","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-232T14:33:00","000T10:30:00","2004-08-19","UVIS","Prime","Saturn","AURORAA","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It uses the GENMOS_P module. It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 10.5 hours.  A similar request (auroralB) is identical except it repeats for 5.0 hours."]
["2004-232T14:33:00","000T10:30:00","2004-08-19","CIRS","SPASS Rider","Saturn","SPTEMPL10","South pole imaging","Saturn South Pole Template","Saturn south pole"]
["2004-232T14:33:00","000T10:30:00","2004-08-19","ISS","SPASS Rider","Saturn","AURORAA","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-232T14:33:00","000T10:30:00","2004-08-19","VIMS","SPASS Rider","Saturn","FARGLO","Saturn far encounter global mosaic","Saturn Far Global Mosaic #19","Saturn Far Encounter Global Mosaic #19"]
["2004-232T23:00:00","000T00:33:00","2004-08-19","INMS","Non-SPASS","Saturn","MRO","Instrument memory readout","MAPS Survey","MAPS magnetospheric survey."]
["2004-232T23:33:00","003T22:20:00","2004-08-19","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","Ride with prime instrument"]
["2004-233T01:03:00","000T04:55:00","2004-08-20","UVIS","Prime","Saturn","MOS00SWAE","Apoapsis mosaic","MOSAIC_APO_01","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with the Saturn spin axis. 1) Slew about Z to +MOS Orb from Saturn Center. 2) Drift at a rate of .0265 mrad/sec about the Z-axis toward -MOS Orb for 15000s. 3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 198.76mrad."]
["2004-233T01:03:00","000T04:55:00","2004-08-20","ISS","SPASS Rider","Saturn","MOS00SWAE","Apoapsis mosaic","UVIS Ride-along for dark images","Ride along during system scans take 5 dark images"]
["2004-233T05:58:00","000T05:00:00","2004-08-20","UVIS","Prime","Saturn","AURORAB","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 5 hours.  A similar request (auroralA) is identical except it repeats for 10.5 hours."]
["2004-233T05:58:00","000T05:00:00","2004-08-20","CIRS","SPASS Rider","Saturn","SPTEMPL05","South pole imaging","Saturn South Pole Template","Saturn south pole"]
["2004-233T05:58:00","000T05:00:00","2004-08-20","ISS","SPASS Rider","Saturn","AURORAB","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-233T05:58:00","000T05:00:00","2004-08-20","VIMS","SPASS Rider","Saturn","FARGLO","Saturn far encounter global mosaic","Saturn Far Global Mosaic #20","Saturn Far Encounter Global Mosaic #20"]
["2004-233T11:28:00","000T08:55:00","2004-08-20","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-233T12:58:00","000T06:00:00","2004-08-20","CIRS","SPASS Rider","InstrumentCalibration","DSCALTMP","Deep space calibration","Saturn South Pole Template","Deep Space Cal"]
["2004-233T21:58:00","000T02:25:00","2004-08-20","UVIS","Prime","Saturn","MOS00SWAE","Apoapsis mosaic","MOSAIC_APO_01","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with the Saturn spin axis. 1) Slew about Z to +MOS Orb from Saturn Center and rotate -64mrad in the YZ plane.  2) Drift at a rate of .0264 mrad/sec about the Z-axis toward -MOS Orb for 6700s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 198.29mrad."]
["2004-234T00:23:00","000T10:30:00","2004-08-21","UVIS","Prime","Saturn","AURORAA","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It uses the GENMOS_P module. It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 10.5 hours.  A similar request (auroralB) is identical except it repeats for 5.0 hours."]
["2004-234T00:23:00","000T10:30:00","2004-08-21","ISS","SPASS Rider","Saturn","AURORAA","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-234T00:23:00","000T10:30:00","2004-08-21","VIMS","SPASS Rider","Saturn","FARGLO","Saturn far encounter global mosaic","Saturn Far Global Mosaic #21","Saturn Far Encounter Global Mosaic #21"]
["2004-234T11:23:00","000T09:00:00","2004-08-21","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-234T20:23:00","000T16:30:00","2004-08-21","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2004-234T20:23:00","000T16:30:00","2004-08-21","RPWS","Non-SPASS","Saturn","SWAURORA","Solar wind campaign","MAPS SW1 Campaign","Part of SW1 MAPS Campaign.  Observe solar wind plasma waves and Saturn radio emissions while ORS instruments simultaneously observe Saturn's aurora and other MAPS observe solar wind conditions."]
["2004-234T21:53:00","000T01:00:00","2004-08-21","ISS","Prime","rings(general)","DIFFUSRNG","Diffuse ring observation","DIFFUSE RINGS, GO WEST TEMPLATE, 004 TH OBSERVATIO","DIFFUSE RINGS IN REV 000, GO WEST TEMPLATE"]
["2004-234T21:53:00","000T01:00:00","2004-08-21","CIRS","SPASS Rider","rings(general)","DIFFUSRNG","Diffuse ring observation","Diffuse Rings, Go West Template Ridealong","Ridealong on ISS diffuse rings, Go West Template"]
["2004-234T22:30:00","000T04:33:04","2004-08-21","CAPS","Non-SPASS","Saturn","BURST16K","16 kbps burst","Burst of 16kbps data","Burst of 16 kbps data (which gives uncollapsed ELS data). 64 B cycles duration. Data is in addition to 1000 bps from SWSKR."]
["2004-234T22:53:00","000T04:25:00","2004-08-21","UVIS","Prime","Saturn","MOS00SWA","Apoapsis mosaic","MOSAIC_APO_01_07k","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with the Saturn spin axis. 1) Slew about Z to -MOS Orb from Saturn Center and rotate 64mrad in the YZ plane.  2) Drift at a rate of .0264 mrad/sec about the Z-axis toward +MOS Orb for 13900s. 3) Slew back to Saturn center and reset pointing. Stare for remaining observation time. MOS Orb (+/-Range): 197.80mrad."]
["2004-234T22:53:00","000T04:25:00","2004-08-21","ISS","SPASS Rider","Saturn","MOS00SWA","Apoapsis mosaic","UVIS Ride-along for dark images","Ride along during system scans take 5 dark images"]
["2004-235T03:53:00","000T09:00:00","2004-08-22","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-235T05:23:00","000T06:00:00","2004-08-22","CIRS","SPASS Rider","InstrumentCalibration","DSCALTMP","Deep space calibration","Deep Space Calibration","Deep Space Cal"]
["2004-235T12:53:00","008T07:01:00","2004-08-22","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2004-235T12:53:00","005T03:23:00","2004-08-22","RPWS","Non-SPASS","Saturn","SWAURORA","Solar wind campaign","MAPS SW1 Campaign","Part of SW1 MAPS Campaign.  Observe solar wind plasma waves and Saturn radio emissions while ORS instruments simultaneously observe Saturn's aurora and other MAPS observe solar wind conditions."]
["2004-235T14:18:00","000T10:30:00","2004-08-22","UVIS","Prime","Saturn","AURORAA","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It uses the GENMOS_P module. It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 10.5 hours.  A similar request (auroralB) is identical except it repeats for 5.0 hours."]
["2004-235T14:18:00","000T10:30:00","2004-08-22","CIRS","SPASS Rider","Saturn","SPTEMPL10","South pole imaging","Saturn South Pole Template","Saturn south pole"]
["2004-235T14:18:00","000T10:30:00","2004-08-22","ISS","SPASS Rider","Saturn","AURORAA","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-235T14:18:00","000T10:30:00","2004-08-22","VIMS","SPASS Rider","Saturn","FARGLO","Saturn far encounter global mosaic","Saturn Far Global Mosaic #1","Saturn Far Encounter Global Mosaic #1"]
["2004-236T00:48:00","000T04:55:00","2004-08-23","UVIS","Prime","Saturn","MOS00SWA","Apoapsis mosaic","MOSAIC_APO_01_07l","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with the Saturn spin axis.  1) Slew about Z to -MOS Orb from Saturn Center.  2) Drift at a rate of .0263 mrad/sec about the Z-axis toward +MOS Orb for 15000s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 197.38mrad"]
["2004-236T00:48:00","000T04:55:00","2004-08-23","ISS","SPASS Rider","Saturn","MOS00SWA","Apoapsis mosaic","UVIS Ride-along for dark images","Ride along during system scans take 5 dark images"]
["2004-236T05:43:00","000T03:30:00","2004-08-23","UVIS","Prime","Saturn","AURORAB","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 5 hours.  A similar request (auroralA) is identical except it repeats for 10.5 hours."]
["2004-236T05:43:00","000T03:30:00","2004-08-23","CIRS","SPASS Rider","Saturn","SPTEMPL05","South pole imaging","Saturn South Pole Template","Saturn south pole"]
["2004-236T05:43:00","000T03:30:00","2004-08-23","ISS","SPASS Rider","Saturn","AURORAB","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-236T05:43:00","000T03:30:00","2004-08-23","VIMS","SPASS Rider","Saturn","FARGLO","Saturn far encounter global mosaic","Saturn Far Global Mosaic #1","Saturn Far Encounter Global Mosaic #2"]
["2004-236T09:53:00","000T12:00:00","2004-08-23","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-236T21:53:00","000T23:45:00","2004-08-23","INMS","Non-SPASS","Saturn","PTOTM","MAPS survey","MAPS Survey","Ride with prime instrument"]
["2004-236T23:23:00","000T09:45:00","2004-08-23","UVIS","Prime","Saturn","AURORAA","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It uses the GENMOS_P module. It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 10.5 hours.  A similar request (auroralB) is identical except it repeats for 5.0 hours."]
["2004-236T23:23:00","000T09:45:00","2004-08-23","ISS","SPASS Rider","Saturn","AURORAA","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-236T23:26:00","000T09:45:00","2004-08-23","VIMS","SPASS Rider","Saturn","FARGLO","Saturn far encounter global mosaic","Saturn Far Global Mosaic #1","Saturn Far Encounter Global Mosaic #3"]
["2004-237T09:38:00","000T12:00:00","2004-08-24","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-237T21:38:00","000T00:33:00","2004-08-24","INMS","Non-SPASS","Saturn","MRO","Instrument memory readout","MAPS Survey","MAPS magnetospheric survey."]
["2004-237T22:11:00","002T14:27:00","2004-08-24","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","Ride with prime instrument"]
["2004-237T22:38:00","000T01:00:00","2004-08-24","ISS","Prime","rings(general)","DIFFUSRNG","Diffuse ring observation","DIFFUSE RINGS, GO WEST TEMPLATE, 005 TH OBSERVATIO","DIFFUSE RINGS IN REV 000, GO WEST TEMPLATE"]
["2004-237T22:38:00","000T01:00:00","2004-08-24","CIRS","SPASS Rider","rings(general)","DIFFUSRNG","Diffuse ring observation","Diffuse Rings, Go West Template Ridealong","Ridealong on ISS diffuse rings, Go West Template"]
["2004-237T23:38:00","000T03:25:00","2004-08-24","UVIS","Prime","Saturn","MOS00SWB","Apoapsis mosaic","MOSAIC_APO_01_07n","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with the Saturn spin axis. 1) Slew about Z to +MOS Orb from Saturn Center. 2) Drift at a rate of .0263 mrad/sec about the Z-axis toward -MOS Orb for 13900s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 196.89mrad."]
["2004-237T23:38:00","000T03:25:00","2004-08-24","ISS","SPASS Rider","Saturn","MOS00SWB","Apoapsis mosaic","UVIS Ride-along for dark images","Ride along during system scans take 5 dark images"]
["2004-238T03:38:00","000T09:00:00","2004-08-25","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-238T14:03:00","000T10:30:00","2004-08-25","UVIS","Prime","Saturn","AURORAA","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It uses the GENMOS_P module. It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 10.5 hours.  A similar request (auroralB) is identical except it repeats for 5.0 hours."]
["2004-238T14:03:00","000T10:30:00","2004-08-25","CIRS","SPASS Rider","Saturn","SPTEMPL10","South pole imaging","Saturn South Pole Template","Saturn south pole"]
["2004-238T14:03:00","000T10:30:00","2004-08-25","ISS","SPASS Rider","Saturn","AURORAA","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-238T14:03:00","000T10:30:00","2004-08-25","VIMS","SPASS Rider","Saturn","FARGLO","Saturn far encounter global mosaic","Saturn Far Global Mosaic #1","Saturn Far Encounter Global Mosaic #4"]
["2004-239T00:33:00","000T04:55:00","2004-08-26","UVIS","Prime","Saturn","MOS00SWB","Apoapsis mosaic","MOSAIC_APO_01_07o","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with the Saturn spin axis. 1) Slew about Z to +MOS Orb from Saturn Center and rotate -64mrad in the YZ plane. 2) Drift at a rate of .0262 mrad/sec about the Z-axis toward -MOS Orb for 15000s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 196.74mrad."]
["2004-239T00:33:00","000T04:55:00","2004-08-26","ISS","SPASS Rider","Saturn","MOS00SWB","Apoapsis mosaic","UVIS Ride-along for dark images","Ride along during system scans take 5 dark images"]
["2004-239T05:28:00","000T05:00:00","2004-08-26","UVIS","Prime","Saturn","AURORAB","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 5 hours.  A similar request (auroralA) is identical except it repeats for 10.5 hours."]
["2004-239T05:28:00","000T05:00:00","2004-08-26","CIRS","SPASS Rider","Saturn","SPTEMPL05","South pole imaging","Saturn South Pole Template","Saturn south pole"]
["2004-239T05:28:00","000T05:00:00","2004-08-26","ISS","SPASS Rider","Saturn","AURORAB","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-239T05:28:00","000T05:00:00","2004-08-26","VIMS","SPASS Rider","Saturn","FARGLO","Saturn far encounter global mosaic","Saturn Far Global Mosaic #5","Saturn Far Encounter Global Mosaic #5"]
["2004-239T10:58:00","000T09:00:00","2004-08-26","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-239T12:28:00","000T06:00:00","2004-08-26","CIRS","SPASS Rider","InstrumentCalibration","DSCALTMP","Deep space calibration","Deep space cal","Deep Space Calibration"]
["2004-239T21:28:00","000T02:25:00","2004-08-26","UVIS","Prime","Saturn","MOS00SWB","Apoapsis mosaic","MOSAIC_APO_01_07p","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel to the Saturn spin axis. 1) Slew about Z to +MOS Orb from Saturn Center and rotate +64mrad in the YZ plane. 2) Drift at a rate of .0262 mrad/sec about the Z-axis toward -MOS Orb 6700s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 196.74mrad"]
["2004-239T23:53:00","000T10:30:00","2004-08-26","UVIS","Prime","Saturn","AURORAA","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It uses the GENMOS_P module. It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 10.5 hours.  A similar request (auroralB) is identical except it repeats for 5.0 hours."]
["2004-239T23:53:00","000T10:30:00","2004-08-26","ISS","SPASS Rider","Saturn","AURORAA","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-239T23:53:00","000T10:30:00","2004-08-26","VIMS","SPASS Rider","Saturn","FARGLO","Saturn far encounter global mosaic","Saturn Far Global Mosaic #6","Saturn Far Encounter Global Mosaic #6"]
["2004-240T11:09:00","000T09:00:00","2004-08-27","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-240T12:38:00","002T09:22:00","2004-08-27","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey."]
["2004-240T16:15:00","007T07:45:00","2004-08-27","MIMI","SPASS Rider","Saturn","SWAURORA","Solar wind campaign","MAPS SW1 Campaign","Part of SW1 MAPS Campaign.   Image the magnetosphere and observe solar wind and pickup ions while ORS instruments make simultaneous observations of Saturns aurora, CAPS observes the solar wind, and RPWS observes SKR. -Y to Saturn (auroral region) and -X ~ to sun."]
["2004-240T16:16:00","007T07:44:00","2004-08-27","CAPS","Non-SPASS","Saturn","SWAURORA","Solar wind campaign","MAPS solar wind/aurora campaign","MAPS magnetospheric survey"]
["2004-240T16:16:00","003T03:38:00","2004-08-27","RPWS","Non-SPASS","Saturn","SWAURORA","Solar wind campaign","MAPS SW1 Campaign","Part of SW1 MAPS Campaign.  Observe solar wind plasma waves and Saturn radio emissions while ORS instruments simultaneously observe Saturn's aurora and other MAPS observe solar wind conditions."]
["2004-240T16:20:00","015T19:15:00","2004-08-27","CDA","Non-SPASS","DustRAM direction","SURVEY","Magnetospheric survey","dust survey","Survey measurements of dust"]
["2004-240T21:39:00","000T01:00:00","2004-08-27","ISS","Prime","rings(general)","DIFFUSRNG","Diffuse ring observation","DIFFUSE RINGS, GO WEST TEMPLATE, 001 TH OBSERVATIO","DIFFUSE RINGS IN REV 00A, GO WEST TEMPLATE"]
["2004-240T22:39:00","000T04:25:00","2004-08-27","UVIS","Prime","Saturn","MOS0ASWC","Apoapsis mosaic","MOSAIC_APO_01_08","Mosaic of Saturn inner magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with the Saturn spin axis. 1) Slew about Z to -MOS Orb from Saturn Center.  2) Drift at a rate of .0262 mrad/sec about the Z-axis toward +MOS Orb for 13900s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 196.67mrad."]
["2004-240T22:39:00","000T04:25:00","2004-08-27","ISS","SPASS Rider","Saturn","MOS0ASWC","Apoapsis mosaic","UVIS Ride-along for dark images","Ride along during system scans take 5 dark images"]
["2004-241T03:34:00","000T09:00:00","2004-08-28","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-241T14:04:00","000T10:30:00","2004-08-28","UVIS","Prime","Saturn","AURORAA","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It uses the GENMOS_P module. It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 10.5 hours.  A similar request (auroralB) is identical except it repeats for 5.0 hours."]
["2004-241T14:04:00","000T10:30:00","2004-08-28","CIRS","SPASS Rider","Saturn","SPTEMPL10","South pole imaging","Saturn South Pole Template","Saturn south pole"]
["2004-241T14:04:00","000T10:30:00","2004-08-28","ISS","SPASS Rider","Saturn","AURORAA","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-241T14:04:00","000T10:30:00","2004-08-28","VIMS","SPASS Rider","Saturn","FARGLO","Saturn far encounter global mosaic","Saturn Far Global Mosaic #7","Saturn Far Encounter Global Mosaic #7"]
["2004-242T00:34:00","000T04:55:00","2004-08-29","UVIS","Prime","Saturn","MOS0ASWC","Apoapsis mosaic","MOSAIC_APO_01_08a","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with the Saturn spin axis. 1) Slew about Z to -MOS Orb from Saturn Center and rotate -64mrad in the YZ plane.  2) Drift at a rate of .0262 mrad/sec about the Z-axis toward +MOS Orb for 15000s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 196.67mrad."]
["2004-242T00:34:00","000T04:55:00","2004-08-29","ISS","SPASS Rider","Saturn","MOS0ASWC","Apoapsis mosaic","UVIS Ride-along for dark images","Ride along during system scans take 5 dark images"]
["2004-242T05:29:00","000T05:00:00","2004-08-29","UVIS","Prime","Saturn","AURORAB","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 5 hours.  A similar request (auroralA) is identical except it repeats for 10.5 hours."]
["2004-242T05:29:00","000T05:00:00","2004-08-29","CIRS","SPASS Rider","Saturn","SPTEMPL05","South pole imaging","Saturn South Pole Template","Saturn south pole"]
["2004-242T05:29:00","000T05:00:00","2004-08-29","ISS","SPASS Rider","Saturn","AURORAB","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-242T05:29:00","000T05:00:00","2004-08-29","VIMS","SPASS Rider","Saturn","FARGLO","Saturn far encounter global mosaic","Saturn Far Global Mosaic #8","Saturn Far Encounter Global Mosaic #8"]
["2004-242T10:59:00","000T09:00:00","2004-08-29","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-242T21:29:00","000T02:25:00","2004-08-29","UVIS","Prime","Saturn","MOS0ASWC","Apoapsis mosaic","MOSAIC_APO_01_08b","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with the Saturn spin axis. 1) Slew about Z to -MOS Orb from Saturn Center and rotate +64mrad in the YZ plane. 2) Drift at a rate of .0262 mrad/sec about the Z-axis toward +MOS Orb for 6700s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 196.87mrad"]
["2004-242T22:00:00","000T00:33:00","2004-08-29","INMS","Non-SPASS","Saturn","MRO","Instrument memory readout","MAPS Survey","MAPS magnetospheric survey."]
["2004-242T22:33:00","004T23:27:00","2004-08-29","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey."]
["2004-242T23:54:00","000T10:30:00","2004-08-29","UVIS","Prime","Saturn","AURORAA","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It uses the GENMOS_P module. It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 10.5 hours.  A similar request (auroralB) is identical except it repeats for 5.0 hours."]
["2004-242T23:54:00","000T10:30:00","2004-08-29","ISS","SPASS Rider","Saturn","AURORAA","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-242T23:54:00","000T10:30:00","2004-08-29","VIMS","SPASS Rider","Saturn","FARGLO","Saturn far encounter global mosaic","Saturn Far Global Mosaic #9","Saturn Far Encounter Global Mosaic #9"]
["2004-243T10:54:00","000T09:00:00","2004-08-30","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-243T12:29:00","000T06:00:00","2004-08-30","CIRS","SPASS Rider","InstrumentCalibration","DSCALTMP","Deep space calibration","Deep space cal","Deep Space Calibration"]
["2004-243T19:54:00","000T16:25:00","2004-08-30","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2004-243T19:54:00","000T16:25:00","2004-08-30","RPWS","Non-SPASS","Saturn","SWAURORA","Solar wind campaign","MAPS SW1 Campaign","Part of SW1 MAPS Campaign.  Observe solar wind plasma waves and Saturn radio emissions while ORS instruments simultaneously observe Saturn's aurora and other MAPS observe solar wind conditions."]
["2004-243T22:54:00","000T01:00:00","2004-08-30","ISS","Prime","rings(general)","DIFFUSRNG","Diffuse ring observation","DIFFUSE RINGS, GO WEST TEMPLATE, 002 TH OBSERVATIO","DIFFUSE RINGS IN REV 00A, GO WEST TEMPLATE"]
["2004-243T23:30:00","000T02:16:32","2004-08-30","CAPS","Non-SPASS","Saturn","BURST16K","16 kbps burst","Burst of 16kbps data","Burst of 16 kbps data (which gives uncollapsed ELS data). 32 B cycles duration. Data is in addition to 1000 bps from SWSKR."]
["2004-243T23:54:00","000T02:55:00","2004-08-30","UVIS","Prime","Saturn","MOS0ASWD","Apoapsis mosaic","MOSAIC_APO_01_08c","Mosaic of Saturn inner magnetosphere.  EUV and FUV low resolution slits on, aligned parallel to the Saturn spin axis. 1) Slew about Z to +MOS Orb from Saturn Center and rotate -64mrad in the YZ plane.  2) Drift at a rate of .0263 mrad/sec about the Z-axis toward -MOS Orb for 8500s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 197.00mrad"]
["2004-243T23:54:00","000T02:55:00","2004-08-30","ISS","SPASS Rider","Saturn","MOS0ASWD","Apoapsis mosaic","UVIS Ride-along for dark images","Ride along during system scans take 5 dark images"]
["2004-244T03:19:00","000T09:00:00","2004-08-31","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-244T12:19:00","003T11:41:00","2004-08-31","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2004-244T12:19:00","003T11:41:00","2004-08-31","RPWS","Non-SPASS","Saturn","SWAURORA","Solar wind campaign","MAPS SW1 Campaign","Part of SW1 MAPS Campaign.  Observe solar wind plasma waves and Saturn radio emissions while ORS instruments simultaneously observe Saturn's aurora and other MAPS observe solar wind conditions."]
["2004-244T13:49:00","000T10:30:00","2004-08-31","UVIS","Prime","Saturn","AURORAA","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It uses the GENMOS_P module. It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 10.5 hours.  A similar request (auroralB) is identical except it repeats for 5.0 hours."]
["2004-244T13:49:00","000T10:30:00","2004-08-31","CIRS","SPASS Rider","Saturn","SPTEMPL10","South pole imaging","Saturn South Pole Template","Saturn south pole"]
["2004-244T13:49:00","000T10:30:00","2004-08-31","ISS","SPASS Rider","Saturn","AURORAA","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-244T13:49:00","000T10:30:00","2004-08-31","VIMS","SPASS Rider","Saturn","FARGLO","Saturn far encounter global mosaic","Saturn Far Global Mosaic #1","Saturn Far Encounter Global Mosaic #10"]
["2004-245T00:19:00","000T04:55:00","2004-09-01","UVIS","Prime","Saturn","MOS0ASWD","Apoapsis mosaic","MOSAIC_APO_01_08d","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with the Saturn spin axis.  1) Slew about Z to +MOS Orb from Saturn Center and rotate +64mrad in the YZ plane.  2) Drift at a rate of .0263 mrad/sec about the Z-axis toward -MOS Orb for 15000s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 197.26mrad"]
["2004-245T00:19:00","000T04:55:00","2004-09-01","ISS","SPASS Rider","Saturn","MOS0ASWD","Apoapsis mosaic","UVIS Ride-along for dark images","Ride along during system scans take 5 dark images"]
["2004-245T05:14:00","000T05:00:00","2004-09-01","UVIS","Prime","Saturn","AURORAB","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 5 hours.  A similar request (auroralA) is identical except it repeats for 10.5 hours."]
["2004-245T05:14:00","000T05:00:00","2004-09-01","CIRS","SPASS Rider","Saturn","SPTEMPL05","South pole imaging","Saturn South Pole Template","Saturn south pole"]
["2004-245T05:14:00","000T05:00:00","2004-09-01","ISS","SPASS Rider","Saturn","AURORAB","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-245T05:14:00","000T05:00:00","2004-09-01","VIMS","SPASS Rider","Saturn","FARGLO","Saturn far encounter global mosaic","Saturn Far Global Mosaic #11","Saturn Far Encounter Global Mosaic #11"]
["2004-245T10:44:00","000T09:00:00","2004-09-01","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-245T12:14:00","000T06:00:00","2004-09-01","CIRS","SPASS Rider","InstrumentCalibration","DSCALTMP","Deep space calibration","Deep space cal","Deep Space Calibration"]
["2004-245T21:14:00","000T02:25:00","2004-09-01","UVIS","Prime","Saturn","MOS0ASWD","Apoapsis mosaic","MOSAIC_APO_01_08e","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel to the Saturn spin axis. 1) Slew about Z to +MOS Orb from Saturn Center.  2) Drift at a rate of .0263 mrad/sec about the Z-axis toward -MOS Orb for 6700s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 197.54mrad."]
["2004-245T23:39:00","000T10:30:00","2004-09-01","UVIS","Prime","Saturn","AURORAA","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It uses the GENMOS_P module. It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 10.5 hours.  A similar request (auroralB) is identical except it repeats for 5.0 hours."]
["2004-245T23:39:00","000T10:30:00","2004-09-01","ISS","SPASS Rider","Saturn","AURORAA","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-245T23:39:00","000T10:30:00","2004-09-01","VIMS","SPASS Rider","Saturn","FARGLO","Saturn far encounter global mosaic","Saturn Far Global Mosaic #12","Saturn Far Encounter Global Mosaic #12"]
["2004-246T10:39:00","000T09:00:00","2004-09-02","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-246T21:09:00","000T01:00:00","2004-09-02","ISS","Prime","rings(general)","DIFFUSRNG","Diffuse ring observation","DIFFUSE RINGS, GO WEST TEMPLATE, 003 TH OBSERVATIO","DIFFUSE RINGS IN REV 00A, GO WEST TEMPLATE"]
["2004-246T22:09:00","000T04:25:00","2004-09-02","UVIS","Prime","Saturn","MOS0ASWE","Apoapsis mosaic","MOSAIC_APO_01_08f","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with the Saturn spin axis. 1) Slew about Z to -MOS Orb from Saturn Center and rotate -64mrad in the YZ plane. 2) Drift at a rate of .0264 mrad/sec about the Z-axis toward +MOS Orb for 13900s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 197.93mrad."]
["2004-246T22:09:00","000T04:25:00","2004-09-02","ISS","SPASS Rider","Saturn","MOS0ASWE","Apoapsis mosaic","UVIS Ride-along for dark images","Ride along during system scans take 5 dark images"]
["2004-247T03:04:00","000T09:00:00","2004-09-03","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-247T13:34:00","000T10:30:00","2004-09-03","UVIS","Prime","Saturn","AURORAA","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It uses the GENMOS_P module. It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 10.5 hours.  A similar request (auroralB) is identical except it repeats for 5.0 hours."]
["2004-247T13:34:00","000T10:30:00","2004-09-03","CIRS","SPASS Rider","Saturn","SPTEMPL10","South pole imaging","Saturn South Pole Template","Saturn south pole"]
["2004-247T13:34:00","000T10:30:00","2004-09-03","ISS","SPASS Rider","Saturn","AURORAA","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-247T13:34:00","000T10:30:00","2004-09-03","VIMS","SPASS Rider","Saturn","FARGLO","Saturn far encounter global mosaic","Saturn Far Global Mosaic #13","Saturn Far Encounter Global Mosaic #13"]
["2004-247T22:00:00","000T00:33:00","2004-09-03","INMS","Non-SPASS","Saturn","MRO","Instrument memory readout","MAPS Survey","MAPS magnetospheric survey."]
["2004-247T22:33:00","002T04:32:00","2004-09-03","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey."]
["2004-248T00:00:00","008T11:35:00","2004-09-04","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey"]
["2004-248T00:00:00","001T19:40:00","2004-09-04","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey."]
["2004-248T00:00:00","008T11:35:00","2004-09-04","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SUR Campaign","Part of SUR MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2004-248T00:00:00","001T19:40:00","2004-09-04","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-248T00:04:00","000T04:55:00","2004-09-04","UVIS","Prime","Saturn","MOS0ASWE","Apoapsis mosaic","MOSAIC_APO_01_08g","Mosaic of Saturn inner magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with the Saturn spin axis. 1) Slew about Z to -MOS Orb from Saturn Center and rotate +64mrad in the YZ plane.  2) Drift at a rate of .0265 mrad/sec about the Z-axis toward +MOS Orb for 15000s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 198.41mrad"]
["2004-248T00:04:00","000T04:55:00","2004-09-04","ISS","SPASS Rider","Saturn","MOS0ASWE","Apoapsis mosaic","UVIS Ride-along for dark images","Ride along during system scans take 5 dark images"]
["2004-248T04:59:00","000T05:00:00","2004-09-04","UVIS","Prime","Saturn","AURORAB","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 5 hours.  A similar request (auroralA) is identical except it repeats for 10.5 hours."]
["2004-248T04:59:00","000T05:00:00","2004-09-04","CIRS","SPASS Rider","Saturn","SPTEMPL05","South pole imaging","Saturn South Pole Template","Saturn south pole"]
["2004-248T04:59:00","000T05:00:00","2004-09-04","VIMS","SPASS Rider","Saturn","FARGLO","Saturn far encounter global mosaic","Saturn Far Global Mosaic #14","Saturn Far Encounter Global Mosaic #14"]
["2004-248T10:29:00","000T09:00:00","2004-09-04","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-248T11:59:00","000T06:00:00","2004-09-04","CIRS","SPASS Rider","InstrumentCalibration","DSCALTMP","Deep space calibration","Saturn South Pole Template","Deep Space Calibration"]
["2004-248T20:59:00","000T02:25:00","2004-09-04","UVIS","Prime","Saturn","MOS0ASWE","Apoapsis mosaic","MOSAIC_APO_01_08h","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel to the Saturn spin axis. 1) Slew about Z to -MOS Orb from Saturn Center.  2) Drift at a rate of .0265 mrad/sec about the Z-axis toward +MOS Orb for 6700s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 198.87mrad."]
["2004-248T23:24:00","000T03:30:00","2004-09-04","UVIS","Prime","Saturn","AURORAA","Saturn aurora movie","Saturn south pole auroral scan","This observation is a repetative half-hour unit for imaging Saturn's south pole during the go-west template in apoapse 0/A.  It uses the GENMOS_P module. It starts with a scan from left limb to central meridian, stop at central meridion for 7 minutes, continue scan to right limb and a fast slew back to left limb.  The full duration is 30 minutes.  This repeats 21 times for 10.5 hours.  A similar request (auroralB) is identical except it repeats for 5.0 hours."]
["2004-248T23:24:00","000T03:30:00","2004-09-04","ISS","SPASS Rider","Saturn","AURORAA","Saturn aurora movie","go west saturn pole movie","Saturn south pole movie"]
["2004-248T23:24:00","000T03:30:00","2004-09-04","VIMS","SPASS Rider","Saturn","FARGLO","Saturn far encounter global mosaic","Saturn Far Global Mosaic #15","Saturn Far Encounter Global Mosaic #15"]
["2004-249T02:54:00","000T07:00:00","2004-09-05","CAPS","Prime","InstrumentCalibration","SWCAL","CAPS solar wind beam calibration","CAPS  Solar Wind Beam Calibration","CAPS solar wind beam calibration.  Need pointing -x to sun, roll +/- 85 degrees about Y.  Need 16kbps.  Need to be placed late in this subphase since we need to have the solar wind beam as narrow as possible (and on average the beam is narrower the farther we are from the sun)."]
["2004-249T10:40:00","000T09:00:00","2004-09-05","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-249T19:40:00","000T16:25:00","2004-09-05","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2004-249T19:40:00","000T16:25:00","2004-09-05","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-249T21:10:00","000T01:00:00","2004-09-05","ISS","Prime","rings(general)","DIFFUSRNG","Diffuse ring observation","DIFFUSE RINGS, GO EAST TEMPLATE, 004 TH OBSERVATIO","DIFFUSE RINGS IN REV 00A, GO EAST TEMPLATE"]
["2004-249T21:30:00","000T04:33:04","2004-09-05","CAPS","Non-SPASS","Saturn","BURST16K","16 kbps burst","Burst of 16kbps data","Burst of 16 kbps data (which gives uncollapsed ELS data). 64 B cycles duration. Data is in addition to 700 bps survey."]
["2004-249T22:10:00","000T04:25:00","2004-09-05","UVIS","Prime","Saturn","MOS0AGEA","Apoapsis mosaic","MOSAIC_APO_01_08i","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with the Saturn spin axis. 1) Slew about Z to +MOS Orb from Saturn Center and rotate +64mrad in the YZ plane.  2) Drift at a rate of .0266 mrad/sec about the z-axis toward -MOS Orb for 13900s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 199.49mrad."]
["2004-249T22:10:00","000T04:25:00","2004-09-05","ISS","SPASS Rider","Saturn","MOS0AGEA","Apoapsis mosaic","UVIS Ride-along for dark images","Ride along during system scans take 5 dark images"]
["2004-250T03:05:00","000T09:00:00","2004-09-06","INMS","Non-SPASS","Saturn","SURVEYA","MAPS survey","Survey 18 a","06/14/2004 - Erin changed time of request. Received additional sponge bits and thus must make adjustments to CIMS request  FSW Testing"]
["2004-250T03:05:00","000T09:00:00","2004-09-06","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-250T12:05:00","001T07:25:00","2004-09-06","INMS","Non-SPASS","Saturn","SURVEYB","MAPS survey","Suvery 19 b","06/14/2004 - Erin changed time of request. Received additional sponge bits and thus must make adjustments to CIMS request  FSW testing"]
["2004-250T12:05:00","005T07:05:00","2004-09-06","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey."]
["2004-250T12:05:00","005T07:05:00","2004-09-06","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-250T13:35:00","000T20:25:00","2004-09-06","ISS","Prime","Saturn","2X2MOVIEA","Saturn movie","Go east global Saturn movie","2X2 Saturn mosaic + spoke movie, repeat every 1:45."]
["2004-250T13:35:00","000T20:25:00","2004-09-06","CIRS","SPASS Rider","Saturn","ISSPCKT20","Saturn movie","Saturn Movie pickets","Saturn Movie pickets"]
["2004-250T13:35:00","000T20:25:00","2004-09-06","UVIS","SPASS Rider","Saturn","2X2MOVIEA","Saturn movie","ISS 2X2MOVIEA Rider","UVIS EUV and FUV riding along with ISS 2X2MOVIEA observation"]
["2004-250T13:35:00","000T20:25:00","2004-09-06","VIMS","SPASS Rider","Saturn","FRGLOB","Saturn far encounter global mosaic","Saturn Far Global Mosaic, Go-East Template  #1","Saturn Far Encounter Global Mosaic under Go-East Template #1. 20-hour duration. 12 pickets acquired over these 20 hours. ISS movie  pickets each last 1:00. Then CD CIRS observations for 45 minutes. Total cycle time is 1:45.  Data volume: 12 observations * 2 exposures * 64*64*352*12 = 420 mbits"]
["2004-251T10:30:00","000T09:00:00","2004-09-07","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-251T12:00:00","000T06:00:00","2004-09-07","CIRS","SPASS Rider","InstrumentCalibration","DSCALTMP","Deep space calibration","Deep Space Calibration","Deep space cal."]
["2004-251T19:30:00","000T23:55:00","2004-09-07","INMS","Non-SPASS","Saturn","PTOTM003","MAPS survey","MAPS Survey","MAPS magnetospheric survey."]
["2004-251T21:00:00","000T05:15:00","2004-09-07","ISS","Prime","Saturn","2X2MOVIEB","Saturn movie","Go east global Saturn movie","2X2 Saturn mosaic + spoke movie, repeat every 1:45."]
["2004-251T21:00:00","000T05:15:00","2004-09-07","CIRS","SPASS Rider","Saturn","ISSPCKT03","Saturn movie","Saturn Movie Pickets","Movie picket rider"]
["2004-251T21:00:00","000T05:15:00","2004-09-07","UVIS","SPASS Rider","Saturn","2X2MOVIEB","Saturn movie","ISS 2X2MOVIEB Rider","UVIS EUV and FUV riding along with ISS 2X2MOVIEB observation"]
["2004-251T21:00:00","000T05:15:00","2004-09-07","VIMS","SPASS Rider","Saturn","FRGLOB","Saturn far encounter global mosaic","Saturn Far Global Mosaic, Go-East Template  #2","Saturn Far Encounter Global Mosaic under Go-East Template #2. 5.25-hour duration. 3 pickets acquired over these 5.25 hours. ISS movie  pickets each last 1:00. Then CD CIRS observations for 45 minutes. Total cycle time is 1:45.  Data volume: 3 observations * 2 exposures * 64*64*352*12 = 105 mbits"]
["2004-252T02:15:00","000T07:30:00","2004-09-08","UVIS","Prime","Saturn","MOS0AGEA","Apoapsis mosaic","MOSAIC_APO_01_08j","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with the Saturn spin axis.  1) Slew about Z to +MOS Orb from Saturn Center.  2) Drift at a rate of .0268 mrad/sec about the Z-axis toward -MOS Orb for 15000s.  3) Rotate -64mrad in the YZ Plane.  Drift at indicated rate about Z for 9500s toward +MOS orb.  4) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 201.02mrad."]
["2004-252T02:15:00","000T04:55:00","2004-09-08","ISS","SPASS Rider","Saturn","MOS0AGEA","Apoapsis mosaic","UVIS Ride-along for dark images","Ride along during system scans take 5 dark images"]
["2004-252T10:25:00","000T09:00:00","2004-09-08","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-252T19:25:00","000T00:33:00","2004-09-08","INMS","Non-SPASS","Saturn","MRO","Instrument memory readout","MAPS Survey","MAPS magnetospheric survey."]
["2004-252T19:58:00","002T23:12:00","2004-09-08","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey."]
["2004-252T20:55:00","000T01:00:00","2004-09-08","ISS","Prime","rings(general)","DIFFUSRNG","Diffuse ring observation","DIFFUSE RINGS, GO EAST TEMPLATE, 005 TH OBSERVATIO","DIFFUSE RINGS IN REV 00A, GO EAST TEMPLATE"]
["2004-252T21:55:00","000T04:25:00","2004-09-08","UVIS","Prime","Saturn","MOS0AGEB","Apoapsis mosaic","MOSAIC_APO_01_08k","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with the Saturn spin axis. 1) Slew about the Z-axis from Saturn Center to -MOS Orb. Rotate +64mrad in the YZ plane. 2) Drift at a rate of .0270 mrad/sec about the Z-axis toward +MOS Orb for 13900s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 201.70mrad."]
["2004-252T21:55:00","000T04:25:00","2004-09-08","ISS","SPASS Rider","Saturn","MOS0AGEB","Apoapsis mosaic","UVIS Ride-along for dark images","Ride along during system scans take 5 dark images"]
["2004-253T02:50:00","000T09:00:00","2004-09-09","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-253T13:20:00","000T20:25:00","2004-09-09","ISS","Prime","Saturn","2X2MOVIEA","Saturn movie","Go east global Saturn movie","2X2 Saturn mosaic + spoke movie, repeat every 1:45."]
["2004-253T13:20:00","000T20:25:00","2004-09-09","CIRS","SPASS Rider","Saturn","ISSPCKT20","Saturn movie","Saturn Movie pickets","Saturn Movie pickets"]
["2004-253T13:20:00","000T20:25:00","2004-09-09","UVIS","SPASS Rider","Saturn","2X2MOVIEA","Saturn movie","ISS 2X2MOVIEA Rider","UVIS EUV and FUV riding along with ISS 2X2MOVIEA observation"]
["2004-253T13:20:00","000T20:25:00","2004-09-09","VIMS","SPASS Rider","Saturn","FRGLOB","Saturn far encounter global mosaic","Saturn Far Global Mosaic, Go-East Template  #3","Saturn Far Encounter Global Mosaic under Go-East Template #3. 20-hour duration. 12 pickets acquired over these 20 hours. ISS movie  pickets each last 1:00. Then CD CIRS observations for 45 minutes. Total cycle time is 1:45.  Data volume: 12 observations * 2 exposures * 64*64*352*12 = 420 mbits"]
["2004-254T10:15:00","000T09:00:00","2004-09-10","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-254T11:00:00","000T06:00:00","2004-09-10","CIRS","SPASS Rider","InstrumentCalibration","DSCALTMP","Deep space calibration","Deep Space Calibration","Deep space cal."]
["2004-254T20:45:00","000T05:15:00","2004-09-10","ISS","Prime","Saturn","2X2MOVIEB","Saturn movie","Go east global Saturn movie","2X2 Saturn mosaic + spoke movie, repeat every 1:45."]
["2004-254T20:45:00","000T05:15:00","2004-09-10","CIRS","SPASS Rider","Saturn","ISSPCKT03","Saturn movie","Saturn Movie Pickets","Movie picket rider"]
["2004-254T20:45:00","000T05:15:00","2004-09-10","UVIS","SPASS Rider","Saturn","2X2MOVIEB","Saturn movie","ISS 2X2MOVIEB Rider","UVIS EUV and FUV riding along with ISS 2X2MOVIEB observation"]
["2004-254T20:45:00","000T05:15:00","2004-09-10","VIMS","SPASS Rider","Saturn","FRGLOB","Saturn far encounter global mosaic","Saturn Far Global Mosaic, Go-East Template  #4","Saturn Far Encounter Global Mosaic under Go-East Template #4. 5.25-hour duration. 3 pickets acquired over these 5.25 hours. ISS movie  pickets each last 1:00. Then CD CIRS observations for 45 minutes. Total cycle time is 1:45.  Data volume: 3 observations * 2 exposures * 64*64*352*12 = 105 mbits"]
["2004-255T02:00:00","000T07:30:00","2004-09-11","UVIS","Prime","Saturn","MOS0AGEB","Apoapsis mosaic","MOSAIC_APO_01_08l","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel to the Saturn spin axis. 1) Slew about the Z-axis from Saturn Center to -MOS Orb. 2) Drift at a rate of .0272 mrad/sec about the Z-axis toward +MOS Orb for 15000s.  3) Rotate -64mrad in the YZ plane. Drift at indicated rate toward -MOS Orb for 9500s.  4) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 203.74mrad."]
["2004-255T02:00:00","000T04:55:00","2004-09-11","ISS","SPASS Rider","Saturn","MOS0AGEB","Apoapsis mosaic","UVIS Ride-along for dark images","Ride along during system scans take 5 dark images"]
["2004-255T10:10:00","000T09:00:00","2004-09-11","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-255T19:10:00","000T16:25:00","2004-09-11","INMS","Non-SPASS","Saturn","SURVEYA","MAPS survey","SURVEY 019A","06/14/2004 - Erin created request. Received additional sponge bits and thus must make adjustments to CIMS request  Will be performing FSW testing"]
["2004-255T19:10:00","000T16:25:00","2004-09-11","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2004-255T19:10:00","000T16:25:00","2004-09-11","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-255T20:40:00","000T01:00:00","2004-09-11","ISS","Prime","rings(general)","DIFFUSRNG","Diffuse ring observation","DIFFUSE RINGS, GO EAST TEMPLATE, 006 TH OBSERVATIO","DIFFUSE RINGS IN REV 00A, GO EAST TEMPLATE"]
["2004-255T21:30:00","000T04:33:04","2004-09-11","CAPS","Non-SPASS","Saturn","BURST16K","16 kbps burst","Burst of 16kbps data","Burst of 16 kbps data (which gives uncollapsed ELS data). 32 B cycles duration. Data is in addition to 700 bps survey rate."]
["2004-255T21:40:00","000T04:25:00","2004-09-11","UVIS","Prime","Saturn","MOS0AGEC","Apoapsis mosaic","MOSAIC_APO_01_09","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with the Saturn spin axis.  1) Slew about the Z-axis from Saturn Center to +MOS Orb.  2) Drift at a rate of .0273 mrad/sec about the Z-axis toward -MOS Orb for 13900s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 204.61mrad"]
["2004-255T21:40:00","000T04:25:00","2004-09-11","ISS","SPASS Rider","Saturn","MOS0AGEC","Apoapsis mosaic","UVIS Ride-along for dark images","Ride along during system scans take 5 dark images"]
["2004-256T02:35:00","000T09:00:00","2004-09-12","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-256T11:35:00","001T22:10:00","2004-09-12","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey"]
["2004-256T11:35:00","001T21:58:00","2004-09-12","CDA","Non-SPASS","DustRAM direction","SURVEY","Magnetospheric survey","dust survey","Survey measurements of dust"]
["2004-256T11:35:00","000T01:22:00","2004-09-12","INMS","Non-SPASS","Saturn","STARTUP","Sequence startup activity","STARTUP","Startup sequence.  Load FSW, MRO, Load IEB from SSR's, MRO"]
["2004-256T11:35:00","001T22:10:00","2004-09-12","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey."]
["2004-256T11:35:00","001T22:03:00","2004-09-12","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SUR Campaign","Part of SUR MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2004-256T11:35:00","000T12:25:00","2004-09-12","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-256T12:57:00","001T20:38:00","2004-09-12","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey."]
["2004-256T13:05:00","000T20:25:00","2004-09-12","ISS","Prime","Saturn","2X2MOVIEA","Saturn movie","Go east global Saturn movie","2X2 Saturn mosaic + spoke movie, repeat every 1:45."]
["2004-256T13:05:00","000T20:25:00","2004-09-12","CIRS","SPASS Rider","Saturn","ISSPCKT20","Saturn movie","Saturn Movie pickets","Saturn Movie pickets"]
["2004-256T13:05:00","000T20:25:00","2004-09-12","UVIS","SPASS Rider","Saturn","2X2MOVIEA","Saturn movie","ISS 2X2MOVIEA Rider","UVIS EUV and FUV riding along with ISS 2X2MOVIEA observation"]
["2004-256T13:05:00","000T20:25:00","2004-09-12","VIMS","SPASS Rider","Saturn","FRGLOB","Saturn far encounter global mosaic","Saturn Far Global Mosaic, Go-East Template  #5","Saturn Far Encounter Global Mosaic under Go-East Template #5. 20-hour duration. 12 pickets acquired over these 20 hours. ISS movie  pickets each last 1:00. Then CD CIRS observations for 45 minutes. Total cycle time is 1:45.  Data volume: 12 observations * 2 exposures * 64*64*352*12 = 420 mbits"]
["2004-257T00:00:00","001T00:00:00","2004-09-13","RPWS","Non-SPASS","InstrumentCalibration","PIM","Periodic Instrument maintenance","RPWS PIM","Perform RPWS PIM, Bias the Langmuir Probe to remove any contamination"]
["2004-257T10:00:00","000T09:00:00","2004-09-13","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-257T10:10:00","000T06:00:00","2004-09-13","CIRS","SPASS Rider","InstrumentCalibration","DSCALTMP","Deep space calibration","Deep Space Calibration","Deep space cal."]
["2004-257T20:30:00","000T04:37:00","2004-09-13","ISS","Prime","Saturn","2X2MOVIEB","Saturn movie","Go east global Saturn movie","2X2 Saturn mosaic + spoke movie, repeat every 1:45."]
["2004-257T20:30:00","000T04:37:00","2004-09-13","CIRS","SPASS Rider","Saturn","ISSPCKT03","Saturn movie","Saturn Movie Pickets","Movie picket rider"]
["2004-257T20:30:00","000T04:37:00","2004-09-13","UVIS","SPASS Rider","Saturn","2X2MOVIEB","Saturn movie","ISS 2X2MOVIEB Rider","UVIS EUV and FUV riding along with ISS 2X2MOVIEB observation"]
["2004-257T20:30:00","000T04:37:00","2004-09-13","VIMS","SPASS Rider","Saturn","FRGLOB","Saturn far encounter global mosaic","Saturn Far Global Mosaic, Go-East Template  #6","Saturn Far Encounter Global Mosaic under Go-East Template #6. 5.25-hour duration. 3 pickets acquired over these 5.25 hours. ISS movie  pickets each last 1:00. Then CD CIRS observations for 45 minutes. Total cycle time is 1:45.  Data volume: 3 observations * 2 exposures * 64*64*352*12 = 105 mbits"]
["2004-258T00:00:00","000T09:40:00","2004-09-14","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-258T01:07:00","000T05:30:00","2004-09-14","UVIS","Prime","Saturn","MOS0AGEC","Apoapsis mosaic","MOSAIC_APO_01_09a","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with the Saturn spin axis.  1) Slew about the Z-axis from Saturn Center to +MOS Orb. Rotate -64mrad in the YZ plane. 2) Drift at a rate of .0276 mrad/sec about the Z-axis toward -MOS Orb for 15000s.  3) Rotate +128mrad in the YZ plane.  Drift at the indicated rate toward +MOS Orb for 9500s.  4) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 207.23mrad."]
["2004-258T01:07:00","000T04:55:00","2004-09-14","ISS","SPASS Rider","Saturn","MOS0AGEC","Apoapsis mosaic","UVIS Ride-along for dark images","Ride along during system scans take 5 dark images"]
["2004-258T09:32:00","000T00:06:00","2004-09-14","CAPS","SPASS Rider","SpacecraftActivity","SLEEP","Instrument to sleep mode","Sleep for Probe activity","sleep instrument"]
["2004-258T09:33:00","000T09:31:00","2004-09-14","CDA","Non-SPASS","Saturn","PCO","Probe Checkout","ProbeCheckOut","CDA Sleep/Mute Unmute/Active pointing: NA; datavolume=0 MB"]
["2004-258T09:34:00","000T00:17:00","2004-09-14","CIRS","Non-SPASS","Other","PROBEMUTE","Huygens Probe support","Sleep/mute placeholder","Put CIRS to sleep/mute for PCO#15, sleep and mute (at epoch-00:06?)"]
["2004-258T09:35:00","000T00:10:00","2004-09-14","INMS","Non-SPASS","SpacecraftActivity","SLEEP","Instrument to sleep mode","INMS Sleep and Mute for Probe C/O","null"]
["2004-258T09:38:00","000T09:24:00","2004-09-14","MIMI","SPASS Rider","co-rotation","PCOMUTE","Mute instrument for Probe Checkout","Probe Checkout Mute","SLEEP/MUTE for PSA; SLEEP 13 minutes before PSA_ON (at REQUEST START), MUTE 7 minutes later.  Duration lasts until UNMUTE, at 6 minutes after PSA_OFF, ACTIVE 7 minutes later."]
["2004-258T09:40:00","000T09:31:00","2004-09-14","RPWS","Non-SPASS","SpacecraftActivity","SLEEPMUTE","Huygens probe support","RPWS Sleep and Mute for Probe activity","RPWS sleep/mute for Probe activity, followed by unmute/sleep."]
["2004-258T09:42:00","000T00:03:00","2004-09-14","UVIS","Non-SPASS","Saturn","SLEEPMUTE","Huygens probe support","UVIS TO SLEEP/MUTE (PCO 15)","UVIS to go to sleep/mute for PCO 15 (MGTWT request)"]
["2004-258T09:43:00","000T00:05:00","2004-09-14","VIMS","Non-SPASS","SpacecraftActivity","SLEEPMUTE","Huygens probe support","VIMS to SLEEP / MUTE","VIMS to SLEEP/ MUTE"]
["2004-258T09:45:00","000T00:01:00","2004-09-14","CAPS","SPASS Rider","SpacecraftActivity","MUTE","Instrument to sleep mode","Mute for Probe activity","mute instrument"]
["2004-258T09:45:00","000T09:17:00","2004-09-14","INMS","Non-SPASS","SpacecraftActivity","MUTE","Instrument to sleep mode","INMS Mute for Probe C/O","null"]
["2004-258T09:45:00","000T09:17:00","2004-09-14","MAG","Non-SPASS","SpacecraftActivity","PROBEMUTE","Huygens Probe support","Mute/Unmute for Probe Checkout 15","Mute instrument for probe checkout, unmute at end. NOTE: MAG does not go to sleep for PCO, other instruments do"]
["2004-258T09:51:00","000T09:05:00","2004-09-14","PROBE","Non-SPASS","Earth","PCO15","Probe Checkout","Probe Checkout #15","Preheating Probe Checkout; MTU Test. This activity, if moved, should remain five days away from Battery Depassivation 1, for thermal reasons. X-band downlink required. The following Orbiter instruments will be ON, in sleep mode, and muted prior to PSA ON: CDA, CAPS, ISS, MIMI, RPWS, MAG, UVIS, and VIMS; other orbiter instruments OFF. The checkout data recorded on the SSR should be played back on a different pass."]
["2004-258T10:06:00","000T00:09:50","2004-09-14","ISS","Non-SPASS","Earth","SLEEPMUTE","Huygens probe support","put ISS to sleep for probe activity","placeholder activity put into CIMS to remenind ISS to go into sleep for probe activity at request of MAG TWT"]
["2004-258T19:02:00","000T00:01:00","2004-09-14","CAPS","SPASS Rider","SpacecraftActivity","UNMUTE","Huygens probe support","Unmute after Probe activity","wake up & unmute biu"]
["2004-258T19:02:00","000T00:07:00","2004-09-14","MIMI","SPASS Rider","co-rotation","PCOUNMUTE","Huygens probe support","Probe Checkout Un-Mute, Active","UNMUTE/ACTIVE post- PSA; UMNUTE 6 minutes after PSA_OFF (at REQUEST START), ACTIVE 7 minutes later."]
["2004-258T19:02:00","004T17:52:00","2004-09-14","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey"]
["2004-258T19:02:00","000T00:04:00","2004-09-14","CIRS","Non-SPASS","Other","PROUNMUTE","Huygens Probe support","wake/unmute placeholder","UNMUTE.  Note power transients! unmute at 00:06, wake at epoch+00:09"]
["2004-258T19:02:00","000T00:04:00","2004-09-14","INMS","Non-SPASS","SpacecraftActivity","UNMUTE","Huygens probe support","INMS UnMute after Probe C/O","null"]
["2004-258T19:02:00","000T00:07:00","2004-09-14","ISS","Non-SPASS","Earth","WAKESLEEP","Wakeup instrument from sleep mode","wake up  ISS after probe activity","placeholder activity put into CIMS to remind ISS to wake up after probe activity at request of MAG TWT"]
["2004-258T19:02:00","002T23:54:00","2004-09-14","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey."]
["2004-258T19:02:00","000T00:11:00","2004-09-14","UVIS","Non-SPASS","Saturn","UNMUTEWAK","Huygens probe support","UVIS to unmute and wake up after PCO 15","Unmute/go to active after PCO 15 (MAGTWT request)"]
["2004-258T19:02:00","000T00:18:00","2004-09-14","VIMS","Non-SPASS","SpacecraftActivity","WAKEUP","Wakeup instrument from sleep mode","VIMS to Active Mode","VIMS to ACTIVE"]
["2004-258T19:03:00","000T02:16:00","2004-09-14","CAPS","SPASS Rider","SpacecraftActivity","WAKEUP","Wakeup instrument from sleep mode","WakeUp after Probe activity","wake up & unmute biu"]
["2004-258T19:04:00","002T23:51:59","2004-09-14","CDA","Non-SPASS","DustRAM direction","SURPCOPPL","Dust survey","dust survey","Survey measurements of dust"]
["2004-258T19:06:00","002T17:51:00","2004-09-14","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey."]
["2004-258T19:09:00","004T17:38:00","2004-09-14","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SUR Campaign","Part of SUR MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2004-258T19:11:00","002T23:45:00","2004-09-14","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-258T20:56:00","000T01:00:00","2004-09-14","ISS","Prime","rings(general)","DIFFUSRNG","Diffuse ring observation","DIFFUSE RINGS, GO EAST TEMPLATE, 007 TH OBSERVATIO","DIFFUSE RINGS IN REV 00A, GO EAST TEMPLATE"]
["2004-258T21:56:00","000T03:55:00","2004-09-14","UVIS","Prime","Saturn","MOS0AGED","Apoapsis mosaic","MOSAIC_APO_01_09b","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with the Saturn spin axis.  1) Slew about the Z-axis from Saturn Center to -MOS Orb.  2) Drift at a rate of .0279 mrad/sec about the Z-axis toward +MOS Orb for 13900s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 208.33mrad."]
["2004-258T21:56:00","000T03:55:00","2004-09-14","ISS","SPASS Rider","Saturn","MOS0AGED","Apoapsis mosaic","UVIS Ride-along for dark images","Ride along during system scans take 5 dark images"]
["2004-259T02:21:00","000T09:00:00","2004-09-15","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-259T12:51:00","000T20:25:00","2004-09-15","ISS","Prime","Saturn","2X2MOVIEA","Saturn movie","Go east global Saturn movie","2X2 Saturn mosaic + spoke movie, repeat every 1:45."]
["2004-259T12:51:00","000T20:25:00","2004-09-15","CIRS","SPASS Rider","Saturn","ISSPCKT20","Saturn movie","Saturn Movie pickets","Saturn Movie pickets"]
["2004-259T12:51:00","000T20:25:00","2004-09-15","UVIS","SPASS Rider","Saturn","2X2MOVIEA","Saturn movie","ISS 2X2MOVIEA Rider","UVIS EUV and FUV riding along with ISS 2X2MOVIEA observation"]
["2004-259T12:51:00","000T20:25:00","2004-09-15","VIMS","SPASS Rider","Saturn","FRGLOB","Saturn far encounter global mosaic","Saturn Far Global Mosaic, Go-East Template  #7","Saturn Far Encounter Global Mosaic under Go-East Template #7. 20-hour duration. 12 pickets acquired over these 20 hours. ISS movie  pickets each last 1:00. Then CD CIRS observations for 45 minutes. Total cycle time is 1:45.  Data volume: 12 observations * 2 exposures * 64*64*352*12 = 420 mbits"]
["2004-260T09:46:00","000T09:00:00","2004-09-16","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-260T11:26:00","000T06:00:00","2004-09-16","CIRS","SPASS Rider","InstrumentCalibration","DSCALTMP","Deep space calibration","Deep Space Calibration","Deep space cal."]
["2004-260T20:16:00","000T05:15:00","2004-09-16","ISS","Prime","Saturn","2X2MOVIEB","Saturn movie","Go east global Saturn movie","2X2 Saturn mosaic + spoke movie, repeat every 1:45."]
["2004-260T20:16:00","000T05:15:00","2004-09-16","CIRS","SPASS Rider","Saturn","ISSPCKT03","Saturn movie","Saturn Movie Pickets","Movie picket rider"]
["2004-260T20:16:00","000T05:15:00","2004-09-16","UVIS","SPASS Rider","Saturn","2X2MOVIEB","Saturn movie","ISS 2X2MOVIEB Rider","UVIS EUV and FUV riding along with ISS 2X2MOVIEB observation"]
["2004-260T20:16:00","000T05:15:00","2004-09-16","VIMS","SPASS Rider","Saturn","FRGLOB","Saturn far encounter global mosaic","Saturn Far Global Mosaic, Go-East Template  #8","Saturn Far Encounter Global Mosaic under Go-East Template #8. 5.25-hour duration. 3 pickets acquired over these 5.25 hours. ISS movie  pickets each last 1:00. Then CD CIRS observations for 45 minutes. Total cycle time is 1:45.  Data volume: 3 observations * 2 exposures * 64*64*352*12 = 105 mbits"]
["2004-261T01:31:00","000T07:30:00","2004-09-17","UVIS","Prime","Saturn","MOS0AGED","Apoapsis mosaic","MOSAIC_APO_01_09c","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel to the Saturn spin axis.  1) Slew about the Z-axis from Saturn Center to -MOS Orb. Rotate -64mrad in the YZ plane.  2) Drift at a rate of .0284 mrad/sec about the Z-axis toward +MOS Orb for 15000s.  3) Rotate +128mrad in the YZ plane.  Drift at the indicated rate toward -MOS Orb for 9500s.  4) Slew back to Saturn center and reset pointing.  Stare for the remaining observation time. MOS Orb (+/-Range): 212.94mrad."]
["2004-261T01:31:00","000T04:55:00","2004-09-17","ISS","SPASS Rider","Saturn","MOS0AGED","Apoapsis mosaic","UVIS Ride-along for dark images","Ride along during system scans take 5 dark images"]
["2004-261T09:56:00","000T09:00:00","2004-09-17","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-261T12:57:00","000T00:33:00","2004-09-17","INMS","Non-SPASS","Saturn","MRO","Instrument memory readout","MAPS Survey","MAPS magnetospheric survey."]
["2004-261T13:30:00","001T23:14:00","2004-09-17","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey."]
["2004-261T18:56:00","000T16:25:00","2004-09-17","CAPS","Non-SPASS","Saturn","SURVEY2","MAPS survey","MAPS Survey","MAPS magnetospheric survey"]
["2004-261T18:56:00","000T16:25:00","2004-09-17","CDA","Non-SPASS","DustRAM direction","SURPCOPPL","Dust survey","dust survey","Survey measurements of dust"]
["2004-261T18:56:00","000T16:25:00","2004-09-17","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey."]
["2004-261T18:56:00","000T16:25:00","2004-09-17","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-261T20:26:00","000T01:00:00","2004-09-17","ISS","Prime","rings(general)","DIFFUSRNG","Diffuse ring observation","DIFFUSE RINGS, GO EAST TEMPLATE, 008 TH OBSERVATIO","DIFFUSE RINGS IN REV 00A, GO EAST TEMPLATE"]
["2004-261T20:26:00","000T01:00:00","2004-09-17","UVIS","SPASS Rider","rings(general)","DIFFUSRNG","Diffuse ring observation","UV Ring Spectroscopy"]
["2004-261T21:26:00","000T04:25:00","2004-09-17","UVIS","Prime","Saturn","MOS0AGEE","Apoapsis mosaic","MOSAIC_APO_01_09e","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with the Saturn spin axis.  1) Slew about the Z-axis from Saturn Center to +MOS Orb. Rotate -64mrad in the YZ plane.  2) Drift at a rate of .0284 mrad/sec about the Z-axis toward -MOS Orb for 13900s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 212.94mrad."]
["2004-261T21:26:00","000T04:25:00","2004-09-17","ISS","SPASS Rider","Saturn","MOS0AGEE","Apoapsis mosaic","UVIS Ride-along for dark images","Ride along during system scans take 5 dark images"]
["2004-261T22:21:00","000T08:00:00","2004-09-17","RSS","SPASS Rider","Earth","USOBSC","RSS HGA boresight calibration","RSS USO Characterization plus Boresight Calibratio","RSS USO characterization plus Boresight Cal. Pointing=XBAND to Earth + two crosshair maneuvers. Last 4 hours required to be tracked at DSS-55 in 1-way mode. Last 4 hours are also desired to be tracked at DSS-63 in 1-way mode."]
["2004-261T23:00:00","000T02:16:32","2004-09-17","CAPS","Non-SPASS","Saturn","BURST16K","16 kbps burst","Burst of 16kbps data","Burst of 16 kbps data (which gives uncollapsed ELS data). 32 B cycles duration. Data is in addition to 1000 bps survey rate."]
["2004-262T02:21:00","000T09:00:00","2004-09-18","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-262T05:21:00","000T01:00:00","2004-09-18","RSS","Prime","Earth","BORESIGHT","HGA boresight calibration","RSS Boresight Calibration","RSS HGA Boresight Calibration.  Pointing:  XBAND to Earth + two crosshair maneuvers"]
["2004-262T06:21:00","000T05:00:00","2004-09-18","CIRS","SPASS Rider","InstrumentCalibration","DSCAL","Deep space calibration","Deep Space Calibration","Deep space cal."]
["2004-262T11:21:00","001T01:33:00","2004-09-18","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey."]
["2004-262T11:21:00","001T01:28:00","2004-09-18","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-262T11:21:01","001T01:20:59","2004-09-18","CDA","Non-SPASS","DustRAM direction","SURPCOPPL","Dust survey","dust survey","Survey measurements of dust"]
["2004-262T12:51:00","000T20:25:00","2004-09-18","ISS","Prime","Saturn","2X2MOVIEA","Saturn movie","Go east global Saturn movie","2X2 Saturn mosaic + spoke movie, repeat every 1:45."]
["2004-262T12:51:00","000T20:25:00","2004-09-18","CIRS","SPASS Rider","Saturn","ISSPCKT20","Saturn movie","Saturn Movie pickets","Saturn Movie pickets"]
["2004-262T12:51:00","000T20:25:00","2004-09-18","UVIS","SPASS Rider","Saturn","2X2MOVIEA","Saturn movie","ISS 2X2MOVIEA Rider","UVIS EUV and FUV riding along with ISS 2X2MOVIEA observation"]
["2004-262T12:51:00","000T20:25:00","2004-09-18","VIMS","SPASS Rider","Saturn","FRGLOB","Saturn far encounter global mosaic","Saturn Far Global Mosaic, Go-East Template  #9","Saturn Far Encounter Global Mosaic under Go-East Template #9. 20-hour duration. 12 pickets acquired over these 20 hours. ISS movie  pickets each last 1:00. Then CD CIRS observations for 45 minutes. Total cycle time is 1:45.  Data volume: 12 observations * 2 exposures * 64*64*352*12 = 420 mbits"]
["2004-263T12:41:00","000T00:06:00","2004-09-19","CAPS","SPASS Rider","SpacecraftActivity","SLEEP","Instrument to sleep mode","Sleep for Probe activity","sleep instrument"]
["2004-263T12:42:00","000T02:26:00","2004-09-19","CDA","Non-SPASS","Saturn","PCO","Probe Checkout","ProbeCheckOut","Mute for PCO. Sleep/Mute Unmute/Active Commands for CDA pointing: NA; datavolume=0 MB"]
["2004-263T12:43:00","000T00:17:00","2004-09-19","CIRS","Non-SPASS","Other","PROBEMUTE","Huygens Probe support","Sleep/mute placeholder","Put CIRS to sleep/mute for DEPASS"]
["2004-263T12:44:00","000T00:10:00","2004-09-19","INMS","Non-SPASS","SpacecraftActivity","SLEEP","Instrument to sleep mode","INMS Sleep and Mute for Probe C/O","null"]
["2004-263T12:45:00","000T00:09:50","2004-09-19","ISS","Non-SPASS","Earth","SLEEPMUTE","Huygens probe support","put ISS to sleep for probe activity","placeholder activity put into CIMS to remenind ISS to go into sleep for probe activity at request of MAG TWT"]
["2004-263T12:47:00","000T02:19:00","2004-09-19","MIMI","SPASS Rider","co-rotation","PCOMUTE","Mute instrument for Probe Checkout","Probe SLEEP","SLEEP/MUTE for Probe depassivation of batteries. SLEEP 13 minutes before PSA_ON (at request start), MUTE 7 minutes later.  Duration lasts until UNMUTE, at 6 minutes after PSA_OFF, ACTIVE 7 minutes later.  Both epoch relative."]
["2004-263T12:49:00","000T02:26:00","2004-09-19","RPWS","Non-SPASS","SpacecraftActivity","SLEEPMUTE","Huygens probe support","RPWS Sleep and Mute for Probe activity","RPWS sleep/mute for Probe activity, followed by unmute/sleep."]
["2004-263T12:51:00","000T00:03:00","2004-09-19","UVIS","Non-SPASS","Saturn","SLEEPMUTE","Huygens probe support","UVIS TO SLEEP/MUTE (Probe depassivation)","UVIS to go to sleep/mute for probe depassivation"]
["2004-263T12:52:00","000T00:05:00","2004-09-19","VIMS","Non-SPASS","SpacecraftActivity","SLEEPMUTE","Huygens probe support","VIMS to SLEEP / MUTE","VIMS to SLEEP/ MUTE"]
["2004-263T12:54:00","000T00:01:00","2004-09-19","CAPS","SPASS Rider","SpacecraftActivity","MUTE","Instrument to sleep mode","Mute for Probe activity","mute instrument"]
["2004-263T12:54:00","000T02:12:00","2004-09-19","INMS","Non-SPASS","SpacecraftActivity","MUTE","Instrument to sleep mode","INMS Mute for Probe Depassivation","null"]
["2004-263T12:54:00","000T02:12:00","2004-09-19","MAG","Non-SPASS","SpacecraftActivity","PROBEMUTE","Huygens Probe support","Mute/Unmute for Probe Depassivation","Mute instrument for probe checkout, unmute at end. NOTE: MAG does not go to sleep for PCO, other instruments do"]
["2004-263T13:30:00","000T01:30:00","2004-09-19","PROBE","Non-SPASS","Earth","DEPASSIV1","Huygens probe support","Probe Battery Depassivation - 1","Prepare Probe batteries for primary mission.  X-band downlink required. Orbiter instruments off/sleep/mute as for probe checkouts. This activity must remain at least five days from probe checkout F15 for thermal reasons."]
["2004-263T15:06:00","000T00:01:00","2004-09-19","CAPS","SPASS Rider","SpacecraftActivity","UNMUTE","Huygens probe support","Unmute after Probe activity","wake up & unmute biu"]
["2004-263T15:06:00","000T00:07:00","2004-09-19","MIMI","SPASS Rider","co-rotation","PCOUNMUTE","Huygens probe support","Probe Checkout Un-Mute, Active","UNMUTE/ACTIVE post- PSA; UMNUTE 6 minutes after PSA_OFF (at REQUEST START), ACTIVE 7 minutes later."]
["2004-263T15:06:00","028T18:24:00","2004-09-19","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey"]
["2004-263T15:06:00","000T00:04:00","2004-09-19","CIRS","Non-SPASS","Other","PROUNMUTE","Huygens Probe support","wake/unmute placeholder","UNMUTE.  Note power transients! unmute at 00:06, wake at epoch+00:09"]
["2004-263T15:06:00","000T00:04:00","2004-09-19","INMS","Non-SPASS","SpacecraftActivity","UNMUTE","Huygens probe support","INMS UnMute after Probe Depassivation","null"]
["2004-263T15:06:00","000T00:07:00","2004-09-19","ISS","Non-SPASS","Earth","WAKESLEEP","Wakeup instrument from sleep mode","wake up  ISS after probe activity","placeholder activity put into CIMS to remind ISS to wake up after probe activity at request of MAG TWT"]
["2004-263T15:06:00","001T03:35:00","2004-09-19","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey."]
["2004-263T15:06:00","000T00:11:00","2004-09-19","UVIS","Non-SPASS","Saturn","UNMUTEWAK","Huygens probe support","UVIS to unmute and wake up after probe dep.","Unmute/go to active after probe depassivation"]
["2004-263T15:06:00","000T00:05:00","2004-09-19","VIMS","Non-SPASS","SpacecraftActivity","WAKEUP","Wakeup instrument from sleep mode","VIMS to Active Mode","VIMS to ACTIVE"]
["2004-263T15:07:00","000T02:16:00","2004-09-19","CAPS","SPASS Rider","SpacecraftActivity","WAKEUP","Wakeup instrument from sleep mode","WakeUp after Probe activity","wake up & unmute biu"]
["2004-263T15:08:00","001T03:32:59","2004-09-19","CDA","Non-SPASS","DustRAM direction","SURPCOPPL","Dust survey","dust survey","Survey measurements of dust"]
["2004-263T15:10:00","001T03:31:00","2004-09-19","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey."]
["2004-263T15:13:00","015T08:47:00","2004-09-19","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SUR Campaign","Part of SUR MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2004-263T15:15:00","001T03:26:00","2004-09-19","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-263T20:16:00","000T05:15:00","2004-09-19","ISS","Prime","Saturn","2X2MOVIEB","Saturn movie","Go east global Saturn movie","2X2 Saturn mosaic + spoke movie, repeat every 1:45."]
["2004-263T20:16:00","000T05:15:00","2004-09-19","CIRS","SPASS Rider","Saturn","ISSPCKT03","Saturn movie","Saturn Movie Pickets","Movie picket rider"]
["2004-263T20:16:00","000T05:15:00","2004-09-19","UVIS","SPASS Rider","Saturn","2X2MOVIEB","Saturn movie","ISS 2X2MOVIEB Rider","UVIS EUV and FUV riding along with ISS 2X2MOVIEB observation"]
["2004-263T20:16:00","000T05:15:00","2004-09-19","VIMS","SPASS Rider","Saturn","FRGLOB","Saturn far encounter global mosaic","Saturn Far Global Mosaic, Go-East Template  #10","Saturn Far Encounter Global Mosaic under Go-East Template #10. 5.25-hour duration. 3 pickets acquired over these 5.25 hours. ISS movie  pickets each last 1:00. Then CD CIRS observations for 45 minutes. Total cycle time is 1:45.  Data volume: 3 observations * 2 exposures * 64*64*352*12 = 105 mbits"]
["2004-264T01:31:00","000T07:30:00","2004-09-20","UVIS","Prime","Saturn","MOS0AGEE","Apoapsis mosaic","MOSAIC_APO_01_09f","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with the Saturn spin axis. 1) Slew about the Z-axis from Saturn Center to +MOS Orb. Rotate +64mrad in the YZ plane. 2) Drift at a rate of .0289 mrad/sec about the Z-axis toward -MOS Orb 15000s.  3) Rotate -64mrad in the YZ plane.  Drift at the indicated rate about the Z-axis toward +MOS Orb for 9500s.  4) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 216.92mrad."]
["2004-264T01:31:00","000T04:55:00","2004-09-20","ISS","SPASS Rider","Saturn","MOS0AGEE","Apoapsis mosaic","UVIS Ride-along for dark images","Ride along during system scans take 5 dark images"]
["2004-264T09:41:00","000T09:00:00","2004-09-20","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-264T18:41:00","000T16:25:00","2004-09-20","CDA","Non-SPASS","DustRAM direction","SURPCOPPL","Dust survey","dust survey","Survey measurements of dust"]
["2004-264T18:41:00","000T16:25:00","2004-09-20","INMS","Non-SPASS","Saturn","SURVEYA","MAPS survey","MAPS Survey","Mag Survey"]
["2004-264T18:41:00","000T16:25:00","2004-09-20","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey."]
["2004-264T18:41:00","000T16:25:00","2004-09-20","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-264T20:11:00","000T01:00:00","2004-09-20","ISS","Prime","rings(general)","DIFFUSRNG","Diffuse ring observation","DIFFUSE RINGS, GO EAST TEMPLATE, 009 TH OBSERVATIO","DIFFUSE RINGS IN REV 00A, GO EAST TEMPLATE"]
["2004-264T20:11:00","000T01:00:00","2004-09-20","UVIS","SPASS Rider","rings(general)","DIFFUSRNG","Diffuse ring observation","UV Ring Spectroscopy"]
["2004-264T20:45:00","000T04:33:04","2004-09-20","CAPS","Non-SPASS","Saturn","BURST16K","16 kbps burst","Burst of 16kbps data","Burst of 16 kbps data (which gives uncollapsed ELS data). 32 B cycles duration. Data is in addition to 1000 bps survey rate."]
["2004-264T21:11:00","000T04:25:00","2004-09-20","UVIS","Prime","Saturn","MOS0AGEF","Apoapsis mosaic","MOSAIC_APO_01_09h","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with the Saturn spin axis.  1) Slew about the Z-axis from Saturn Center to -MOS Orb. Rotate -64mrad in the YZ plane.  2) Drift at a rate of .0291 mrad/sec about the Z-axis toward +MOS Orb for 13900s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 218.57mrad."]
["2004-264T21:11:00","000T04:25:00","2004-09-20","ISS","SPASS Rider","Saturn","MOS0AGEF","Apoapsis mosaic","UVIS Ride-along for dark images","Ride along during system scans take 5 dark images"]
["2004-265T02:06:00","000T09:00:00","2004-09-21","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-265T11:06:00","001T01:51:00","2004-09-21","INMS","Non-SPASS","Saturn","SURVEYB","MAPS survey","MAPS Survey","MAPS magnetospheric survey."]
["2004-265T11:06:00","002T07:21:00","2004-09-21","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey."]
["2004-265T11:06:00","002T07:21:00","2004-09-21","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-265T11:06:01","002T07:20:58","2004-09-21","CDA","Non-SPASS","DustRAM direction","SURPCOPPL","Dust survey","dust survey","Survey measurements of dust"]
["2004-265T12:36:00","000T20:25:00","2004-09-21","ISS","Prime","Saturn","2X2MOVIEA","Saturn movie","Go east global Saturn movie","2X2 Saturn mosaic + spoke movie, repeat every 1:45."]
["2004-265T12:36:00","000T20:25:00","2004-09-21","CIRS","SPASS Rider","Saturn","ISSPCKT20","Saturn movie","Saturn Movie pickets","Saturn Movie pickets"]
["2004-265T12:36:00","000T20:25:00","2004-09-21","UVIS","SPASS Rider","Saturn","2X2MOVIEA","Saturn movie","ISS 2X2MOVIEA Rider","UVIS EUV and FUV riding along with ISS 2X2MOVIEA observation"]
["2004-265T12:36:00","000T20:25:00","2004-09-21","VIMS","SPASS Rider","Saturn","FRGLOB","Saturn far encounter global mosaic","Saturn Far Global Mosaic, Go-East Template  #11","Saturn Far Encounter Global Mosaic under Go-East Template #11. 20-hour duration. 12 pickets acquired over these 20 hours. ISS movie  pickets each last 1:00. Then CD CIRS observations for 45 minutes. Total cycle time is 1:45.  Data volume: 12 observations * 2 exposures * 64*64*352*12 = 420 mbits"]
["2004-266T09:31:00","000T09:00:00","2004-09-22","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-266T11:11:00","000T06:00:00","2004-09-22","CIRS","SPASS Rider","InstrumentCalibration","DSCALTMP","Deep space calibration","Deep Space Calibration","Deep space cal."]
["2004-266T12:57:00","000T00:33:00","2004-09-22","INMS","Non-SPASS","Saturn","MRO","Instrument memory readout","MAPS Survey","MAPS magnetospheric survey."]
["2004-266T13:30:00","001T04:57:00","2004-09-22","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey."]
["2004-266T20:01:00","000T05:15:00","2004-09-22","ISS","Prime","Saturn","2X2MOVIEB","Saturn movie","Go east global Saturn movie","2X2 Saturn mosaic + spoke movie, repeat every 1:45."]
["2004-266T20:01:00","000T05:15:00","2004-09-22","CIRS","SPASS Rider","Saturn","ISSPCKT03","Saturn movie","Saturn Movie Pickets","Movie picket rider"]
["2004-266T20:01:00","000T05:15:00","2004-09-22","UVIS","SPASS Rider","Saturn","2X2MOVIEB","Saturn movie","ISS 2X2MOVIEB Rider","UVIS EUV and FUV riding along with ISS 2X2MOVIEB observation"]
["2004-266T20:01:00","000T05:15:00","2004-09-22","VIMS","SPASS Rider","Saturn","FRGLOB","Saturn far encounter global mosaic","Saturn Far Global Mosaic, Go-East Template  #12","Saturn Far Encounter Global Mosaic under Go-East Template #12. 5.25-hour duration. 3 pickets acquired over these 5.25 hours. ISS movie  pickets each last 1:00. Then CD CIRS observations for 45 minutes. Total cycle time is 1:45.  Data volume: 3 observations * 2 exposures * 64*64*352*12 = 105 mbits"]
["2004-267T01:16:00","000T07:30:00","2004-09-23","UVIS","Prime","Saturn","MOS0AGEF","Apoapsis mosaic","MOSAIC_APO_01_09j","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with the Saturn spin axis. 1) Slew about the Z-axis from Saturn Center to -MOS Orb. Rotate +64mrad in the YZ plane. 2) Drift at a rate of .0298 mrad/sec about the Z-axis toward +MOS Orb for 15000s.  3) Rotate -64mrad in the YZ Plane. Drift at indicated rate about the Z-axis toward -MOS Orb for 9500s.  4) Slew back to Saturn center and reset pointing.  Stare for remaining observation time.  MOS Orb (+/-Range): 223.43mrad."]
["2004-267T01:16:00","000T04:55:00","2004-09-23","ISS","SPASS Rider","Saturn","MOS0AGEF","Apoapsis mosaic","UVIS Ride-along for dark images","Ride along during system scans take 5 dark images"]
["2004-267T09:27:00","000T09:00:00","2004-09-23","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-267T18:27:00","000T16:25:00","2004-09-23","CDA","Non-SPASS","DustRAM direction","SURPCOPPL","Dust survey","dust survey","Survey measurements of dust"]
["2004-267T18:27:00","000T16:25:00","2004-09-23","INMS","Non-SPASS","Saturn","SURVEYA","MAPS survey","MAPS Survey","MAPS magnetospheric survey."]
["2004-267T18:27:00","000T16:25:00","2004-09-23","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey."]
["2004-267T18:27:00","000T16:25:00","2004-09-23","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-267T19:57:00","000T01:00:00","2004-09-23","ISS","Prime","rings(general)","DIFFUSRNG","Diffuse ring observation","DIFFUSE RINGS, GO EAST TEMPLATE, 010 TH OBSERVATIO","DIFFUSE RINGS IN REV 00A, GO EAST TEMPLATE"]
["2004-267T19:57:00","000T01:00:00","2004-09-23","UVIS","SPASS Rider","rings(general)","DIFFUSRNG","Diffuse ring observation","UV Ring Spectroscopy"]
["2004-267T20:30:00","000T04:33:04","2004-09-23","CAPS","Non-SPASS","Saturn","BURST16K","16 kbps burst","Burst of 16kbps data","Burst of 16 kbps data (which gives uncollapsed ELS data). 32 B cycles duration. Data is in addition to 1000 bps survey rate."]
["2004-267T20:57:00","000T04:25:00","2004-09-23","UVIS","Prime","Saturn","MOS0AGEG","Apoapsis mosaic","MOSAIC_APO_01_09k","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel to the Saturn spin axis. 1) Slew about the Z-Axis from Saturn Center to +MOS Orb. Rotate +64mrad in the YZ plane.  2) Drift at a rate of .0301 mrad/sec about the Z-axis toward -MOS Orb for 13900s.  3) Slew to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 225.46mrad."]
["2004-267T20:57:00","000T04:25:00","2004-09-23","ISS","SPASS Rider","Saturn","MOS0AGEG","Apoapsis mosaic","UVIS Ride-along for dark images","Ride along during system scans take 5 dark images"]
["2004-268T01:52:00","000T09:00:00","2004-09-24","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-268T10:52:00","002T07:35:00","2004-09-24","INMS","Non-SPASS","Saturn","SURVEYB","MAPS survey","MAPS Survey","MAPS magnetospheric survey."]
["2004-268T10:52:00","000T23:55:00","2004-09-24","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey."]
["2004-268T10:52:00","002T07:35:00","2004-09-24","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-268T10:52:01","002T07:34:58","2004-09-24","CDA","Non-SPASS","DustRAM direction","SURPCOPPL","Dust survey","dust survey","Survey measurements of dust"]
["2004-268T12:22:00","000T20:25:00","2004-09-24","ISS","Prime","Saturn","2X2MOVIEA","Saturn movie","Go east global Saturn movie","2X2 Saturn mosaic + spoke movie, repeat every 1:45."]
["2004-268T12:22:00","000T20:25:00","2004-09-24","CIRS","SPASS Rider","Saturn","ISSPCKT20","Saturn movie","Saturn Movie pickets","Saturn Movie pickets"]
["2004-268T12:22:00","000T20:25:00","2004-09-24","UVIS","SPASS Rider","Saturn","2X2MOVIEA","Saturn movie","ISS 2X2MOVIEA Rider","UVIS EUV and FUV riding along with ISS 2X2MOVIEA observation"]
["2004-268T12:22:00","000T20:25:00","2004-09-24","VIMS","SPASS Rider","Saturn","FRGLOB","Saturn far encounter global mosaic","Saturn Far Global Mosaic, Go-East Template  #13","Saturn Far Encounter Global Mosaic under Go-East Template #13. 20-hour duration. 12 pickets acquired over these 20 hours. ISS movie  pickets each last 1:00. Then CD CIRS observations for 45 minutes. Total cycle time is 1:45.  Data volume: 12 observations * 2 exposures * 64*64*352*12 = 420 mbits"]
["2004-269T09:17:00","000T09:00:00","2004-09-25","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-269T10:47:00","000T06:05:00","2004-09-25","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey."]
["2004-269T16:52:00","000T18:05:00","2004-09-25","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey."]
["2004-269T19:47:00","000T05:15:00","2004-09-25","ISS","Prime","Saturn","2X2MOVIEB","Saturn movie","Go east global Saturn movie","2X2 Saturn mosaic + spoke movie, repeat every 1:45."]
["2004-269T19:47:00","000T05:15:00","2004-09-25","CIRS","SPASS Rider","Saturn","ISSPCKT03","Saturn movie","Saturn Movie Pickets","Movie picket rider"]
["2004-269T19:47:00","000T05:15:00","2004-09-25","UVIS","SPASS Rider","Saturn","2X2MOVIEB","Saturn movie","ISS 2X2MOVIEB Rider","UVIS EUV and FUV riding along with ISS 2X2MOVIEB observation"]
["2004-269T19:47:00","000T05:15:00","2004-09-25","VIMS","SPASS Rider","Saturn","FRGLOB","Saturn far encounter global mosaic","Saturn Far Global Mosaic, Go-East Template  #14","Saturn Far Encounter Global Mosaic under Go-East Template #14. 5.25-hour duration. 3 pickets acquired over these 5.25 hours. ISS movie  pickets each last 1:00. Then CD CIRS observations for 45 minutes. Total cycle time is 1:45.  Data volume: 3 observations * 2 exposures * 64*64*352*12 = 105 mbits"]
["2004-270T01:02:00","000T07:30:00","2004-09-26","UVIS","Prime","Saturn","MOS0AGEG","Apoapsis mosaic","MOSAIC_APO_01_09l","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel to the Saturn spin axis. 1) Slew about the Z axis from Saturn Center to +MOS Orb. 2) Drift at a rate of .0309 mrad/sec about the Z-axis to -MOS Orb for 15000s.  3) Rotate -64mrad in the YZ plane.  Drift at indicated rate toward +MOS Orb for 9500s.  4) Slew back to Saturn center and resest pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 231.38mrad."]
["2004-270T01:02:00","000T04:55:00","2004-09-26","ISS","SPASS Rider","Saturn","MOS0AGEG","Apoapsis mosaic","UVIS Ride-along for dark images","Ride along during system scans take 5 dark images"]
["2004-270T09:27:00","000T09:00:00","2004-09-26","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-270T10:57:00","000T06:05:00","2004-09-26","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey."]
["2004-270T17:02:00","000T01:25:00","2004-09-26","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey."]
["2004-270T18:27:00","000T16:25:00","2004-09-26","CDA","Non-SPASS","DustRAM direction","SURPCOPPL","Dust survey","dust survey","Survey measurements of dust"]
["2004-270T18:27:00","000T16:25:00","2004-09-26","INMS","Non-SPASS","Saturn","SURVEYC","MAPS survey","MAPS Survey","MAPS magnetospheric survey."]
["2004-270T18:27:00","000T16:25:00","2004-09-26","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey."]
["2004-270T18:27:00","000T16:25:00","2004-09-26","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-270T19:57:00","000T01:00:00","2004-09-26","ISS","Prime","rings(general)","DIFFUSRNG","Diffuse ring observation","DIFFUSE RINGS, GO EAST TEMPLATE, 011 TH OBSERVATIO","DIFFUSE RINGS IN REV 00A, GO EAST TEMPLATE"]
["2004-270T19:57:00","000T01:00:00","2004-09-26","UVIS","SPASS Rider","rings(general)","DIFFUSRNG","Diffuse ring observation","UV Ring Spectroscopy"]
["2004-270T20:30:00","000T06:49:36","2004-09-26","CAPS","Non-SPASS","Saturn","BURST16K","16 kbps burst","Burst of 16kbps data","Burst of 16 kbps data (which gives uncollapsed ELS data). 32 B cycles duration. Data is in addition to 1000 bps survey rate."]
["2004-270T20:57:00","000T04:25:00","2004-09-26","UVIS","Prime","Saturn","MOS0AGEH","Apoapsis mosaic","MOSAIC_APO_01_09n","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with the Saturn spin axis.  1) Slew about the Z-axis from Saturn Center to -MOS Orb. Rotate +64mrad in the YZ plane. 2) Drift at a rate of .0312 mrad/sec about the Z-axis toward +MOS Orb for 13900s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time.  MOS Orb (+/-Range): 233.88mrad."]
["2004-270T20:57:00","000T04:25:00","2004-09-26","ISS","SPASS Rider","Saturn","MOS0AGEH","Apoapsis mosaic","UVIS Ride-along for dark images","Ride along during system scans take 5 dark images"]
["2004-271T01:52:00","000T09:00:00","2004-09-27","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-271T10:52:00","002T07:19:59","2004-09-27","CDA","Non-SPASS","DustRAM direction","SURPCOPPL","Dust survey","dust survey","Survey measurements of dust"]
["2004-271T10:52:00","000T02:05:00","2004-09-27","INMS","Non-SPASS","Saturn","SURVEYD","MAPS survey","MAPS Survey","MAPS magnetospheric survey."]
["2004-271T10:52:00","002T07:20:00","2004-09-27","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey."]
["2004-271T10:52:00","002T07:20:00","2004-09-27","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-271T12:22:00","000T20:25:00","2004-09-27","ISS","Prime","Saturn","2X2MOVIEA","Saturn movie","Go east global Saturn movie","2X2 Saturn mosaic + spoke movie, repeat every 1:45."]
["2004-271T12:22:00","000T20:25:00","2004-09-27","CIRS","SPASS Rider","Saturn","ISSPCKT20","Saturn movie","Saturn Movie pickets","Saturn Movie pickets"]
["2004-271T12:22:00","000T20:25:00","2004-09-27","UVIS","SPASS Rider","Saturn","2X2MOVIEA","Saturn movie","ISS 2X2MOVIEA Rider","UVIS EUV and FUV riding along with ISS 2X2MOVIEA observation"]
["2004-271T12:22:00","000T20:25:00","2004-09-27","VIMS","SPASS Rider","Saturn","FRGLOB","Saturn far encounter global mosaic","Saturn Far Global Mosaic, Go-East Template  #15","Saturn Far Encounter Global Mosaic under Go-East Template #15. 20-hour duration. 12 pickets acquired over these 20 hours. ISS movie  pickets each last 1:00. Then CD CIRS observations for 45 minutes. Total cycle time is 1:45.  Data volume: 12 observations * 2 exposures * 64*64*352*12 = 420 mbits"]
["2004-271T12:57:00","000T00:33:00","2004-09-27","INMS","Non-SPASS","Saturn","MRO","Instrument memory readout","MAPS Survey","MAPS magnetospheric survey."]
["2004-271T13:30:00","002T04:42:00","2004-09-27","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey."]
["2004-272T09:17:00","000T09:00:00","2004-09-28","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-272T10:57:00","000T06:00:00","2004-09-28","CIRS","SPASS Rider","InstrumentCalibration","DSCALTMP","Deep space calibration","Deep Space Calibration","Deep space cal."]
["2004-272T19:47:00","000T05:15:00","2004-09-28","ISS","Prime","Saturn","2X2MOVIEB","Saturn movie","Go east global Saturn movie","2X2 Saturn mosaic + spoke movie, repeat every 1:45."]
["2004-272T19:47:00","000T05:15:00","2004-09-28","CIRS","SPASS Rider","Saturn","ISSPCKT03","Saturn movie","Saturn Movie Pickets","Movie picket rider"]
["2004-272T19:47:00","000T05:15:00","2004-09-28","UVIS","SPASS Rider","Saturn","2X2MOVIEB","Saturn movie","ISS 2X2MOVIEB Rider","UVIS EUV and FUV riding along with ISS 2X2MOVIEB observation"]
["2004-272T19:47:00","000T05:15:00","2004-09-28","VIMS","SPASS Rider","Saturn","FRGLOB","Saturn far encounter global mosaic","Saturn Far Global Mosaic, Go-East Template  #16","Saturn Far Encounter Global Mosaic under Go-East Template #16. 5.25-hour duration. 3 pickets acquired over these 5.25 hours. ISS movie  pickets each last 1:00. Then CD CIRS observations for 45 minutes. Total cycle time is 1:45.  Data volume: 3 observations * 2 exposures * 64*64*352*12 = 105 mbits"]
["2004-273T01:02:00","000T07:30:00","2004-09-29","UVIS","Prime","Saturn","MOS0AGEH","Apoapsis mosaic","MOSAIC_APO_01_09o","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with the Saturn spin axis.  1) Slew about the Z-axis from Saturn Center to -MOS Orb. 2) Drift at a rate of .0322 mrad/sec about the Z-axis for 15000s to +MOS Orb.  3) Rotate -64mrad in the YZ plane.  Drift at the indicated rate toward -MOS Orb for 9500s.  4) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 241.13mrad."]
["2004-273T01:02:00","000T04:55:00","2004-09-29","ISS","SPASS Rider","Saturn","MOS0AGEH","Apoapsis mosaic","UVIS Ride-along for dark images","Ride along during system scans take 5 dark images"]
["2004-273T09:12:00","000T09:00:00","2004-09-29","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-273T18:12:00","000T16:25:00","2004-09-29","CDA","Non-SPASS","DustRAM direction","SURPCOPPL","Dust survey","dust survey","Survey measurements of dust"]
["2004-273T18:12:00","000T16:25:00","2004-09-29","INMS","Non-SPASS","Saturn","SURVEYA","MAPS survey","MAPS Survey","MAPS magnetospheric survey."]
["2004-273T18:12:00","000T16:25:00","2004-09-29","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey."]
["2004-273T18:12:00","000T16:25:00","2004-09-29","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-273T19:42:00","000T01:00:00","2004-09-29","ISS","Prime","rings(general)","DIFFUSRNG","Diffuse ring observation","DIFFUSE RINGS, GO EAST TEMPLATE, 012 TH OBSERVATIO","DIFFUSE RINGS IN REV 00A, GO EAST TEMPLATE"]
["2004-273T19:42:00","000T01:00:00","2004-09-29","UVIS","SPASS Rider","rings(general)","DIFFUSRNG","Diffuse ring observation","UV Ring Spectroscopy"]
["2004-273T20:30:00","000T06:49:36","2004-09-29","CAPS","Non-SPASS","Saturn","BURST16K","16 kbps burst","Burst of 16kbps data","Burst of 16 kbps data (which gives uncollapsed ELS data). 32 B cycles duration. Data is in addition to 1000 bps survey rate."]
["2004-273T20:42:00","000T04:25:00","2004-09-29","UVIS","Prime","Saturn","MOS0AGEI","Apoapsis mosaic","MOSAIC_APO_01_09q","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with the Saturn spin axis. 1) Slew about the Z-axis from Saturn Center to +MOS Orb.  2) Drift at a rate of .0326 mrad/sec about the Z-axis toward -MOS Orb for 13900s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 244.16mrad."]
["2004-273T20:42:00","000T04:25:00","2004-09-29","ISS","SPASS Rider","Saturn","MOS0AGEI","Apoapsis mosaic","UVIS Ride-along for dark images","Ride along during system scans take 5 dark images"]
["2004-274T01:37:00","000T09:00:00","2004-09-30","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-274T10:37:00","002T02:20:00","2004-09-30","INMS","Non-SPASS","Saturn","SURVEYB","MAPS survey","MAPS Survey","MAPS magnetospheric survey."]
["2004-274T10:37:00","004T13:23:00","2004-09-30","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey."]
["2004-274T10:37:00","004T13:23:00","2004-09-30","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-274T10:37:01","011T00:03:58","2004-09-30","CDA","Non-SPASS","DustRAM direction","SURPCOPPL","Dust survey","dust survey","Survey measurements of dust"]
["2004-274T12:07:00","000T20:25:00","2004-09-30","ISS","Prime","Saturn","2X2MOVIEA","Saturn movie","Go east global Saturn movie","2X2 Saturn mosaic + spoke movie, repeat every 1:45."]
["2004-274T12:07:00","000T20:25:00","2004-09-30","CIRS","SPASS Rider","Saturn","ISSPCKT20","Saturn movie","Saturn Movie pickets","Saturn Movie pickets"]
["2004-274T12:07:00","000T20:25:00","2004-09-30","UVIS","SPASS Rider","Saturn","2X2MOVIEA","Saturn movie","ISS 2X2MOVIEA Rider","UVIS EUV and FUV riding along with ISS 2X2MOVIEA observation"]
["2004-274T12:07:00","000T20:25:00","2004-09-30","VIMS","SPASS Rider","Saturn","FRGLOB","Saturn far encounter global mosaic","Saturn Far Global Mosaic, Go-East Template  #17","Saturn Far Encounter Global Mosaic under Go-East Template #17. 20-hour duration. 12 pickets acquired over these 20 hours. ISS movie  pickets each last 1:00. Then CD CIRS observations for 45 minutes. Total cycle time is 1:45.  Data volume: 12 observations * 2 exposures * 64*64*352*12 = 420 mbits"]
["2004-275T09:02:00","000T09:00:00","2004-10-01","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-275T19:32:00","000T05:15:00","2004-10-01","ISS","Prime","Saturn","2X2MOVIEB","Saturn movie","Go east global Saturn movie","2X2 Saturn mosaic + spoke movie, repeat every 1:45."]
["2004-275T19:32:00","000T05:15:00","2004-10-01","CIRS","SPASS Rider","Saturn","ISSPCKT03","Saturn movie","Saturn Movie Pickets","Movie picket rider"]
["2004-275T19:32:00","000T05:15:00","2004-10-01","UVIS","SPASS Rider","Saturn","2X2MOVIEB","Saturn movie","ISS 2X2MOVIEB Rider","UVIS EUV and FUV riding along with ISS 2X2MOVIEB observation"]
["2004-275T19:32:00","000T05:15:00","2004-10-01","VIMS","SPASS Rider","Saturn","FRGLOB","Saturn far encounter global mosaic","Saturn Far Global Mosaic, Go-East Template  #18","Saturn Far Encounter Global Mosaic under Go-East Template #18. 5.25-hour duration. 3 pickets acquired over these 5.25 hours. ISS movie  pickets each last 1:00. Then CD CIRS observations for 45 minutes. Total cycle time is 1:45.  Data volume: 3 observations * 2 exposures * 64*64*352*12 = 105 mbits"]
["2004-276T00:47:00","000T07:30:00","2004-10-02","UVIS","Prime","Saturn","MOS0AGEI","Apoapsis mosaic","MOSAIC_APO_01_09r","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel to the Saturn spin axis. 1) Slew about the Z-axis from Saturn Center to +MOS Orb. Rotate -64mrad in the YZ plane.  2) Drift at a rate of .0115 mrad/sec about the Z-axis for 15000s to -MOS Orb. 3) Rotate +128mrad in the YZ plane. Drift at indicated rate toward +MOS Orb for 9500s. 4) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 86.00mrad."]
["2004-276T00:47:00","000T04:55:00","2004-10-02","ISS","SPASS Rider","Saturn","MOS0AGEI","Apoapsis mosaic","UVIS Ride-along for dark images","Ride along during system scans take 5 dark images"]
["2004-276T08:58:00","000T09:00:00","2004-10-02","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-276T12:57:00","000T00:33:00","2004-10-02","INMS","Non-SPASS","Saturn","MRO","Instrument memory readout","MAPS Survey","MAPS magnetospheric survey."]
["2004-276T13:30:00","004T23:27:00","2004-10-02","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey."]
["2004-277T01:23:00","000T09:00:00","2004-10-03","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-278T08:48:00","000T09:00:00","2004-10-04","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-279T00:00:00","006T10:54:00","2004-10-05","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2004-279T00:00:00","006T17:29:00","2004-10-05","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-279T00:00:01","006T17:06:59","2004-10-05","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SUR Campaign","Part of SUR MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2004-279T08:43:00","000T09:00:00","2004-10-05","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-279T19:13:00","000T01:00:00","2004-10-05","ISS","Prime","rings(general)","DIFFUSRNG","Diffuse ring observation","DIFFUSE RINGS, GO EAST TEMPLATE, 014 TH OBSERVATIO","DIFFUSE RINGS IN REV 00A, GO EAST TEMPLATE"]
["2004-279T20:13:00","000T04:25:00","2004-10-05","UVIS","Prime","Saturn","MOS0AGEK","Apoapsis mosaic","MOSAIC_APO_01_10c","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel to the Saturn spin axis.  1) Slew about the Z-Axis from Saturn Center to +MOS Orb and rotate +64mrad in the YZ plane.  2) Drift at a rate of .0124 mrad/sec about the Z-axis toward -MOS Orb for 13900s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb(+/-Range): 92.85mrad."]
["2004-280T01:13:00","000T09:00:00","2004-10-06","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-280T12:00:00","000T00:30:00","2004-10-06","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 120 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [PA-EP-TL-EN-DI (602, 604, 611, 613, 617)]"]
["2004-280T12:30:00","000T03:00:00","2004-10-06","ISS","Prime","Saturn","SATSYSTEM","Saturn system image","Saturn system PR observation","Do observations of satellites (NAC), Saturn, and rings (NAC and WAC), turn to WP. For a detailed description, see notes entry field."]
["2004-280T15:30:00","000T00:30:00","2004-10-06","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 121 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [AT-JA-CP-PM-PA (610, 614, 615, 616, 617)]"]
["2004-280T16:30:00","000T09:00:00","2004-10-06","UVIS","Prime","Star","URXICET","Stellar occultation","URSTAR","Instance of URSTAR. This very slow occultation near apoapse provides an excellent opportunity for high resolution studies of low optical depth regions in the rings. This part of the occultation covers the ring system interior to the B Ring."]
["2004-281T02:00:00","000T05:50:00","2004-10-07","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-281T03:30:00","000T06:00:00","2004-10-07","CIRS","SPASS Rider","InstrumentCalibration","DSCALTMP","Deep space calibration","Deep Space Calibration","Deep space cal."]
["2004-281T08:20:00","000T07:20:00","2004-10-07","UVIS","Prime","Star","URXICET","Stellar occultation","URSTAR","Instance of URSTAR. This very slow occultation near apoapse provides an excellent opportunity for high resolution studies of low optical depth regions in the rings. This part of the occultation covers the ring system exterior to the B Ring."]
["2004-281T12:57:00","000T00:33:00","2004-10-07","INMS","Non-SPASS","Saturn","MRO","Instrument memory readout","MAPS Survey","MAPS magnetospheric survey."]
["2004-281T13:30:00","003T21:13:00","2004-10-07","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey."]
["2004-281T16:26:00","000T01:15:00","2004-10-07","ISS","Prime","Iapetus","GLOBCOLA","Global coverage observation","Iapetus global color observation","Turn -Y to Iapetus; do 1x1 mosaic 2 NAC clear + 25 NAC color + 9 NAC polarizer + 4 WAC polarizer filters; turn -Y to WP"]
["2004-281T16:26:00","000T01:15:00","2004-10-07","CIRS","SPASS Rider","Iapetus","GLOBCOLA","Global coverage observation","Iapetus rider","Integrate FP3, FP4 at high spectral resolution (0.5 cm-1).  AD~0.6 mrad, long~245 (Roncevaux Terra), phase~45."]
["2004-281T16:26:00","000T01:15:00","2004-10-07","UVIS","SPASS Rider","Iapetus","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2004-281T16:26:00","000T01:15:00","2004-10-07","VIMS","SPASS Rider","Iapetus","GLOBCOLA","Global coverage observation","Iapetus southern anti-Saturn hemisphere","Multiple 640ms 12x12 cubes"]
["2004-281T20:00:00","000T00:30:00","2004-10-07","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 124 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [PM-AT-DI-EP-EN (602, 604, 611, 615, 616)]"]
["2004-281T20:30:00","000T10:45:00","2004-10-07","ISS","Prime","Phoebe","002PHO","Phoebe spectrophotometery","Phoebe Spectrophotometry","Turn -Y to Phoebe, do during one Phoebe rotation 6 1x1 mosaics, 4 color, 3 polarizer filters, turn to WP."]
["2004-281T20:30:00","000T10:45:00","2004-10-07","UVIS","SPASS Rider","Phoebe","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2004-282T08:44:00","000T09:00:00","2004-10-08","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-282T19:14:00","000T01:00:00","2004-10-08","ISS","Prime","rings(general)","DIFFUSRNG","Diffuse ring observation","DIFFUSE RINGS, GO EAST TEMPLATE, 015 TH OBSERVATIO","DIFFUSE RINGS IN REV 00A, GO EAST TEMPLATE"]
["2004-282T20:14:00","000T04:15:00","2004-10-08","UVIS","Prime","Saturn","MOS0AGEL","Apoapsis mosaic","MOSAIC_APO_01_10f","Mosaic of Saturn inner magnetosphere.  EUV and FUV low resolution slits on, aligned parallel to the Saturn spin axis. 1) Slew about the Z-Axis from Saturn Center to -MOS Orb. Rotate -64mrad in the YZ Plane.   2) Drift at a rate of .0134 mrad/sec about the Z-axis toward +MOS Orb for 13900s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 100.18mrad."]
["2004-283T00:59:00","000T09:00:00","2004-10-09","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-283T11:34:00","000T07:00:00","2004-10-09","ISS","Prime","Saturn","2X2MOVIEA","Saturn movie","Go east global Saturn movie","2X2 Saturn mosaic + spoke movie, repeat every 1:30."]
["2004-283T11:34:00","000T09:10:00","2004-10-09","CAPS","SPASS Rider","InstrumentCalibration","CALIBRATE","Calibration","CAPS Calibration","CAPS periodic gain test and calibration. The specified rate and data volume are the delta above the CAPS survey rate (1000 bps), and the rate is the average over the entire request (current plans are to conduct the test in two different rates.)"]
["2004-283T11:34:00","000T20:25:00","2004-10-09","CIRS","SPASS Rider","Saturn","ISSPCKT20","Saturn movie","Saturn Movie pickets","Saturn Movie pickets"]
["2004-283T11:34:00","000T07:00:00","2004-10-09","UVIS","SPASS Rider","Saturn","2X2MOVIEA","Saturn movie","ISS 2X2MOVIEA Rider","UVIS EUV and FUV riding along with ISS 2X2MOVIEA observation"]
["2004-283T11:34:00","000T20:25:00","2004-10-09","VIMS","SPASS Rider","Saturn","FRGLOB","Saturn far encounter global mosaic","Saturn Far Global Mosaic, Go-East Template  #23","Saturn Far Encounter Global Mosaic under Go-East Template #23. 20-hour duration. 12 pickets acquired over these 20 hours. ISS movie  pickets each last 1:00. Then CD CIRS observations for 45 minutes. Total cycle time is 1:45.  Data volume: 12 observations * 2 exposures * 64*64*352*12 = 420 mbits"]
["2004-283T18:34:00","000T00:30:00","2004-10-09","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 129 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [PM-EN-DI-JA-PA (602, 604, 610, 616, 617)]"]
["2004-283T19:04:00","000T04:00:00","2004-10-09","ISS","Prime","Saturn","2X2MOVI2A","Saturn movie","Go east global Saturn movie","2X2 Saturn mosaic + spoke movie, repeat every 1:30."]
["2004-283T19:04:00","000T04:00:00","2004-10-09","UVIS","SPASS Rider","Saturn","2X2MOVI2A","Saturn movie","ISS 2X2MOVIEA Rider","UVIS EUV and FUV riding along with ISS 2X2MOVIEA observation"]
["2004-283T23:04:00","000T00:30:00","2004-10-09","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 130 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [TL-AT-PM-EP-HE (611, 612, 613, 615, 616)]"]
["2004-283T23:34:00","000T05:30:00","2004-10-09","ISS","Prime","Saturn","2X2MOVI3A","Saturn movie","Go east global Saturn movie","2X2 Saturn mosaic + spoke movie, repeat every 1:30."]
["2004-283T23:34:00","000T05:30:00","2004-10-09","UVIS","SPASS Rider","Saturn","2X2MOVI3A","Saturn movie","ISS 2X2MOVIEA Rider","UVIS EUV and FUV riding along with ISS 2X2MOVIEA observation"]
["2004-284T05:04:00","000T00:30:00","2004-10-10","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 131 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [EP-AT-PM-EN-JA (602, 610, 611, 615, 616)]"]
["2004-284T05:34:00","000T02:25:00","2004-10-10","ISS","Prime","Saturn","2X2MOVI4A","Saturn movie","Go east global Saturn movie","2X2 Saturn mosaic + spoke movie, repeat every 1:30."]
["2004-284T05:34:00","000T02:25:00","2004-10-10","UVIS","SPASS Rider","Saturn","2X2MOVI4A","Saturn movie","ISS 2X2MOVIEA Rider","UVIS EUV and FUV riding along with ISS 2X2MOVIEA observation"]
["2004-284T08:29:00","000T09:00:00","2004-10-10","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-284T09:59:00","000T06:00:00","2004-10-10","CIRS","SPASS Rider","InstrumentCalibration","DSCALTMP","Deep space calibration","Deep Space Calibration","Deep space cal."]
["2004-284T19:59:00","000T00:30:00","2004-10-10","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 133 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [CP-PM-AT-HE-JA (610, 612, 614, 615, 616)]"]
["2004-284T20:29:00","000T10:50:00","2004-10-10","UVIS","Prime","Saturn","MOS0AGEL","Apoapsis mosaic","MOSAIC_APO_01_10i","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel to the Saturn spin axis. 1) Slew about the Z-Axis from Saturn Center to +MOS Orb. Rotate +64mrad in the YZ Plane.  2) Drift at a rate of .0143 mrad/sec about the Z-axis for 15000s to -MOS Orb.  3) Rotate -64mrad in the YZ Plane.  Drift at indicated rate about the Z-axis for 15000s to +MOS Orb.  4) Rotate -64mrad in the YZ Plane.  Drift at indicated rate about the Z-axis toward -MOS Orb for 7000s.  5) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb(+/-Range): 106.81mrad."]
["2004-285T07:19:00","000T00:30:00","2004-10-11","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 134 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [EP-EN-TL-DI-PA (602, 604, 611, 613, 617)]"]
["2004-285T10:41:00","000T06:19:00","2004-10-11","CDA","Non-SPASS","Saturn","PPL","Huygens Probe support","Probe Patch Load","Mute for PPL. Sleep/Mute Unmute/Active Commands pointing: NA; datavolume=0 MB"]
["2004-285T10:42:00","000T00:17:00","2004-10-11","CIRS","Non-SPASS","Other","PROBEMUTE","Huygens Probe support","Sleep/mute placeholder","Put CIRS to sleep/mute for probe patch load, mute at epoch -00:06"]
["2004-285T10:43:00","000T00:10:00","2004-10-11","INMS","Non-SPASS","SpacecraftActivity","SLEEP","Instrument to sleep mode","INMS Sleep and Mute for Probe C/O","null"]
["2004-285T10:44:00","000T00:09:50","2004-10-11","ISS","Non-SPASS","Earth","SLEEPMUTE","Huygens probe support","put ISS to sleep for probe activity","placeholder activity put into CIMS to remenind ISS to go into sleep for probe activity at request of MAG TWT"]
["2004-285T10:50:00","000T00:03:00","2004-10-11","UVIS","Non-SPASS","Saturn","SLEEPMUTE","Huygens probe support","UVIS TO SLEEP/MUTE (Probe Patch Load)","UVIS to go to sleep/mute for Probe Patch Load (MGTWT request)"]
["2004-285T10:51:00","000T00:05:00","2004-10-11","VIMS","Non-SPASS","SpacecraftActivity","SLEEPMUTE","Huygens probe support","VIMS to SLEEP / MUTE","VIMS to SLEEP/ MUTE"]
["2004-285T10:53:00","000T06:07:00","2004-10-11","INMS","Non-SPASS","SpacecraftActivity","MUTE","Instrument to sleep mode","INMS Mute for Probe Patch","null"]
["2004-285T10:54:00","000T06:05:00","2004-10-11","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey."]
["2004-285T16:59:00","000T00:30:00","2004-10-11","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2004-285T17:00:00","000T00:28:59","2004-10-11","CDA","Non-SPASS","DustRAM direction","SURAFTPPL","Dust survey","dust survey","Survey measurements of dust"]
["2004-285T17:00:00","000T00:04:00","2004-10-11","CIRS","Non-SPASS","Other","PROUNMUTE","Huygens Probe support","wake/unmute placeholder","UNMUTE.  Note power transients!, unmute at 00:06, wake at epoch+00:09"]
["2004-285T17:00:00","000T00:04:00","2004-10-11","INMS","Non-SPASS","SpacecraftActivity","UNMUTE","Huygens probe support","INMS UnMute after Probe Patch","null"]
["2004-285T17:00:00","000T00:07:00","2004-10-11","ISS","Non-SPASS","Earth","WAKESLEEP","Wakeup instrument from sleep mode","wake up  ISS after probe activity","placeholder activity put into CIMS to remind ISS to wake up after probe activity at request of MAG TWT"]
["2004-285T17:00:00","000T00:11:00","2004-10-11","UVIS","Non-SPASS","Saturn","UNMUTEWAK","Huygens probe support","UVIS to unmute and wake up after probe patch load","Unmute/go to active after probe patch load (MAGTWT request)"]
["2004-285T17:00:00","000T00:05:00","2004-10-11","VIMS","Non-SPASS","SpacecraftActivity","WAKEUP","Wakeup instrument from sleep mode","VIMS to Active Mode","VIMS to ACTIVE"]
["2004-285T17:04:00","000T00:25:00","2004-10-11","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey."]
["2004-285T17:07:00","002T23:45:00","2004-10-11","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SUR Campaign","Part of SUR MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2004-285T17:29:00","000T16:15:00","2004-10-11","CDA","Non-SPASS","DustRAM direction","SURAFTPPL","Dust survey","dust survey","Survey measurements of dust"]
["2004-285T17:29:00","000T16:15:00","2004-10-11","INMS","Non-SPASS","Saturn","SURVEYA","MAPS survey","MAPS Survey","MAPS magnetospheric survey."]
["2004-285T17:29:00","000T16:15:00","2004-10-11","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2004-285T17:29:00","000T16:15:00","2004-10-11","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-285T18:59:00","000T01:15:00","2004-10-11","ISS","Prime","Iapetus","GLOBCOLB","Global coverage observation","Iapetus global color observation","Turn -Y to Iapetus; do 1x1 mosaic 2 NAC clear + 25 NAC color + 9 NAC polarizer + 4 WAC polarizer filters; turn -Y to WP"]
["2004-285T18:59:00","000T01:15:00","2004-10-11","CIRS","SPASS Rider","Iapetus","GLOBCOLB","Global coverage observation","Iapetus rider","Integrate FP3, FP4 at high spectral resolution (0.5 cm-1).  AD~0.75 mrad, long~220 (Roncevaux Terra), phase~58."]
["2004-285T18:59:00","000T01:15:00","2004-10-11","UVIS","SPASS Rider","Iapetus","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2004-285T18:59:00","000T01:15:00","2004-10-11","VIMS","SPASS Rider","Iapetus","GLOBCOLB","Global coverage observation","Iapetus","Multiple 640ms 12x12 cubes (double resolution)"]
["2004-285T20:14:00","000T00:30:00","2004-10-11","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 136 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [PA-EN-JA-PM-AT (602, 610, 615, 616, 617)]"]
["2004-285T20:30:00","000T04:33:04","2004-10-11","CAPS","Non-SPASS","Saturn","BURST16K","16 kbps burst","Burst of 16kbps data","Burst of 16 kbps data (which gives uncollapsed ELS data). 32 B cycles duration. Data is in addition to 1000 bps survey rate."]
["2004-285T20:44:00","000T03:30:00","2004-10-11","UVIS","Prime","Saturn","MOS0AGEM","Apoapsis mosaic","MOSAIC_APO_01_11b","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel to the Saturn spin axis. 1) Slew about the Z-axis from Saturn Center to +MOS Orb. Rotate +64mrad in the YZ Plane.  2) Drift at a rate of .0147 mrad/sec about the Z-axis toward -MOS Orb for 10600s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 109.96mrad."]
["2004-286T00:44:00","000T09:00:00","2004-10-12","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-286T09:44:00","000T03:13:00","2004-10-12","INMS","Non-SPASS","Saturn","SURVEYB","MAPS survey","MAPS Survey","MAPS magnetospheric survey."]
["2004-286T09:44:00","002T00:55:00","2004-10-12","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2004-286T09:44:00","002T07:30:00","2004-10-12","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-286T09:44:01","002T00:41:59","2004-10-12","CDA","Non-SPASS","DustRAM direction","SURAFTPPL","Dust survey","dust survey","Survey measurements of dust"]
["2004-286T11:14:00","000T06:25:00","2004-10-12","ISS","Prime","Saturn","2X2MOVIEA","Saturn movie","Go east global Saturn movie","2X2 Saturn mosaic + spoke movie, repeat every 1:45."]
["2004-286T11:14:00","000T11:40:00","2004-10-12","CIRS","SPASS Rider","Saturn","ISSPCKT20","Saturn movie","Saturn Movie pickets","Saturn Movie pickets with SATELORBS"]
["2004-286T11:14:00","000T06:25:00","2004-10-12","UVIS","SPASS Rider","Saturn","2X2MOVIEA","Saturn movie","ISS 2X2MOVIEA Rider","UVIS EUV and FUV riding along with ISS 2X2MOVIEA observation"]
["2004-286T11:14:00","000T20:25:00","2004-10-12","VIMS","SPASS Rider","Saturn","FRGLOB","Saturn far encounter global mosaic","Saturn Far Global Mosaic, Go-East Template  #25","Saturn Far Encounter Global Mosaic under Go-East Template #25. 20-hour duration. 12 pickets acquired over these 20 hours. ISS movie  pickets each last 1:00. Then CD CIRS observations for 45 minutes. Total cycle time is 1:45.  Data volume: 12 observations * 2 exposures * 64*64*352*12 = 420 mbits"]
["2004-286T12:57:00","000T00:33:00","2004-10-12","INMS","Non-SPASS","Saturn","MRO","Instrument memory readout","MAPS Survey","MAPS magnetospheric survey."]
["2004-286T13:30:00","001T20:58:00","2004-10-12","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey."]
["2004-286T17:39:00","000T00:30:00","2004-10-12","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 139 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [JA-EN-PM-AT-EP (602, 610, 611, 615, 616)]"]
["2004-286T18:14:00","000T04:40:00","2004-10-12","ISS","Prime","Saturn","2X2MOVI2A","Saturn movie","Go east global Saturn movie","2X2 Saturn mosaic + spoke movie, repeat every 1:45."]
["2004-286T18:14:00","000T04:40:00","2004-10-12","UVIS","SPASS Rider","Saturn","2X2MOVI2A","Saturn movie","ISS 2X2MOVIEA Rider","UVIS EUV and FUV riding along with ISS 2X2MOVIEA observation"]
["2004-286T22:54:00","000T00:30:00","2004-10-12","ISS","Prime","Iapetus","GLOBMAPC","Global coverage mapping","Iapetus global mapping","Turn -Y to Iapetus; do 1x1 mosaic 2 NAC clear + 3 NAC color filters; turn to WP"]
["2004-286T22:54:00","000T00:30:00","2004-10-12","CIRS","SPASS Rider","Iapetus","GLOBMAPC","Global coverage mapping","Iapetus rider","Integrate FP3, FP4 at high spectral resolution (0.5 cm-1).  AD~0.75 mrad, long~230 (Roncevaux Terra), phase~65."]
["2004-286T22:54:00","000T00:30:00","2004-10-12","UVIS","SPASS Rider","Iapetus","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2004-286T23:29:00","000T04:40:00","2004-10-12","ISS","Prime","Saturn","2X2MOVI3A","Saturn movie","Go east global Saturn movie","2X2 Saturn mosaic + spoke movie, repeat every 1:45."]
["2004-286T23:29:00","000T08:05:00","2004-10-12","CIRS","SPASS Rider","Saturn","ISSPCKT2I","Saturn movie","Saturn Movie pickets","Saturn Movie pickets and SATELORBs."]
["2004-286T23:29:00","000T04:40:00","2004-10-12","UVIS","SPASS Rider","Saturn","2X2MOVI3A","Saturn movie","ISS 2X2MOVIEA Rider","UVIS EUV and FUV riding along with ISS 2X2MOVIEA observation"]
["2004-287T04:09:00","000T00:30:00","2004-10-13","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 140 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [PA-EP-EN-JA-DI (602, 604, 610, 611, 617)]"]
["2004-287T04:39:00","000T02:55:00","2004-10-13","ISS","Prime","Saturn","2X2MOVI4A","Saturn movie","Go east global Saturn movie","2X2 Saturn mosaic + spoke movie, repeat every 1:45."]
["2004-287T04:39:00","000T02:55:00","2004-10-13","UVIS","SPASS Rider","Saturn","2X2MOVI4A","Saturn movie","ISS 2X2MOVIEA Rider","UVIS EUV and FUV riding along with ISS 2X2MOVIEA observation"]
["2004-287T08:14:00","000T09:00:00","2004-10-13","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-287T08:44:00","000T06:00:00","2004-10-13","CIRS","SPASS Rider","InstrumentCalibration","DSCALTMP","Deep space calibration","Deep Space Calibration","Deep space cal."]
["2004-287T18:49:00","000T00:30:00","2004-10-13","ISS","Prime","Iapetus","LIMBTOPOD","Limb topography and geodesy observation","Iapetus limb topography and geodesy obs.","Turn -Y to Iapetus; do 1x1 mosaic 2 NAC clear + 3 NAC color filters"]
["2004-287T18:49:00","000T00:30:00","2004-10-13","CIRS","SPASS Rider","Iapetus","LIMBTOPOD","Limb topography and geodesy observation","Iapetus rider","Integrate FP3, FP4 at high spectral resolution (0.5 cm-1).  AD~1.1 mrad, long~220 (Roncevaux Terra), phase~80."]
["2004-287T18:49:00","000T00:30:00","2004-10-13","UVIS","SPASS Rider","Iapetus","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2004-287T19:19:00","000T01:20:00","2004-10-13","ISS","Prime","Iapetus","HILLSPHEC","Hill sphere observation","Iapetus Hill sphere observation","Do 5x5 NAC clear filter mosaic of Hill sphere around Iapetus two times."]
["2004-287T19:19:00","000T01:20:00","2004-10-13","CIRS","SPASS Rider","Iapetus","HILLSPHEC","Hill sphere observation","Iapetus rider","Integrate FP3, FP4 at high spectral resolution (0.5 cm-1).  AD~1.05 mrad, long~230 (W. Cassini Regio), phase~80."]
["2004-287T19:19:00","000T01:20:00","2004-10-13","UVIS","SPASS Rider","Iapetus","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2004-287T20:50:00","000T00:30:00","2004-10-13","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 142 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [TL-PM-AT-EP-PA (611, 613, 615, 616, 617)]"]
["2004-287T22:00:00","000T00:45:00","2004-10-13","ISS","Prime","rings(general)","RNGPHOTMA","Ring photometry","RING PHOTOM","3X3 NACS IN 5 COLORS ON RIGHT ANSA;"]
["2004-287T22:45:00","000T01:00:00","2004-10-13","RADAR","SPASS Rider","Other","ENGTEST","Engineering test","Engineering Test of Diagnostic Modes","Engineering test of diagnostic modes on the flight unit."]
["2004-288T00:04:00","000T07:30:00","2004-10-14","UVIS","Prime","Saturn","MOS0AGEM","Apoapsis mosaic","MOSAIC_APO_01_11c","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with the Saturn spin axis. 1) Slew about the Z-Axis from Saturn Center to +MOS Orb.  2) Drift at a rate of .0159 mrad/sec about the Z-axis for 15000s to -MOS Orb.  3) Rotate -64mrad in the YZ Plane.  Drift at indicated rate about the Z-Axis toward +MOS Orb for 9500s.  4) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 119.21mrad."]
["2004-288T10:26:00","000T06:21:00","2004-10-14","CDA","Non-SPASS","Saturn","PPL","Huygens Probe support","Probe Patch Load BU","Mute for PPL. Sleep/Mute Unmute/Active activities for CDA pointing: NA; datavolume=0 MB"]
["2004-288T10:27:00","000T00:17:00","2004-10-14","CIRS","Non-SPASS","Other","PROBEMUTE","Huygens Probe support","Sleep/mute placeholder","Put CIRS to sleep/mute for probe patch load BU, mute at epoch -00:06"]
["2004-288T10:28:00","000T00:10:00","2004-10-14","INMS","Non-SPASS","SpacecraftActivity","SLEEP","Instrument to sleep mode","INMS Sleep and Mute for Probe C/O","null"]
["2004-288T10:29:00","000T00:09:50","2004-10-14","ISS","Non-SPASS","Earth","SLEEPMUTE","Huygens probe support","put ISS to sleep for probe activity","placeholder activity put into CIMS to remenind ISS to go into sleep for probe activity at request of MAG TWT"]
["2004-288T10:35:00","000T00:03:00","2004-10-14","UVIS","Non-SPASS","Saturn","SLEEPMUTE","Huygens probe support","UVIS TO SLEEP/MUTE for probe patch backup","UVIS to go to sleep/mute for probe patch backup"]
["2004-288T10:36:00","000T00:05:00","2004-10-14","VIMS","Non-SPASS","SpacecraftActivity","SLEEPMUTE","Huygens probe support","VIMS to SLEEP / MUTE","VIMS to SLEEP/ MUTE"]
["2004-288T10:38:00","000T06:07:00","2004-10-14","INMS","Non-SPASS","SpacecraftActivity","MUTE","Instrument to sleep mode","INMS Mute for Probe Patch  Back Up","null"]
["2004-288T10:39:00","000T06:05:00","2004-10-14","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey."]
["2004-288T16:44:00","000T00:30:00","2004-10-14","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2004-288T16:45:00","000T00:04:00","2004-10-14","CIRS","Non-SPASS","Other","PROUNMUTE","Huygens Probe support","wake/unmute placeholder","UNMUTE.  Note power transients!, unmute at 00:06, wake at epoch+00:09"]
["2004-288T16:45:00","000T00:04:00","2004-10-14","INMS","Non-SPASS","SpacecraftActivity","UNMUTE","Huygens probe support","INMS UnMute after Probe Patch BackUp","null"]
["2004-288T16:45:00","000T00:07:00","2004-10-14","ISS","Non-SPASS","Earth","WAKESLEEP","Wakeup instrument from sleep mode","wake up  ISS after probe activity","placeholder activity put into CIMS to remind ISS to wake up after probe activity at request of MAG TWT"]
["2004-288T16:45:00","000T00:11:00","2004-10-14","UVIS","Non-SPASS","Saturn","UNMUTEWAK","Huygens probe support","UVIS to unmute and wake up after patch backup","Unmute/go to active after probe depassivation"]
["2004-288T16:45:00","000T00:05:00","2004-10-14","VIMS","Non-SPASS","SpacecraftActivity","WAKEUP","Wakeup instrument from sleep mode","VIMS to Active Mode","VIMS to ACTIVE"]
["2004-288T16:47:00","000T00:26:59","2004-10-14","CDA","Non-SPASS","DustRAM direction","SURAFTPPL","Dust survey","Dust Survey","survey measurement of dust"]
["2004-288T16:49:00","002T20:08:00","2004-10-14","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey."]
["2004-288T16:52:00","003T16:38:00","2004-10-14","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SUR Campaign","Part of SUR MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2004-288T17:14:00","000T16:30:00","2004-10-14","CDA","Non-SPASS","DustRAM direction","SURAFTPPL","Dust survey","Dust Survey","survey measurement of dust"]
["2004-288T17:14:00","000T16:30:00","2004-10-14","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2004-288T17:14:00","000T16:30:00","2004-10-14","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-288T18:44:00","000T04:40:00","2004-10-14","UVIS","Prime","Saturn","MOS0AGEN","Apoapsis mosaic","MOSAIC_APO_01_11d","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with the Saturn spin axis. 1) Slew about the Z-axis from Saturn Center to -MOS Orb. Rotate +64mrad in the YZ Plane. 2) Drift at a rate of .0165 mrad/sec about the Z-axis toward +MOS Orb for 14800s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 123.40mrad."]
["2004-288T19:00:00","000T04:33:04","2004-10-14","CAPS","Non-SPASS","Saturn","BURST16K","16 kbps burst","Burst of 16kbps data","Burst of 16 kbps data (which gives uncollapsed ELS data). 32 B cycles duration. Data is in addition to 1000 bps survey rate."]
["2004-288T23:24:00","000T00:45:00","2004-10-14","ISS","Prime","rings(general)","RNGPHOTMA","Ring photometry","RING PHOTOMETRY OF RING ANSA","3X3 NACS IN 4 COLORS ON RIGHT ANSA"]
["2004-288T23:24:00","000T00:45:00","2004-10-14","UVIS","SPASS Rider","rings(general)","RNGPHOTMA","Ring photometry","UV Ring Spectroscopy"]
["2004-288T23:24:00","000T00:45:00","2004-10-14","VIMS","SPASS Rider","rings(general)","RNGPHOTMA","Ring photometry","Ring Mosaic","TBD"]
["2004-289T00:44:00","000T09:00:00","2004-10-15","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-289T09:44:00","002T07:16:00","2004-10-15","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2004-289T09:44:00","002T07:16:00","2004-10-15","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-289T09:44:01","002T07:15:58","2004-10-15","CDA","Non-SPASS","DustRAM direction","SURAFTPPL","Dust survey","Dust Survey","survey measurement of dust"]
["2004-289T11:14:00","000T06:25:00","2004-10-15","ISS","Prime","Saturn","2X2MOVIEA","Saturn movie","Go east global Saturn movie","2X2 Saturn mosaic + spoke movie, repeat every 1:45."]
["2004-289T11:14:00","000T11:25:00","2004-10-15","CIRS","SPASS Rider","Saturn","ISSPCKT20","Saturn movie","Saturn Movie pickets","Saturn Movie pickets and SATELORBS."]
["2004-289T11:14:00","000T06:25:00","2004-10-15","UVIS","SPASS Rider","Saturn","2X2MOVIEA","Saturn movie","ISS 2X2MOVIEA Rider","UVIS EUV and FUV riding along with ISS 2X2MOVIEA observation"]
["2004-289T11:14:00","000T20:25:00","2004-10-15","VIMS","SPASS Rider","Saturn","FRGLOB","Saturn far encounter global mosaic","Saturn Far Global Mosaic, Go-East Template  #27","Saturn Far Encounter Global Mosaic under Go-East Template #27. 20-hour duration. 12 pickets acquired over these 20 hours. ISS movie  pickets each last 1:00. Then CD CIRS observations for 45 minutes. Total cycle time is 1:45.  Data volume: 12 observations * 2 exposures * 64*64*352*12 = 420 mbits"]
["2004-289T17:39:00","000T00:30:00","2004-10-15","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 147 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [HE-PM-AT-PA-JA (610, 612, 615, 616, 617)]"]
["2004-289T18:14:00","000T04:25:00","2004-10-15","ISS","Prime","Saturn","2X2MOVI2A","Saturn movie","Go east global Saturn movie","2X2 Saturn mosaic + spoke movie, repeat every 1:45."]
["2004-289T18:14:00","000T04:25:00","2004-10-15","UVIS","SPASS Rider","Saturn","2X2MOVI2A","Saturn movie","ISS 2X2MOVIEA Rider","UVIS EUV and FUV riding along with ISS 2X2MOVIEA observation"]
["2004-289T22:39:00","000T01:00:00","2004-10-15","ISS","Prime","Iapetus","GLOBCOLF","Global coverage observation","Iapetus global color and global mapping observatio","Turn -Y to Iapetus; do 1x1 mosaic 2 NAC clear + 25 NAC color + 9 NAC polarizer + 4 WAC polarizer filters; turn -Y to WP"]
["2004-289T22:39:00","000T01:00:00","2004-10-15","CIRS","SPASS Rider","Iapetus","GLOBCOLF","Global coverage observation","Iapetus rider","Integrate FP3, FP4 at high spectral resolution (0.5 cm-1).  AD~1.2 mrad, long~200 (W. Cassini Regio), phase~95."]
["2004-289T22:39:00","000T01:00:00","2004-10-15","UVIS","SPASS Rider","Iapetus","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2004-289T22:39:00","000T01:00:00","2004-10-15","VIMS","SPASS Rider","Iapetus","GLOBCOLF","Global coverage observation","Iapetus southern anti-Saturn hemisphere","Multiple 640ms 12x12 cubes (double resolution)"]
["2004-289T23:39:00","000T04:30:00","2004-10-15","ISS","Prime","Saturn","2X2MOVI3A","Saturn movie","Go east global Saturn movie","2X2 Saturn mosaic + spoke movie, repeat every 1:45."]
["2004-289T23:39:00","000T08:00:00","2004-10-15","CIRS","SPASS Rider","Saturn","ISSPCKT2I","Saturn movie","Saturn Movie pickets","Saturn Movie pickets and SATELORBS."]
["2004-289T23:39:00","000T04:30:00","2004-10-15","UVIS","SPASS Rider","Saturn","2X2MOVI3A","Saturn movie","ISS 2X2MOVIEA Rider","UVIS EUV and FUV riding along with ISS 2X2MOVIEA observation"]
["2004-290T04:09:00","000T00:30:00","2004-10-16","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 149 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [EP-EN-TL-PM-DI (602, 604, 611, 613, 616)]"]
["2004-290T04:44:00","000T02:55:00","2004-10-16","ISS","Prime","Saturn","2X2MOVI4A","Saturn movie","Go east global Saturn movie","2X2 Saturn mosaic + spoke movie, repeat every 1:45."]
["2004-290T04:44:00","000T02:55:00","2004-10-16","UVIS","SPASS Rider","Saturn","2X2MOVI4A","Saturn movie","ISS 2X2MOVIEA Rider","UVIS EUV and FUV riding along with ISS 2X2MOVIEA observation"]
["2004-290T08:15:00","000T09:00:00","2004-10-16","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-290T18:45:00","000T00:45:00","2004-10-16","ISS","Prime","Iapetus","LIMBTOPOG","Limb topography and geodesy observation","Iapetus limb topography and geodesy obs.","Turn -Y to Iapetus; Do 1x1 mosaic 2 NAC clear + 3 NAC color filters"]
["2004-290T18:45:00","000T00:45:00","2004-10-16","CIRS","SPASS Rider","Iapetus","LIMBTOPOG","Limb topography and geodesy observation","Iapetus rider","Integrate FP3, FP4 at high spectral resolution (0.5 cm-1).  AD~1.28 mrad, long~200 (W. Cassini Regio), phase~100."]
["2004-290T18:45:00","000T00:45:00","2004-10-16","UVIS","SPASS Rider","Iapetus","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2004-290T18:45:00","000T00:45:00","2004-10-16","VIMS","SPASS Rider","Iapetus","LIMBTOPOG","Limb topography and geodesy observation","Iapetus southern anti-Saturn hemisphere","Multiple 640ms 12x12 cubes"]
["2004-290T19:30:00","000T04:00:00","2004-10-16","ISS","Prime","Iapetus","HILLSPHEF","Hill sphere observation","Iapetus Hill sphere observation","Do 5x5 NAC clear filter mosaic of Hill sphere around Iapetus two times."]
["2004-290T19:30:00","000T04:00:00","2004-10-16","CIRS","SPASS Rider","Iapetus","HILLSPHEF","Hill sphere observation","Iapetus rider","Integrate FP3, FP4 at high spectral resolution (0.5 cm-1).  AD~1.3 mrad, long~210 (W. Cassini Regio), phase~100."]
["2004-290T19:30:00","000T04:00:00","2004-10-16","UVIS","SPASS Rider","Iapetus","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2004-290T23:49:00","000T07:30:00","2004-10-16","UVIS","Prime","Saturn","MOS0AGEN","Apoapsis mosaic","MOSAIC_APO_01_12","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel to the Saturn spin axis. 1) Slew about the Z-Axis from Saturn Center to -MOS Orb. 2) Drift at a rate of .0183 mrad/sec about the Z-axis for 15000s to +MOS Orb.  3) Rotate -64mrad in the YZ Plane.  Drift at indicated rate toward -MOS Orb for 9500s.  4) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 137.18mrad."]
["2004-291T08:00:00","000T09:00:00","2004-10-17","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-291T12:57:00","000T00:33:00","2004-10-17","INMS","Non-SPASS","Saturn","MRO","Instrument memory readout","MAPS Survey","MAPS magnetospheric survey."]
["2004-291T13:30:00","000T03:30:00","2004-10-17","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey."]
["2004-291T17:00:00","000T16:30:00","2004-10-17","CDA","Non-SPASS","DustRAM direction","SURAFTPPL","Dust survey","Dust Survey","survey measurement of dust"]
["2004-291T17:00:00","000T16:30:00","2004-10-17","INMS","Non-SPASS","Saturn","SURVEYA","MAPS survey","MAPS Survey","MAPS magnetospheric survey."]
["2004-291T17:00:00","000T16:30:00","2004-10-17","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2004-291T17:00:00","000T16:30:00","2004-10-17","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-291T18:45:00","000T01:00:00","2004-10-17","ISS","Prime","rings(general)","DIFFUSRNG","Diffuse ring observation","DIFFUSE RINGS, GO EAST TEMPLATE, 018 TH OBSERVATIO","DIFFUSE RINGS IN REV 00A, GO EAST TEMPLATE"]
["2004-291T18:45:00","000T01:00:00","2004-10-17","UVIS","SPASS Rider","rings(general)","DIFFUSRNG","Diffuse ring observation","UV Ring Spectroscopy"]
["2004-291T19:00:00","000T06:49:36","2004-10-17","CAPS","Non-SPASS","Saturn","BURST16K","16 kbps burst","Burst of 16kbps data","Burst of 16 kbps data (which gives uncollapsed ELS data). 32 B cycles duration. Data is in addition to 1000 bps survey rate."]
["2004-291T19:45:00","000T00:45:00","2004-10-17","ISS","Prime","Iapetus","GLOBMAPH","Global coverage mapping","Iapetus global mapping","Turn -Y to Iapetus; do 1x1 mosaic 2 NAC clear + 3 NAC color filters; turn to WP."]
["2004-291T19:45:00","000T00:45:00","2004-10-17","CIRS","SPASS Rider","Iapetus","GLOBMAPH","Global coverage mapping","Iapetus rider","Integrate FP3, FP4 at high spectral resolution (0.5 cm-1).  AD~1.25 mrad, long~200 (W. Cassini Regio), phase~100."]
["2004-291T19:45:00","000T00:45:00","2004-10-17","UVIS","SPASS Rider","Iapetus","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2004-291T19:45:00","000T00:45:00","2004-10-17","VIMS","SPASS Rider","Iapetus","LIMBTOPOH","Limb topography and geodesy observation","Iapetus southern anti-Saturn hemisphere","Multiple 640ms 12x12 cubes"]
["2004-291T20:30:00","000T00:30:00","2004-10-17","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 154 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [PA-DI-EN-AT-JA (602, 604, 610, 615, 617)]"]
["2004-291T21:00:00","000T02:55:00","2004-10-17","UVIS","Prime","Saturn","MOS0AGEO","Apoapsis mosaic","MOSAIC_APO_01_12a","Mosaic of Saturn magnetosphere.  EUV and FUV low resolution slits on, aligned parallel to the Saturn spin axis. 1) Slew about the Z-Axis from Saturn Center to +MOS Orb. 2) Drift at a rate of .0192 mrad/sec about the Z-axis toward -MOS Orb for 8500s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 143.64mrad."]
["2004-292T00:30:00","000T09:00:00","2004-10-18","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-292T09:30:00","005T23:31:00","2004-10-18","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey"]
["2004-292T09:30:00","010T08:14:00","2004-10-18","CDA","Non-SPASS","DustRAM direction","SURAFTPPL","Dust survey","dust survey","Survey measurements of dust"]
["2004-292T09:30:00","000T01:22:00","2004-10-18","INMS","Non-SPASS","Saturn","STARTUP","Sequence startup activity","STARTUP","Startup sequence.  Load FSW, MRO, Load IEB from SSR's, MRO"]
["2004-292T09:30:00","004T07:16:00","2004-10-18","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps). Request includes clear of DPU timetagged buffer (commands left within from S2 SOI)."]
["2004-292T09:30:00","004T07:16:00","2004-10-18","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SUR Campaign","Part of SUR MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2004-292T09:30:00","004T07:16:00","2004-10-18","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-292T10:52:00","004T22:24:00","2004-10-18","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey."]
["2004-292T11:00:00","000T20:25:00","2004-10-18","CIRS","Prime","Saturn","COMPSITA","Sit and stare at one location to derive composition","CIRS_00ASA_COMPSITA13","Measure oxygen compounds (H2O, CO2) in stratosphere as a function of latitude.  Pointing: -Y to Saturn, Z to pole"]
["2004-292T11:00:00","000T20:25:00","2004-10-18","ISS","SPASS Rider","Saturn","COMPSITA","Sit and stare at one location to derive composition","Shutter, Linearity and RBI calibration","Linearity and Shutter cal and RBI cal"]
["2004-292T11:00:00","000T20:25:00","2004-10-18","UVIS","SPASS Rider","Saturn","COMPSITA","Sit and stare at one location to derive composition","UVIS Rider to CIRS Far Nadir Comp","UVIS Rider to CIRS Far-IR Nadir Comp"]
["2004-292T11:00:00","000T20:25:00","2004-10-18","VIMS","SPASS Rider","Saturn","GLOMAP","Saturn global map","Saturn GlobalMap: CIRS Ridealong","Saturn Global Map. Ridealong for first 20 hours of CIRS  COMPSIT observation"]
["2004-293T08:00:00","000T09:00:00","2004-10-19","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-293T09:30:00","000T06:00:00","2004-10-19","CIRS","SPASS Rider","InstrumentCalibration","DSCAL1","Deep space calibration",null,"Deep space obervations for calibration."]
["2004-293T18:30:00","000T13:00:00","2004-10-19","CIRS","Prime","Saturn","COMPSITB","Sit and stare at one location to derive composition","CIRS_00ASA_COMPSITB13","Measure oxygen compounds (H2O, CO2) in stratosphere as a function of latitude.  Pointing: -Y to Saturn, Z to pole"]
["2004-293T18:30:00","000T13:00:00","2004-10-19","ISS","SPASS Rider","Saturn","COMPSITB","Sit and stare at one location to derive composition","Saturn BOTSIM imaging","Photometry/polarimetry"]
["2004-293T18:30:00","000T13:00:00","2004-10-19","UVIS","SPASS Rider","Saturn","COMPSITB","Sit and stare at one location to derive composition","UVIS Rider to CIRS Far Nadir Comp","UVIS Rider to CIRS Far-IR Nadir Comp"]
["2004-293T18:30:00","000T13:00:00","2004-10-19","VIMS","SPASS Rider","Saturn","GLOMAP","Saturn global map","Saturn GlobalMap: CIRS Ridealong #2","Saturn Global Map. Ridealong for first 20 hours of CIRS  COMPSIT observation"]
["2004-294T08:00:00","000T09:00:00","2004-10-20","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-294T18:30:00","000T01:00:00","2004-10-20","ISS","Prime","Iapetus","GRAYLITEK","Graylight observstion","Iapetus graylight observation","Turn to Iapetus; do 1x1 mosaic at various exposure times"]
["2004-294T18:30:00","000T01:00:00","2004-10-20","CIRS","SPASS Rider","Iapetus","GRAYLITEK","Graylight observstion","Iapetus rider","Integrate FP3, FP4 at high spectral resolution (0.5 cm-1).  AD~1.0 mrad, long~190 (W. Cassini Regio), phase~150."]
["2004-294T18:30:00","000T01:00:00","2004-10-20","UVIS","SPASS Rider","Iapetus","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2004-294T19:30:00","000T01:00:00","2004-10-20","ISS","Prime","Iapetus","LIMBTOPOK","Limb topography and geodesy observation","Iapetus limb topography and geodesy obs.","Do 1x1 mosaic 2 NAC clear + 3 NAC color filters + various exp times for graylight; turn to WP."]
["2004-294T19:30:00","000T01:00:00","2004-10-20","CIRS","SPASS Rider","Iapetus","LIMBTOPOK","Limb topography and geodesy observation","Iapetus rider","Integrate FP3, FP4 at high spectral resolution (0.5 cm-1).  AD~0.9 mrad, long~170 (W. Cassini Regio), phase~150."]
["2004-294T19:30:00","000T01:00:00","2004-10-20","UVIS","SPASS Rider","Iapetus","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2004-294T20:30:00","000T00:30:00","2004-10-20","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 163 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [JA-DI-HE-AT-EP (604, 610, 611, 612, 615)]"]
["2004-294T21:00:00","000T02:45:00","2004-10-20","UVIS","Prime","Saturn","MOS0AGEP","Apoapsis mosaic","MOSAIC_APO_01_14a","Mosaic of Saturn inner magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with the Saturn spin axis. 1) Slew about the Z-Axis from Saturn Center to -MOS Orb. 2)  Drift at a rate of .0238 mrad/sec about the Z-axis toward +MOS Orb for 7900s.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 177.50mrad"]
["2004-295T00:15:00","000T09:00:00","2004-10-21","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-295T11:45:00","000T01:00:00","2004-10-21","ISS","Prime","Iapetus","LIMBTOPOL","Limb topography and geodesy observation","Iapetus limb topography and geodesy obs.","Turn -Y to Iapetus; do 1x1 mosaic 3 NAC clear + 3 NAC color filters for limbtopo; do various exp. times for graylight imaging; do two more NAC clear for limbtopo."]
["2004-295T11:45:00","000T01:00:00","2004-10-21","CIRS","SPASS Rider","Iapetus","LIMBTOPOL","Limb topography and geodesy observation","Iapetus rider","Integrate FP3, FP4 at high spectral resolution (0.5 cm-1).  AD~0.9 mrad, long~160 (W. Cassini Regio), phase~150."]
["2004-295T11:45:00","000T01:00:00","2004-10-21","UVIS","SPASS Rider","Iapetus","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2004-295T12:45:00","000T01:00:00","2004-10-21","ISS","Prime","Iapetus","GRAYLITEL","Graylight observstion","Iapetus graylight observation","Do 1x1 mosaic NAC clear filters at various exposure times; do 2 NAC clear for limbtopo; turn to WP."]
["2004-295T12:45:00","000T01:00:00","2004-10-21","CIRS","SPASS Rider","Iapetus","GRAYLITEL","Graylight observstion","Iapetus rider","Integrate FP3, FP4 at high spectral resolution (0.5 cm-1).  AD~0.9 mrad, long~180 (W. Cassini Regio), phase~160."]
["2004-295T12:45:00","000T01:00:00","2004-10-21","UVIS","SPASS Rider","Iapetus","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2004-295T13:45:00","000T00:30:00","2004-10-21","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 166 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [PA-PM-EN-DI-EP (602, 604, 611, 616, 617)]"]
["2004-295T14:46:00","000T16:00:00","2004-10-21","ISS","Prime","rings(general)","RNGHAZARD","Diffuse ring satellite search","RING HAZARD AND SATELLITE SEARCH","SEARCH FOR DIFFUSE RINGS AND NEW SATELLITES AT EACH ANSAE WITH SINGLE WACS"]
["2004-296T06:46:00","000T00:30:00","2004-10-22","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","Early tour Hyperion color observation","Turn to Hyperion; do multi-color NAC images; turn to WP. Was orbit determination, but changed to a satellite observation at SOP update."]
["2004-296T07:46:00","000T09:00:00","2004-10-22","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-296T09:16:00","000T06:00:00","2004-10-22","CIRS","SPASS Rider","InstrumentCalibration","DSCALTMP","Deep space calibration","Deep Space Calibration","Deep space cal."]
["2004-296T16:46:00","001T16:15:00","2004-10-22","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2004-296T16:46:00","001T16:15:00","2004-10-22","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SUR Campaign","Part of SUR MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2004-296T16:46:00","001T16:15:00","2004-10-22","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-296T18:20:00","000T01:00:00","2004-10-22","ISS","Prime","rings(general)","DIFFUSRNG","Diffuse ring observation","DIFFUSE RINGS, GO EAST TEMPLATE, 020 TH OBSERVATIO","DIFFUSE RINGS IN REV 00A, GO EAST TEMPLATE"]
["2004-296T18:30:00","000T02:16:32","2004-10-22","CAPS","Non-SPASS","Saturn","BURST16K","16 kbps burst","Burst of 16kbps data","Burst of 16 kbps data (which gives uncollapsed ELS data). 32 B cycles duration. Data is in addition to 1000 bps survey rate."]
["2004-296T19:20:00","000T01:00:00","2004-10-22","ISS","Prime","Iapetus","LIMBTOPOM","Limb topography and geodesy observation","Iapetus limb topography and geodesy obs.","Turn -Y to Iapetus; do 1x1 mosaic 2 NAC clear + 3 NAC color filters for limbtopo; do 5 NAC for dust search; do 2 NAC clear for limbtopo."]
["2004-296T19:20:00","000T01:00:00","2004-10-22","CIRS","SPASS Rider","Iapetus","LIMBTOPOM","Limb topography and geodesy observation","Iapetus rider","Integrate FP3, FP4 at high spectral resolution (0.5 cm-1).  AD~0.85 mrad, long~140 (W. Cassini Regio), phase~160."]
["2004-296T19:20:00","000T01:00:00","2004-10-22","UVIS","SPASS Rider","Iapetus","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2004-296T20:20:00","000T01:00:00","2004-10-22","ISS","Prime","Iapetus","GRAYLITEM","Graylight observstion","Iapetus graylight observation","Do 1x1 mosaic 7 NAC clear filters (varying exposure times)"]
["2004-296T20:20:00","000T01:00:00","2004-10-22","CIRS","SPASS Rider","Iapetus","GRAYLITEM","Graylight observstion","Iapetus rider","Integrate FP3, FP4 at high spectral resolution (0.5 cm-1).  AD~0.85 mrad, long~170 (W. Cassini Regio), phase~165."]
["2004-296T20:20:00","000T01:00:00","2004-10-22","UVIS","SPASS Rider","Iapetus","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2004-296T21:20:00","000T01:00:00","2004-10-22","ISS","Prime","Iapetus","DUSTSEAR","Dust observation","Iapetus very high-phase Hill sphere obs.","Do 10 NAC clear and 5 NAC UV3 filter images (combined with polarizers); do 1 NAC clear for limbtopo; turn to WP"]
["2004-296T21:20:00","000T01:00:00","2004-10-22","CIRS","SPASS Rider","Iapetus","DUSTSEAR","Dust observation","Iapetus rider","Integrate FP3, FP4 at high spectral resolution (0.5 cm-1).  AD~0.8 mrad, long~140 (W. Cassini Regio), phase~165."]
["2004-296T21:20:00","000T01:00:00","2004-10-22","UVIS","SPASS Rider","Iapetus","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2004-296T22:20:00","000T01:25:00","2004-10-22","UVIS","Prime","Saturn","MOS0AGEP","Apoapsis mosaic","MOSAIC_APO_01_15","Mosaic of Saturn inner magnetosphere.  EUV and FUV low resolution slits on, aligned parallel to the Saturn spin axis.  1) Drift at a rate of 0.0369 mrad/s about the z-axis from Saturn Center for 4100s toward -MOS Orb.  3) Slew back to Saturn center and reset pointing.  Stare for remaining observation time. MOS Orb (+/-Range): 221.48mrad."]
["2004-297T00:16:00","000T09:00:00","2004-10-23","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-297T01:16:00","000T06:00:00","2004-10-23","CIRS","SPASS Rider","InstrumentCalibration","DSCALTMP","Deep space calibration","Deep Space Calibration","Deep space cal."]
["2004-297T09:16:00","000T23:45:00","2004-10-23","INMS","Non-SPASS","Saturn","PSTOTM004","Magetospheric survey","MAPS Survey","MAPS magnetospheric survey."]
["2004-297T10:46:00","000T12:45:00","2004-10-23","ISS","Prime","Titan","MOVIEA","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds.  9 images every hour for duration"]
["2004-297T10:46:00","000T12:45:00","2004-10-23","VIMS","SPASS Rider","Titan","MOVIEA","Surface/winds/cloud movie","Titan Movie, ridealong with ISS","Titan movie ride-along with ISS. Part 1 of 4 parts."]
["2004-298T00:01:00","000T09:00:00","2004-10-24","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-298T09:01:00","001T07:30:00","2004-10-24","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey"]
["2004-298T09:01:00","001T05:49:00","2004-10-24","INMS","Non-SPASS","Saturn","PSTOTM4BU","Magetospheric survey","MAPS Survey","MAPS magnetospheric survey."]
["2004-298T09:01:00","001T07:30:00","2004-10-24","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2004-298T09:01:00","001T07:30:00","2004-10-24","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SUR Campaign","Part of SUR MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2004-298T09:01:00","001T07:30:00","2004-10-24","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-298T10:31:00","000T01:30:00","2004-10-24","ISS","Prime","rings(general)","RADCOLOR","Radial color scan","RING RADIAL COLOR SCAN","RADIAL COLOR SCAN, 15 COLORS, NAC"]
["2004-298T10:31:00","000T01:30:00","2004-10-24","VIMS","SPASS Rider","rings(general)","COMPLOLIT","Low phase sunlit ring radial scan","radial scan, low phase, lit face.","Cube Size (X,Z) = 64*12 hires, 80 msec, + 12*12, 320 msec, Time per SC pointing (mins) = 3 Number of SC pointings = 16?,  Time of observation (hours) = 1.5,  Desc = ISS rider with ISS RAD_COLOR001 observation."]
["2004-298T12:01:00","000T11:55:00","2004-10-24","ISS","Prime","Titan","MOVIEB","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds.  9 images every hour for duration"]
["2004-298T12:01:00","000T14:55:00","2004-10-24","VIMS","SPASS Rider","Titan","MOVIEB","Surface/winds/cloud movie","Titan Movie, ridealong with ISS","Titan movie ride-along with ISS. Part 2 of 4 parts."]
["2004-298T23:56:00","000T00:20:00","2004-10-24","ISS","Prime","Titan","MOVIEB1","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds.  9 images every hour for duration"]
["2004-298T23:56:00","000T03:00:00","2004-10-24","RADAR","SPASS Rider","Other","WARMUP","RADAR warmup","Distant Titan Latitude Study, Southern Latitudes","Warmup for calibration and science data collection."]
["2004-299T00:16:00","000T02:40:00","2004-10-25","ISS","Prime","Titan","MOVIEB2","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds.  9 images every hour for duration"]
["2004-299T02:56:00","000T01:20:00","2004-10-25","RADAR","Prime","Titan","SOUTH7CAL","Distant Titan radiometery and calibration","Distant Titan Radiometry, Southern Latitudes","Obtain distant Titan radiometer science and calibration data.  One of a set that provides coverage of Titan southern latitude variation along with some obtainable associated longitude variation."]
["2004-299T04:16:00","000T00:10:00","2004-10-25","ISS","Prime","Titan","MOVIEB","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds.  9 images."]
["2004-299T04:16:00","000T00:10:00","2004-10-25","VIMS","SPASS Rider","Titan","MOVIEB","Surface/winds/cloud movie","Titan Movie, ridealong with ISS","Titan movie ride-along with ISS. Part 3 of 4 parts."]
["2004-299T04:26:00","000T01:40:00","2004-10-25","RADAR","Prime","Titan","SOUTHSCAT","Distant Titan radiometery and calibration","Distant Titan Scatterometry, Southern Latitudes","Obtain distant Titan scatterometry science and calibration data.  One of a set that provides coverage of Titan southern latitude variation along with some obtainable associated longitude variation."]
["2004-299T06:06:00","000T00:55:00","2004-10-25","ISS","Prime","Titan","MOVIEB","Surface/winds/cloud movie","Titan Surface/winds/clouds","Surface/winds/clouds.  9 images twice."]
["2004-299T06:06:00","000T00:55:00","2004-10-25","VIMS","SPASS Rider","Titan","MOVIEB","Surface/winds/cloud movie","Titan Movie, ridealong with ISS","Titan movie ride-along with ISS. Part 4 of 4 parts."]
["2004-299T07:31:00","000T09:00:00","2004-10-25","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-299T09:01:00","000T06:00:00","2004-10-25","CIRS","SPASS Rider","InstrumentCalibration","DSCALTMP","Deep space calibration","Deep Space Calibration","Deep space cal."]
["2004-299T14:50:00","000T12:40:23","2004-10-25","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey."]
["2004-299T16:31:00","000T20:59:09","2004-10-25","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey"]
["2004-299T16:31:00","000T19:27:16","2004-10-25","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps."]
["2004-299T16:31:00","000T20:59:09","2004-10-25","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2004-299T16:31:01","000T21:13:46","2004-10-25","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SUR Campaign","Part of SUR MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2004-299T17:16:09","000T00:14:00","2004-10-25","ISS","Prime","Titan","LRMONITOR","Long range monitor","Long Range NAC Monitoring of Surface and Atmospher","monitoring for surface/atmosphere changes; attempt to see surface color variations; monitor limb hazes, 1-3 km/px"]
["2004-299T17:16:09","000T00:14:00","2004-10-25","VIMS","SPASS Rider","Titan","ISS",null,"Dark_Side VIMS_4868","Ridealong with ISS Image. 64X64"]
["2004-299T17:30:09","000T05:15:00","2004-10-25","CIRS","Prime","Titan","MIDIRTMAP","Mid infrared thermal map",null,"Obtain information on the thermal structure of Titan's stratosphere. Slew across disk at 4 microrad/s."]
["2004-299T17:30:09","000T05:15:00","2004-10-25","CIRS","SPASS Rider","Titan","MIDIRTMAP","Mid infrared thermal map","ISS_PHOT_1x1","ISS WAC support imaging, 2 images per integration (6 integrations total = 12 frames, 0.5 Mb/frame)"]
["2004-299T17:30:09","000T05:15:00","2004-10-25","ISS","SPASS Rider","Titan","MIDIRTMAP","Mid infrared thermal map","RCI (Ridealong Context Imaging)","wind/cloud motions, 3-12 km/px, 3 images/timestep in CB1 filter to increase SNR, 12-bit lossless"]
["2004-299T17:30:09","000T05:15:00","2004-10-25","VIMS","SPASS Rider","Titan","MIDIR","Mid infrared thermal map","Dark_Side VIMS_4868","Ridealong with CIRS MID IR Temp map. Mode will be 64 square for entire period."]
["2004-299T22:45:09","000T01:15:00","2004-10-25","ISS","Prime","Titan","MONITORNA","Monitoring of surface and atmosphere","NMA (NAC Monitoring of Surface and Atmosphere)","monitoring for surface/atmosphere changes; attempt to see surface color variations; monitor limb hazes, 1-3 km/px"]
["2004-299T22:45:09","000T01:15:00","2004-10-25","CIRS","SPASS Rider","Titan","FIRNADCMP","Far infrared nadir composition map",null,"Ride-along with ISS."]
["2004-299T22:45:09","000T01:15:00","2004-10-25","VIMS","SPASS Rider","Titan","ISS",null,"Dark_Side VIMS_4868","Ridealong with ISS Monitor (both NAC &  WAC). 64X64 all the way."]
["2004-300T00:00:09","000T04:00:00","2004-10-26","CIRS","Prime","Titan","FIRNADCMP","Far infrared nadir composition map",null,"Obtain information on CO, HCN, CH4. Integrate on disk at airmass 1.5--2.0."]
["2004-300T00:00:09","000T04:00:00","2004-10-26","CIRS","SPASS Rider","Titan","FIRNADCMP","Far infrared nadir composition map","ISS_PHOT_1x1","ISS WAC support imaging, 2 images per integration (4 integrations total = 8 frames, 0.5 Mb/frame)"]
["2004-300T00:00:09","000T04:00:00","2004-10-26","ISS","SPASS Rider","Titan","FIRNADCMP","Far infrared nadir composition map","RCI (Ridealong Context Imaging)","wind/cloud motions, 3-12 km/px, 3 images/timestep in CB1 filter to increase SNR, 12-bit lossless"]
["2004-300T00:00:09","000T04:00:00","2004-10-26","VIMS","SPASS Rider","Titan","FARIRNAD",null,"Dark_Side VIMS_4868","Ridealong with CIRS Far IR nadir comp map. Sit and stare. Mode will be 64  square for entire period."]
["2004-300T03:30:23","000T10:59:46","2004-10-26","INMS","Non-SPASS","Titan","TAINBD",null,"MAPS TOST Campaign","Part of TOST MAPS Campaign.  Determine"]
["2004-300T04:00:09","000T06:30:00","2004-10-26","VIMS","Prime","Titan","MEDRES","Medium resolution global mapping","Med_Res_Regional VIMS_4868","Medium resolution global mapping. Start sequence with  64X64, and then do a 3X2 mosaic (64 hi-res mode) with  at least 2 integration times."]
["2004-300T04:00:09","000T06:30:00","2004-10-26","CIRS","SPASS Rider","Titan","FIRNADCMP","Far infrared nadir composition map",null,"Ride-along with VIMS. 1 minute dwells."]
["2004-300T04:00:09","000T06:30:00","2004-10-26","ISS","SPASS Rider","Titan","MEDRES","Medium resolution global mapping","WMO (WAC Movie)","wind/cloud motions, 3-12 km/px, 3 images/timestep in CB1 filter to increase SNR, 12-bit lossless"]
["2004-300T04:00:09","000T06:30:00","2004-10-26","UVIS","SPASS Rider","Titan","EUVFUV","UVIS EUV / FUV imaging","EUVFUV Imaging of  Titan","Several slow wcans across Titan's visible hemisphere to form spectral images"]
["2004-300T10:15:09","000T03:27:00","2004-10-26","RADAR","SPASS Rider","Titan","TAWARMUP",null,"Warmup for Ta Radiomeetry","Warmup needed for Radiometry period following"]
["2004-300T10:30:09","000T01:40:00","2004-10-26","ISS","Prime","Titan","REGMAP","Regional mapping","NRM (NAC Regional Map)","regional map"]
["2004-300T10:30:09","000T03:12:00","2004-10-26","CIRS","SPASS Rider","Titan","FIRNADCMP","Far infrared nadir composition map",null,"Ride-along with ISS."]
["2004-300T10:30:09","000T03:12:00","2004-10-26","VIMS","SPASS Rider","Titan","HIGHRES","High resolution observartion","Dark_Side VIMS_4868","Ridealong with ISS High Res. 12X12 all the way."]
["2004-300T11:58:16","000T07:03:46","2004-10-26","MAG","Non-SPASS","Titan","MAGTITAN","MAG Titan observation","TA Flyby","TA is the first close encounter at Titan at 1200 km during the Cassini mission and thus the first encounter after the Voyager-1 encounter in November 1980. It will thus be of extreme scientific interest to the mission, the science community and for PR purposes. If the various approaches to obtain an improved neutral atmosphere model of Titan during this encounter possibly find a denser atmosphere, it may turn out to be among the closest encounters of the whole mission. The trajectory is on the downstream or wake side and therefore very suitable for studies of the tail formation processes. It thus has to be of highest priority i.e. grade 1 priority which assumes +- four hours (total duration eight hours) of high resolution data at 1976 bps (32 vps) total around closest approach."]
["2004-300T12:10:09","000T01:31:00","2004-10-26","ISS","Prime","Titan","HIRESNAC","High resolution map","HRI (High Resolution Imaging)","high-resolution imaging, 50-200 m/px, special targets, emission angles < 45 prefer IR-polarizer (phase 45-110)"]
["2004-300T13:30:09","000T01:21:00","2004-10-26","CAPS","SPASS Rider","Titan","TAINBND",null,"MAPS 00ATI Campaign","Part of 00ATI MAPS Campaign.  Inbound approach observations and context for the interaction between Titan and Saturn's magnetosphere"]
["2004-300T13:30:09","000T01:32:30","2004-10-26","RPWS","Non-SPASS","Titan","TIINTRMED","Titan magnetosphere interaction","Titan Interaction - Intermediate","Study the interaction of the magnetosphere with Titan at intermediate distances for evidence of ion pickup, radio emissions, density profiles, and the general wave environment.  Prefer Langmuir probe within 90 degrees of plasma ram."]
["2004-300T13:42:09","000T00:21:00","2004-10-26","CIRS","SPASS Rider","Titan","FIRNADCMP","Far infrared nadir composition map",null,"Ride-along with VIMS landing site obs, actually during RCS/RWA  transition."]
["2004-300T13:42:09","000T00:21:00","2004-10-26","ISS","SPASS Rider","Titan","RADRCS",null,"RCS/RWA Transition Imaging","ISS on, max data rate = 182.784 kbps, number of frames and bits/frame are input parameters, data volume = number of frames x bits/frame, average data rate = data volume/duration."]
["2004-300T13:42:09","000T00:21:49","2004-10-26","VIMS","SPASS Rider","Titan","TRANS",null,"Hi_Res_Trans VIMS_4868","During the transition from RW to thrusters, take two 64 square cubes  if possible."]
["2004-300T13:44:36","000T00:45:33","2004-10-26","MIMI","SPASS Rider","Titan","TAINBND",null,"MAPS 00ATI(TA) Campaign","Part of 00ATI(TA) MAPS Campaign.   Investigate micro-scale and near aspects of the Titan interaction by observing during about one hour period around an encounter. With -Y pointed toward Titan, when within 30 minutes of the targeted flyby, optimize secondary axis for corotation flow as close to the S/C -X, +/- Z plane as works with the other constraints on pointing. Also, measure Titan exosphere/magnetosphere interaction by imaging in ENA with INCA (when sun is not in INCA FOV)."]
["2004-300T14:02:09","000T00:02:00","2004-10-26","ISS","Prime","Titan","WAYPTTURN","Waypoint turn","Return To Waypoint Following Transition","ISS on, max data rate = 182.784 kbps, number of frames and bits/frame are input parameters, data volume = number of frames x bits/frame, average data rate = data volume/duration."]
["2004-300T14:11:09","000T00:34:00","2004-10-26","RADAR","Prime","Titan","TAINSCAT",null,"Inbound Scatterometry of Ta","Inbound Scatterometry during Ta flyby"]
["2004-300T14:30:09","000T02:00:00","2004-10-26","MIMI","SPASS Rider","Titan","TACLOSE",null,"MAPS 00ATI(TA) Campaign","Part of 00ATI(TA) MAPS Campaign.   Investigate micro-scale and near aspects of the Titan interaction by observing during about one hour period around an encounter. With -Y pointed toward Titan, when within 30 minutes of the targeted flyby, optimize secondary axis for corotation flow as close to the S/C -X, +/- Z plane as works with the other constraints on pointing. Also, measure Titan exosphere/magnetosphere interaction by imaging in ENA with INCA (when sun is not in INCA FOV)."]
["2004-300T14:30:09","000T00:47:00","2004-10-26","INMS","Non-SPASS","Titan","TACLOSE",null,"MAPS TOST Campaign","Part of TOST MAPS Campaign.  Determine"]
["2004-300T14:45:09","000T00:33:00","2004-10-26","VIMS","Prime","Titan","HIRES","High resolution image","Hi_Res_Regional VIMS_4868","High resolution, low phase angle mapping. Line of 64X64 cubes probabaly best."]
["2004-300T14:45:09","000T00:32:00","2004-10-26","CIRS","SPASS Rider","Titan","FIRNADMAP","Far infrared nadir composition map",null,"Ridealong with VIMS"]
["2004-300T14:45:09","000T00:32:00","2004-10-26","ISS","SPASS Rider","Titan","HIRES","High resolution image","RCI (Ridealong Context Imaging)","wind/cloud motions, 3-12 km/px, 3 images/timestep in CB1 filter to increase SNR, 12-bit lossless"]
["2004-300T14:51:09","000T01:18:00","2004-10-26","CAPS","SPASS Rider","Titan","TACLOSE",null,"MAPS 00ATI Campaign","Part of 00ATI MAPS Campaign.  Observations of Titan's interaction with Saturn's magnetosphere"]
["2004-300T15:02:39","000T00:21:30","2004-10-26","RPWS","Non-SPASS","Titan","TICA","Titan closest approach","Titan closest approach observations","RPWS observations in the immediate vicinity of Titan, including thermal plasma density and temperature measurements with the Langmuir probe, search for lightning and other radio emissions, characterization of plasma wave spectrum, search for evidence of pickup ions.  Langmuir  probe within 90 degrees of spacecraft ram at closest approach, corotational ram outside of +/- 15 minutes."]
["2004-300T15:17:09","000T00:13:00","2004-10-26","INMS","SPASS Rider","Titan","TARAMPNT",null,"MAPS TOST Campaign","Ta is an engineering pass"]
["2004-300T15:18:09","000T00:12:00","2004-10-26","RADAR","Prime","Titan","TAPT4INMS",null,"TA Ride Along SAR","Ride along SAR of Titan with INMS."]
["2004-300T15:57:39","000T01:32:30","2004-10-26","RPWS","Non-SPASS","Titan","TIINTRMED","Titan magnetosphere interaction","Titan Interaction - Intermediate","Study the interaction of the magnetosphere with Titan at intermediate distances for evidence of ion pickup, radio emissions, density profiles, and the general wave environment.  Prefer Langmuir probe within 90 degrees of plasma ram."]
["2004-301T09:30:01","000T14:29:59","2004-10-27","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SUR Campaign","Part of SUR MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2004-302T07:15:00","000T01:45:00","2004-10-28","CIRS","Prime","RingC","SHADCIN","Ring shadow scan","CIRS_00ARC_SHADCIN","Longitudinal scan of  ring in the early mission (highest temperature contrasts), in and around shadow, Low Phase, lit face, dawn side -Y to ring, +Z perpendicular to rings (if not possible, +Z parallel to pole)"]
["2004-302T19:00:00","000T02:05:00","2004-10-28","CDA","Prime","RingE","RPC","Ring plane crossing","Ring Plane Crossing @ 8 Rs","Ring Plane Crossing @ 302T20:15?, pointing=CDA to Kepler RAM or windshield-wiper mode or roll;rate=524"]
["2004-302T23:00:00","000T00:29:49","2004-10-28","RPWS","Non-SPASS","Saturn","WHISTLER","RPWS lightning search","Obtain wideband examples of lightning whistlers","Obtain wideband evidence of lightning whistlers.  These would verify the existence of lightning already suspected from Saturn Electrostatic Discharges (SED) and would provide information on the electron density along the field line to the source.  No pointing requirement."]
["2004-304T01:00:00","000T02:16:32","2004-10-30","CAPS","Non-SPASS","Saturn","BURST16K","16 kbps burst","Burst of 16kbps data","Burst of 16 kbps data (which gives uncollapsed ELS data). 32 B cycles duration. Data is in addition to 1000 bps survey rate."]
["2004-306T18:15:00","000T05:02:00","2004-11-01","CIRS","SPASS Rider","rings(general)","IMPACT",null,"CIRS_00ARI_IMPACT","Radial scan of main rings to obtain submillimeter measurement of rings at a variety of geometries.  -Y to rings, Z perp to rings"]
["2004-308T16:02:01","011T15:46:59","2004-11-03","MIMI","SPASS Rider","co-rotation","MAGBOUND","MAPS magnetosphere boundary campaign","MAPS MB/high Campaign","Part of MB/high MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2004-311T22:48:00","000T06:30:00","2004-11-06","CIRS","Prime","rings(general)","FMONITOR","F ring monitor","Ring FP3/FP4 integrations","Integration on the main rings with FP3 and FP4"]
["2004-315T23:15:00","000T09:00:00","2004-11-10","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-319T22:49:00","000T09:00:00","2004-11-14","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-320T07:49:00","000T01:22:00","2004-11-15","INMS","Non-SPASS","Saturn","STARTUP","Sequence startup activity","STARTUP","Startup sequence.  Load FSW, MRO, Load IEB from SSR's, MRO"]
["2004-324T15:04:00","003T13:50:00","2004-11-19","MAG","Non-SPASS","Other","MAGBOUND","MAPS magnetosphere boundary campaign","MAG MAPS Magbound Campaign","Observe magnetospheric boundaries at a variety of radial distances."]
["2004-326T10:00:00","000T12:00:00","2004-11-21","VIMS","SPASS Rider","Saturn","SPKMOVIE","Ring spoke movie","Saturn Spoke Movie #7: ISS ridealong","Saturn far global imagery, rideing along with ISS spoke movie #7 (First one in  Rev 00B).. Images acquired close to apoapsis. Assume Saturn is smaller than  16 mrads across, and use double-sampling.  Image once every 1.5 hours, using three exposures. 9 image sets  in  12 hours.  Volume (downlinked) = 352*12*64*32*9*3*1.05/2 = 123 mbits downlinked Call it 130 mbits."]
["2004-328T03:30:00","000T01:20:00","2004-11-23","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-330T15:35:00","000T06:00:00","2004-11-25","UVIS","Prime","Saturn","MOS02APOB","Apoapsis mosaic","MOSAIC_APO_02_31b","Mosaic of Saturn inner magnetosphere.  EUV and FUV low resolution slits on, aligned parallel to the Saturn spin axis. 1) Slew about the Z-axis from Saturn Center to +MOS Orb. Rotate +128mrad in the YZ plane. 2) Drift at a rate of 0.0933 mrad/sec about the Z-axis for 8000s to -MOS Orb. 3) Rotate -64mrad in the YZ Plane. Drift at indicated rate about the Z-axis for 8000s to +MOS Orb. 4) Rotate -64mrad in the YZ Plane. Drift at indicated rate about the Z-axis for 4000s toward -MOS Orb. 7) Slew back to Saturn center and reset pointing. Stare for remaining observation time. MOS Orb (+/-Range): 373.5mrad."]
["2004-333T16:20:00","000T12:00:00","2004-11-28","UVIS","Prime","Saturn","MOS02APOB","Apoapsis mosaic","MOSAIC_APO_02_32b","Mosaic of Saturn inner magnetosphere.  EUV and FUV low resolution slits on, aligned parallel to the Saturn spin axis.  1) Slew about the Z-axis from Saturn Center to +MOS Orb. Rotate +128mrad in the YZ Plane.  2) Drift at a rate of 0.034 mrad/sec about the Z-axis for 8000s to -MOS Orb. 3) Rotate -64mrad in the YZ Plane. Drift at indicated rate about the Z-axis for 8000s to +MOS Orb. 4) Rotate -64mrad in the YZ Plane. Drift at indicated rate about the Z-axis for 8000s to -MOS Orb. 5) Rotate -64mrad in the YZ Plane. Drift at indicated rate about the Z-axis for 8000s to +MOS Orb. 6) Rotate -64mrad in the YZ Plane. Drift at indicated rate about the Z-axis for 8000s to -MOS Orb. 7) Slew back to SAturn center and reset pointing. Stare for remaining observation time. MOS Orb (+/-Range): 135.61mrad."]
["2004-335T10:20:00","000T06:00:00","2004-11-30","UVIS","SPASS Rider","rings(general)","FMONITOR","F ring monitor","FUV and EUV ring spectroscopy"]
["2004-338T15:36:00","000T16:15:00","2004-12-03","RPWS","Non-SPASS","co-rotation","MAGBOUND","MAPS magnetosphere boundary campaign","MAPS MB,A Campaign","Part of MB,A MAPS Campaign.  Observe plasma waves on dawn-side magnetospheric boundaries at a variety of radial distances"]
["2004-340T08:08:00","000T01:52:00","2004-12-05","CDA","Non-SPASS","DustRAM direction","SURVEY","Magnetospheric survey","survey","dust survey measurements"]
["2004-343T23:21:00","000T05:15:00","2004-12-08","CIRS","SPASS Rider","InstrumentCalibration","DSCAL1","Deep space calibration",null,"Deep space obervations for calibration."]
["2004-345T21:05:00","000T09:30:00","2004-12-10","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-347T06:17:00","000T07:19:00","2004-12-12","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2004-348T09:38:13","000T01:30:00","2004-12-13","ISS","Prime","Titan","HIRESNAC","High resolution map","HRI (High Resolution Imaging)","high-resolution imaging, 50-200 m/px, special targets, emission angles < 45 prefer IR-polarizer (phase 45-110)"]
["2004-348T23:38:13","000T08:14:31","2004-12-13","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey."]
["2004-349T09:00:00","000T07:52:00","2004-12-14","ISS","SPASS Rider","Saturn","CYLMAP","Saturn cylindrical map","Saturn CYLMAP rider","Saturn rider to VIMS observation"]
["2004-350T00:52:00","000T00:48:00","2004-12-15","ISS","Prime","Dione","REGMAP","Regional mapping","Dione regional mapping","Turn -Y to Dione; do 5-NAC-frames mosaic (three shutters per footprint) (IR1, GRN, Clr filters) + 3 WAC rgb; turn to Dione center."]
["2004-351T00:00:00","000T13:22:00","2004-12-16","CDA","Non-SPASS","DustRAM direction","SURVEY","Magnetospheric survey","survey","dust survey measurements"]
["2004-353T04:22:00","000T09:00:00","2004-12-18","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-354T04:07:00","000T09:00:00","2004-12-19","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-356T13:07:00","000T03:53:00","2004-12-21","ISS","Prime","InstrumentCalibration","DARKCAL","Dark image calibration","Dark images, NAC and WAC plus three cal lamp image","Ride along during system scans take 5 dark images"]
["2004-359T20:00:00","000T00:00:00","2004-12-24","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey."]
["2004-360T18:37:00","000T09:00:00","2004-12-25","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2004-366T03:32:00","000T00:57:00","2004-12-31","UVIS","SPASS Rider","Iapetus","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2004-366T14:00:00","000T00:30:00","2004-12-31","VIMS","SPASS Rider","Iapetus","GLOBMAPC","Global coverage mapping","Iapetus global mapping","12x12 low res IR and Vis at 320ms (50sec), one  cube per ISS NAC footprint == 13 cubes; 32x32 low res IR and Vis at 320ms (5,5 min),  while ISS dwells to Iapetus center for WAC  images."]
["2004-366T21:00:00","000T01:00:00","2004-12-31","UVIS","SPASS Rider","Iapetus","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2005-001T04:00:00","000T01:00:00","2005-01-01","ISS","Prime","Iapetus","GRAYLITEH","Graylight observstion","Iapetus close flyby 00B/00C graylight imaging","Do NAC 3+3+24 mosaic + WAC 4-color context; do 1x4 NAC graylight mosaic."]
["2005-002T08:30:00","001T12:30:00","2005-01-02","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey."]
["2005-006T11:53:00","004T00:01:00","2005-01-06","RPWS","Non-SPASS","Earth","OFF",null,"RPWS OFF","Perform RPWS OFF for Probr relay test"]
["2005-015T11:00:00","000T06:00:00","2005-01-15","MIMI","SPASS Rider","co-rotation","POWERON","Huygens Probe support","Turn on after Probe activity","Part of MB/high MAPS Campaign.   Set up MIMI for magnetospheric boundaries campaign with corotation pointing. Pointing: -X to corotation, Saturn B in X, Z plane; or spin about Z. Observe dawn-side magnetospheric boundaries at a variety of radial distances."]
["2005-015T23:42:00","000T14:00:00","2005-01-15","RPWS","Non-SPASS","Saturn","SEDDF","Saturn Electrical Discharge direction finding","SED Direction-finding","Perform direction-finding on SED to a) verify source in Saturn's atmosphere (or refute this and find source in rings), and b) if source is in atmosphere, use location to characterize the location of thunderstorms.  Need to do this inside 6 RS on at least half of the periapses inside of 6RS.  No pointing requirement"]
["2005-016T03:20:00","000T09:00:00","2005-01-16","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2005-016T13:56:00","000T01:04:00","2005-01-16","ISS","SPASS Rider","Enceladus","ICYLON","Icy satellite longitudinal coverage","ENCELADUS Color Photometry/Polarization","2; Enceladus photometry/polarization. NP09+N05"]
["2005-016T22:20:00","000T00:15:00","2005-01-16","UVIS","SPASS Rider","Rhea","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2005-017T12:30:00","000T21:30:00","2005-01-17","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SUR Campaign","Part of SUR MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2005-017T22:40:00","000T02:00:00","2005-01-17","UVIS","Prime","rings(general)","IMPACT",null,null,"Use UVIS HSP and FUV to detect flashes from meter-sized interplanetary impactors on rings to constrain flux of important impact population for ring origin/evolution."]
["2005-018T02:10:00","000T07:50:00","2005-01-18","RPWS","Non-SPASS","co-rotation","HIRATE","High rate mode","MAPS MB,A Campaign","Part of MB,A MAPS Campaign.  Observe plasma waves on dawn-side magnetospheric boundaries at a variety of radial distances"]
["2005-019T13:00:00","000T00:30:00","2005-01-19","ISS","Prime","Mimas","LONPHA","Spectrophotometry / phase coverage","Mimas spectrophotometry/ phase coverage","Turn -Y to Tethys; Do 1x1 mosiac 4 NAC color + 9 NAC polarizer + 4 WAC polarizer filters"]
["2005-022T11:45:00","000T00:30:00","2005-01-22","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 050 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [JA-TL-HY-PM-EP (607, 610, 611, 613, 616)]"]
["2005-024T01:23:00","000T09:00:00","2005-01-24","CDA","Non-SPASS","DustRAM direction","DRATE","Data volume adjustment","add data rate","dust survey measurements"]
["2005-024T22:00:00","000T14:00:00","2005-01-24","RSS","SPASS Rider","Earth","PATTERN","HGA pattern calibration","HGA Pattern Calibration","HGA Pattern Calibration; Pointing: XBAND to Earth + two rastor scan maneuvers (one smaller for X and Ka bands, one larger for X and S bands).  Last 10 hours required to be tracked at both DSS-25 and DSS-15 in 1-way mode.  Playback of telemetry required afterwards for C-Kernel generation,"]
["2005-025T13:30:00","000T10:00:00","2005-01-25","CAPS","Prime","Other","MAGBNDPTG","MAPS magnetosphere boundary campaign","Magnetospheric Boundary Campaign","Part of MB,High MAPS Campaign. Observe dawn-side magnetospheric boundaries at a variety of radial distances"]
["2005-029T01:08:00","000T09:00:00","2005-01-29","CDA","Non-SPASS","DustRAM direction","DRATE","Data volume adjustment","add data rate","dust survey measurements"]
["2005-029T17:38:00","000T09:00:00","2005-01-29","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2005-031T23:22:00","000T12:00:00","2005-01-31","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2005-034T11:22:00","000T12:30:00","2005-02-03","RPWS","Non-SPASS","co-rotation","HIRATE","High rate mode","MAPS MB,A Campaign","Part of MB,A MAPS Campaign.  Observe plasma waves on dawn-side magnetospheric boundaries at a variety of radial distances"]
["2005-035T11:07:00","001T22:30:00","2005-02-04","CAPS","SPASS Rider","co-rotation","MAGBOUND","MAPS magnetosphere boundary campaign","MAPS","Part of  MB,A  MAPS Campaign.  Observe dawn-side magnetospheric boundaries at a variety of radial distances"]
["2005-037T09:37:00","001T14:45:00","2005-02-06","CAPS","SPASS Rider","co-rotation","MAGBOUND","MAPS magnetosphere boundary campaign","MAPS","Part of  MB,A  MAPS Campaign.  Observe dawn-side magnetospheric boundaries at a variety of radial distances"]
["2005-039T10:22:00","000T05:30:00","2005-02-08","VIMS","SPASS Rider","Saturn","3X3MOVIEA","3 x 3 mosaic","Saturn ISS/VIMS Movie #3","Saturn ISS/VIMS  Movie #2of 3. 5.5 Hours observing, once per hour. 2*2 mosiac, each taking 4*7 + 12 = 40 minutes. Each mosaic uses  352*12*64*64*4/2*(1.05) = 36.3 mbits. For  6 hours = 220 mbits."]
["2005-041T16:37:00","000T09:00:00","2005-02-10","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously during downlink periods.  No special pointing is  required."]
["2005-042T13:07:00","000T10:00:00","2005-02-11","VIMS","Prime","Saturn","GLOMOV","Saturn global movie","Saturn Global Movie #2","Saturn Global Movie #2 of 4. 10 Hours observing, once per hour. 2*2 mosiac, each taking 4*7 + 12 = 40 minutes. Each mosaic uses  352*12*64*64*4/2*(1.05) = 36.3 mbits. For 10 hours = 370 mbits.  Modified 9/26/02: Volume decreased to 100 Mbits to fit SSR"]
["2005-045T09:07:00","000T04:53:00","2005-02-14","MAG","Non-SPASS","co-rotation","MAGBOUND","MAPS magnetosphere boundary campaign","MAG_MAPS_MB_A_Campaign","Observe_dawn-side_magnetospheric_boundaries_at_a_variety_of_radial_distances. (Alternate_MB_A)"]
["2005-045T19:57:53","000T04:00:00","2005-02-14","UVIS","SPASS Rider","Titan","MIRLMBINT","Mid infrared limb integration","UVIS Rider to CIRS MIRLMBINT","UVIS Rider to CIRS Mid IR Limb INT"]
["2005-046T01:57:53","000T03:00:00","2005-02-15","MIMI","SPASS Rider","Titan","T3INBND",null,"MAPS 003TI Campaign","Part of 003TI MAPS Campaign.   Investigate micro-scale and near aspects of the Titan interaction by observing during about one hour period around an encounter. With -Y pointed toward Titan, when within 30 minutes of the targeted flyby, optimize secondary axis for corotation flow as close to the S/C -X, +/- Z plane as works with the other constraints on pointing. Also, measure Titan exosphere/magnetosphere interaction by imaging in ENA with INCA (when sun is not in INCA FOV)."]
["2005-046T08:30:53","000T14:47:00","2005-02-15","VIMS","SPASS Rider","Titan","NIGHT",null,"VIMS_ride VIMS_4870","Titan Night"]
["2005-047T09:00:00","000T13:20:00","2005-02-16","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2005-047T22:20:29","000T01:16:00","2005-02-16","CDA","Non-SPASS","RingE","ERING","E ring observation","Dust survey within dust hazard zone","Dust survey within dust hazard zone, CDA defines secondary axis, rate: 150 bps, volume: 1. Mb"]
["2005-048T03:00:29","000T02:00:00","2005-02-17","RSS","SPASS Rider","Enceladus","THERMAL","Thermal stabilization period","RSS Enceladus Gravity Thermal Stabilization","A period of thermal stabilization is required immediately prior to any radio science experiment and test using Ka-band or S-band."]
["2005-048T05:25:29","000T02:50:00","2005-02-17","RSS","SPASS Note","Enceladus","GRAVITYN","RSS gravity field determination","RSS Enceladus Gravity Field Determination","Enceladus mass determination"]
["2005-048T14:46:00","000T08:22:00","2005-02-17","UVIS","SPASS Rider","Saturn","EUVFUV","UVIS EUV / FUV imaging","EUVFUV Imaging of Saturn","Rider opportunity"]
["2005-049T14:35:00","000T00:25:00","2005-02-18","ISS","Prime","Mimas","166W100PH","Spectrophotometery","Mimas spectrophotometry/ phase coverage","Turn -Y to Mimas; do 1x1 mosaic 3 clear + 4 NAC color + 9 NAC polarizer + 4 WAC polarizer filters; turn to WP"]
["2005-050T11:40:00","000T01:00:00","2005-02-19","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 040 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 8 targets: [CP-HE-MI-EP-TE-EN-JA-PA (601, 602, 603, 610, 611, 612, 614, 617)]"]
["2005-051T12:56:00","000T10:25:00","2005-02-20","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2005-054T08:21:00","002T23:45:00","2005-02-23","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2005-055T23:06:00","000T09:00:00","2005-02-24","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously during downlink periods.  No special pointing is  required."]
["2005-057T08:06:00","000T16:30:00","2005-02-26","MIMI","SPASS Rider","co-rotation","MAGBOUND","MAPS magnetosphere boundary campaign","MAPS MB/A Campaign","Part of MB/A MAPS Campaign.   Set up MIMI for magnetospheric boundaries campaign with corotation pointing. Pointing: -X to corotation, Saturn B in X, Z plane; or spin about Z. Observe dawn-side magnetospheric boundaries at a variety of radial distances."]
["2005-058T07:00:00","003T00:00:00","2005-02-27","RPWS","Non-SPASS","co-rotation","HIRATE","High rate mode","MAPS MB,A Campaign","Part of MB,A MAPS Campaign.  Observe plasma waves on dawn-side magnetospheric boundaries at a variety of radial distances"]
["2005-058T19:02:00","000T00:40:00","2005-02-27","VIMS","SPASS Rider","Saturn","1X6MOVIEA","Saturn movie","ISS 1X6 Movie Ride Along","ISS Movie Ride Along"]
["2005-059T16:34:00","000T00:40:00","2005-02-28","VIMS","SPASS Rider","Saturn","1X6MOVIEB","Saturn movie","ISS 1X6 Movie Ride Along","ISS Movie Ride Along"]
["2005-064T08:35:00","000T00:55:00","2005-03-05","ISS","Prime","Janus","MUTUALEVE","Mutual event satellite transit observation","MUTUAL EVENTS, TRANSIT OF Janus     ACROSS Encelad","Turn to satellite, take 1 NAC every ~ minute for duration of event while tracking satellite"]
["2005-065T17:35:00","000T00:30:00","2005-03-06","UVIS","SPASS Rider","Dione","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2005-066T07:20:00","001T00:26:33","2005-03-07","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey."]
["2005-066T19:55:00","000T00:30:00","2005-03-07","UVIS","SPASS Rider","Rhea","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2005-067T19:50:00","000T03:50:00","2005-03-08","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously during downlink periods.  No special pointing is  required."]
["2005-068T01:30:47","000T01:21:07","2005-03-09","CDA","Non-SPASS","DustRAM direction","0700DUST","Dust survey","E Ring dense - survey - 0.15<lat< 0.15 deg 6.90...","E Ring dense - survey - $ 251.06305 $ 251.11939 $ 7.557 to 6.899 Rs lat: -0.149 to -0.151 deg ring-alt: 1186. to 1097.km,pointing=CDA to Kepler RAM,rate=524,dataVolume=2.432"]
["2005-068T06:50:24","000T00:24:28","2005-03-09","CDA","Non-SPASS","Tethys","0500TEORX","Tethys orbit crossing","Tethys Orbit Xing 0.00<lat< 1.20 deg 4.79... 4.99","Tethys Orbit Xing$ 251.28500$ 251.30200$ 4.987 to 4.798 Rs lat: -0.139 to -0.135 deg ring-alt: 730. to 682.km 002OF018 no ADJ: 0 was:...,pointing=CDA to Kepler RAM,rate=4192,dataVolume=5.868"]
["2005-068T08:10:36","000T00:58:28","2005-03-09","CDA","Non-SPASS","DustRAM direction","0400DUST","Dust survey","E Ring dense - survey - 0.10<lat< 0.12 deg 4.03...","E Ring dense - survey - $ 251.34069 $ 251.38131 $ 4.372 to 4.033 Rs lat: -0.121 to -0.100 deg ring-alt: 557. to 425.km,pointing=CDA to Kepler RAM,rate=524,dataVolume=1.753"]
["2005-068T09:53:09","000T17:21:47","2005-03-09","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey"]
["2005-068T14:30:45","000T00:52:43","2005-03-09","CDA","Non-SPASS","DustRAM direction","0400DUST","Dust survey","E Ring dense - survey - 0.11<lat< 0.13 deg 4.08...","E Ring dense - survey - $ 251.60469 $ 251.64131 $ 4.076 to 4.389 Rs lat: 0.110 to 0.127 deg ring-alt: 472. to 587.km,pointing=CDA to Kepler RAM,rate=524,dataVolume=1.580"]
["2005-069T00:56:14","000T00:43:02","2005-03-10","CDA","Non-SPASS","DustRAM direction","0900DUST","Dust survey","Ring Margin - survey - 0.14<lat< 0.14 deg 8.98...","Ring Margin - survey - $ 252.03905 $ 252.06895 $ 8.983 to 9.296 Rs lat: 0.144 to 0.143 deg ring-alt: 1362. to 1400.km,pointing=CDA to Kepler RAM,rate=524,dataVolume=1.290"]
["2005-069T08:35:00","000T00:55:00","2005-03-10","ISS","Prime","Mimas","166W113PH","Spectrophotometery","Mimas spectrophotometry/ phase coverage","Turn -Y to Mimas; Do 1x1 mosaic 3 clear + 4 NAC color + 9 NAC polarizer + 4 WAC polarizer filters"]
["2005-070T02:23:05","000T03:37:49","2005-03-11","CDA","Non-SPASS","DustRAM direction","1900DUST","Dust survey","Dust survey 0.09<lat< 0.10 deg 18.83... 19.98 Rs v","Dust survey $ 253.09936 $ 253.25064 $ 18.834 to 19.983 Rs lat: 0.096 to 0.091 deg ring-alt: 1904. to 1915.km,pointing=CDA to Kepler RAM,rate=150,dataVolume=1.869"]
["2005-070T21:19:56","000T01:59:59","2005-03-11","CDA","Non-SPASS","Hyperion","2400HYORX","Hyperion orbit crossing","Hyperion Orbit Xing 0.00<lat< 0.50 deg 24.31... 24","Hyperion Orbit Xing$ 253.88884$ 253.97217$ 24.322 to 24.704 Rs lat: 0.075 to 0.074 deg ring-alt: 1921. to 1925.km 002OF035 no ADJ: 29 was:2005-070T21:34:34...2005-070T23:05:17,pointing=CDA to Kepler RAM,rate=524,dataVolume=3.597"]
["2005-071T13:45:00","000T03:00:00","2005-03-12","CIRS","SPASS Rider","InstrumentCalibration","DSCAL1","Deep space calibration",null,"Deep space obervations for calibration."]
["2005-074T05:15:00","000T00:45:00","2005-03-15","ISS","Prime","Iapetus","LIMBTOPOC","Limb topography and geodesy observation","Iapetus limb topography and geodesy observation","Turn -Y to Iapetus; do 1x1 mosaic 1 NAC clear + 4 NAC color + 9 NAC polarizer filters; turn to WP."]
["2005-078T12:19:00","000T05:06:00","2005-03-19","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting H data at a low rate continuously during downlink periods.  No special pointing is  required."]
["2005-081T07:00:00","000T12:15:00","2005-03-22","UVIS","Prime","Saturn","MOS04APO","Apoapsis mosaic","MOSAIC_APO_04_012","Mosaic of Saturn inner magnetosphere.  EUV and FUV low resolution slits on, perpendicular to the orbital plane (FOV Twist: 93.207 deg).  1) Drift at a rate of .152836972 mrad/sec about the Z-axis from START RA/DEC (planet center) to +MOS orb for 4000s.  Drift back to center, reset pointing for planet center. Drift in opposite direction to -MOS orb, drift back and reset pointing.  Total cycle time 16000 seconds.  Rotate 64 mr in the YZ plane from planet center.  Repeat (1) for a cycle time of another 16000 seconds.  Slew back to planet center and reset pointing.  Rotate -64 mr in the YZ plane from planet center.  Drift at the given rate about the Z-axis to +MOS orb for 4000s.  Drift back to start. Total scan time is 40000s. Slew back to planet center and reset pointing.  Stare at Saturn center for remaining time.  MOS orb (+/-range): 609.2888163 mrad"]
["2005-084T05:45:00","000T00:45:00","2005-03-25","ISS","Prime","Iapetus","LIMBTOPOM","Limb topography and geodesy observation","Iapetus limb topography and geodesy observation","Turn -Y to Iapetus; do 1x1 mosaic 1 NAC clear + 4 NAC color + 9 NAC polarizer filters; turn to WP."]
["2005-087T03:42:14","000T02:00:00","2005-03-28","CDA","Non-SPASS","Titan","2000TIORX","Titan orbit crossing","Titan Orbit Xing 0.00<lat< 0.60 deg 20.12... 20.42","Titan Orbit Xing$ 270.15433$ 270.23767$ 20.397 to 20.119 Rs lat: -0.121 to -0.123 deg ring-alt: 2599. to 2606.km 003OF031 no ADJ: 65 was:2005-087T04:14:53...2005-087T05:09:36,pointing=CDA to Kepler RAM,rate=200,dataVolume=1.373"]
["2005-088T20:10:00","000T07:05:00","2005-03-29","MAG","SPASS Rider","Other","INTFLD","MAG Internal field observation","MAG_Internal_Field_Measurements","This request will yield unique observations of Saturns internal magnetic field over a unique orbit track in latitude and longitude space. Port3 C kernal check shows field stays in -X 45deg fov for whole observation."]
["2005-089T11:00:00","000T00:32:00","2005-03-30","ISS","Prime","Rhea","REGMAPA","Regional map","Rhea regional mapping","Turn -Y to Rhea; do 3x3 mosaic in NAC clear."]
["2005-089T14:57:00","000T00:33:00","2005-03-30","CIRS","Prime","Rhea","FP13MAPS","CIRS FP1 / FP3 mapping","FP1 disk scan, FP3 map of subsolar region","FP1 disk scan, FP3 map of Rhea subsolar region.  AD=10.1-9.8 mrad, phase=78-82, LT=6.9-6.6, Sub S/C=(0, 118)-(0, 124), Subsolar=(-22, 41).  Duration 00:33.    Handoff point:  NAC to Rhea center, POS_Z to NSP  Make single FP1 diametric scan from dark to light side.  Length 23 mrad; rate 24 microrad/sec  (00:16).  Then make 2-scan FP3 mosaic centered on lighted side (adjust to provide lateral shift in space off bright limb); each scan 7 mrad at 16 microrad/sec (00:15).  Return to handoff point.  CIRS: 38 RTI, pairs, shutter closed 00:14 to 00:16;  38 RTI, blink 00:16 to 00:33, shutter closed first (and last?) 2 min.  Request one WAC image at beginning (14:57), another at turning point to second scan (ca. T15:20)."]
["2005-090T11:35:16","000T03:00:00","2005-03-31","ISS","Prime","Titan","COMBINED",null,"WAC Photometry, Medium Phase NAC Global Map","particle properties, vertical distributions  about 6 km/px.  0.6 Mbit/frame with 2x2 summing. special S/C orientation requested moderate-phase global map, 200-1000 m/px, emission < 45, need IR-polarizer filter, (special S/C orientation); stereo maps"]
["2005-090T11:35:16","000T03:00:00","2005-03-31","VIMS","SPASS Rider","Titan","MEDRESMAP","Medium resolution regional map","Med_Res_Regional VIMS_4868","Titan Medres Map"]
["2005-090T21:20:16","000T00:45:00","2005-03-31","CIRS","SPASS Rider","Titan","FIRLMBINT","Vertical limb sounding","ISS_PHOT_1x1","ISS WAC support imaging, 2 images per integration (~2 integrations total = 4 frames, 0.5 Mb/frame)"]
["2005-092T20:22:00","000T09:15:00","2005-04-02","CAPS","SPASS Rider","Other","MAGBNDDNL","MAPS magnetosphere boundary campaign","MAPS","Part of  MB,B  MAPS Campaign.  Observe variability of magnetospheric boundaries at several geometrically similar apoapsis"]
["2005-094T16:22:00","000T09:15:00","2005-04-04","CAPS","SPASS Rider","Other","MAGBNDDNL","MAPS magnetosphere boundary campaign","MAPS","Part of  MB,B  MAPS Campaign.  Observe variability of magnetospheric boundaries at several geometrically similar apoapsis"]
["2005-096T05:30:00","000T14:45:00","2005-04-06","CAPS","SPASS Rider","Other","MAGBNDRPW","MAPS magnetosphere boundary campaign","MAPS","Part of  MB,B  MAPS Campaign.  Observe variability of magnetospheric boundaries at several geometrically similar apoapsis"]
["2005-098T20:00:00","000T09:15:00","2005-04-08","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously during downlink periods.  No special pointing is  required."]
["2005-100T05:15:00","000T10:45:00","2005-04-10","CAPS","SPASS Rider","co-rotation","MAGBNDCOR","MAPS magnetosphere boundary campaign","MAPS","Part of  MB,B  MAPS Campaign.  Observe variability of magnetospheric boundaries at several geometrically similar apoapsis"]
["2005-101T01:15:00","000T18:09:33","2005-04-11","INMS","Non-SPASS","Sun","MAGBNDSW","MAPS magnetosphere boundary campaign","MAPS","Part of MB,A MAPS Campaign.  Observe dawn-side magnetospheric boundaries at a variety of radial distances"]
["2005-102T10:10:07","001T10:34:53","2005-04-12","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2005-103T20:45:00","000T09:15:00","2005-04-13","RPWS","Non-SPASS","Saturn","INSURVEY","Inner magnetosphere survey","RPWS Inner Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2005-104T14:37:48","000T00:30:00","2005-04-14","CDA","Non-SPASS","RingE","0707ERNGM","E ring margin","E-Ring Margin 7.00<lat< 8.20 deg 6.68... 6.92 Rs v","E-Ring Margin$ 287.60958$ 287.63041$ 6.879 to 6.740 Rs lat: -7.018 to -7.000 deg ring-alt: 50705. to 49552.km 001OF003 no ADJ: 15 was:2005-104T14:45:35...2005-104T15:00:00,pointing=CDA to Kepler RAM,rate=524,dataVolume=0.899"]
["2005-105T02:10:00","000T08:45:00","2005-04-15","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2005-105T11:25:00","000T02:30:00","2005-04-15","CIRS","Prime","rings(general)","SUBMU04HP","Ring radial scan","CIRS_006RI_SubmU04HP","Radial scan of main rings to obtain submillimeter measurement of rings at a variety of geometries.  NAC to rings, +Z  to NEP 9 WA frames, highly compressed.  Starting T0 + 0:40:00  --  Shutter first image, 1 frame every 10 min for 9 frames."]
["2005-105T18:25:00","000T22:46:46","2005-04-15","RPWS","Non-SPASS","Titan","TINTERACT","MAPS TI/EE Campaign","MAPS TI/EE Campaign","Part of TI/EE MAPS Campaign.  Investigate large-scale and distant aspects of the Titan interaction by observing during entire period around an encounter from 10 to 25 RS"]
["2005-106T13:18:16","007T09:26:15","2005-04-16","CDA","Non-SPASS","DustRAM direction","1901DUST","Dust survey","Dust survey 0.52<lat< 12.18 deg 18.83... 40.52 Rs","Dust survey $ 289.55435 $ 296.94759 $ 18.833 to 40.521 Rs lat: 0.519 to -12.182 deg ring-alt: 10292. to 515861.km,pointing=CDA to Kepler RAM,rate=150,dataVolume=91.377"]
["2005-107T22:25:00","000T03:00:00","2005-04-17","CAPS","Prime","Other","MAGBNDPTG","MAPS magnetosphere boundary campaign","Magnetospheric Boundary Campaign","Part of MB,High MAPS Campaign. Observe dawn-side magnetospheric boundaries at a variety of radial distances. Data volume is included in another, overlapping request."]
["2005-109T06:15:00","000T08:15:00","2005-04-19","UVIS","SPASS Rider","rings(general)","FMONITOR","F ring monitor",null,"UV spectral mapping of Saturn's rings."]
["2005-110T06:15:00","000T00:30:00","2005-04-20","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 028 TH OBS","Turn to first satellite, take 1 NAC (CL1,CL2). Turn to second satellite take 1 NAC (CL1,CL2), repeat for up to 8 satellites if visible"]
["2005-112T05:43:00","000T11:44:00","2005-04-22","UVIS","SPASS Rider","rings(general)","FMONITOR","F ring monitor",null,"UV spectral mapping of Saturn's rings."]
["2005-113T23:14:31","008T17:07:23","2005-04-23","CDA","Non-SPASS","DustRAM direction","0612DUST","Dust survey","Dust survey 12.20<lat< 17.53 deg 6.39... 40.52 Rs","Dust survey $ 296.96842 $ 305.68189 $ 40.521 to 6.388 Rs lat:-12.203 to -17.528 deg ring-alt: 516737. to 116076.km,pointing=CDA to Kepler RAM,rate=150,dataVolume=107.695"]
["2005-117T08:30:00","000T05:30:00","2005-04-27","ISS","Prime","rings(general)","SPKLRSLPB","Ring spoke campaign","Spoke campaign","SPOKE TRACKING: FOLLOW SPOKES AROUND FOR 5.5 HRS; INCLUDE WACS FOR F RING MONITORING"]
["2005-119T05:30:00","000T00:30:00","2005-04-29","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 016 TH OBS","Turn to first satellite, take 1 NAC (CL1,CL2). Turn to second satellite take 1 NAC (CL1,CL2), repeat for up to 8 satellites if visible"]
["2005-120T09:30:00","000T07:00:00","2005-04-30","VIMS","Prime","rings(general)","LATPHASE","Latitude phase coverage","latitude-phase coverage: 3x1 mosaic on each ansa","Orbit 007, Cube Size (X,Z) = 64*64 hires, 80 ms and 320 ms at each pointing. Time per SC pointing (mins) = 30, Number of SC pointings = 12, Time of observation (hours) = 6.0, Volume (Mbits) = 416, Desc = Obtain 6x1 mosaic on each ring ansa on sunlit face. Orient Z-axis parallel to Saturn's pole. Distance 20 R_S."]
["2005-122T18:58:00","000T05:50:00","2005-05-02","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2005-123T01:30:17","000T09:08:22","2005-05-03","CDA","Non-SPASS","DustRAM direction","0416DUST","Dust survey","Dust survey inside 8 Rs 15.99<lat< 17.67 deg 3.71.","Dust survey inside 8 Rs $ 306.06270 $ 306.44353 $ 3.710 to 7.545 Rs lat: 17.666 to 15.989 deg ring-alt: 67916. to 125388.km,pointing=CDA to Kepler RAM,rate=200,dataVolume=6.275"]
["2005-123T10:29:00","000T00:20:00","2005-05-03","CIRS","SPASS Rider","InstrumentCalibration","DEEPSPACE","Deep space calibration",null,"Deep space obervations for calibration during turns"]
["2005-124T12:10:00","000T06:00:00","2005-05-04","CIRS","SPASS Rider","InstrumentCalibration","DSCAL1","Deep space calibration",null,"Deep space obervations for calibration."]
["2005-125T08:10:00","000T09:00:00","2005-05-05","CIRS","SPASS Rider","Saturn","EUVFUV","UVIS EUV / FUV imaging","CIRS_007SA_EUVFUV002_UVIS","Rider to EUVFUV scans"]
["2005-126T03:40:00","002T23:47:00","2005-05-06","MAG","Non-SPASS","co-rotation","MAGBOUND","MAPS magnetosphere boundary campaign","MAG_MAPS_MB_B_Campaign","Observe_variability_of_magnetospheric_boundaries_at_several_geometrically_similar_apoapsis."]
["2005-129T03:27:00","002T23:55:50","2005-05-09","INMS","Non-SPASS","co-rotation","MAGBOUND","MAPS magnetosphere boundary campaign","MAPS","Part of MB,B MAPS Campaign.  Observe variability of magnetospheric boundaries at several geometrically similar apoapsis"]
["2005-133T02:41:00","000T15:14:00","2005-05-13","CDA","Non-SPASS","Other","DRATE","Data volume adjustment","add data rate","dust survey measurements"]
["2005-134T04:12:00","003T22:48:00","2005-05-14","INMS","Non-SPASS","co-rotation","MAGBOUND","MAPS magnetosphere boundary campaign","MAPS","Part of MB,B MAPS Campaign.  Observe variability of magnetospheric boundaries at several geometrically similar apoapsis"]
["2005-135T22:41:00","002T04:19:00","2005-05-15","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2005-139T16:10:00","000T00:20:00","2005-05-19","CIRS","SPASS Rider","InstrumentCalibration","DEEPSPACE","Deep space calibration","Deep Space Cal","Deep space observation for calibration during turns"]
["2005-140T20:26:00","000T01:15:00","2005-05-20","CIRS","Prime","Saturn","CWLEON","CW Leo occultation","CW Leo ingress occultation by Saturn","Ingress latitude TBD; apparent drift rate ca. 17 km/sec.  The apparent passage of CW Leo through the atmosphere of Saturn provides information on the composition and chemistry at high altitudes. One FP3 pixel is targeted on the star throughout the occultation.  The FP3 array axis (Z) is aligned with the apparent drift direction across the planet. FK5 2000.0/2000.0 coordinates 09h 47m 57.3s, +13d 16m 44s = 146.989d, 13.279d."]
["2005-140T21:41:00","000T01:55:00","2005-05-20","ISS","SPASS Rider","Enceladus","ENCELADUS","Enceladus","ENCELADUS Color Photometry","2;N04 or NP03 + 1 NAC Color"]
["2005-141T09:40:21","000T01:28:00","2005-05-21","UVIS","SPASS Rider","Enceladus","HTSPT31KM","Enceladus hot spot imaging","ICYLON:  Longitude / Phase Space Coverage","Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible but north-south is prefered."]
["2005-141T23:40:00","000T01:50:00","2005-05-21","CIRS","SPASS Rider","rings(general)","VERTULHP","Ring scan","CIRS_008RI_VERTULHP_SI","vert"]
["2005-144T04:03:00","000T05:13:00","2005-05-24","VIMS","Prime","Star","OMICETOCC","OmiCet occultation","omiCet","Orbits = 006-052, Cube Size (X,Z) = 64*64 IR-only, Time per SC pointing (mins) = 3.0, Number of SC pointings = 20/hr, Time of observation (hours) = 1.0, Volume (Mbits) = 32/hr, Desc = Stellar_occ mode. same as 7, Phase=90.4, Dist=1.70(10^6km)"]
["2005-145T13:53:00","000T11:16:00","2005-05-25","CAPS","SPASS Rider","Other","MAGBNDDNL","MAPS magnetosphere boundary campaign","MAPS","Part of  MB,B  MAPS Campaign.  Observe dawn-side magnetospheric boundaries at a variety of radial distances"]
["2005-146T16:09:00","000T11:00:00","2005-05-26","MAG","Non-SPASS","Other","MAGBNDDNL","MAPS magnetosphere boundary campaign","MAG_MAPS_MB_B_Campaign","Observe variability of magnetospheric boundaries at several geometrically similar apoapsis. Note datarate assumes 600bps survey."]
["2005-147T16:54:00","000T09:07:00","2005-05-27","CAPS","SPASS Rider","Other","MAGBNDDNL","MAPS magnetosphere boundary campaign","MAPS","Part of  MB,B  MAPS Campaign.  Observe dawn-side magnetospheric boundaries at a variety of radial distances"]
["2005-149T01:01:00","000T14:53:00","2005-05-29","CAPS","SPASS Rider","co-rotation","MAGBNDCOR","MAPS magnetosphere boundary campaign","MAPS","Part of  MB,B  MAPS Campaign.  Observe dawn-side magnetospheric boundaries at a variety of radial distances"]
["2005-150T11:30:00","000T05:00:00","2005-05-30","CIRS","SPASS Rider","rings(general)","APOMOSAIC","Apoapsis mosaic","VIMS Apomosaic Ridealong","4:00 integration on main rings with FP3/4."]
["2005-152T14:30:00","000T00:30:00","2005-06-01","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 007 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [AT-PA-DI-CP-EN (602, 604, 614, 615, 617)]"]
["2005-154T09:00:00","000T02:00:00","2005-06-03","ISS","SPASS Rider","rings(general)","IMPACT",null,"URIMPACT spoke and F ring imaging on each ansa","One WAC at each ansa beginning and end; pointing by UVIS; occasionally try to insert a second exposure"]
["2005-155T01:00:00","003T00:30:00","2005-06-04","CDA","Non-SPASS","Other","SPGBITP0","Data volume adjustment",null,"Sponge bit adds"]
["2005-155T13:10:00","000T01:20:00","2005-06-04","ISS","Prime","Titan","1X1WND10","Wind observation","Titan Surface/winds/clouds imaging","Titan Surface/winds/clouds imaging"]
["2005-157T14:23:00","000T11:10:00","2005-06-06","RSS","SPASS Rider","Saturn","OCCORT","Operations Readiness Test to demonstrate DSN and RSSG preparedness to support upcoming occultations","RSS Operational Readiness Test","RSS Operational Readiness Test (ORT). Pointing=XBAND to Earth.  Last 9 hours required to be tracked by DSS-14, DSS-25, and DSS-26; and last 3.5 hours required to be tracked by DSS-63 and DSS-55."]
["2005-158T22:10:00","000T02:50:00","2005-06-07","ISS","Prime","Dione","GLOCOL","Global coverage mapping","Dione global color and mapping","Turn -Y to Dione; do 1x1 mosaic NAC color + polarizer filters: do CIRS scan; do 1x1 sitNstare; do 2x2 NAC clear mosaic (REGMAP) immediately before return to WP."]
["2005-159T08:44:10","001T09:01:00","2005-06-08","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SURVEY Campaign","Part of SURVEY MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2005-160T06:13:00","000T11:10:00","2005-06-09","RSS","SPASS Rider","Saturn","KADOWN","RSS Ka-Band downlink","Gravity downlink pass","Additional downlink pass at Ka-band to improve Saturn's gravity field determination.  This request includes 5 minutes of Ka-band TWTA maintenance and 2 hours RFIS thermal stabilization."]
["2005-160T06:32:53","000T02:00:00","2005-06-09","CDA","Non-SPASS","DustRAM direction","1207SUOUT","Dust survey","Dust survey outside 8 Rs 7.00<lat< 8.20 deg 12.40.","Dust survey outside 8 Rs$ 343.27283$ 343.35617$ 12.431 to 12.599 Rs lat: 7.714 to 7.508 deg ring-alt: 100666. to 99316.km 002OF012 no ADJ: 95 was:2005-160T07:20:38...2005-160T07:45:07,pointing=CDA to Kepler RAM,rate=200,dataVolume=1.373"]
["2005-161T05:30:14","000T02:00:00","2005-06-10","CDA","Non-SPASS","Titan","2000TIORX","Titan orbit crossing","Titan Orbit Xing 0.00<lat< 0.60 deg 20.12... 20.42","Titan Orbit Xing$ 344.22933$ 344.31266$ 20.218 to 20.410 Rs lat: 0.600 to 0.467 deg ring-alt: 12773. to 10036.km 004OF031 no ADJ: 79 was:2005-161T06:10:04...2005-161T06:50:24,pointing=CDA to Kepler RAM,rate=200,dataVolume=1.373"]
["2005-161T23:45:00","000T01:10:00","2005-06-10","CIRS","SPASS Rider","Hyperion","FP1FAZ0P5","CIRS FP1 phase coverage","FP1 phase coverage at 0.5 cm-1 resolution","FP1 observation of Hyperion for high spectral resolution integration for  composition, and for phase angle coverage. Phase= 18.3, Local time= 11.9, sub S/C=(   17.7, 214.7), AD=   1.9 mrad.  Note that for objects of small apparent size, the 4 mrad  +X offset of CIRS FP1 may make this observation incompatible with simultaneous UVIS  and NAC observations; VIMS retains adequate overlap for simultaneous  observations."]
["2005-162T16:25:00","000T09:00:00","2005-06-11","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously during downlink periods.  No special pointing is  required."]
["2005-163T02:35:00","000T00:30:00","2005-06-12","UVIS","SPASS Rider","rings(general)","FMONITOR","F ring monitor",null,"UV spectral mapping of Saturn's rings."]
["2005-166T01:07:00","002T11:53:00","2005-06-15","MIMI","SPASS Rider","co-rotation","MAGBOUND","MAPS magnetosphere boundary campaign","MAPS MB/B Campaign","APS Campaign.   Observe variability of magnetospheric boundaries at several geometrically similar apoapsis. Set up MIMI for magnetospheric boundaries campaign Pointing: -X to sun and/or corotation, internal B in X, Z plane; or spin about Z."]
["2005-166T11:04:00","000T08:30:00","2005-06-15","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously during downlink periods.  No special pointing is  required."]
["2005-167T05:15:00","000T00:40:00","2005-06-16","ISS","Prime","Saturn","1X6MOVIEB","Saturn movie","NAC Southern Hemisphere Saturn movie","1x6 mos in two filters plus one extra WAC, repeat every two hours, eight minutes."]
["2005-168T11:48:00","000T01:28:00","2005-06-17","CIRS","Prime","rings(general)","FMONITOR","F ring monitor","Ring FP3/FP4 integrations","Integration on the main rings with FP3 and FP4"]
["2005-169T09:08:00","000T01:28:00","2005-06-18","ISS","SPASS Rider","rings(general)","FMONITOR","F ring monitor","F ring imaging on each ansa","One WAC exposures at left ansa, one at right ansa"]
["2005-171T16:00:00","000T09:52:00","2005-06-20","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously during downlink periods.   No special pointing is required."]
["2005-173T20:00:00","000T03:00:00","2005-06-22","CIRS","SPASS Rider","InstrumentCalibration","DSCAL2","Deep space calibration",null,"Deep space obervations for calibration."]
["2005-174T02:00:00","000T23:00:00","2005-06-23","RPWS","Non-SPASS","co-rotation","MAGBOUND","MAPS magnetosphere boundary campaign","MAPS MB,B Campaign","Part of MB,B MAPS Campaign.  Observe variability of magnetospheric boundaries at several geometrically similar apoapsis"]
["2005-175T07:45:00","000T05:15:00","2005-06-24","UVIS","SPASS Rider","rings(general)","COMP","Sit and stare to derive composition",null,"Hi spectral resolution UV map of complete ring system at low phase angle in evening quadrant of rings."]
["2005-177T07:50:25","000T03:34:01","2005-06-26","CDA","Non-SPASS","DustRAM direction","0508DUST","Dust survey","Dust survey inside 8 Rs 8.18<lat< 16.55 deg 4.58..","Dust survey inside 8 Rs $ 360.32668 $ 360.47532 $ 6.190 to 4.582 Rs lat:-16.548 to -8.175 deg ring-alt: 106359. to 39307.km,pointing=CDA to Kepler RAM,rate=200,dataVolume=2.449"]
["2005-177T19:00:57","000T00:36:00","2005-06-26","RSS","Prime","Saturn","OCC","Occultation","RSS Early Diametric Occ. Atm. Ingress 010","THIS REQUEST:  Observations begin at the inner edge of the D ring, roughly corresponding with the beginning of the ionosphere, and continue for 20 minutes after the 2-bar level is reached. GENERAL: This is the first of a set of diametric radio occultations by Saturn's rings and atmosphere. We will observe at Ka, X, and S bands. Observations will commence after a 2-hour period of thermal stabilization in RSS WARMUP mode. In the most general case, we will begin with a 30-min calibration period of free-space observation, and then observe continuously through the entire ingress ring occultation, during the free-space interval between the ring and atmospheric ingress, and we will track the position of the virtual Earth along Saturn's limb as the atmospheric occultation progresses. (For an ingress-only event, this observation will stop at the end of the atmosphere occultation. For an egress-only event, the observing sequence will begin with a two-hour thermal stabilization in RSS WARMUP mode prior to atmospheric egress.) After the ingress atmospheric occultation is over, the S/C may be switched to RSS WARMUP mode, if there is time and power for observations by other instruments while the S/C is in the Earth's shadow. Then the egress atmospheric event will commence with a limb track maneuver, followed by the egress atmosphere and ring occultations, and ending with another 30-minute free-space baseline calibration."]
["2005-178T02:53:28","000T04:35:07","2005-06-27","CDA","Non-SPASS","DustRAM direction","0811DUST","Dust survey","Dust survey outside 8 Rs 10.74<lat< 14.49 deg 8.10","Dust survey outside 8 Rs $ 361.12046 $ 361.31153 $ 8.101 to 10.203 Rs lat: 14.493 to 10.741 deg ring-alt: 122311. to 114716.km,pointing=CDA to Kepler RAM,rate=200,dataVolume=3.148"]
["2005-178T11:00:00","000T02:00:00","2005-06-27","CIRS","SPASS Rider","rings(general)","TEMPU08HP","Thermal map","CIRS_010RI_TempU08HP","Afternoon radial scan of main rings to obtain thermal measurement of rings.  -Y to rings, Z perp to rings"]
["2005-179T13:08:00","000T00:59:00","2005-06-28","VIMS","SPASS Rider","Saturn","1X2WPH120","Photopolarimetry","ISS 1X2WPH120","ISS 1X2WPH120"]
["2005-181T05:40:00","005T13:14:19","2005-06-30","INMS","Non-SPASS","co-rotation","MAGBOUND","MAPS magnetosphere boundary campaign","MAPS","Part of MB,B MAPS Campaign.  Observe variability of magnetospheric boundaries at several geometrically similar apoapsis"]
["2005-183T15:07:00","000T09:15:00","2005-07-02","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously during downlink periods.   No special pointing is required."]
["2005-185T20:37:00","000T01:33:00","2005-07-04","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey"]
["2005-186T07:14:00","000T00:40:00","2005-07-05","ISS","Prime","Saturn","1X6MOVIEE","Saturn movie","NAC Southern Hemisphere Saturn movie","1x6 mos in two filters plus one extra WAC, repeat every two hours, eight minutes."]
["2005-187T16:40:00","000T08:50:00","2005-07-06","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously during downlink periods.   No special pointing is required."]
["2005-191T10:05:00","000T08:00:00","2005-07-10","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously during downlink periods.   No special pointing is required."]
["2005-192T23:30:00","000T03:15:00","2005-07-11","RADAR","SPASS Rider","Other","SOUTHWARM","Instrument warmup","Distant Titan Latitude Study, Southern Latitudes","Warmup for calibration and science data collection."]
["2005-193T07:40:00","000T16:03:00","2005-07-12","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2005-194T00:00:00","000T04:00:00","2005-07-13","CIRS","SPASS Rider","RingC","SHADLLP","Saturn ring shadow observation","CIRS_0011RC_SHADLLP_SI","Stare at West ansa, low phase, lit face -Y to ring, +Z perpendicular to ring radius"]
["2005-194T18:10:00","001T21:50:00","2005-07-13","RPWS","Non-SPASS","Saturn","INSURVEY","Inner magnetosphere survey","RPWS Inner Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2005-195T10:25:00","000T00:55:00","2005-07-14","CIRS","SPASS Rider","Rhea","RHEA","Rhea","Rhea","42i2-63v3 80ms, 640 ms (13 min/cycle) repeat 3  each hour"]
["2005-195T12:24:22","000T01:15:00","2005-07-14","VIMS","SPASS Rider","Enceladus","ENCELADUS","Enceladus","Enceladus targeted","24i2-36v3 80ms, 640ms/cycle 4min/cycle, 5.7 mbits repeat 3 times = 8.55 mbits compressed"]
["2005-195T16:14:22","000T00:25:00","2005-07-14","VIMS","SPASS Rider","Enceladus","ENCELADUS","Enceladus","Enceladus targeted","36i2-54v3 80ms, 640ms/cycle 9min/cycle,  12.8 mbits total uncomp, 1 time"]
["2005-195T18:41:00","000T07:34:00","2005-07-14","MAG","SPASS Rider","Other","INTFLD","MAG Internal field observation","MAG_Internal_Field_Measurements","This request will yield unique observations of Saturns internal magnetic field over a unique orbit track in latitude and longitude space."]
["2005-195T20:53:57","000T19:04:00","2005-07-14","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SURVEY Campaign","Part of SURVEY MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2005-196T02:03:22","000T01:17:00","2005-07-15","VIMS","Prime","rings(general)","HIPHASE","High phase observation","High phase ring observation","Ring hi-phase observations. 2 64*64 frames, 320 msec. First pointing at C ring just off Saturn's left limb. Second pointing is at Saturn's left equatorial limb for CIRS limb observations."]
["2005-196T09:55:56","000T06:07:33","2005-07-15","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey."]
["2005-197T13:15:00","000T00:50:00","2005-07-16","VIMS","SPASS Rider","Saturn","1X2WPH120","Photopolarimetry","ISS 1X2WPH120","ISS 1X2WPH120"]
["2005-197T21:15:00","000T05:15:00","2005-07-16","CIRS","SPASS Rider","Saturn","EUVFUV","UVIS EUV / FUV imaging","CIRS_011SA_EUVFUV004_UVIS","Rider to EUVFUV scans"]
["2005-203T10:06:00","000T09:15:00","2005-07-22","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously during downlink periods.   No special pointing is required."]
["2005-208T14:22:00","000T03:00:00","2005-07-27","CIRS","SPASS Rider","InstrumentCalibration","DSCAL1","Deep space calibration",null,"Deep space obervations for calibration."]
["2005-209T00:00:00","000T04:33:04","2005-07-28","CAPS","Non-SPASS","Saturn","BURST16K","16 kbps burst","Burst of 16kbps data","Burst of 16 kbps data (which gives uncollapsed ELS data). 64 B cycles duration. Data is in addition to 1000 bps from survey."]
["2005-210T22:00:00","000T04:00:00","2005-07-29","ISS","SPASS Rider","rings(general)","IMPACT",null,"URIMPACT spoke and F ring imaging on each ansa","One WAC at each ansa beginning, middle, and end; pointing by UVIS; occasionally insert a second exposure"]
["2005-212T10:07:00","000T11:53:00","2005-07-31","MIMI","SPASS Rider","Saturn","MAGDYN","MAPS magnetosphere dynamics campaign","MAPS IM/DYN Campaign","Part of IM/DYN MAPS Campaign.   Image the dynamics of the inner magnetosphere in ENA with MIMI/INCA. With -Y pointed toward Saturn, corotation as close to the S/C -X, +/- Z plane as possible."]
["2005-213T14:10:00","000T00:10:00","2005-08-01","UVIS","SPASS Rider","Rhea","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2005-213T17:55:00","000T00:45:00","2005-08-01","CIRS","SPASS Rider","Dione","ICYLON","Icy satellite longitudinal coverage","DIONE_FP3","RIDER"]
["2005-213T21:10:04","000T00:50:24","2005-08-01","CDA","Non-SPASS","DustRAM direction","0615SURIN","Dust survey","Dust survey inside 8 Rs 15.00<lat< 17.50 deg 6.20.","Dust survey inside 8 Rs$ 396.88199$ 396.91699$ 6.605 to 6.201 Rs lat:-17.485 to -16.402 deg ring-alt: 119731. to 105636.km 008OF013 no ADJ: 0 was:...,pointing=CDA to Kepler RAM,rate=200,dataVolume=0.576"]
["2005-213T23:46:02","000T00:45:00","2005-08-01","CIRS","SPASS Rider","Mimas","MIMAS","Mimas","MI rider on  VIMS","VIMS rider.  Mimas:  2.7-3.4 mrad, 55, (-25, 155); duration 00:45."]
["2005-214T01:42:02","000T00:29:00","2005-08-02","ISS","SPASS Rider","Mimas","FP3REGION","CIRS FP3 regional map","MIMAS FLYBY(NT) Color","ISS on, max data rate = 182.784 kbps, number of frames and bits/frame are input parameters, data volume = number of frames x bits/frame, average data rate = data volume/duration."]
["2005-214T05:08:02","000T00:25:00","2005-08-02","CIRS","Prime","Mimas","FP1REGION","CIRS FP1 regional map","Regional_FP1_Map","Nighttime observation; 8.0<\\.lt.AD.lt.7.2 mrad; (55, 209); phase=106; LT~1730.  08/02/05. Perform three 6-scan FP1 Nyquist box mosaics (9.8 mrad x 9.8 mrad) of disk at 15.5 cm-1 resolution (4.75 sec /frame).  (3 x 6.5 min).  Then FP1 to 1 mrad in -X of disk center and stare (5 min).  Return to waypoint."]
["2005-214T10:08:16","000T01:30:00","2005-08-02","RSS","SPASS Rider","Saturn","THERMAL","Thermal stabilization period","RSS 012RI MID-OCC Thermal Stabilization","A two-hour period of thermal stabilization is required immediately prior to any radio science experiment and test using Ka-band or S-band."]
["2005-215T07:25:40","000T02:00:00","2005-08-03","CDA","Non-SPASS","rings(general)","1404RINGM","Ring margin","Ring Margin 4.00<lat< 5.00 deg 14.40... 14.60 Rs v","Ring Margin$ 398.30949$ 398.39282$ 14.569 to 14.569 Rs lat: 4.980 to 4.980 deg ring-alt: 76301. to 76301.km 000OF006 yes ADJ: 119 was:2005-215T08:25:28...2005-215T08:25:52,pointing=CDA to Kepler RAM,rate=524,dataVolume=3.598"]
["2005-215T14:50:00","001T07:10:00","2005-08-03","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps). Note: Does NOT overlap XD campaign."]
["2005-217T02:59:00","000T00:40:00","2005-08-05","UVIS","Prime","Star","ALPERI","Alpha Eri occultation","USTRCAL01","INSTANCE OF USTRCAL01. Stellar Calibration: ALPHA ERI"]
["2005-219T19:37:00","000T17:15:00","2005-08-07","CAPS","SPASS Rider","co-rotation","MAGBNDCOR","MAPS magnetosphere boundary campaign","MAPS","Part of  MB,B  MAPS Campaign.  Observe variability of magnetospheric boundaries at several geometrically similar apoapsis"]
["2005-221T12:52:00","000T09:15:00","2005-08-09","MAG","Non-SPASS","Other","MAGBNDDNL","MAPS magnetosphere boundary campaign","MAG_MAPS_MB_B_Campaign","Observe_dawn-side_magnetospheric_boundaries_at_a_variety_of_radial_distances"]
["2005-222T19:00:00","001T03:07:00","2005-08-10","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps). Note: Does NOT overlap XD campaign."]
["2005-224T01:00:00","000T10:15:00","2005-08-12","ISS","SPASS Rider","rings(general)","IMPACT",null,"URIMPACT spoke and F ring imaging on each ansa","One WAC at each ansa beginning, then every 2 hours, and at end; pointing by UVIS; occasionally try to insert a second exposure"]
["2005-225T19:22:00","000T16:00:00","2005-08-13","CAPS","SPASS Rider","co-rotation","MAGBNDCOR","MAPS magnetosphere boundary campaign","MAPS","Part of  MB,B  MAPS Campaign.  Observe variability of magnetospheric boundaries at several geometrically similar apoapsis"]
["2005-226T12:37:00","000T09:00:00","2005-08-14","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting H data at a low rate continuously during downlink periods.   No special pointing is required."]
["2005-228T02:15:00","000T02:00:00","2005-08-16","VIMS","SPASS Rider","rings(general)","IMPACT",null,null,"VIMS uses an offset FOV to make continuous map of the F ring as it rotates underneath."]
["2005-229T02:15:00","000T00:20:00","2005-08-17","ISS","Prime","Hyperion","GEOLOG","Geologic study","GEOLOGY STUDY N03 & NP03","GEOLOGY STUDY N03 & NP03"]
["2005-229T21:10:00","001T16:50:00","2005-08-17","CAPS","Non-SPASS","Saturn","4KSURVEY","MAPS survey","MAPS Survey with extra bits","MAPS magnetospheric survey"]
["2005-230T15:00:00","000T05:00:00","2005-08-18","UVIS","SPASS Rider","RingB","BMOVIE1","B ring movie",null,"UV spectral mapping of Saturn's rings."]
["2005-231T14:00:00","000T17:44:00","2005-08-19","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Normal magnetospheric survey prior to start of internal field observation."]
["2005-232T05:00:00","000T02:34:02","2005-08-20","CDA","Non-SPASS","DustRAM direction","DOWNLK002",null,"Dust survey inside 8 Rs 7.91<lat< 16.36 deg 4.57..","Dust survey inside 8 Rs $ 415.16768 $ 415.31532 $ 6.187 to 4.574 Rs lat:-16.362 to -7.912 deg ring-alt: 105149. to 37984.km,pointing=CDA to Kepler RAM,rate=200,dataVolume=2.432"]
["2005-232T11:50:00","000T00:05:00","2005-08-20","RPWS","Non-SPASS","Saturn","HRSED","Highest resolution saturn kilometric radiation observation","Highest Resolution SED Observations","Obtain the highest resolution observations of Saturn Electrostatic Discharges (SED) by using the RPWS HF-WBR mode at ~180 kbps within 6 RS for a total of 60 minutes within the first 12 periapses inside of 6 RS.  Results will help to verify the source as lightning, or provide evidence that they could be of some other origin (e.g. rings).  No attitude requirement."]
["2005-233T21:12:32","000T01:22:28","2005-08-21","INMS","Non-SPASS","Titan","T6INBD",null,"MAPS/TOST","Coming soon..."]
["2005-234T06:38:37","000T02:30:00","2005-08-22","ISS","SPASS Rider","Titan","FIRLMBINT","Vertical limb sounding","High Resolution Imaging","limb photometry"]
["2005-234T09:53:37","000T11:00:00","2005-08-22","INMS","Non-SPASS","Titan","T6OUTBD",null,"MAPS/TOST Campaign","Coming soon..."]
["2005-234T11:12:32","001T02:29:28","2005-08-22","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2005-235T13:42:00","001T07:40:00","2005-08-23","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2005-238T19:59:00","000T15:54:00","2005-08-26","INMS","Non-SPASS","co-rotation","MAGBNDCOR","MAPS magnetosphere boundary campaign","MAPS","Part of MB,A MAPS Campaign.  Observe dawn-side magnetospheric boundaries at a variety of radial distances"]
["2005-239T21:08:00","000T14:30:16","2005-08-27","INMS","Non-SPASS","Sun","MAGBNDSW","MAPS magnetosphere boundary campaign","MAPS","Part of MB,A MAPS Campaign.  Observe dawn-side magnetospheric boundaries at a variety of radial distances"]
["2005-240T12:01:24","000T00:00:01","2005-08-28","MP","SPASS Note","Saturn","APOAPSE","Apoapse",null,"Apoapse per = 16.0 d, inc = 15.8 deg, r = 37.8 Rs, phase = 75 deg"]
["2005-242T21:43:00","001T00:10:00","2005-08-30","MIMI","SPASS Rider","co-rotation","MAGBOUND","MAPS magnetosphere boundary campaign","MAPS MB/A Campaign","Part of MB/A MAPS Campaign.   Set up MIMI for magnetospheric boundaries campaign with corotation pointing. Pointing: -X to corotation, Saturn B in X, Z plane; or spin about Z. Observe dawn-side magnetospheric boundaries at a variety of radial distances."]
["2005-243T21:53:00","000T08:29:00","2005-08-31","MAG","Non-SPASS","co-rotation","MAGBNDSW","MAPS magnetosphere boundary campaign","MAG_MAPS_MB_A_Campaign","Observe_dawn-side_magnetospheric_boundaries_at_a_variety_of_radial_distances"]
["2005-244T06:22:00","000T14:15:00","2005-09-01","MAG","Non-SPASS","Other","MAGBNDDNL","MAPS magnetosphere boundary campaign","MAG_MAPS_MB_A_Campaign","Observe_dawn-side_magnetospheric_boundaries_at_a_variety_of_radial_distances"]
["2005-245T21:20:00","000T00:40:00","2005-09-02","CIRS","SPASS Rider","Tethys","OPNAV","Optical navigation image","FP3_High_Res","Rider OPNAV of Tethys; AD=0.59 mrad, Phase=60; LT=08; subS/C=(-5,333).  Would like OPNAV image as Support Image."]
["2005-247T05:10:00","000T14:20:00","2005-09-04","INMS","Non-SPASS","Saturn","FULLSURV","MAPS magnetospheric survey","MAPS Survey","MAPS magnetospheric survey."]
["2005-247T20:00:00","000T05:50:00","2005-09-04","CIRS","Prime","rings(general)","SUBML15LP","Ring radial scan","CIRS_014RI_SubmL15LP","Radial scan of main rings to obtain submillimeter measurement of rings at a variety of geometries."]
["2005-248T05:57:14","000T00:30:00","2005-09-05","CDA","Non-SPASS","RingE","0507ERNGM","E ring margin","E-Ring Margin 7.00<lat< 8.20 deg 5.38... 5.62 Rs v","E-Ring Margin$ 431.24808$ 431.26892$ 5.611 to 5.465 Rs lat: -7.119 to -7.039 deg ring-alt: 41950. to 40403.km 001OF002 no ADJ: 14 was:2005-248T06:04:18...2005-248T06:20:10,pointing=CDA to Kepler RAM,rate=524,dataVolume=0.899"]
["2005-249T01:20:00","000T18:52:07","2005-09-06","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey."]
["2005-249T12:00:00","000T00:34:08","2005-09-06","CAPS","Non-SPASS","InstrumentCalibration","ELSCAL","CAPS Electron Spectrometer calibration","Calibration/Gain curve of ELS sensor","Calibration/gain curve of ELS sensor. 8 B cycles duration in 16 kbps. Data is in addition to 1000 bps from SWSKR."]
["2005-250T03:11:57","000T04:08:00","2005-09-07","ISS","Prime","Titan","COMBINED",null,"Medium Phase NAC Global Map combined with higher r","moderate-phase global map, 200-1000 m/px, emission < 45, need IR-polarizer filter, (special S/C orientation); stereo maps"]
["2005-250T13:51:57","000T03:20:00","2005-09-07","CIRS","Prime","Titan","MIRLMBINT","Mid infrared limb integration","CIRS_013TI_MIRLIMBINT_01","Obtain information on trace constituents in Titan's stratosphere.  Integrate on limb at two positions  POINTING: -y to Titan, z within 30 degrees of normal to limb."]
["2005-252T11:09:00","000T10:00:00","2005-09-09","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2005-254T20:30:00","000T01:20:00","2005-09-11","ISS","Prime","Tethys","MUTUALEVE","Mutual event satellite transit observation","MUTUAL EVENTS, TRANSIT OF Tethys    ACROSS Dione","Turn to satellite, take 1 NAC every ~ minute for duration of event while tracking satellite"]
["2005-256T20:09:00","000T21:30:00","2005-09-13","MAG","Non-SPASS","co-rotation","MAGBOUND","MAPS magnetosphere boundary campaign","MAG_MAPS_MB_A_Campaign","Observe_dawn-side_magnetospheric_boundaries_at_a_variety_of_radial_distances"]
["2005-258T19:54:00","001T00:00:00","2005-09-15","MAG","Non-SPASS","co-rotation","MAGBOUND","MAPS magnetosphere boundary campaign","MAG_MAPS_MB_A_Campaign","Observe_dawn-side_magnetospheric_boundaries_at_a_variety_of_radial_distances"]
["2005-259T19:54:00","000T21:30:00","2005-09-16","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2005-263T16:35:00","002T02:15:00","2005-09-20","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey"]
["2005-263T23:05:00","000T00:20:00","2005-09-20","UVIS","SPASS Rider","Dione","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2005-264T13:30:00","001T05:20:00","2005-09-21","MAG","Non-SPASS","co-rotation","MAGBOUND","MAPS magnetosphere boundary campaign","MAG_MAPS_MB_A_Campaign","Observe_dawn-side_magnetospheric_boundaries_at_a_variety_of_radial_distances"]
["2005-265T03:10:00","000T00:20:00","2005-09-22","UVIS","SPASS Rider","Dione","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2005-265T19:10:00","000T00:30:00","2005-09-22","UVIS","SPASS Rider","Mimas","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2005-266T13:20:47","000T00:52:57","2005-09-23","CDA","Non-SPASS","DustRAM direction","0600DUST","Dust survey","E Ring dense - survey - 0.12<lat< 0.14 deg 5.63...","E Ring dense - survey - $ 449.55610 $ 449.59288 $ 6.075 to 5.627 Rs lat: -0.139 to -0.115 deg ring-alt: 889. to 681.km,pointing=CDA to Kepler RAM,rate=524,dataVolume=1.587"]
["2005-266T23:10:36","000T00:33:59","2005-09-23","CDA","Non-SPASS","DustRAM direction","0400DUST","Dust survey","E Ring dense - survey - 0.25<lat< 0.27 deg 3.65...","E Ring dense - survey - $ 449.96569 $ 449.98930 $ 3.652 to 3.864 Rs lat: 0.273 to 0.254 deg ring-alt: 1050. to 1033.km,pointing=CDA to Kepler RAM,rate=524,dataVolume=1.018"]
["2005-267T01:10:00","000T00:30:00","2005-09-24","UVIS","SPASS Rider","Tethys","ICYLON","Icy satellite longitudinal coverage","ICYMAP","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2005-267T04:38:47","000T00:30:38","2005-09-24","CDA","Non-SPASS","DustRAM direction","0600DUST","Dust survey","E Ring dense - survey - 0.07<lat< 0.08 deg 6.41...","E Ring dense - survey - $ 450.19360 $ 450.21489 $ 6.412 to 6.678 Rs lat: 0.084 to 0.072 deg ring-alt: 567. to 506.km,pointing=CDA to Kepler RAM,rate=524,dataVolume=0.918"]
["2005-268T14:24:53","000T00:45:53","2005-09-25","CIRS","SPASS Rider","Hyperion","ISSRIDER","ISS ride along activity","Hyperion Rider on ISS","CIRS coverage of morning hemisphere."]
["2005-268T17:19:46","000T00:01:45","2005-09-25","ISS","Prime","Hyperion","ROTCOL","Satellite rotation and color imaging","HYPERION Rotation Monitor","GRN"]
["2005-268T21:31:46","000T00:23:00","2005-09-25","VIMS","Prime","Hyperion","HYPERION","Hyperion","Hyperion","vis and IR hi-res 16 x 16. 320 IR int time, 30 cyclics<p>Reaction Wheels Required"]
["2005-269T01:29:46","000T00:49:00","2005-09-26","ISS","Prime","Hyperion","MORPHO","Morphology","HYPERION Morphology","CUSTOM GRN NAC + WAC fast-geometry closeup imaging."]
["2005-269T01:54:46","000T00:15:00","2005-09-26","INMS","Non-SPASS","Hyperion","ICYSATIB","Icy satellite imaging","SOST","Measurements of magnetospheric/exospheric interaction and the determination of surface composition."]
["2005-269T08:57:02","000T01:25:51","2005-09-26","ISS","SPASS Rider","Hyperion","HYPERION","Hyperion","HYPERION Color","N05 color"]
["2005-271T19:46:00","000T08:00:00","2005-09-28","CIRS","Prime","rings(general)","FP34INTEG","CIRS FP3 / FP4 integration","CIRS_015RI_F34INTEG_PRIME","FP3/4 integration on main rings"]
["2005-273T09:41:00","000T09:45:00","2005-09-30","CAPS","SPASS Rider","Other","MAGBNDDNL","MAPS magnetosphere boundary campaign","CAPS","Part of  MB,A  MAPS Campaign.  Observe dawn-side magnetospheric boundaries at a variety of radial distances"]
["2005-274T02:50:00","000T00:40:00","2005-10-01","VIMS","SPASS Rider","Saturn","1X6MOVIEA","Saturn movie","ISS 1X6 Movie Ride Along","ISS Movie Ride Along"]
["2005-276T01:46:00","000T00:40:00","2005-10-03","ISS","Prime","Saturn","1X6MOVIEA","Saturn movie","NAC Southern Hemisphere Saturn movie","1x6 mos in two filters plus one extra WAC, repeat every two hours, eight minutes."]
["2005-277T03:22:00","000T00:40:00","2005-10-04","ISS","Prime","Saturn","1X6MOVIEB","Saturn movie","NAC Southern Hemisphere Saturn movie","1x6 mos in two filters plus one extra WAC, repeat every two hours, eight minutes."]
["2005-277T19:09:00","001T23:33:00","2005-10-04","MIMI","SPASS Rider","co-rotation","MAGBOUND","MAPS magnetosphere boundary campaign","MAPS MB/A Campaign","Part of MB/A MAPS Campaign.   Set up MIMI for magnetospheric boundaries campaign with corotation pointing. Pointing: -X to corotation, Saturn B in X, Z plane; or spin about Z. Observe dawn-side magnetospheric boundaries at a variety of radial distances."]
["2005-279T18:42:00","001T00:00:00","2005-10-06","INMS","Non-SPASS","co-rotation","MAGBNDCOR","MAPS magnetosphere boundary campaign","MAPS","Part of MB,A MAPS Campaign.  Observe dawn-side magnetospheric boundaries at a variety of radial distances"]
["2005-281T12:30:00","001T01:44:06","2005-10-08","CDA","Non-SPASS","DustRAM direction","2500DUST","Dust survey","Dust survey 0.28<lat< 0.30 deg 24.76... 41.17 Rs v","Dust survey $ 458.97941 $ 465.59314 $ 41.172 to 24.756 Rs lat: -0.277 to -0.301 deg ring-alt: 12009. to 7846.km,pointing=CDA to Kepler RAM,rate=78"]
["2005-283T05:57:35","000T02:00:00","2005-10-10","CDA","Non-SPASS","Titan","2000TIORX","Titan orbit crossing","Titan Orbit Xing 0.00<lat< 0.60 deg 20.12... 20.42","Titan Orbit Xing$ 466.24833$ 466.33166$ 20.407 to 20.134 Rs lat: -0.297 to -0.297 deg ring-alt: 6382. to 6297.km 010OF031 no ADJ: 65 was:2005-283T06:30:14...2005-283T07:24:57,pointing=CDA to Kepler RAM,rate=200,dataVolume=1.373"]
["2005-284T00:00:00","000T00:20:00","2005-10-11","CIRS","SPASS Rider","Dione","ICYLON","Icy satellite longitudinal coverage","UVIS rider","."]
["2005-284T07:38:00","000T01:00:00","2005-10-11","CIRS","Prime","Dione","FP3MAP","CIRS FP3 map","FP3 mapping","FP3 observation of Dione."]
["2005-284T10:08:00","000T00:20:00","2005-10-11","CIRS","Prime","Dione","FP3MAP","CIRS FP3 map","FP3 mapping of midday disk","FP3 observation of Dione.  R=360K km; AD=3.1 mrad; ss/c=(-0, 129); phase=21; LT=12.5; Tmax~110K.  Design:  Single 4 mrad FP3 scan in X at 16 microrad/sec, centered on disk (20 min).  CIRS at 15.5 cm-1 res.; blink; shutter closed first 60 sec."]
["2005-284T15:42:02","000T02:02:00","2005-10-11","CIRS","SPASS Rider","Dione","TARGFLYBY",null,"ISS Dione rider","Ride on ISS Telesto observation"]
["2005-284T19:22:02","000T01:00:00","2005-10-11","ISS","Prime","Telesto","MORPHO","Morphology","TELESTO Morphology","8-color NAC"]
["2005-285T01:24:57","000T00:54:42","2005-10-12","CDA","Non-SPASS","Mimas","0300MIORX","Mimas orbit crossing","Mimas Orbit Xing 0.00<lat< 1.70 deg 3.05... 3.11 R","Mimas Orbit Xing$ 468.05899$ 468.09698$ 3.103 to 3.108 Rs lat: 0.298 to 0.336 deg ring-alt: 974. to 1100.km 001OF002 no ADJ: 0 was:...,pointing=CDA to Kepler RAM,rate=4192,dataVolume=13.120"]
["2005-285T08:57:00","000T10:01:00","2005-10-12","INMS","Non-SPASS","Saturn","POTM38PRM","MAPS survey","MAPS Survey","MAPS magnetospheric survey."]
["2005-285T19:45:00","000T01:55:00","2005-10-12","CDA","Non-SPASS","RingE","ECCENDV","Eccentricity scan","DV Corrector","E Ring particle eccentricity scan between 8 and 12 Rs"]
["2005-286T19:55:00","002T14:48:00","2005-10-13","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey"]
["2005-286T22:50:00","000T00:30:00","2005-10-13","UVIS","SPASS Rider","Tethys","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2005-287T21:45:00","000T00:30:00","2005-10-14","UVIS","SPASS Rider","Mimas","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible and may be adjusted to minimize slew time."]
["2005-288T23:20:00","000T00:30:00","2005-10-15","ISS","Prime","Rhea","166W087PH","Spectrophotometery","Rhea spectrophotometry/ phase coverage","Turn -Y to Rhea; Do 1x1 mosaic clear + 4 NAC color + 9 NAC polarizer + 4 WAC polarizer filters"]
["2005-289T04:40:00","001T13:33:00","2005-10-16","MIMI","SPASS Rider","co-rotation","MAGBOUND","MAPS magnetosphere boundary campaign","MAPS MB/A Campaign","Part of MB/A MAPS Campaign.   Set up MIMI for magnetospheric boundaries campaign with corotation pointing. Pointing: -X to corotation, Saturn B in X, Z plane; or spin about Z. Observe dawn-side magnetospheric boundaries at a variety of radial distances."]
["2005-290T18:33:00","000T00:30:00","2005-10-17","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 032 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [EP-TL-PM-DI-TI (604, 606, 611, 613, 616)]"]
["2005-293T17:58:00","000T06:24:24","2005-10-20","CAPS","SPASS Rider","co-rotation","MAGBNDCOR","MAPS magnetosphere boundary campaign","CAPS","Part of  MB,A  MAPS Campaign.  Observe dawn-side magnetospheric boundaries at a variety of radial distances"]
["2005-294T00:35:10","006T10:23:49","2005-10-21","CDA","Non-SPASS","DustRAM direction","2500DUST","Dust survey","Dust survey 0.34<lat< 0.36 deg 24.75... 40.64 Rs v","Dust survey $ 477.02442 $ 483.45764 $ 40.636 to 24.755 Rs lat: -0.339 to -0.360 deg ring-alt: 14505. to 9384.km,pointing=CDA to Kepler RAM,rate=150,dataVolume=79.511"]
["2005-295T10:29:00","002T23:45:00","2005-10-22","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2005-298T12:14:00","000T06:25:00","2005-10-25","MIMI","Prime","co-rotation","MAGBNDCOR","MAPS magnetosphere boundary campaign","Magnetospheric Boundary Campaign, Co-rotation","Pointing for MAGBOUNDARY Campaign, Co-rotation attitude"]
["2005-300T11:00:00","000T02:00:00","2005-10-27","CDA","Non-SPASS","Hyperion","2400HYORX","Hyperion orbit crossing","Hyperion Orbit Xing 0.00<lat< 0.50 deg 24.31... 24","Hyperion Orbit Xing$ 483.45833$ 483.54167$ 24.695 to 24.330 Rs lat: -0.360 to -0.360 deg ring-alt: 9361. to 9223.km 009OF035 no ADJ: 30 was:2005-300T11:15:21...2005-300T12:44:39,pointing=CDA to Kepler RAM,rate=524,dataVolume=3.598"]
["2005-300T18:29:00","000T07:46:25","2005-10-27","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey"]
["2005-301T04:12:25","000T00:06:00","2005-10-28","RADAR","Prime","Titan","TI8P5HSAR",null,"T8 High Resolution Synthetic Aperture RADAR SAR","High Resolution Synthetic Aperture RADAR (SAR) Imaging."]
["2005-301T16:03:10","000T03:26:17","2005-10-28","CDA","Non-SPASS","DustRAM direction","1500DUST","Dust survey","Ring Margin - survey - 0.38<lat< 0.38 deg 14.85...","Ring Margin - survey - $ 484.66887 $ 484.81214 $ 16.131 to 14.849 Rs lat: -0.375 to -0.381 deg ring-alt: 6369. to 5957.km,pointing=CDA to Kepler RAM,rate=524,dataVolume=6.185"]
["2005-302T00:19:00","000T00:30:00","2005-10-29","CIRS","SPASS Rider","InstrumentCalibration","DSCALSHRT","Deep space calibration","Short Deep Space Calibration","Deep space obervations for calibration.   Short cal done during turn."]
["2005-302T17:00:00","001T00:15:00","2005-10-29","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2005-303T00:30:00","000T02:30:00","2005-10-30","CIRS","Prime","Saturn","LIMBINT","Limb integration","CIRS_017SA_LIMBINT01","obtain stratospheric thermal structure by means of limb sounding in the mid-IR, longitude coverage."]
["2005-303T06:00:00","000T01:45:00","2005-10-30","UVIS","SPASS Rider","Saturn","FEATRACK","Imaging selected lattitudes at a range of emission angles as the planet rotates","UVIS Rider to VIMS FEATRACK","UVIS Rider to VIMS FEATRACK"]
["2005-303T17:15:00","000T23:59:00","2005-10-30","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2005-304T17:40:00","000T00:30:00","2005-10-31","UVIS","SPASS Rider","Rhea","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2005-305T17:29:00","000T00:20:00","2005-11-01","INMS","Non-SPASS","Saturn","FULLSURVY","MAPS magnetospheric survey","MAPS Survey","MAPS magnetospheric survey."]
["2005-306T17:50:00","000T01:30:00","2005-11-02","ISS","Prime","Iapetus","LIMBTOPOB","Limb topography and geodesy observation","Iapetus limb topography and geodesy observation","Turn -Y to Iapetus; Do 1x1 mosaic 3 NAC clear + 4 NAC color filters"]
["2005-307T07:50:00","000T00:30:00","2005-11-03","ISS","Prime","Tethys","238W119PH","Spectrophotometery","Tethys spectrophotometry/ phase coverage","Turn -Y to Tethys; Do 1x1 mosaic 3 clear + 4 NAC color + 9 NAC polarizer + 4 WAC polarizer filters; turn to WP"]
["2005-308T17:30:00","001T00:00:00","2005-11-04","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SURVEY Campaign","Part of SURVEY MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2005-311T00:11:00","000T09:05:00","2005-11-07","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting H data at a low rate continuously.  No special pointing is  required."]
["2005-312T07:36:00","000T09:25:00","2005-11-08","CAPS","SPASS Rider","Other","MAGBNDDNL","MAPS magnetosphere boundary campaign","CAPS","Part of  MB,A  MAPS Campaign.  Observe dawn-side magnetospheric boundaries at a variety of radial distances"]
["2005-313T10:00:00","000T06:00:00","2005-11-09","CIRS","SPASS Rider","InstrumentCalibration","DSCAL1","Deep space calibration",null,"Deep space obervations for calibration."]
["2005-315T17:01:00","000T14:35:00","2005-11-11","CAPS","SPASS Rider","Sun","MAGBNDSW","MAPS magnetosphere boundary campaign","CAPS","Part of  MB,A  MAPS Campaign.  Observe dawn-side magnetospheric boundaries at a variety of radial distances"]
["2005-315T17:01:00","001T00:00:00","2005-11-11","MAG","Non-SPASS","co-rotation","MAGBOUND","MAPS magnetosphere boundary campaign","MAG_MAPS_MB_A_Campaign","Observe_dawn-side_magnetospheric_boundaries_at_a_variety_of_radial_distances"]
["2005-316T17:01:00","000T12:18:07","2005-11-12","RPWS","Non-SPASS","co-rotation","MAGBOUND","MAPS magnetosphere boundary campaign","MAPS MB,A Campaign","Part of MB,A MAPS Campaign.  Observe plasma waves on dawn-side magnetospheric boundaries at a variety of radial distances"]
["2005-317T17:02:00","001T00:00:00","2005-11-13","MIMI","SPASS Rider","co-rotation","MAGBOUND","MAPS magnetosphere boundary campaign","MAPS MB/A Campaign","Part of MB/A MAPS Campaign.   Set up MIMI for magnetospheric boundaries campaign with corotation pointing. Pointing: -X to corotation, Saturn B in X, Z plane; or spin about Z. Observe dawn-side magnetospheric boundaries at a variety of radial distances."]
["2005-318T17:02:00","008T23:01:00","2005-11-14","INMS","Non-SPASS","co-rotation","MAGBOUND","MAPS magnetosphere boundary campaign","MAPS","Part of MB,A MAPS Campaign.  Observe dawn-side magnetospheric boundaries at a variety of radial distances"]
["2005-319T05:47:00","000T11:15:00","2005-11-15","CAPS","SPASS Rider","Other","MAGBNDDNL","MAPS magnetosphere boundary campaign","CAPS","Part of  MB,A  MAPS Campaign.  Observe dawn-side magnetospheric boundaries at a variety of radial distances"]
["2005-321T16:02:00","002T00:00:00","2005-11-17","MIMI","SPASS Rider","co-rotation","MAGBOUND","MAPS magnetosphere boundary campaign","MAPS MB/A Campaign","Part of MB/A MAPS Campaign.   Set up MIMI for magnetospheric boundaries campaign with corotation pointing. Pointing: -X to corotation, Saturn B in X, Z plane; or spin about Z. Observe dawn-side magnetospheric boundaries at a variety of radial distances."]
["2005-322T17:52:00","000T12:45:00","2005-11-18","UVIS","SPASS Rider","Sun","MAGBNDPTG","MAPS magnetosphere boundary campaign","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting H data at a low rate continuously.  No special pointing is  required."]
["2005-323T23:58:00","000T08:49:00","2005-11-19","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting H data at a low rate continuously.  No special pointing is  required."]
["2005-325T16:03:00","000T15:10:00","2005-11-21","MAG","Non-SPASS","co-rotation","MAGBOUND","MAPS magnetosphere boundary campaign","MAG_MAPS_MB_A_Campaign","Observe_dawn-side_magnetospheric_boundaries_at_a_variety_of_radial_distances"]
["2005-327T16:38:00","000T00:30:00","2005-11-23","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 032 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [EN-CP-MI-TL-PM (601, 602, 613, 614, 616)]"]
["2005-329T15:48:00","001T06:19:39","2005-11-25","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey. 834 bps is 8 B cycles in 500 and one in 4000."]
["2005-329T15:48:00","001T06:33:10","2005-11-25","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SURVEY Campaign","Part of SURVEY MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2005-330T16:03:39","000T01:30:00","2005-11-26","ISS","Prime","Rhea","REGCOL",null,"Rhea regional color observation","Turn -Y to selected area on Rhea; Do 2x2 mosaic 24 NAC color + 9 NAC polarizer filters; then 1x1 mosaic 4 WAC polarizer filters"]
["2005-330T20:33:39","000T04:20:00","2005-11-26","CDA","Non-SPASS","RingE","RHE1DUST","Rhea dust observation","Dust envelope around Rhea","Study dust envelope around Rhea. CDA shares this observation with RSS.  pointing: primary: RSS, secondary (-x): RA 210.3, Dec -35.8 @ Rhea C/A power: 11 W data volume:  15 Mbits data rate: 4192 bps"]
["2005-331T01:43:39","000T00:50:00","2005-11-27","UVIS","SPASS Rider","Rhea","ICYMAP","Icy satellite surface map","ICYMAP:  UV Surface Map of Rhea, ORS Rider","UV albedo map of Rhea's surface plus limb drifts"]
["2005-331T08:49:38","000T05:00:00","2005-11-27","RPWS","Non-SPASS","Saturn","SEDMSEC","Saturn Electrical Discharge observation","High temporal observations of SED","Obtain millisecond temporal resolution observations of Saturn Electrostatic Discharges (SED) in order to characterize their temporal structure and to verify their source as lightning (or to refute this).  Dayside high frequency observation --need 1 of 4. No pointing requirement."]
["2005-331T16:00:00","000T02:20:00","2005-11-27","CIRS","SPASS Rider","Enceladus","ORSRIDER",null,"UVIS Cooperative","FP1 observation of Enceladus to be inserted for 15  minutes as part of this observation. At 05:00, approximate phase= 96.3, Local  time= 18.5, sub S/C=(  -0.2, 115.3), AD=   4.1 mrad.  Note that for objects of  small apparent size, the 4 mrad +X offset of CIRS FP1 may make this observation  incompatible with simultaneous UVIS and NAC observations; VIMS retains adequate  overlap for simultaneous observations."]
["2005-331T18:00:00","000T00:20:00","2005-11-27","UVIS","Prime","Enceladus","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is +X to Enceladus north pole, so center illuminated crescent in FUV low res slit (~40 deg south latitude)."]
["2005-331T22:15:00","000T01:41:19","2005-11-27","CDA","Non-SPASS","DustRAM direction","0800DUST","Dust survey","Ring Margin - survey - 0.35<lat< 0.37 deg 8.01...","Ring Margin - survey - $ 514.94157 $ 514.99745 $ 8.009 to 8.584 Rs lat: 0.366 to 0.353 deg ring-alt: 3087. to 3191.km,pointing=CDA to Kepler RAM,rate=524,dataVolume=2.412"]
["2005-332T20:40:00","000T00:30:00","2005-11-28","VIMS","Prime","Tethys","TETH","Tethys","Tethys","6 x 6 hi res vis and IR 640ms and 160ms, 30 of each"]
["2005-333T15:33:00","001T23:46:00","2005-11-29","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2005-334T19:15:00","000T10:29:00","2005-11-30","ISS","SPASS Rider","RingE","E105PHASE","E ring observation","RIDE ALONG E RING OBSERVATIONS","RIDE ALONG E RING OBSERVATIONS"]
["2005-335T15:49:00","001T00:11:00","2005-12-01","ISS","SPASS Rider","rings(general)","RPX110PH","Ring plane crossing","RIDE ALONG RPX OBSERVATIONS","RIDE ALONG RPX OBSERVATIONS"]
["2005-337T11:15:00","000T11:00:00","2005-12-03","UVIS","SPASS Rider","Phoebe","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2005-340T02:19:00","000T03:26:00","2005-12-06","UVIS","Prime","InstrumentCalibration","IMPACT",null,null,"Calibrate HSP and FUV instrument response on dark sky for statistical baseline comparison to IMPACT detection measurements."]
["2005-340T19:20:00","000T00:30:00","2005-12-06","ISS","Prime","Saturn","1X2PLRNCI","Polarimetry","NAC polarimetry Phase 90-135","NAC polarimetry Phase 90-135"]
["2005-341T15:05:00","000T00:30:00","2005-12-07","ISS","Prime","Saturn","1X2PLRNCJ","Polarimetry","NAC polarimetry Phase 90-135","NAC polarimetry Phase 90-135"]
["2005-342T22:50:00","000T00:30:00","2005-12-08","ISS","Prime","Saturn","1X2PLRNCK","Polarimetry","NAC polarimetry Phase 90-135","NAC polarimetry Phase 90-135"]
["2005-343T05:45:00","001T09:05:00","2005-12-09","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SURVEY Campaign","Part of SURVEY MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2005-344T01:05:00","000T00:30:00","2005-12-10","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 050 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [PA-EN-HY-DI-EP (602, 604, 607, 611, 617)]"]
["2005-346T14:50:00","004T14:16:00","2005-12-12","MIMI","SPASS Rider","co-rotation","MAGBOUND","MAPS magnetosphere boundary campaign","MAPS MB/A Campaign","Part of MB/A MAPS Campaign.   Set up MIMI for magnetospheric boundaries campaign with corotation pointing. Pointing: -X to corotation, Saturn B in X, Z plane; or spin about Z. Observe dawn-side magnetospheric boundaries at a variety of radial distances."]
["2005-348T15:15:00","000T10:45:00","2005-12-14","UVIS","SPASS Rider","Phoebe","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2005-350T07:31:00","000T21:20:00","2005-12-16","MIMI","Prime","SolarWind","MAGBNDSWD","MAPS solar wind campaign","Magnetospheric Boundary Campaign, Solar Wind","Pointing for MAGBOUNDARY Campaign, Solar Wind Attitude"]
["2005-354T14:21:00","000T14:45:00","2005-12-20","CAPS","SPASS Rider","co-rotation","MAGBNDCOR","MAPS magnetosphere boundary campaign","CAPS","Part of  MB,A  MAPS Campaign.  Observe dawn-side magnetospheric boundaries at a variety of radial distances"]
["2005-356T08:55:00","000T05:26:00","2005-12-22","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey"]
["2005-356T15:00:00","000T00:11:50","2005-12-22","RPWS","Non-SPASS","co-rotation","HIRATE","High rate mode","MAPS MB,A Campaign"]
["2005-357T18:40:00","000T00:29:59","2005-12-23","CDA","Non-SPASS","Other","DATAVOL","Data volume adjustment","Datavol addition due to SAP","sponge bit adjust"]
["2005-358T01:22:00","000T00:08:00","2005-12-24","ISS","Prime","Rhea","REGGEODC","Regional geodesy","Rhea regional geodesy","Do 1x2 mosaic in NAC clear filter (two shutters per footprint)."]
["2005-358T03:25:00","000T00:45:00","2005-12-24","VIMS","SPASS Rider","Dione","DIONE","Dione","Dione","42i2-63v3 80ms, 640 ms (13 min/cycle) repeat 3 times 17.5 Mbits/cycle, uncompressed"]
["2005-358T16:50:25","000T01:28:42","2005-12-24","CDA","Non-SPASS","DustRAM direction","0500DUST","Dust survey","E Ring dense - survey - 0.06<lat< 0.15 deg 4.98...","E Ring dense - survey - $ 541.70168 $ 541.76329 $ 5.370 to 4.980 Rs lat: -0.146 to -0.059 deg ring-alt: 826. to 309.km,pointing=CDA to Kepler RAM,rate=524,dataVolume=2.659"]
["2005-358T21:23:13","000T00:00:01","2005-12-24","MP","SPASS Note","Saturn","PERIAPSE","Periapse",null,"Periapse per = 27.6 d, inc = 0.4 deg, r = 4.6 Rs, phase = 91 deg"]
["2005-359T01:20:00","000T01:26:00","2005-12-25","CIRS","SPASS Rider","Saturn","LIMBMAPC","Limb sounding","CIRS_019SA_LIMBMAPC005 SI","obtain stratospheric thermal structure by means of limb sounding in the mid-IR, latitude coverage.  POINTING: -y to Saturn, z to limb"]
["2005-359T08:00:00","000T00:55:00","2005-12-25","VIMS","SPASS Rider","Epimetheus","MUTUAL","Mutual event satellite transit observation","MutualEvent","36i2-54v3 160ms, 640 ms (10 min/cycle) 12.8mbits/cycle. 5 cycles  (we may need to make thisdescription"]
["2005-360T06:54:00","000T11:05:30","2005-12-26","INMS","Non-SPASS","Titan","T9INBD",null,"MAPS TI/EE Campaign","Part of TI/EE MAPS Campaign.  Investigate large-scale and distant aspects of the Titan interaction by observing during entire period around an encounter from 10 to 25 RS"]
["2005-360T14:59:30","000T06:30:00","2005-12-26","CIRS","SPASS Rider","Titan","FIRNADCMP","Far infrared nadir composition map","CIRS_019TI_FIRNADIRCOMPINT_01","Obtain information on trace constituents in Titan's stratosphere.  Integrate on limb at two positions  POINTING: Obtain information on CO, HCN, CH4. Integrate on disk at airmass 1.5-2.0. POINTING: -y to Titan, x away from sun."]
["2005-361T09:34:56","000T03:59:04","2005-12-27","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey. Datarate is composed of continuous 494bps (8vps) plus bursts of 1976bps (32vps)."]
["2005-361T13:33:30","002T16:18:30","2005-12-27","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SURVEY Campaign","Part of SURVEY MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2005-363T13:53:00","000T06:13:00","2005-12-29","ISS","SPASS Rider","RingG","G105PHASE","G ring observation","RIDE ALONG G RING OBSERVATIONS","RIDE ALONG G RING OBSERVATIONS"]
["2006-002T13:52:00","000T01:00:00","2006-01-02","ISS","Prime","Other","SATELLORC","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 008 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [PA-DI-EN-CP-JA (602, 604, 610, 614, 617)]"]
["2006-004T13:52:00","000T11:30:00","2006-01-04","UVIS","SPASS Rider","Phoebe","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2006-006T05:02:00","000T03:00:00","2006-01-06","CIRS","SPASS Rider","InstrumentCalibration","DSCAL1","Deep space calibration",null,"Deep space obervations for calibration."]
["2006-007T05:22:00","005T07:16:00","2006-01-07","MIMI","SPASS Rider","co-rotation","MAGBOUND","MAPS magnetosphere boundary campaign","MAPS MB/A Campaign","Part of MB/A MAPS Campaign.   Set up MIMI for magnetospheric boundaries campaign with corotation pointing. Pointing: -X to corotation, Saturn B in X, Z plane; or spin about Z. Observe dawn-side magnetospheric boundaries at a variety of radial distances."]
["2006-012T12:38:00","001T00:00:00","2006-01-12","MAG","Non-SPASS","co-rotation","MAGBOUND","MAPS magnetosphere boundary campaign","MAG_MAPS_MB_A_Campaign","Observe_dawn-side_magnetospheric_boundaries_at_a_variety_of_radial_distances"]
["2006-013T12:38:00","000T16:35:00","2006-01-13","CAPS","SPASS Rider","Sun","MAGBNDSW","MAPS magnetosphere boundary campaign","CAPS","Part of  MB,A  MAPS Campaign.  Observe dawn-side magnetospheric boundaries at a variety of radial distances"]
["2006-014T20:00:00","000T01:59:59","2006-01-14","CDA","Non-SPASS","Hyperion","2400HYORX","Hyperion orbit crossing","Hyperion Orbit Xing 0.00<lat< 0.50 deg 24.31... 24","Hyperion Orbit Xing$ 562.83333$ 562.91667$ 24.711 to 24.316 Rs lat: -0.302 to -0.305 deg ring-alt: 7858. to 7809.km 015OF035 no ADJ: 30 was:2006-014T20:15:21...2006-014T21:44:39,pointing=CDA to Kepler RAM,rate=524,dataVolume=3.597"]
["2006-015T10:41:27","000T02:00:00","2006-01-15","CAPS","SPASS Rider","Titan","T10CLOSE",null,"MAPS 020TI(T10) Campaign","Part of 020TI(T10) MAPS Campaign.  Observations of Titan's interaction with Saturn's magnetosphere"]
["2006-015T12:41:27","000T01:00:00","2006-01-15","CIRS","SPASS Rider","Titan","FIRLMBINT","Vertical limb sounding","ISS_PHOT_1x1","ISS WAC support imaging, 2 images per integration (2 integrations total = 4 frames, 0.5 Mb/frame)"]
["2006-016T14:09:00","000T10:00:00","2006-01-16","CIRS","SPASS Rider","Saturn","CYLMAP","Saturn cylindrical map","VIMS Rider","Rider on VIMS cylindrical map."]
["2006-016T17:02:37","000T00:49:59","2006-01-16","CDA","Non-SPASS","rings(general)","0900RINGM","Ring margin","Ring Margin 0.00<lat< 1.00 deg 9.40... 9.60 Rs v2.","Ring Margin$ 564.71015$ 564.74487$ 9.587 to 9.424 Rs lat: -0.375 to -0.373 deg ring-alt: 3785. to 3701.km 016OF033 no ADJ: 25 was:2006-016T17:15:21...2006-016T17:39:52,pointing=CDA to Kepler RAM,rate=524,dataVolume=1.498"]
["2006-017T05:30:00","000T00:45:00","2006-01-17","UVIS","SPASS Rider","Enceladus","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2006-017T14:19:00","000T00:40:00","2006-01-17","VIMS","Prime","Rhea","RHEA","Rhea","Rhea","48x48i2v3 160, 640 ms (32.3 min/cycle) 23.4 mbits uncomp. do only one cycle VIMS point and stare Rhea is ~30 degrees phase, <11.9 pixels  (R. Clark 3/11/2003)"]
["2006-017T19:22:16","000T00:49:59","2006-01-17","CDA","Non-SPASS","Rhea","0900RHORX","Rhea orbit crossing","Rhea Orbit Xing 0.00<lat< 0.50 deg 8.64... 8.84 Rs","Rhea Orbit Xing$ 565.80713$ 565.84185$ 8.651 to 8.811 Rs lat: 0.376 to 0.378 deg ring-alt: 3425. to 3507.km 017OF032 no ADJ: 25 was:2006-017T19:35:01...2006-017T19:59:32,pointing=CDA to Kepler RAM,rate=4192,dataVolume=11.989"]
["2006-017T22:13:30","000T01:37:45","2006-01-17","CDA","Non-SPASS","DustRAM direction","1000DUST","Dust survey","Ring Margin - survey - 0.38<lat< 0.38 deg 9.68...","Ring Margin - survey - $ 565.92604 $ 565.99394 $ 9.685 to 10.339 Rs lat: 0.381 to 0.380 deg ring-alt: 3885. to 4137.km,pointing=CDA to Kepler RAM,rate=524,dataVolume=2.930"]
["2006-018T00:49:00","000T00:40:00","2006-01-18","UVIS","SPASS Rider","Rhea","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Preferred slit orientation is Z parallel to spin axis."]
["2006-018T12:05:00","000T23:54:00","2006-01-18","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2006-018T19:30:00","000T00:30:00","2006-01-18","ISS","Prime","Tethys","094W147PH","Spectrophotometery","Tethys spectrophotometry/ phase coverage","Turn -Y to Tethys; Do 1x1 mosaic 3 clear + 4 NAC color + 9 NAC polarizer + 4 WAC polarizer filters; turn to WP"]
["2006-019T11:59:00","001T23:54:00","2006-01-19","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2006-019T22:00:00","000T02:25:00","2006-01-19","CIRS","SPASS Rider","InstrumentCalibration","DSCAL1","Deep space calibration",null,"Deep space obervations for calibration."]
["2006-021T12:20:00","000T01:20:00","2006-01-21","UVIS","SPASS Rider","Enceladus","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2006-022T04:23:00","002T07:15:00","2006-01-22","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SURVEY Campaign","Part of SURVEY MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2006-022T21:34:00","000T04:54:00","2006-01-22","UVIS","SPASS Rider","Iapetus","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2006-025T03:33:00","000T03:00:00","2006-01-25","CIRS","SPASS Rider","InstrumentCalibration","DSCAL2","Deep space calibration",null,"Deep space obervations for calibration."]
["2006-025T23:38:00","000T00:30:00","2006-01-25","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 009 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [EP-JA-CP-HE-PA (610, 611, 612, 614, 617)]"]
["2006-026T19:03:00","000T09:00:00","2006-01-26","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting H data at a low rate continuously.  No special pointing is  required."]
["2006-027T05:25:00","006T05:28:00","2006-01-27","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey."]
["2006-030T00:23:00","000T00:30:00","2006-01-30","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 022 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [AT-EP-DI-EN-PA (602, 604, 611, 615, 617)]"]
["2006-032T12:46:00","000T01:30:00","2006-02-01","VIMS","Prime","Star","MUGEMCAL","Mu Gem calibration","Mu Gem calibration","Turn to star : 15 min Multiple cubes w/12x12 FOV IR @ 40/160/640 ms; OCC mode tests.  Time: 75 min;  Volume: 26 Mbits; CompRatio: 2.0 Do not return to waypoint. Not time critical. RWA REQUIRED."]
["2006-034T11:53:00","000T10:00:00","2006-02-03","CIRS","SPASS Rider","Saturn","2X3LGTSEA","Lightning search","ISS Rider","ISS Rider"]
["2006-036T02:48:00","000T03:00:00","2006-02-05","CIRS","SPASS Rider","InstrumentCalibration","DSCAL1","Deep space calibration",null,"Deep space obervations for calibration."]
["2006-036T11:23:00","000T06:24:00","2006-02-05","CIRS","SPASS Rider","Saturn","2X3LGTSEA","Lightning search","ISS Rider","ISS Rider"]
["2006-038T12:08:00","000T10:00:00","2006-02-07","ISS","Prime","Saturn","3X5LIGHTB","3 x 5 mosaic lightning search","NAC Northern Hemisphere Saturn lightning search","Each picket is 3x5 NAC mos using the HAL filter with 56 second exp times, picket duration 01:28:00.  Repeat interval for the pickets is every 02:08:00.   There are 5 pickets in this ob."]
["2006-040T01:33:00","000T09:05:00","2006-02-09","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting H data at a low rate continuously.  No special pointing is  required."]
["2006-041T10:38:00","000T16:30:00","2006-02-10","CAPS","Non-SPASS","Saturn","2KSURVEY","2 kbps survey mode","MAPS Survey","MAPS magnetospheric survey"]
["2006-042T08:08:00","000T10:00:00","2006-02-11","VIMS","SPASS Rider","Saturn","2X3LGTSEA","Lightning search","Saturn Lightning during CIRS F Ring movie","Saturn Lightning during ISS mosaic."]
["2006-045T01:18:00","000T09:05:00","2006-02-14","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting H data at a low rate continuously.  No special pointing is  required."]
["2006-047T03:07:00","000T01:00:00","2006-02-16","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 011 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [PM-EN-CP-MI-TE (601, 602, 603, 614, 616)]"]
["2006-047T04:07:00","000T02:08:00","2006-02-16","VIMS","SPASS Rider","Saturn","2X3LGTSEA","Lightning search","Saturn Lightning during CIRS F Ring movie","Saturn Lightning during ISS search."]
["2006-049T22:07:00","000T02:10:00","2006-02-18","UVIS","SPASS Rider","InstrumentCalibration","IMPACT",null,null,"Calibrate HSP and FUV instrument response on dark sky for statistical baseline comparison to IMPACT detection measurements."]
["2006-051T09:52:00","000T16:15:00","2006-02-20","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_Survey_Measurements","Continuous_low_rate_magnetospheric_survey."]
["2006-052T06:15:00","000T00:30:00","2006-02-21","ISS","Prime","Mimas","166W075PH","Spectrophotometery","Mimas spectrophotometry/ phase coverage","Turn -Y to Mimas; Do 1x1 mosaic 3 clear + 4 NAC color + 9 NAC polarizer + 4 WAC polarizer filters; turn to WP"]
["2006-053T23:50:00","001T02:10:00","2006-02-22","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey."]
["2006-054T16:00:00","000T01:00:00","2006-02-23","UVIS","SPASS Rider","Hyperion","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2006-054T19:50:00","000T01:20:00","2006-02-23","ISS","Prime","Hyperion","GEOLOG","Geologic study","GEOLOGY STUDY","GEOLOGY STUDY"]
["2006-055T09:52:00","000T00:20:00","2006-02-24","CIRS","Prime","Rhea","FP3GLOBAL","CIRS FP3 global map","Global_FP3_map, integration.","Sub-S/C=(0, 107), phase=18, AD=2.9 mrad...A) Displace FP3 2 mrad in +X, then drift in -X at 7.5 microrad/sec for 8 min (4.75 sec/frame, blink, shutter closed for first 2 min)....B) NAC to disk center for 12 min (center detectors, shutter closed for last 2 min)  JRS 05/09/30:  Can we make the scan a bit longer so we have a couple more fovs of sky on each side of Rhea?"]
["2006-056T01:05:00","000T00:47:50","2006-02-25","CDA","Non-SPASS","RingE","0800ERNGX","Ring plane crossing","E Ring Xing 0.00<lat< 1.00 deg 7.68... 7.92 Rs v2.","E Ring Xing$ 604.04364$ 604.07837$ 7.919 to 7.705 Rs lat: -0.338 to -0.330 deg ring-alt: 2818. to 2677.km 018OF032 no ADJ: 15 was:2006-056T01:10:35...2006-056T01:45:07,pointing=CDA to Kepler RAM,rate=4192,dataVolume=11.989"]
["2006-056T10:55:42","000T00:00:01","2006-02-25","MP","SPASS Note","Saturn","PERIAPSE","Periapse",null,"Periapse per = 39.3 d, inc = 0.4 deg, r = 5.6 Rs, phase = 72 deg"]
["2006-057T02:06:01","000T01:25:35","2006-02-26","CDA","Non-SPASS","DustRAM direction","1000DUST","Dust survey","Ring Margin - survey - 0.37<lat< 0.37 deg 9.67...","Ring Margin - survey - $ 605.07555 $ 605.14696 $ 9.674 to 10.366 Rs lat: 0.374 to 0.373 deg ring-alt: 3810. to 4071.km,pointing=CDA to Kepler RAM,rate=524,dataVolume=3.082"]
["2006-057T09:55:19","000T12:30:00","2006-02-26","UVIS","SPASS Rider","Titan","MEDRES","Medium resolution global mapping","UVIS Rider to VIMS Medium Res Map","Ride along with VIMS MEDRES on Titan"]
["2006-058T04:25:19","000T02:30:00","2006-02-27","ISS","Prime","Titan","REGMAPNA","Regional map","NAC Regional Map","regional map"]
["2006-059T08:51:00","002T00:00:00","2006-02-28","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey"]
["2006-059T16:21:00","000T07:00:00","2006-02-28","RADAR","Prime","Other","SRCRADCAL","RADAR microwave source radiometric calibration","Radiometric Calibration Using Microwave Sources","Scan the Sun, Saturn, and microwave sources while collecting radiometry data."]
["2006-061T11:21:00","000T01:24:00","2006-03-02","ISS","Prime","Enceladus","MUTUALEVE","Mutual event satellite transit observation","MUTUAL EVENTS, TRANSIT OF Enceladus ACROSS Rhea","Turn to satellite, take 1 NAC every ~ minute for duration of event while tracking satellite"]
["2006-062T13:15:00","000T03:05:00","2006-03-03","UVIS","SPASS Rider","InstrumentCalibration","IMPACT",null,null,"Calibrate HSP and FUV instrument response on dark sky for statistical baseline comparison to IMPACT detection measurements."]
["2006-062T17:40:00","000T03:10:00","2006-03-03","CAPS","Prime","co-rotation","MAGBNDPTG","MAPS magnetosphere boundary campaign","CAPS Control Pointing during MAG BND Campaign","Part of  MB,C  MAPS Campaign.  Observe dusk-side magnetospheric boundaries at a variety of latitudes"]
["2006-064T19:52:00","000T02:44:00","2006-03-05","CIRS","SPASS Rider","InstrumentCalibration","DSCAL1","Deep space calibration",null,"Deep space obervations for calibration."]
["2006-067T20:36:00","000T00:30:00","2006-03-08","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 049 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [MI-HE-TL-EP-AT (601, 611, 612, 613, 615)]"]
["2006-069T08:20:00","000T16:15:00","2006-03-10","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2006-070T00:35:00","001T07:30:00","2006-03-11","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2006-072T17:30:00","000T04:35:00","2006-03-13","CAPS","Prime","co-rotation","MAGBNDPTG","MAPS magnetosphere boundary campaign","CAPS Control Pointing during MAG BND Campaign","Part of  MB,C  MAPS Campaign.  Observe dusk-side magnetospheric boundaries at a variety of latitudes"]
["2006-073T15:20:00","000T09:00:00","2006-03-14","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting H data at a low rate continuously.  No special pointing is  required."]
["2006-074T00:50:00","000T21:15:00","2006-03-15","VIMS","Prime","RingE","E105PHASE","E ring observation","E Ring near phase 105","Orbits = 017-023, Cube Size (X,Z) = 32*12, Time per SC pointing (mins) = 7, Number of SC pointings = 180, Time of observation (hours) = 20, Volume (Mbits) = 289, Desc = Stare at core of E ring from 30-40 R_S to build up spectra at different phase angles. Orient X-axis parallel to Saturn's pole to measure vertical ring profile. Observations at each phase angle need NOT be contiguous. 32x12; 1 sec exp; do any 1 of 5 at Priority 1; also any 1 of 5 at Priority 2; can be split"]
["2006-076T07:50:00","000T23:59:00","2006-03-17","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_SURVEY","Continuous low-rate magnetospheric survey"]
["2006-077T10:05:57","000T07:00:00","2006-03-18","UVIS","SPASS Rider","Titan","FIRNADCMP","Far infrared nadir composition map","UVIS Rider to CIRS Far Nadir Comp","UVIS Rider to CIRS Far-IR Nadir Comp"]
["2006-078T01:05:57","000T11:00:00","2006-03-19","INMS","Non-SPASS","Titan","T12OUTBD",null,"MAPS TOST Campaign","Part of TOST MAPS Campaign.  Observe magnetospheric/ionospheric interatction."]
["2006-078T15:04:00","000T09:00:00","2006-03-19","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting H data at a low rate continuously.  No special pointing is  required."]
["2006-079T01:45:00","000T01:20:00","2006-03-20","ISS","SPASS Rider","Star","BETORI","Beta Orion occultation","Stellar Occultation by Saturn NAC Rider","NAC high resolution limb images during star occ"]
["2006-079T09:32:00","000T00:30:00","2006-03-20","ISS","Prime","Other","RETHIEQPL","Retargetable observation","DETERMINING THE ORBITS OF NEWLY DISCOVERED SATELLI","Turn to satellite, take 3x1 BOTSIM 4 colour mosaic"]
["2006-079T15:25:31","000T02:43:35","2006-03-20","CDA","Non-SPASS","DustRAM direction","0600DUST","Dust survey","E Ring dense - survey - 0.26<lat< 0.35 deg 5.61...","E Ring dense - survey - $ 627.64272 $ 627.75633 $ 6.143 to 5.611 Rs lat: -0.350 to -0.263 deg ring-alt: 2264. to 1554.km,pointing=CDA to Kepler RAM,rate=524,dataVolume=4.904"]
["2006-080T01:30:00","000T00:15:00","2006-03-21","UVIS","SPASS Rider","Rhea","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible. Crosses multiple CIRS and ISS observations."]
["2006-080T04:30:00","000T00:30:00","2006-03-21","VIMS","SPASS Rider","Rhea","RHEA","Rhea","Rhea","32x64 lo/hi 320ms; 32x32 lo/lo 640ms"]
["2006-080T16:50:00","000T00:10:00","2006-03-21","CIRS","SPASS Rider","Saturn","WAYPTTURN","Waypoint turn","deep space rider","Waypoint turn rider for deep space calibration of following observation.  CIRS 15.5 cm-1 res (4.75 sec/frame); blink. 7 min shutter open (space), then 3 min shutter closed."]
["2006-080T18:17:00","000T00:43:00","2006-03-21","ISS","Prime","Other","RETHIEQPL","Retargetable observation","DETERMINING THE ORBITS OF NEWLY DISCOVERED SATELLI","Turn to satellite, take 3x1 BOTSIM 4 colour mosaic"]
["2006-081T09:30:00","000T01:59:59","2006-03-22","CDA","Non-SPASS","rings(general)","1800RINGM","Ring margin","Ring Margin 0.00<lat< 1.00 deg 18.40... 18.60 Rs v","Ring Margin$ 629.39583$ 629.47917$ 18.420 to 18.590 Rs lat: 0.385 to 0.385 deg ring-alt: 7467. to 7536.km 019OF029 no ADJ: 89 was:2006-081T10:14:53...2006-081T10:45:07,pointing=CDA to Kepler RAM,rate=524,dataVolume=3.597"]
["2006-083T11:10:00","000T00:30:00","2006-03-24","UVIS","SPASS Rider","Mimas","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2006-084T20:50:00","000T00:43:00","2006-03-25","ISS","Prime","Rhea","094W149PH","Spectrophotometery","Rhea spectrophotometry/ phase coverage","Turn -Y to Rhea; Do 1x1 mosaic 3 clear + 4 NAC color + 9 NAC polarizer + 4 WAC polarizer filters; turn to WP"]
["2006-086T13:35:00","000T06:23:00","2006-03-27","CAPS","Prime","Other","MTAILPTG","Magnetotail pointing","CAPS Control Pointing during MAG TAIL Campaign","Part of  MB,A  MAPS Campaign.  Observe dawn-side magnetospheric boundaries at a variety of radial distances"]
["2006-087T22:03:00","000T09:00:00","2006-03-28","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting H data at a low rate continuously.  No special pointing is  required."]
["2006-092T07:18:00","000T11:35:00","2006-04-02","CDA","SPASS Rider","Other","DECON","Decontamination","Decontamination","CDA boresight off-sun, no resources (Watts, bps), resources covered by other request"]
["2006-096T21:17:00","000T09:00:00","2006-04-06","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting H data at a low rate continuously.  No special pointing is  required."]
["2006-099T12:27:00","001T23:20:08","2006-04-09","RPWS","Non-SPASS","Other","MAGTAIL","MAPS magnetotail observation","MAPS MT,distant Campaign","Part of MT,distant MAPS Campaign.  Observe the structure and dynamics of Saturn's magnetotail at large distances downstream"]
["2006-101T11:47:08","005T10:28:52","2006-04-11","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2006-101T20:20:00","000T00:10:00","2006-04-11","ISS","Prime","Iapetus","GLOBMAPS","Global coverage mapping","Iapetus global mapping","Turn -Y to Iapetus; do 2 clr + N08 + NP03; turn to WP"]
["2006-103T21:31:00","000T03:00:00","2006-04-13","CIRS","SPASS Rider","InstrumentCalibration","DSCAL2","Deep space calibration",null,"Deep space obervations for calibration."]
["2006-106T07:16:00","000T05:00:00","2006-04-16","VIMS","SPASS Rider","Saturn","1X2PLRNCP","Polarimetry","VIMS ISS Polarimetry ridealong","Global observation: ridealong with SSI polarimetry observation"]
["2006-107T19:00:00","000T01:00:00","2006-04-17","UVIS","SPASS Rider","Iapetus","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2006-111T07:00:00","000T11:00:00","2006-04-21","CIRS","Prime","Saturn","MIRMAPA","Mid infrared map","CIRS_023SA_MIRMAPA10","Determine upper troposphere and tropopause temperature with spatial resolution of about two degrees of latitude and longitude  POINTING: -y to Saturn, z to pole"]
["2006-113T20:15:00","000T09:00:00","2006-04-23","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2006-116T05:29:00","000T08:30:00","2006-04-26","UVIS","Prime","Hyperion","ICYLONA","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2006-116T17:29:00","000T10:15:09","2006-04-26","CDA","Non-SPASS","DustRAM direction","2100DUST","Dust survey","Dust survey 0.14<lat< 0.18 deg 20.59... 24.22 Rs v","Dust survey $ 664.66235 $ 665.15567 $ 24.216 to 20.591 Rs lat: -0.144 to -0.181 deg ring-alt: 3672. to 3924.km,pointing=CDA to Kepler RAM,rate=150,dataVolume=6.097"]
["2006-118T07:05:00","000T00:45:00","2006-04-28","ISS","Prime","Janus","MUTUALEVE","Mutual event satellite transit observation","MUTUAL EVENTS, TRANSIT OF Janus     ACROSS Titan","Turn to satellite, take 1 NAC every ~ minute for duration of event while tracking satellite"]
["2006-118T18:30:00","000T06:00:00","2006-04-28","CIRS","Prime","Saturn","FTRACK","Feature track","CIRS_023SA_FTRACK05","Limb integration, slow nadir scans at 100 microrad/s, interleaved with ISS and VIMS integrations.  POINTING: -y to saturn, Z to limb for limb integrations, X to pole for scans"]
["2006-119T00:30:00","000T01:00:00","2006-04-29","ISS","Prime","Janus","COLORF","Color image","JANUS Color","N09 + 2 WAC GRN"]
["2006-120T02:15:07","000T01:59:59","2006-04-30","CDA","Non-SPASS","rings(general)","1400RINGM","Ring margin","Ring Margin 0.00<lat< 1.00 deg 14.40... 14.60 Rs v","Ring Margin$ 668.09383$ 668.17716$ 14.408 to 14.595 Rs lat: 0.373 to 0.374 deg ring-alt: 5659. to 5748.km 023OF034 no ADJ: 89 was:2006-120T03:00:00...2006-120T03:30:14,pointing=CDA to Kepler RAM,rate=524,dataVolume=3.597"]
["2006-120T14:58:14","000T02:00:00","2006-04-30","CIRS","SPASS Rider","Titan","MIRLMBMAP","Mid infrared limb map","ISS_PHOT_1x1","ISS WAC support imaging, 2 images per integration (5 integrations total = 10 frames, 0.5 Mb/frame)"]
["2006-120T18:58:14","000T00:44:00","2006-04-30","ISS","SPASS Rider","Titan","HIGHRESNA","High resolution observartion","RCI (Ridealong Context Imaging)","high-resolution imaging, 50-200 m/px, special targets, emission angles < 45 prefer IR-polarizer (phase 45-110)"]
["2006-120T22:33:31","000T13:41:29","2006-04-30","RPWS","Non-SPASS","co-rotation","TINTERACT","MAPS TI/EE Campaign","MAPS TI/EE Campaign","Part of TI/EE MAPS Campaign.  Investigate large-scale and distant aspects of the Titan interaction by observing during entire period around an encounter from 10 to 25 RS"]
["2006-121T21:55:00","000T00:35:00","2006-05-01","ISS","Prime","Mimas","238W161PH","Spectrophotometery","Mimas spectrophotometry/ phase coverage","Turn -Y to Mimas; do 1x1 mosaic 1 NAC clear + 4 NAC color + 9 NAC polarizer filters + 1 WAC context; turn to WP"]
["2006-122T09:30:00","000T00:50:00","2006-05-02","UVIS","SPASS Rider","Rhea","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2006-123T06:50:00","000T00:30:00","2006-05-03","UVIS","SPASS Rider","Mimas","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2006-124T14:00:00","000T01:00:00","2006-05-04","MIMI","Prime","Saturn","TAILPADIS","Magnetotail campaign","Magnetotail Campaign, pitch angle distribution","Pointing for MAGNETOTAIL Campaign, pitchangle distribution attitude"]
["2006-124T15:00:00","000T01:00:00","2006-05-04","ISS","Prime","Dione","310W162PH","Spectrophotometery","Dione spectrophotometry/ phase coverage","Turn -Y to Dione; do 1x1 mosaic 1 NAC clear + 4 NAC color + 9 NAC polarizer filters + 1 WAC context; turn to WP"]
["2006-126T22:00:00","000T01:30:00","2006-05-06","MIMI","Prime","Saturn","TAILPADIS","Magnetotail campaign","Magnetotail Campaign, pitch angle distribution","Pointing for MAGNETOTAIL Campaign, pitchangle distribution attitude"]
["2006-131T04:12:00","001T23:45:00","2006-05-11","CAPS","Non-SPASS","Other","MAGTAIL","MAPS magnetotail observation","MAPS","Part of  MT,lowlat  MAPS Campaign.  Observe the structure and dynamics of Saturn's magnetotail at low latitudes and moderate distances downstream"]
["2006-134T20:27:00","002T07:15:00","2006-05-14","MIMI","SPASS Rider","Other","MAGTAIL","MAPS magnetotail observation","MAPS MT/lowlat Campaign","Part of MT/lowlat MAPS Campaign.   MIMI setup for MAPS Magnetotail observations; observe plasma flows. Pointing: corotation and Saturn both in -X, Z half-plane; or rotate about -X to sun, or rotate about -Z to Earth. Observe the structure and dynamics of Saturns magnetotail at large distances downstream."]
["2006-135T18:42:00","000T09:00:00","2006-05-15","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting H data at a low rate continuously.  No special pointing is  required."]
["2006-138T03:41:00","001T00:00:00","2006-05-18","INMS","Non-SPASS","Saturn","PTOTM61","MAPS survey","MAPS Survey","MAPS magnetospheric survey."]
["2006-140T09:48:11","000T01:25:00","2006-05-20","CIRS","SPASS Rider","Titan","FIRLMBINT","Vertical limb sounding","ISS_PHOT_1x1","ISS WAC support imaging, 2 images per integration (2 integrations total = 4 frames, 0.5 Mb/frame)"]
["2006-140T11:18:11","000T02:00:00","2006-05-20","INMS","Non-SPASS","Titan","T14CLOSE",null,"MAPS TOST Campaign","Part of TOST MAPS Campaign.  Determine atmospheric and ionospheric composition and thermal structure."]
["2006-140T16:18:11","001T03:37:48","2006-05-20","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_SURVEY","Continuous low-rate magnetospheric survey"]
["2006-141T18:42:43","000T00:49:59","2006-05-21","CDA","Non-SPASS","rings(general)","0900RINGM","Ring margin","Ring Margin 0.00<lat< 1.00 deg 9.40... 9.60 Rs v2.","Ring Margin$ 689.77967$ 689.81439$ 9.569 to 9.402 Rs lat: -0.268 to -0.274 deg ring-alt: 2700. to 2713.km 024OF033 no ADJ: 24 was:2006-141T18:54:45...2006-141T19:20:41,pointing=CDA to Kepler RAM,rate=524,dataVolume=1.498"]
["2006-142T03:40:00","000T01:00:00","2006-05-22","VIMS","Prime","Saturn","ALPCMIOCC","Alpha CMI occultation","Alp CMi Stellar Occultation of Saturn","Alp CMi Stellar Occultation of Saturn"]
["2006-142T04:55:49","000T08:00:00","2006-05-22","RPWS","Non-SPASS","Saturn","SEDDF","Saturn Electrical Discharge direction finding","SED Direction-finding","Perform direction-finding on SED to a) verify source in Saturn's atmosphere (or refute this and find source in rings), and b) if source is in atmosphere, use location to characterize the location of thunderstorms.  Need to do this inside 6 RS on at least half of the periapses inside of 6RS.  No pointing requirement"]
["2006-143T04:32:00","000T01:30:00","2006-05-23","ISS","SPASS Rider","Tethys","ICYOCC","Icy satellite occultation observation","UVIS Tethys rider","Take series of GRN filter images as Tethys passes in front of NAC FOV"]
["2006-144T05:46:10","000T11:50:16","2006-05-24","CDA","Non-SPASS","DustRAM direction","2100DUST","Dust survey","Dust survey 0.38<lat< 0.38 deg 20.61... 24.24 Rs v","Dust survey $ 692.24039 $ 692.73364 $ 20.611 to 24.238 Rs lat: 0.377 to 0.384 deg ring-alt: 8182. to 9800.km,pointing=CDA to Kepler RAM,rate=150,dataVolume=6.096"]
["2006-145T03:41:00","000T13:59:00","2006-05-25","VIMS","Prime","RingE","E145MAP","E ring mapping","E Ring map near phase 145","Cube Size (X,Z) = 64*64, Time per SC pointing (mins) = 48, Number of SC pointings = 12-18, Time of observation (hours) = 14, Volume (Mbits) = 160, Desc = 1xN mosaic of both E Ring ansas for vertical and radial structure. Radial limits 3-8 Rs. Individual frames need to be timed to avoid bright satellites."]
["2006-152T04:00:00","000T02:10:30","2006-06-01","RPWS","Non-SPASS","co-rotation","HIRATE","High rate mode","MAPS MB,A Campaign"]
["2006-154T02:39:00","007T20:16:26","2006-06-03","RPWS","Non-SPASS","Other","MAGTAIL","MAPS magnetotail observation","MAPS MT,distant Campaign","Part of MT,distant MAPS Campaign.  Observe the structure and dynamics of Saturn's magnetotail at large distances downstream"]
["2006-155T12:00:00","000T00:34:08","2006-06-04","CAPS","Non-SPASS","InstrumentCalibration","ELSCAL","CAPS Electron Spectrometer calibration","Calibration/Gain curve of ELS sensor","Calibration/gain curve of ELS sensor. 8 B cycles duration in 16 kbps. Data is in addition to 1000 bps from SWSKR."]
["2006-158T12:00:00","000T01:00:00","2006-06-07","ISS","Prime","Mimas","MUTUALEVE","Mutual event satellite transit observation","MUTUAL EVENTS, TRANSIT OF Mimas     ACROSS Janus","Turn to satellite, take 1 NAC every ~ minute for duration of event while tracking satellite"]
["2006-161T02:45:00","000T07:00:00","2006-06-10","ISS","SPASS Rider","Saturn","ANTCAL","Antenna calibration","ISS WAC dark current calibration","ISS WAC dark current calibration"]
["2006-164T07:15:00","000T07:30:00","2006-06-13","CAPS","Prime","Sun","TAILROLL","Magnetotail campaign (rolling)","MAPS","Part of  MT,lowlat  MAPS Campaign.  Observe the structure and dynamics of Saturn's magnetotail at low latitudes and moderate distances downstream.  CAPS will be rolling the s/c."]
["2006-167T11:30:00","000T04:45:00","2006-06-16","CAPS","Prime","Sun","TAILROLL","Magnetotail campaign (rolling)","MAPS","Part of  MT,lowlat  MAPS Campaign.  Observe the structure and dynamics of Saturn's magnetotail at low latitudes and moderate distances downstream.  CAPS will be rolling the s/c."]
["2006-168T10:30:00","000T00:30:00","2006-06-17","ISS","Prime","Janus","MUTUALEVE","Mutual event satellite transit observation","MUTUAL EVENTS, TRANSIT OF Janus     ACROSS Epimeth","Turn to satellite, take 1 NAC every ~ minute for duration of event while tracking satellite"]
["2006-171T02:45:00","000T01:00:00","2006-06-20","ISS","Prime","Iapetus","SPECPHOTC","Spectrophotometry/phase coverage","Iapetus spectrophotometry/ phase coverage","Do 1x1 mosaic 1 NAC clear + 4 NAC color + 9 NAC polarizer"]
["2006-175T01:52:00","000T01:00:00","2006-06-24","ISS","Prime","Helene","MUTUALEVE","Mutual event satellite transit observation","MUTUAL EVENTS, TRANSIT OF Helene    ACROSS Dione","Turn to satellite, take 1 NAC every ~ minute for duration of event while tracking satellite"]
["2006-176T02:12:00","000T00:20:00","2006-06-25","UVIS","SPASS Rider","Iapetus","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2006-178T02:37:00","000T11:00:00","2006-06-27","CIRS","SPASS Rider","Saturn","EUVFUV","UVIS EUV / FUV imaging","CIRS_025SA_EUVFUV002","Rider to UVIS EUVFUV scans"]
["2006-179T11:37:00","000T03:00:00","2006-06-28","VIMS","Prime","Saturn","FEATRACK","Imaging selected lattitudes at a range of emission angles as the planet rotates","Saturn Feature Track #1","Saturn FeaTrak #1"]
["2006-179T16:07:00","003T01:15:00","2006-06-28","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_SURVEY","Continuous low-rate magnetospheric survey"]
["2006-180T17:37:00","000T08:57:00","2006-06-29","INMS","Non-SPASS","Saturn","PTOTM64BU","MAPS survey","MAPS Survey","MAPS magnetospheric survey"]
["2006-181T13:05:10","000T00:00:01","2006-06-30","MP","SPASS Note","Saturn","PERIAPSE","Periapse",null,"Periapse R = 5.4 Rs, lat = -0 deg, phase = 20 deg"]
["2006-182T00:45:00","000T02:30:00","2006-07-01","CDA","Non-SPASS","Other","DRATEC","Data volume adjustment","adjust datavolume for E-Ring measurements","E-Ring dust measurements"]
["2006-182T17:22:00","000T00:13:00","2006-07-01","RPWS","Non-SPASS","Saturn","INSURVEY","Inner magnetosphere survey","RPWS Inner Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2006-183T08:50:47","000T01:00:00","2006-07-02","RPWS","Non-SPASS","Titan","TICA","Titan closest approach","Titan closest approach observations","RPWS observations in the immediate vicinity of Titan, including thermal plasma density and temperature measurements with the Langmuir probe, search for lightning and other radio emissions, characterization of plasma wave spectrum, search for evidence of pickup ions.  Langmuir  probe within 90 degrees of spacecraft ram at closest approach, corotational ram outside of +/- 15 minutes."]
["2006-183T13:20:47","000T11:54:13","2006-07-02","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_SURVEY","Continuous low-rate magnetospheric survey"]
["2006-183T21:20:47","000T03:54:12","2006-07-02","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey"]
["2006-185T01:22:00","000T05:45:00","2006-07-04","VIMS","Prime","RingG","G150PHASE","G ring observation","G Ring near phase 150","12x12; 1 sec exp; do any 2 of 5 at Priority 1; also any 1 of 5 at Priority 2"]
["2006-189T02:24:00","002T21:57:00","2006-07-08","INMS","Non-SPASS","Other","MAGTAIL","MAPS magnetotail observation","MAPS","Part of MT,lowlat MAPS Campaign.  Observe the structure and dynamics of Saturn's magnetotail at low latitudes and moderate distances downstream"]
["2006-190T15:21:00","000T09:00:00","2006-07-09","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting H data at a low rate continuously.  No special pointing is required."]
["2006-197T00:06:00","000T15:00:00","2006-07-16","CDA","Non-SPASS","Other","DRATESAP","Data volume adjustment","additional DV due to sponge bits","dust measurements"]
["2006-198T07:36:00","002T16:15:00","2006-07-17","CDA","Non-SPASS","Other","DRATESAP","Data volume adjustment","additional DV due to sponge bits","dust measurements"]
["2006-200T00:21:00","000T14:00:00","2006-07-19","UVIS","Prime","Saturn","EUVFUV","UVIS EUV / FUV imaging","EUVFUV Imaging of Saturn","Several slow scans across Saturn's visible hemisphere to form spectral images. Distance to Saturn is 2 million Km.  Phase is 135-160"]
["2006-201T18:47:00","000T05:00:00","2006-07-20","CIRS","SPASS Rider","InstrumentCalibration","DSCAL1","Deep space calibration",null,"Deep space obervations for calibration.  CO-ADD FOR CONSISTENCY WITH PREVIOUS E-RING OBSERVATION."]
["2006-202T22:41:26","000T00:52:00","2006-07-21","RADAR","Prime","Titan","T16INSCAT",null,"T16 Inbound Scatterometry","Scatterometry of Titan.  -Z scanned over Titan.  Y axis controlled for different polarizations"]
["2006-203T02:25:26","000T21:34:47","2006-07-22","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SURVEY Campaign","Part of SURVEY MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2006-203T05:25:26","000T02:15:00","2006-07-22","ISS","SPASS Rider","Titan","MIRLMBMAP","Mid infrared limb map","NGM (NAC Global Map)","global map"]
["2006-204T07:00:00","000T01:30:00","2006-07-23","CIRS","SPASS Rider","Rhea","RHEA","Rhea","FP1, FP3 VIMS rider","FP1, FP3 rider on Rhea for composition, phase angle coverage, and dark side FP1 thermal map. Phase=133, Local time= 00, sub S/C=(-30, 270), AD=9.1 mrad.  CIRS Design request: 15.5 cm-1 resolution (38 RTI), blink.  Request 15 min for darkside Nyquist map of 6 FP1 scans at 28 RTI (15.5 cm-1, one-sided).  Shutter closed first 3 min, last 3 min."]
["2006-204T17:00:00","000T01:00:00","2006-07-23","UVIS","SPASS Rider","Tethys","TETHYS","Tethys","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2006-205T04:00:00","000T07:00:00","2006-07-24","CIRS","SPASS Rider","rings(general)","LPHRDFMOV","Ansa movie","CIRS_ISS  Movie Rider","Ride along with ISS observation. No FP4."]
["2006-205T23:30:00","000T15:00:00","2006-07-24","RPWS","Non-SPASS","co-rotation","HIRATE","High rate mode","MAPS MB,A Campaign"]
["2006-206T11:10:00","000T12:20:00","2006-07-25","INMS","Non-SPASS","Saturn","FULLSURV","MAPS magnetospheric survey","MAPS Survey","MAPS magnetospheric survey."]
["2006-208T06:30:00","000T07:51:00","2006-07-27","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_SURVEY","Continuous low-rate magnetospheric survey"]
["2006-210T04:45:00","000T11:05:00","2006-07-29","RSS","SPASS Rider","Earth","SCE3","Solar Corona Experiment","Solar Conjunction Experiment (SCE) #3","Characterize the solar corona at 2 frequency bands (X and Ka1), and assess the electron content and possible Faraday rotation, during the solar conjunction period."]
["2006-210T23:30:00","000T00:34:08","2006-07-29","CAPS","Non-SPASS","InstrumentCalibration","ELSCAL","CAPS Electron Spectrometer calibration","Calibration/Gain curve of ELS sensor","Calibration/gain curve of ELS sensor. 8 B cycles duration in 16 kbps. Data is in addition to 1000 bps from SWSKR."]
["2006-213T04:05:00","000T04:30:00","2006-08-01","ISS","Prime","Star","CHARGEXF","Instrument calibration","ISS CCD Charge Transfer Calibration","Point to Pleiades. Rotate about -Y and image every 20-30 degrees."]
["2006-216T13:50:00","000T09:00:00","2006-08-04","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously during downlink periods.   No special pointing is required."]
["2006-216T21:59:38","010T02:34:24","2006-08-04","CDA","Non-SPASS","DustRAM direction","2100DUST","Dust survey","Dust survey 0.30<lat< 10.12 deg 20.57... 48.96 Rs","Dust survey $ 764.91642 $ 775.02365 $ 48.959 to 20.573 Rs lat: 10.123 to 0.297 deg ring-alt: 519151. to 6434.km,pointing=CDA to Kepler RAM,rate=150,dataVolume=124.921"]
["2006-223T01:15:00","000T02:15:00","2006-08-11","ISS","SPASS Rider","rings(general)","FMONITOR","F ring monitor","F ring imaging on each ansa","One WAC each ansa repeated every 2 hours"]
["2006-225T13:20:00","000T09:40:00","2006-08-13","CAPS","Non-SPASS","Saturn","4KBURST","4 kbps burst","Burst of 4k data","Burst of 4k data"]
["2006-226T08:50:08","001T20:40:00","2006-08-14","MAG","Non-SPASS","co-rotation","DISTTORUS","Distant Titan torus observation","MAG MAPS TI_DT Campaign","Measure the properties of the Titan torus and Titan interaction at large distances from Titan."]
["2006-227T22:21:00","000T07:09:08","2006-08-15","CAPS","SPASS Rider","co-rotation","DISTTORUS","Distant Titan torus observation","MAPS TI/DT Campaign","Part of TI/DT MAPS Campaign.  Measure the properties of the Titan torus and Titan interaction at large distances from Titan"]
["2006-228T14:23:57","000T07:31:03","2006-08-16","RPWS","Non-SPASS","Saturn","SEDDF","Saturn Electrical Discharge direction finding","SED Direction-finding","Perform direction-finding on SED to a) verify source in Saturn's atmosphere (or refute this and find source in rings), and b) if source is in atmosphere, use location to characterize the location of thunderstorms.  Need to do this inside 6 RS on at least half of the periapses inside of 6RS.  No pointing requirement"]
["2006-229T01:30:00","000T01:55:00","2006-08-17","CDA","Non-SPASS","DustRAM direction","0403DUST","Dust survey","E Ring dense - survey - 2.85<lat< 3.61 deg 4.42...","E Ring dense - survey - $ 776.97330 $ 776.98533 $ 4.422 to 4.479 Rs lat: -3.606 to -2.852 deg ring-alt: 16779. to 13446.km,pointing=CDA to Kepler RAM,rate=524,dataVolume=0.518"]
["2006-229T03:25:00","000T01:50:00","2006-08-17","CIRS","SPASS Rider","Helene","ISS",null,"Helene rider","Rider on ISS Helene.  AD=0.38, phase=102, (61, 211).  Duration 01:50.  CIRS 38 RTI, center detectors, coadd."]
["2006-230T04:00:00","000T06:00:00","2006-08-18","VIMS","Prime","Saturn","FTRACK","Feature track","Saturn Feature Track","Saturn Feature Track. Third of three.  This one is near 140 degrees phase angle.  11/25/02: Downlinked volume reduced to 275 Mbits from 375 Mbits due to antennae maintenance 11/17/03: Antennae completely gone! Going to 34 M. New volume: 120 Mbits downlinked"]
["2006-231T22:06:00","008T21:07:51","2006-08-19","MIMI","SPASS Rider","Other","MAGTAIL","MAPS magnetotail observation","MAPS MT/antiS Campaign","Part of MT/antiS MAPS Campaign.   MIMI setup for MAPS Magnetotail observations; observe plasma flows. Pointing: corotation and Saturn both in -X, Z half-plane; or rotate about -X to sun, or rotate about -Z to Earth. Observe the structure and dynamics of Saturns magnetotail at large distances downstream."]
["2006-232T13:06:00","000T09:00:00","2006-08-20","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2006-236T09:21:00","000T01:00:00","2006-08-24","CIRS","Prime","rings(general)","FMONITOR","F ring monitor","F RING monitoring","F Ring monitoring"]
["2006-238T12:51:00","000T09:00:00","2006-08-26","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2006-240T02:30:00","000T02:00:00","2006-08-28","ISS","Prime","Star","MONITOR",null,"ISS Sensitivity monitor","Periodic standard star image to monitor ISS sensitivity"]
["2006-242T23:00:00","000T06:00:00","2006-08-30","CIRS","SPASS Rider","InstrumentCalibration","DSCAL3","Deep space calibration",null,"Deep space obervations for calibration."]
["2006-249T21:06:00","000T19:38:21","2006-09-06","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_SURVEY","Continuous low-rate magnetospheric survey"]
["2006-250T12:46:51","000T04:45:00","2006-09-07","ISS","SPASS Rider","Titan","EUVFUV","UVIS EUV / FUV imaging","WNI (WAC Nightside Imaging)","search for and monitor lightning/aurora"]
["2006-250T19:31:51","000T00:30:00","2006-09-07","CIRS","SPASS Rider","Titan","FIRLMBT","Far Infrared limb tracking","ISS_PHOT_1x1","ISS WAC support imaging, 4 images (4 frames, 0.5 Mb/frame)"]
["2006-250T20:35:56","000T00:40:55","2006-09-07","INMS","Non-SPASS","Titan","T17RMPNT",null,"MAPS TOST Campaign","Part of TOST MAPS Campaign.  Determine atmospheric and ionospheric thermal structure."]
["2006-250T23:49:21","000T21:10:39","2006-09-07","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_SURVEY","Continuous low-rate magnetospheric survey"]
["2006-252T00:30:00","000T02:00:00","2006-09-09","CIRS","Prime","rings(general)","TEMPL10MP","Thermal map","CIRS_028RI_TEMPL10MP","Changed from ridealong with UVIS on URIMPACT;  TEMP measurement"]
["2006-252T05:45:00","000T02:45:00","2006-09-09","UVIS","SPASS Rider","Star","URLAMCET","Stellar occultation","URSTAR","1 NAC at start of UVIS data. 1 NAC at end of UVIS data."]
["2006-252T12:15:00","000T01:58:00","2006-09-09","CIRS","SPASS Rider","rings(general)","RDHRESSCN","Radial scan","CIRS_028RI_RDHRESSCN_ISS","ride with ISS"]
["2006-252T22:50:00","000T01:10:00","2006-09-09","CIRS","Prime","Tethys","TETHYSORS","ORS Tethys observation","Tethys observations by ORS","Joint ORS observations of Tethys."]
["2006-252T22:50:00","000T01:10:00","2006-09-09","UVIS","SPASS Rider","Tethys","TETHYSORS","ORS Tethys observation","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2006-253T19:33:23","000T03:25:36","2006-09-10","CDA","Non-SPASS","DustRAM direction","1423DUST","Dust survey","Dust survey outside 8 Rs 23.48<lat< 23.90 deg 14.4","Dust survey outside 8 Rs $ 801.81485 $ 801.95764 $ 14.397 to 15.645 Rs lat: 23.904 to 23.481 deg ring-alt: 351954. to 376073.km,pointing=CDA to Kepler RAM,rate=200,dataVolume=2.352"]
["2006-254T21:00:00","000T11:25:04","2006-09-11","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2006-255T12:00:00","000T09:00:00","2006-09-12","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously during downlink periods.   No special pointing is required."]
["2006-256T03:50:00","000T08:02:00","2006-09-13","MIMI","Prime","Sun","TAILPLSFL","Magnetotail campaign","Magnetotail Campaign, tailward flow","Pointing for MAGNETOTAIL Campaign, tailward flow attitude"]
["2006-258T17:40:00","000T03:50:00","2006-09-15","RSS","Prime","rings(general)","OCC","Occultation","RSS Ring  Ingress Occulation 028","THIS REQUEST:  Because this is a slow event, we include one hour of baseline prior to the F ring ingress time. GENERAL: We will observe at Ka, X, and S bands. Observations will commence after a 2-hour period of thermal stablization in RSS WARMUP mode. We will commence observations with a 60-minute baseline and calibration period, followed by the ring ingress, which ends at the D ring.  After a two-hour thermal stabilization period, we commence observations of the ingress atmosphere occultation 60 minutes before the 1.3-bar level.  Atmosphere ingress observations end 5 hours after the 1.3-bar level."]
["2006-260T17:08:58","001T04:57:02","2006-09-17","INMS","Non-SPASS","Other","MAGTAIL","MAPS magnetotail observation","MAPS","Part of MT,antiS MAPS Campaign.  Observe the structure and dynamics of Saturn's magnetotail in the anti-solar direction"]
["2006-261T22:39:00","001T21:43:00","2006-09-18","INMS","Non-SPASS","Other","MAGTAIL","MAPS magnetotail observation","MAPS","Part of MT,antiS MAPS Campaign.  Observe the structure and dynamics of Saturn's magnetotail in the anti-solar direction"]
["2006-265T11:00:00","000T15:05:04","2006-09-22","MAG","Non-SPASS","Other","MAGTAIL","MAPS magnetotail observation","MAG_MAPS_MT_antiS_Campaign","Observe_the_structure_and_dynamics_of_Saturn's_magnetotail_in_the_anti-solar_direction. (0)"]
["2006-266T11:28:49","000T04:30:00","2006-09-23","CIRS","SPASS Rider","Titan","FIRNADMAP","Far infrared nadir composition map","CIRS_029TI_FIRNADIRMAP_01","Obtain information on surface & tropopause temperatures, and on tropospheric CH4.  Scan  or contiguous steps across disk.  POINTING: -y to Titan, x away from sun.  Z axis generally aligned N/S or E/W, perpendicular to scan or steps.  Substitutes: T19in"]
["2006-266T18:35:49","000T00:46:00","2006-09-23","INMS","Prime","Titan","T18RMPNT",null,"MAPS TOST Campaign","INMS Titan observation, -X to RAM, second axis favorable to MAPS/RADAR"]
["2006-267T04:34:49","000T00:15:00","2006-09-24","VIMS","Prime","Titan","COMPMAP","Composition map","Comp_map_VIMS","Nested mapping, high, medium and global resolution.  From 00:40 to +5:00 do 12X12 with ISS, high  resolution From +5 to +9 use a medium resolution template From +9 out, 64X64 or 48X48 global mapping  On March 20, 2003 BJB truncated 97 minutes to accommodate a CIRS ring observation."]
["2006-267T20:00:00","002T05:00:00","2006-09-24","RPWS","Non-SPASS","Saturn","INSURVEY","Inner magnetosphere survey","RPWS Inner Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2006-268T19:10:26","000T00:45:00","2006-09-25","RPWS","Non-SPASS","Saturn","WHISTLER","RPWS lightning search","Obtain wideband examples of lightning whistlers","Obtain wideband evidence of lightning whistlers.  These would verify the existence of lightning already suspected from Saturn Electrostatic Discharges (SED) and would provide information on the electron density along the field line to the source.  No pointing requirement."]
["2006-269T02:30:00","000T03:30:00","2006-09-26","CIRS","Prime","rings(general)","TEMPU30MP","Thermal map","CIRS_029RI_TempU30MP","Afternoon radial scan of main rings to obtain thermal measurement of rings.  -Y to rings, Z perp to rings"]
["2006-270T03:45:00","000T07:15:00","2006-09-27","CIRS","Prime","rings(general)","SUBMU36HP","Ring radial scan","CIRS_029RI_SubmU36HP","Radial scan of main rings to obtain submillimeter measurement of rings at a variety of geometries.  -Y to rings, Z perp to rings"]
["2006-271T04:00:00","000T06:30:00","2006-09-28","ISS","SPASS Rider","rings(general)","LATPHASE","Latitude phase coverage","Rev 29 VIMS rider","TWT RINGS  Range 25.37 to 23.74 B -6.08 to -6.26 Phase (start) 52.22-57.13 Phase (end) 49.94-55.19"]
["2006-272T06:52:44","000T00:33:00","2006-09-29","INMS","Non-SPASS","Saturn","MRO","Instrument memory readout","MAPS Survey","MAPS magnetospheric survey."]
["2006-273T11:38:00","000T04:00:00","2006-09-30","CIRS","SPASS Rider","InstrumentCalibration","DSCAL1","Deep space calibration",null,"Deep space obervations for calibration."]
["2006-277T06:52:44","000T00:33:00","2006-10-04","INMS","Non-SPASS","Saturn","MRO","Instrument memory readout","MAPS Survey","MAPS magnetospheric survey."]
["2006-280T08:00:00","000T01:45:00","2006-10-07","RADAR","Prime","Titan","NORTH7CAL","Distant Titan latitude study","Distant Titan Latitude Study, Northern Latitudes","Obtain distant Titan radiometer science and calibration data.  One of a set that provides coverage of Titan northern latitude variation along with some obtainable associated longitude variation."]
["2006-281T23:25:00","000T09:10:00","2006-10-08","CAPS","SPASS Rider","InstrumentCalibration","CALIBRATE","Calibration","CAPS Calibration","CAPS periodic gain test and calibration. The specified rate and data volume are the delta above the CAPS survey rate (1000 bps), and the rate is the average over the entire request (current plans are to conduct the test in two different rates.)"]
["2006-282T17:00:07","000T00:15:00","2006-10-09","RADAR","Prime","Titan","T19INALT",null,"T19 Inbound Altimetry","Collect altimetry data while maintaining nadir pointing."]
["2006-282T18:00:07","000T01:30:00","2006-10-09","RPWS","Non-SPASS","Titan","TIINTRMED","Titan magnetosphere interaction","Titan Interaction - Intermediate","Study the interaction of the magnetosphere with Titan at intermediate distances for evidence of ion pickup, radio emissions, density profiles, and the general wave environment.  Prefer Langmuir probe within 90 degrees of plasma ram."]
["2006-283T03:30:07","000T05:51:00","2006-10-10","VIMS","SPASS Rider","Titan","COMPMAP","Composition map","VIMS_ride_CIRS","Ridealong with CIRS map. Long integration with focal plane 1."]
["2006-284T10:47:30","000T00:49:59","2006-10-11","CDA","Non-SPASS","DustRAM direction","0838SURVY","Dust survey","Dust survey 37.50<lat< 40.00 deg 7.70... 8.30 Rs v","Dust survey$ 832.44965$ 832.48437$ 8.287 to 8.085 Rs lat:-38.900 to -39.973 deg ring-alt: 313945. to 313371.km 000OF006 no ADJ: 15 was:2006-284T10:55:13...2006-284T11:29:46,pointing=CDA to Kepler RAM,rate=100,dataVolume=0.286"]
["2006-284T23:00:01","000T01:05:03","2006-10-11","MIMI","SPASS Rider","Saturn","MAGDYN","MAPS magnetosphere dynamics campaign","MAPS IM/DYN Campaign","Part of IM/DYN MIMI Campaign.   Image the dynamics of the inner magnetosphere in ENA with MIMI/INCA. With -Y pointed generally toward Saturn, corotation as close to the S/C -X, +/- Z plane as possible."]
["2006-285T03:38:00","000T01:07:01","2006-10-12","MIMI","SPASS Rider","DustRAM direction","INCADUST","MIMI INCA dust observation","MAPS RS Campaign","Part of RS MAPS Campaign.   Spacecraft must be pointed such that the dust ram is not entering the INCA FOV. Required to satisfy FR76C3. This means INCA boresight (in S/C X, Y plane, 9.5 deg toward +X from -Y) >70 deg from dust ram."]
["2006-286T07:00:00","000T02:30:00","2006-10-13","CIRS","Prime","rings(general)","TEMPU45MP","Thermal map","CIRS_030RI_TempU45MP","Afternoon radial scan of main rings to obtain thermal measurement of rings.  -Y to rings, Z perp to rings"]
["2006-287T07:50:00","000T01:45:00","2006-10-14","UVIS","SPASS Rider","RingA","VERTULMP","Unlit face radial scan observation",null,"UV spectral mapping of Saturn's rings."]
["2006-287T19:55:00","000T11:22:40","2006-10-14","CAPS","Non-SPASS","Saturn","BURST16K","16 kbps burst","Burst of 16kbps data","Burst of 16 kbps data (which gives uncollapsed ELS data)."]
["2006-290T18:40:00","000T16:30:00","2006-10-17","INMS","Non-SPASS","Saturn","PTOTM78","MAPS survey","MAPS Survey","MAPS magnetospheric survey."]
["2006-292T22:30:00","000T00:34:08","2006-10-19","CAPS","Non-SPASS","InstrumentCalibration","ELSCAL","CAPS Electron Spectrometer calibration","Calibration/Gain curve of ELS sensor","Calibration/gain curve of ELS sensor. 8 B cycles duration in 16 kbps. Data is in addition to 1000 bps from SWSKR."]
["2006-296T01:56:00","000T06:18:00","2006-10-23","RPWS","Non-SPASS","Other","MAGTAIL","MAPS magnetotail observation","MAPS MT,vert Campaign","Part of MT,vert MAPS Campaign.  Observe the vertical structure of Saturn's magnetotail on an inclined apoapsis"]
["2006-297T10:11:00","000T08:00:00","2006-10-24","CIRS","SPASS Rider","InstrumentCalibration","DSCAL1","Deep space calibration","CIRS Deep Space Calibration","Deep space obervations for calibration."]
["2006-297T19:54:56","000T18:03:11","2006-10-24","MAG","Non-SPASS","co-rotation","TINTERACT","MAPS TI/EE Campaign","MAG MAPS TI_EE Campaign","Investigate large-scale and distant aspects of the Titan interaction by observing during entire period around an encounter from 10 to 25 RS. (31TI (T20))"]
["2006-298T14:58:07","000T03:00:00","2006-10-25","MIMI","SPASS Rider","Titan","T20CLOSE",null,"MAPS 031TI(T20) Campaign","Part of 031TI(T20) MAPS Campaign.   Investigate micro-scale and near aspects of the Titan interaction by observing during about one hour period around an encounter. With -Y pointed toward Titan, when within 30 minutes of the targeted flyby, optimize secondary axis for corotation flow as close to the S/C -X, +/- Z plane as works with the other constraints on pointing. Also, measure Titan exosphere/magnetosphere interaction by imaging in ENA with INCA (when sun is not in INCA FOV)."]
["2006-298T20:28:07","000T03:00:00","2006-10-25","ISS","SPASS Rider","Titan","MIRLMBMAP","Mid infrared limb map","NGM/RCI","regional map"]
["2006-300T00:30:00","000T08:30:00","2006-10-27","CIRS","SPASS Rider","RingC","SHADLMP","Saturn ring shadow observation","CIRS_030RC_SHADLMP_SI"]
["2006-300T16:35:00","000T00:15:00","2006-10-27","CIRS","SPASS Rider","InstrumentCalibration","DEEPSPACE","Deep space calibration","Deep Space Cal","Deep space observation for calibration during turns"]
["2006-300T20:00:00","000T03:00:00","2006-10-27","ISS","Prime","rings(general)","RDHRCOMP","High resolution radial scan of ring system","High res radial scan of the main rings","HI RES RAD SCAN OF MAIN RINGS, OUT TO F RING, AT LONGITUDE OF HIGHEST RADIAL RESOLUTION."]
["2006-301T01:00:00","000T03:40:00","2006-10-28","MAG","Non-SPASS","co-rotation","IMVP5N","Inner Magnetosphere vertical profile","MAG MAPS IM_VP Campaign","Measure the vertical structure and dynamics of the inner magnetosphere on orbits nearly tangent to L-shells at a variety of local times and L-shells. (L~4.5-5 noon)"]
["2006-301T06:00:00","000T06:17:57","2006-10-28","INMS","Non-SPASS","Saturn","INMAGSURV","Observing neutral molecules in the inner magnetosphere","MAPS Survey","MAPS magnetospheric survey."]
["2006-302T22:12:00","000T10:15:00","2006-10-29","VIMS","SPASS Rider","Saturn","1X2WPH161","Photopolarimetry","Saturn ISS Hi-Phase Ridealong","Saturn ISS High-Phase ridealong.   64*64 images along with ISS frames.Assume four images per hour. Datavolume = 4*10 hrs*64*64*12*352 = 692 Mbits, or about 350 mbits compressed. Assume actually take 2/3 of the wavelengths.. Ask for 250 mbits (compressed).   9/11/06: Data volume reduced to 165 Mbits to accomodate DSN outage."]
["2006-304T06:57:00","000T01:30:00","2006-10-31","CIRS","SPASS Rider","InstrumentCalibration","STARCAL","Star calibration",null,"Deepspace rider with VIMS Star Calibration"]
["2006-305T21:27:00","000T03:03:00","2006-11-01","ISS","SPASS Rider","RingF","FMOVIE","F ring movie","F RING OBSERVATION RIDING ALONG WITH VIMS","F ring rider observation"]
["2006-307T00:20:45","001T00:00:00","2006-11-03","RPWS","Non-SPASS","InstrumentCalibration","PIM","Periodic Instrument maintenance","RPWS PIM","Perform RPWS PIM, Bias the Langmuir Probe to remove any contamination"]
["2006-309T05:12:00","000T02:00:00","2006-11-05","ISS","Prime","rings(general)","SHADSCANI","Saturn ring shadow observation","SEARCH FOR INCLINED RINGS AT SHADOW BDY","RADIAL SCAN FOLLOWING SHADOW BOUNDARY ON MAIN RINGS, BOTH ANSAE."]
["2006-310T20:30:00","000T01:30:00","2006-11-06","CIRS","SPASS Rider","InstrumentCalibration","LONG4CAL","Titan longitude study","CIRS_032IC_LONG4CAL001_RADAR","rider"]
["2006-311T23:00:00","000T02:30:00","2006-11-07","CIRS","SPASS Rider","Rhea","FP1FAZ0P5","CIRS FP1 phase coverage","FP1 phase coverage at 3.0 cm-1 resolution","VIMS rider observation of Rhea for high spectral resolution integration for composition, and for phase angle coverage.   Duration=02:30.  At start: AD=3.4 mrad, phase=76, LT=6.4,  (-41, 108);  at end:  AD=3.8, phase=69, LT=7.0,  (-51, 107).   CIRS: 96 RTI, shutter closed 00:20 to 00:25, and 02:15 to 02:20, blink.  Request 15 min of FP1 time."]
["2006-312T15:45:31","000T04:18:43","2006-11-08","CDA","Non-SPASS","DustRAM direction","0552DUST","Dust survey","Dust survey inside 8 Rs 52.47<lat< 52.94 deg 5.28.","Dust survey inside 8 Rs $ 860.65661 $ 860.83629 $ 6.636 to 5.282 Rs lat:-52.935 to -52.465 deg ring-alt: 319472. to 252681.km,pointing=CDA to Kepler RAM,rate=200,dataVolume=2.960"]
["2006-312T20:40:00","000T04:05:00","2006-11-08","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_SURVEY","Continuous low-rate magnetospheric survey"]
["2006-313T00:45:00","000T02:05:00","2006-11-09","MIMI","SPASS Rider","co-rotation","IMVP5N","Inner Magnetosphere vertical profile","MAPS IM/VP Campaign","Part of IM/VP MAPS Campaign.   Set up MIMI for Inner Magnetospheric Campaign vertical structure measurement at L=4.5-5, near 1200 LT; maximize pitch angle coverage. Corotation flow into -X, Z half-plane, B field in X, Z plane; or Rotate about Z. Measure the vertical structure and dynamics of the inner magnetosphere on orbits nearly tangent to L shells, at a variety of local times and L shells."]
["2006-313T18:00:00","000T02:10:00","2006-11-09","UVIS","Prime","Star","URGAMLUP","Stellar occultation","URSTAR","Instance of URSTAR."]
["2006-314T09:58:00","002T07:15:00","2006-11-10","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2006-316T00:43:00","000T07:00:00","2006-11-12","ISS","Prime","rings(general)","SHADBOUND","Ring shadow boundary","DIFFUSE RING SRCH/STRUCTURE VIA SHAD BDY OBS","FIVE FOOTPRINTS ALONG EVENING SHADOW BOUNDARY FROM ENCKE DIVISION OUT TO ORBIT OF MIMAS.  DO BOTSIMS IN SEVERAL COLORS.~ 30 MIN TOTAL FOOTPRINT TIME.  TOTAL TIME: ~ 7 HOURS WITH TURNS."]
["2006-319T07:59:00","000T09:00:00","2006-11-15","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2006-322T07:44:00","000T09:00:00","2006-11-18","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously during downlink periods.   No special pointing is required."]
["2006-322T17:15:00","000T10:00:00","2006-11-18","ISS","Prime","rings(general)","HPMRLFMOV","High phase ring movie","HI PHASE ANSA MOVIE OF CASSINI DIVISION","Lit face ansa movie of Cassini Division to study azimuthally variable structure in outer B ring and CD."]
["2006-324T00:42:58","000T03:56:27","2006-11-20","CDA","Non-SPASS","DustRAM direction","1026DUST","Dust survey","Dust survey outside 8 Rs 25.81<lat< 31.85 deg 10.4","Dust survey outside 8 Rs $ 872.02984 $ 872.19406 $ 11.801 to 10.401 Rs lat:-25.812 to -31.853 deg ring-alt: 309998. to 331145.km,pointing=CDA to Kepler RAM,rate=200,dataVolume=2.705"]
["2006-324T19:45:00","000T04:05:00","2006-11-20","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey"]
["2006-324T22:30:00","000T01:10:00","2006-11-20","UVIS","SPASS Rider","Mimas","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2006-325T13:30:00","000T02:00:00","2006-11-21","ISS","Prime","rings(general)","WNHIEL1","Ring photometry","Campaign to study ring photometry","Multi-color WAC mosaic of half of the rings at high elevation unlit face."]
["2006-326T22:00:00","000T03:00:00","2006-11-22","CIRS","SPASS Rider","rings(general)","SHADULHP","Saturn ring shadow observation","CIRS_033RI_SHADULHP_SI"]
["2006-328T16:30:00","003T23:46:00","2006-11-24","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_SURVEY","Continuous low-rate magnetospheric survey"]
["2006-330T22:23:57","001T17:53:39","2006-11-26","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2006-333T07:16:00","000T09:00:00","2006-11-29","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting H data at a low rate continuously.  No special pointing is  required."]
["2006-334T20:00:00","000T02:00:00","2006-11-30","CIRS","Prime","Rhea","ORS",null,"FP3 Disk scan, FP1 stare, FP3 (ORS) stare of Rhea","FP1, FP3, ORS observation of Rhea for phase angle coverage. Phase=147, Local time=1.7, sub S/C=(-6, 200), AD=2.34 mrad.  Turn from waypoint (8.3 degrees from Saturn, est. 6 min turn); 1) single FP3 scan centered on disk of length 4.35 mrad at 4 microrad/sec (4x Nyquist) (00:30).  CIRS at 15.5 cm-1 resolution (4.875 sec/scan, 39 RTI); blink;  first 5 min with shutter closed; 2)  FP1 to Rhea; stare 00:40 (shutter closed last 5 min); 3) FP3 to disk center; stare 00:40 for ORS; 4) return to waypoint (00:10, shutter closed final 5 min; 13.3 degrees to Saturn, est 7 min turn)."]
["2006-335T16:50:39","000T04:23:14","2006-12-01","CDA","Non-SPASS","DustRAM direction","1318DUST","Dust survey","Dust survey outside 8 Rs 18.27<lat< 23.10 deg 12.5","Dust survey outside 8 Rs $ 883.70184 $ 883.88465 $ 13.890 to 12.511 Rs lat:-18.273 to -23.101 deg ring-alt: 262748. to 296137.km,pointing=CDA to Kepler RAM,rate=200,dataVolume=3.012"]
["2006-336T04:06:32","000T04:24:28","2006-12-02","CDA","Non-SPASS","DustRAM direction","0833DUST","Dust survey","Dust survey outside 8 Rs 33.25<lat< 44.97 deg 7.97","Dust survey outside 8 Rs $ 884.17121 $ 884.41093 $ 10.114 to 7.969 Rs lat:-33.247 to -44.974 deg ring-alt: 334520. to 339792.km,pointing=CDA to Kepler RAM,rate=200,dataVolume=3.950"]
["2006-336T12:00:00","000T02:20:00","2006-12-02","VIMS","SPASS Rider","Star","ALPAUROCC","Alpha Aur occultation","ALP AUR Stellar Occultation SI","ISS Support Imaging:  Time is a place holder until PDT designs are done."]
["2006-336T22:25:00","000T03:40:00","2006-12-02","INMS","Non-SPASS","co-rotation","IMVP5N","Inner Magnetosphere vertical profile","MAPS IM/VP Campaign","Part of IM/VP MAPS Campaign.   Measure the vertical structure and dynamics of the inner magnetosphere on orbits nearly tangent to L shells, at a variety of local times and L shells"]
["2006-337T01:50:00","000T04:35:01","2006-12-03","CDA","Non-SPASS","DustRAM direction","0630SURIN","Dust survey","Dust survey inside 8 Rs 30.00<lat< 32.50 deg 6.20.","Dust survey inside 8 Rs$ 885.23959$ 885.26737$ 6.457 to 6.636 Rs lat: 30.162 to 32.292 deg ring-alt: 195742. to 213889.km 004OF006 no ADJ: 9 was:2006-337T05:49:54...2006-337T06:20:08,pointing=CDA to Kepler RAM,rate=200,dataVolume=0.457"]
["2006-337T17:00:00","000T04:00:00","2006-12-03","CIRS","SPASS Rider","rings(general)","SHADULMP","Saturn ring shadow observation","CIRS_033RI_SHADULMP_SI"]
["2006-339T06:47:00","000T09:00:00","2006-12-05","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting H data at a low rate continuously.  No special pointing is  required."]
["2006-340T16:00:00","002T05:07:04","2006-12-06","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2006-341T17:45:00","000T12:00:00","2006-12-07","CDA","SPASS Rider","Other","DECON","Decontamination","Decontamination","CDA boresight off-sun, no resources (Watts, bps), resources covered by other request"]
["2006-344T06:32:00","000T09:00:00","2006-12-10","CDA","SPASS Rider","DustRAM direction","DATART","Data volume adjustment","DataVolume"]
["2006-345T14:32:00","000T13:09:31","2006-12-11","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_SURVEY","Continuous low-rate magnetospheric survey"]
["2006-346T02:41:31","000T01:30:00","2006-12-12","CIRS","Prime","Titan","MIRLMBINT","Mid infrared limb integration","CIRS_035TI_MIRLIMBINT_2","Obtain information on trace constituents in Titan's stratosphere.  Integrate on limb at two positions  POINTING: -y to Titan, z within 30 degrees of normal to limb.  Substitute: T19out."]
["2006-346T10:41:31","000T02:00:00","2006-12-12","CAPS","SPASS Rider","Titan","T21CLOSE",null,"MAPS 035TI(T21) Campaign","Part of 035TI(T21) MAPS Campaign.  Observations of Titan's interaction with Saturn's magnetosphere"]
["2006-347T02:21:00","000T08:00:00","2006-12-13","CIRS","SPASS Rider","InstrumentCalibration","DSCAL06","Deep space calibration","CIRS Deep Space Calibration","Deep space obervations for calibration."]
["2006-347T12:48:00","000T09:30:00","2006-12-13","ISS","SPASS Rider","Saturn","CYLMAP","Saturn cylindrical map","Saturn CYLMAP rider","Saturn rider to VIMS observation"]
["2006-348T17:15:00","000T10:15:00","2006-12-14","CIRS","SPASS Rider","rings(general)","AZSCNLOPH","Azimuthal ring scan","CIRS_035RI_AZSCNLOPH_ISS","ride with ISS"]
["2006-349T05:11:05","000T08:13:59","2006-12-15","INMS","Non-SPASS","co-rotation","IMVP9N","Inner Magnetosphere vertical profile","MAPS IM/VP Campaign","Part of IM/VP MAPS Campaign.   Measure the vertical structure and dynamics of the inner magnetosphere on orbits nearly tangent to L shells, at a variety of local times and L shells"]
["2006-349T17:15:00","000T08:00:00","2006-12-15","UVIS","SPASS Rider","rings(general)","SUBMU20MP","Ring radial scan",null,"UV spectral mapping of Saturn's rings."]
["2006-350T20:30:00","000T04:50:00","2006-12-16","ISS","SPASS Rider","Star","URKAPCEN","Stellar ring occultation","Stellar Occultation by Saturn NAC Rider","NAC high resolution limb images during star occ"]
["2006-351T15:30:00","000T07:00:00","2006-12-17","VIMS","Prime","rings(general)","LATPHASE","Latitude phase coverage","latitude-phase coverage: 3x1 mosaic on each ansa","Orbits = 026-064, Cube Size (X,Z) = 64*64,  Time per SC pointing (mins) = 60, Number of SC pointings = 6,  Time of observation (hours) = 6.0,  Desc = Obtain 3x1 mosaic on each ring ansa on unlit face, or at high phase angle.  Distance 20 R_S. unlit side 3x1 mosaic each ansa"]
["2006-353T18:18:00","000T07:00:00","2006-12-19","RADAR","Prime","Other","SRCRADCAL","RADAR microwave source radiometric calibration","Radiometric Calibration Using Microwave Sources, S","Scan the Sun, Saturn, and microwave sources while collecting radiometry data."]
["2006-355T14:49:00","001T08:36:31","2006-12-21","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey."]
["2006-359T14:34:00","000T14:45:00","2006-12-25","CDA","SPASS Rider","DustRAM direction","DATART","Data volume adjustment","DataVolume"]
["2006-361T15:04:22","000T05:01:00","2006-12-27","CIRS","Prime","Titan","MIDIRTMAP","Mid infrared thermal map","CIRS_036TI_MIDIRTEMPMAP01","obtain information on the thermal structure of Titan's stratosphere.  Slew across disk at 4 microrad/s.  POINTING: -y to Titan, x to pole.  Substitutes:  T20in, T21in."]
["2006-361T20:05:22","000T05:30:00","2006-12-27","UVIS","SPASS Rider","Titan","FIRNADCMP","Far infrared nadir composition map","UVIS Rider to CIRS Far Nadir CMP","UVIS Rider to CIRS Far-IR Nadir CMP"]
["2006-362T11:00:13","000T01:00:00","2006-12-28","CAPS","SPASS Rider","Titan","T22OUTBND",null,"MAPS 036TI(T22) Campaign","Part of 036TI(T22) MAPS Campaign.  Outbound approach observations and context for the interaction between Titan and Saturn's magnetosphere"]
["2006-362T21:49:00","000T09:00:00","2006-12-28","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2006-364T04:30:00","000T00:30:00","2006-12-30","CIRS","SPASS Rider","InstrumentCalibration","DEEPSPACE","Deep space calibration","Deep Space Cal","Deep space observation for calibration during turns"]
["2006-364T18:30:00","000T01:00:00","2006-12-30","CIRS","Prime","rings(general)","TEMPL57LP","Thermal map","CIRS_036RI_TempL57LP","Afternoon radial scan of main rings to obtain thermal measurement of rings.  -Y to rings, Z perp to rings"]
["2006-365T05:05:00","000T08:10:00","2006-12-31","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_SURVEY","Continuous low-rate magnetospheric survey"]
["2006-365T14:30:00","000T00:30:00","2006-12-31","UVIS","SPASS Rider","Saturn","FEATRACK","Imaging selected lattitudes at a range of emission angles as the planet rotates","UVIS Rider to VIMS FEATRACK","UVIS Rider to VIMS FEATRACK"]
["2007-001T02:00:00","000T02:30:00","2007-01-01","UVIS","SPASS Rider","rings(general)","TEMPU05LP","Thermal map",null,"UV spectral mapping of Saturn's rings."]
["2007-002T00:30:00","000T00:34:08","2007-01-02","CAPS","Non-SPASS","InstrumentCalibration","ELSCAL","CAPS Electron Spectrometer calibration","Calibration/Gain curve of ELS sensor","Calibration/gain curve of ELS sensor. 8 B cycles duration in 16 kbps. Data is in addition to 1000 bps from SWSKR."]
["2007-003T14:10:00","000T04:10:00","2007-01-03","ISS","Prime","Saturn","NALGTNG02","Lightning/aurora search","Northern hemisphere NAC lightning/aurora search","Eight 2x4 NAC mosaics in dark northern hemisphere. One filter (HAL). Acquire a mosaic in same geometry every 30 minutes for a total of eight."]
["2007-004T04:20:00","000T00:30:00","2007-01-04","CIRS","SPASS Rider","InstrumentCalibration","DEEPSPACE","Deep space calibration","Deep Space Cal","Deep space observation for calibration during turns"]
["2007-008T04:34:53","005T02:03:38","2007-01-08","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey"]
["2007-010T04:20:00","000T09:00:00","2007-01-10","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2007-010T15:50:00","000T09:00:00","2007-01-10","UVIS","SPASS Rider","rings(general)","AZDKMRHPH","Azimuthal ring scan"]
["2007-012T16:38:31","000T01:00:00","2007-01-12","UVIS","SPASS Rider","Titan","NIGHTNAC","ISS lightning / aurora observation","UVIS Rider to ISS NIGHTNAC","Ride along with ISS NightNAC"]
["2007-013T06:38:31","000T01:00:00","2007-01-13","MIMI","SPASS Rider","Titan","T23INBND",null,"MAPS 037TI(T23) Campaign","Part of 037TI(T23) MAPS Campaign.   Investigate micro-scale and near aspects of the Titan interaction by observing during about one hour period around an encounter. With -Y pointed toward Titan, when within 30 minutes of the targeted flyby, optimize secondary axis for corotation flow as close to the S/C -X, +/- Z plane as works with the other constraints on pointing. Also, measure Titan exosphere/magnetosphere interaction by imaging in ENA with INCA (when sun is not in INCA FOV)."]
["2007-013T08:45:31","000T00:08:00","2007-01-13","RADAR","Prime","Titan","T23OTLSAR",null,"T23 Outbound Low Resolution SAR Imaging","Outbound low resolution SAR imaging on T23 flyby"]
["2007-013T19:38:31","000T02:00:00","2007-01-13","ISS","Prime","Titan","MONITORNA","Monitoring of surface and atmosphere","NMA (NAC Monitoring of Surface and Atmosphere)","monitoring for surface/atmosphere changes; attempt to see surface color variations; monitor limb hazes, 1-3 km/px"]
["2007-015T04:30:00","000T01:06:00","2007-01-15","RPWS","Non-SPASS","Saturn","INSURVEY","Inner magnetosphere survey","RPWS Inner Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2007-015T13:10:00","000T03:20:00","2007-01-15","UVIS","SPASS Rider","Star","URDELPER","Del Per occultation","URSTAR","Adding precise timing for support imaging based on new trajectory. NAC and WAC images at the following times: 2007-015T15:18:33 2007-015T14:10:51 2007-015T13:36:31 2007-015T13:25:22"]
["2007-016T06:00:00","000T02:00:00","2007-01-16","UVIS","SPASS Rider","RingB","SPOKE","Ring spoke movie",null,"UV spectral mapping of Saturn's rings."]
["2007-017T10:05:15","000T01:59:59","2007-01-17","CDA","Non-SPASS","DustRAM direction","1415SUOUT","Dust survey","Dust survey outside 8 Rs 15.00<lat< 17.50 deg 13.7","Dust survey outside 8 Rs$ 930.42031$ 930.50364$ 13.706 to 13.804 Rs lat:-16.680 to -15.077 deg ring-alt: 237329. to 216618.km 005OF011 no ADJ: 59 was:2007-017T10:35:01...2007-017T11:35:29,pointing=CDA to Kepler RAM,rate=200,dataVolume=1.373"]
["2007-018T03:45:05","003T12:14:56","2007-01-18","MIMI","SPASS Rider","Saturn","MAGDYN","MAPS magnetosphere dynamics campaign","MAPS IM/DYN Campaign","Part of IM/DYN MAPS Campaign.   Image the dynamics of the inner magnetosphere in ENA with MIMI/INCA. With -Y pointed toward Saturn, corotation as close to the S/C -X, +/- Z plane as possible."]
["2007-019T14:20:00","000T07:00:00","2007-01-19","VIMS","SPASS Rider","rings(general)","PHOTDRK","Ring system photometry","latitude-phase coverage: 3x1 mosaic on each ansa","24 frame WAC mosaic. Take 2 VIMS 24*24 cubes at each WAC piointing, tau_IR = 160 & 640 msec."]
["2007-020T03:51:00","000T09:00:00","2007-01-20","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2007-021T03:36:00","000T09:00:00","2007-01-21","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2007-024T12:25:00","000T06:00:00","2007-01-24","VIMS","Prime","rings(general)","APOMOSAIC","Apoapsis mosaic","APOAPSE MOSAIC","Orbits = 026-074, Cube Size (X,Z) = 64*64, Time per SC pointing (mins) = 24, Number of SC pointings = 4-30, Time of observation (hours) = 1.5-11, Volume (Mbits) = 69-519  Mosaic of entire ring system near apoapse. Unlit face. Various mosaic sizes (4x1 - 6x5)., Desc =  5x6. Second half of APOMOSAIC; first half is at 2007-021T15:30."]
["2007-025T14:00:00","000T10:00:00","2007-01-25","INMS","Non-SPASS","Saturn","SURVEYCS","MAPS survey","MAPS Survey","MAPS magnetospheric survey."]
["2007-027T12:51:00","000T03:45:00","2007-01-27","UVIS","SPASS Rider","Star","UREPSPSA","Eps PsA ring occultation","URSTAR","Adding precise timing for support imaging based on new trajectory. NAC and WAC images at the following times: 2007-027T14:40:01 2007-027T16:29:21 2007-027T12:59:40"]
["2007-028T11:32:52","000T00:39:08","2007-01-28","CAPS","Non-SPASS","Other","BURST4K","4 kbps burst","Burst of 4kbps data","Burst of 16 kbps data (which gives uncollapsed ELS data)."]
["2007-029T06:15:55","000T02:00:00","2007-01-29","INMS","Non-SPASS","Titan","T24CLOSE",null,"MAPS TOST Campaign","Part of the MAPS/TOST Campaign. Determine atmospheric and ionospheric composition and thermal structure."]
["2007-029T08:15:55","000T11:00:00","2007-01-29","INMS","Non-SPASS","Titan","T24OUTBD",null,"MAPS TOST Campaign","Part of the MAPS/TOST Campaign. Determine atmospheric and ionospheric composition and thermal structure."]
["2007-030T04:00:00","000T08:00:00","2007-01-30","CIRS","SPASS Rider","InstrumentCalibration","DSCAL07","Deep space calibration","Deep Space Calibration","Deep space obervations for calibration."]
["2007-031T22:20:00","000T02:57:00","2007-01-31","CIRS","Prime","Saturn","REGMAPB","Regional map","CIRS_038SA_REGMAPB14","Produce a regional map of atmospheric  composition at about 12Rs by building a raster  by scanning North/South over a region 16 [32]  milliradians on a side at 13 [26] microrad/s. POINTING: -y to Saturn, +x to pole"]
["2007-032T13:22:00","000T06:00:00","2007-02-01","CIRS","SPASS Rider","rings(general)","SPKHRLPF","Ring spoke campaign","CIRS_038RI_SPKHRLPF_ISS","ride with ISS, FP1 and FP3 only"]
["2007-034T04:22:00","001T01:15:00","2007-02-03","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2007-035T17:52:00","000T03:00:00","2007-02-04","RADAR","SPASS Rider","Other","WARM4RING","RADAR warmup","Warm Up for the Ring Observation","Warmup for the Ring observation on rev 38."]
["2007-036T22:07:00","000T03:30:00","2007-02-05","ISS","Prime","Saturn","HILTATMAF","Saturn high latitude photopolarimetry","High Lat Photopol","Saturn High latitude photopolarimetry"]
["2007-038T11:37:00","000T14:44:00","2007-02-07","RPWS","Non-SPASS","Saturn","HIRATE","High rate mode","MAPS MB,A Campaign","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2007-038T21:45:00","000T00:20:00","2007-02-07","ISS","Prime","Saturn","HILTATMBA","Saturn high latitude photopolarimetry","High Lat Photopol","Saturn High latitude photopolarimetry"]
["2007-039T14:20:00","000T00:40:00","2007-02-08","UVIS","SPASS Rider","Saturn","GLOAURTRI","Saturn global aurora map","Rider to VIMS_038SA_GLOAURTRI","adding UVIS auroral riders to VIMS auroral observations as part of the recently approved HST/Cassini International Heliophysical Year campaign."]
["2007-039T16:00:00","000T00:20:00","2007-02-08","ISS","Prime","Saturn","HILTATMBB","Saturn high latitude photopolarimetry","High Lat Photopol","Saturn High latitude photopolarimetry"]
["2007-040T12:00:00","000T00:34:08","2007-02-09","CAPS","Non-SPASS","InstrumentCalibration","ELSCAL","CAPS Electron Spectrometer calibration","Calibration/Gain curve of ELS sensor","Calibration/gain curve of ELS sensor. 8 B cycles duration in 16 kbps. Data is in addition to 1000 bps from SWSKR."]
["2007-040T18:30:00","000T06:15:00","2007-02-09","UVIS","SPASS Rider","rings(general)","SHADBOUND","Ring shadow boundary","ISS SHADBOUND RIDER"]
["2007-041T11:22:00","000T14:45:00","2007-02-10","VIMS","Prime","RingF","FMOVIE","F ring movie","TBD","TBD"]
["2007-045T09:45:00","000T00:25:00","2007-02-14","CIRS","SPASS Rider","InstrumentCalibration","DEEPSPACE","Deep space calibration",null,"rider"]
["2007-046T00:10:00","000T01:20:00","2007-02-15","VIMS","SPASS Rider","Iapetus","LOWPHASED","Low phase imaging","Iapetus","12x12 hi/hi 80ms, 160ms, 640 ms (3.6 min/cycle) repeat 18 times"]
["2007-046T12:55:00","000T04:00:00","2007-02-15","VIMS","Prime","rings(general)","LATPHASE","Latitude phase coverage","latitude-phase coverage: 3x1 mosaic on each ansa","Orbits = 026-064, Cube Size (X,Z) = 64*64, Time per SC pointing (mins) = 60, Number of SC pointings = 3, Time of observation (hours) = 3.0, Volume (Mbits) = 208, Desc = Obtain 3x1 mosaic on each ring ansa on unlit face, or at high phase angle. Distance 20 R_S.  Left ansa only."]
["2007-046T23:30:00","000T02:00:00","2007-02-15","RADAR","Prime","Hyperion","SCATTRADL","RADAR Scatterometry / Radiometry","Scatterometry/Radiometry of Hyperion.","Point -Z axis at target and execute raster scan(s) centered on target. Obtain simultaneous scatterometry and radiometry."]
["2007-048T10:52:00","000T03:27:39","2007-02-17","CDA","Non-SPASS","DustRAM direction","1823SUOUT","Dust survey","Dust survey outside 8 Rs 22.50<lat< 25.00 deg 17.7","Dust survey outside 8 Rs$ 961.49298$ 961.59698$ 18.184 to 17.959 Rs lat:-22.565 to -25.000 deg ring-alt: 420970. to 457896.km 003OF006 no ADJ: 0 was:...,pointing=CDA to Kepler RAM,rate=200,dataVolume=1.713"]
["2007-049T15:55:00","000T01:35:00","2007-02-18","CIRS","SPASS Rider","rings(general)","SHADLMP","Saturn ring shadow observation","CIRS_039RI_SHADLMP005_SI","rider"]
["2007-050T20:40:00","000T04:30:00","2007-02-19","CIRS","SPASS Rider","rings(general)","PHOTLIT","Ring system photometry",null,"rider"]
["2007-051T10:37:00","000T00:23:00","2007-02-20","CIRS","SPASS Rider","InstrumentCalibration","DEEPSPACE","Deep space calibration",null,"rider"]
["2007-052T11:10:38","000T03:30:50","2007-02-21","CDA","Non-SPASS","DustRAM direction","1812DUST","Dust survey","Dust survey outside 8 Rs 11.57<lat< 14.99 deg 18.1","Dust survey outside 8 Rs $ 965.46572 $ 965.61215 $ 18.111 to 18.432 Rs lat:-14.994 to -11.568 deg ring-alt: 282682. to 222986.km,pointing=CDA to Kepler RAM,rate=200,dataVolume=2.412"]
["2007-052T17:12:24","000T01:00:00","2007-02-21","ISS","Prime","Titan","PHOTOMWAC","Photometry map","WPH (WAC Photometry)","particle properties, vertical distributions ~6 km/px.  0.6 Mbit/frame with 2x2 summing. special S/C orientation requested."]
["2007-053T08:23:24","000T03:25:00","2007-02-22","ISS","Prime","Titan","GLOBMAP","Global coverage mapping","NGM (NAC Global Map)","global map"]
["2007-053T17:12:24","000T07:15:00","2007-02-22","CIRS","Prime","Titan","MIDIRTMAP","Mid infrared thermal map",null,"Obtain information on the thermal structure of Titan's stratosphere. Slew across disk at 4 microrad/s."]
["2007-056T02:15:00","000T04:00:00","2007-02-25","CIRS","SPASS Rider","InstrumentCalibration","DSCAL07","Deep space calibration","Deep Space Calibration","Deep space obervations for calibration."]
["2007-056T11:22:00","000T03:00:00","2007-02-25","UVIS","SPASS Rider","Hyperion","ICYLON","Icy satellite longitudinal coverage"]
["2007-058T07:50:38","003T02:00:22","2007-02-27","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2007-061T11:00:01","003T05:10:00","2007-03-02","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SURVEY Campaign","Part of SURVEY MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2007-064T01:21:40","000T22:17:37","2007-03-05","CDA","SPASS Rider","DustRAM direction","1503DUST","Dust survey","Dust survey outside 8 Rs 3.08<lat< 22.48 deg 14.65","Dust survey outside 8 Rs $ 977.05672 $ 977.98563 $ 17.837 to 14.653 Rs lat: 22.476 to -3.075 deg ring-alt: 411403. to 47421.km,pointing=CDA to Kepler RAM,rate=200,dataVolume=15.307"]
["2007-064T14:36:00","000T02:15:00","2007-03-05","ISS","Prime","rings(general)","HIPHAMOVD","High phase observation","Ansa movie of the D ring at high phase","Brief ansa movie of D ring at very high phase"]
["2007-065T14:00:00","000T01:00:00","2007-03-06","ISS","Prime","Saturn","LIMBSCAN","Limb scan","Saturn Limb Scan","Rings behind Saturn nightside limb"]
["2007-066T13:36:00","000T08:15:00","2007-03-07","CIRS","SPASS Rider","Saturn","POLEMAP","Saturn polar map","CIRS_040SA_AURMAP","Determine upper troposphere and tropopause temperature with spatial resolution of about two degrees of latitude and longitude  POINTING: -y to Saturn, z to pole"]
["2007-067T09:41:00","000T02:40:00","2007-03-08","CIRS","Prime","rings(general)","TEMPL40LP","Thermal map","CIRS_040RI_TempL40LP","Afternoon radial scan of main rings to obtain thermal measurement of rings.  -Y to rings, Z perp to rings"]
["2007-068T09:47:00","000T03:27:22","2007-03-09","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey."]
["2007-068T20:49:00","000T02:45:00","2007-03-09","CIRS","SPASS Rider","Titan","FIRNADMAP","Far infrared nadir composition map","ISS_PHOT_1x1","ISS WAC support imaging, 2 images per integration (3 integrations total = 6 frames, 0.5 Mb/frame)"]
["2007-069T02:49:00","000T01:00:00","2007-03-10","MIMI","SPASS Rider","Titan","T26OUTBND",null,"MAPS 040TI(T26) Campaign","Part of 040TI(T26) MAPS Campaign.   Investigate micro-scale and near aspects of the Titan interaction by observing during about one hour period around an encounter. With -Y pointed toward Titan, when within 30 minutes of the targeted flyby, optimize secondary axis for corotation flow as close to the S/C -X, +/- Z plane as works with the other constraints on pointing. Also, measure Titan exosphere/magnetosphere interaction by imaging in ENA with INCA (when sun is not in INCA FOV)."]
["2007-069T03:35:00","000T00:37:00","2007-03-10","CIRS","Prime","Titan","FIRLMBINT","Vertical limb sounding",null,"Vertical sounding of stratospheric compounds on Titan, including H2O. Integrations at 2 locations on the limb displaced vertically."]
["2007-069T12:49:00","000T02:00:00","2007-03-10","VIMS","SPASS Rider","Titan","MOSAIC","Mosaic","Global_mosaic_VIMS","Ridealong global mosiac  with ISS. Template D."]
["2007-070T10:00:00","004T02:51:44","2007-03-11","MIMI","SPASS Rider","Sun","MAGBOUND","MAPS magnetosphere boundary campaign","MAPS MB/C Campaign","Part of MB/C MAPS Campaign.   Observe afternoon magnetospheric boundaries at 35 RS apoapsis distance and a range of inclinations. Set up MIMI for magnetospheric boundaries campaign Pointing: -X to sun and/or corotation, internal B in X, Z plane; or spin about Z."]
["2007-071T10:06:00","000T12:00:00","2007-03-12","UVIS","SPASS Rider","Saturn","GLOAURTRI","Saturn global aurora map"]
["2007-073T22:45:00","000T00:30:00","2007-03-14","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 014 TH OBS","Images of small satellites for orbit determination purposes. One NAC (CL1,CL2) of each target. This observation has 5 targets: [PN-JA-PA-PM-AT (610, 615, 616, 617, 618)]"]
["2007-075T10:00:00","000T05:15:00","2007-03-16","CAPS","Prime","co-rotation","MAGBNDPTG","MAPS magnetosphere boundary campaign","CAPS Control Pointing during MAG BND Campaign","Part of  MB,C  MAPS Campaign.  Observe dusk-side magnetospheric boundaries at a variety of latitudes"]
["2007-077T17:00:00","000T06:00:00","2007-03-18","UVIS","SPASS Rider","rings(general)","SHADBOUND","Ring shadow boundary"]
["2007-078T08:35:00","000T00:30:00","2007-03-19","CIRS","SPASS Rider","InstrumentCalibration","DEEPSPACE","Deep space calibration",null,"rider"]
["2007-079T08:50:00","000T06:25:00","2007-03-20","UVIS","SPASS Rider","Star","URBETSGR","Stellar occultation","Support Imaging","Adding precise timing for support imaging based on new trajectory. NAC and WAC images at the following times: 2007-079T09:11:38 2007-079T13:58:10 2007-079T14:47:07"]
["2007-081T05:00:00","000T01:59:59","2007-03-22","CDA","Non-SPASS","DustRAM direction","1415SUOUT","Dust survey","Dust survey outside 8 Rs 15.00<lat< 17.50 deg 13.7","Dust survey outside 8 Rs$ 994.20833$ 994.29167$ 13.768 to 13.701 Rs lat: 17.444 to 16.972 deg ring-alt: 249005. to 241283.km 006OF011 no ADJ: 99 was:2007-081T05:49:54...2007-081T06:10:06,pointing=CDA to Kepler RAM,rate=200,dataVolume=1.373"]
["2007-081T23:30:00","000T00:30:00","2007-03-22","CIRS","SPASS Rider","InstrumentCalibration","DEEPSPACE","Deep space calibration",null,"rider"]
["2007-082T11:40:00","000T03:00:00","2007-03-23","CIRS","SPASS Rider","rings(general)","URDELPER","Del Per occultation",null,"rider"]
["2007-082T16:20:00","000T04:00:00","2007-03-23","VIMS","SPASS Rider","Star","ALPAUROCC","Alpha Aur occultation","ALPAUR Occultation SI","ISS Support Imaging:  Need two Images: 1. First image within 3 minutes after arriving on target 2. Second image within 3 minutes before leaving target.  ISS parameters should be the same as we used before:  ISS_WAC image clear filter 2x2 on-chip summing mode slightly-lossy compression data vol = 0.5 Mbit/image"]
["2007-084T08:20:01","000T15:03:26","2007-03-25","MIMI","SPASS Rider","Titan","T27EXTINB",null,"MAPS TI/EE Campaign","Part of TI/EE MAPS Campaign.   Investigate large-scale and distant aspects of the Titan interaction by observing during entire period around an encounter from 10 to 25 RS. With -Y pointed toward Titan, when far from Titan (more than 30 minutes to either side of a targeted flyby), measure Titan exosphere/magnetosphere interaction by imaging in ENA with INCA (when sun is not in INCA FOV). Also, optimize secondary axis for corotation flow as close to the S/C -X, +/- Z plane as works with the other constraints on pointing."]
["2007-084T11:23:27","000T03:00:00","2007-03-25","UVIS","SPASS Rider","Titan","FIRNADCMP","Far infrared nadir composition map","UVIS Rider to CIRS FIRNADCMP001","UVIS Rider to CIRS FIRNADCMP"]
["2007-084T23:23:27","000T02:00:00","2007-03-25","CAPS","SPASS Rider","Titan","T27CLOSE",null,"MAPS 041TI(T27) Campaign","Part of 041TI(T27) MAPS Campaign.  Observations of Titan's interaction with Saturn's magnetosphere"]
["2007-085T03:23:27","000T05:00:00","2007-03-26","ISS","SPASS Rider","Titan","EUVFUV","UVIS EUV / FUV imaging","RCI (Ridealong Context Imaging)","ISS on, max data rate = 182.784 kbps, number of frames and bits/frame are input parameters, data volume = number of frames x bits/frame, average data rate = data volume/duration."]
["2007-085T09:03:27","000T00:20:00","2007-03-26","ISS","Prime","Titan","PHOTOMWAC","Photometry map","WPH (WAC Photometry)","particle properties, vertical distributions ~6 km/px.  0.6 Mbit/frame with 2x2 summing. special S/C orientation requested."]
["2007-086T05:02:23","001T03:01:37","2007-03-27","INMS","Non-SPASS","Sun","MAGBOUND","MAPS magnetosphere boundary campaign","MAPS","Part of MB,C MAPS Campaign.  Observe afternoon magnetospheric boundaries at 35 RS apoapsis distance and a range of inclinations"]
["2007-088T05:40:00","000T06:15:00","2007-03-29","VIMS","SPASS Rider","Star","RHYAOCC","R Hya occultation","RHYOCC Occultation SI","ISS Support Imaging:  Need two Images: 1. First image within 3 minutes after arriving on target 2. Second image within 3 minutes before leaving target.  ISS parameters should be the same as we used before:  ISS_WAC image clear filter 2x2 on-chip summing mode slightly-lossy compression data vol = 0.5 Mbit/image"]
["2007-089T23:35:00","000T08:00:00","2007-03-30","CIRS","SPASS Rider","InstrumentCalibration","DSCAL07","Deep space calibration","Deep Space Calibration","Deep space obervations for calibration."]
["2007-091T07:49:00","000T05:20:00","2007-04-01","CAPS","Non-SPASS","Saturn","BURST16K","16 kbps burst","Burst of 16kbps data","Burst of 16 kbps data (which gives uncollapsed ELS data)."]
["2007-094T07:33:00","000T23:27:00","2007-04-04","INMS","Non-SPASS","Saturn","PTOTM102B","MAPS survey","MAPS Survey","MAPS magnetospheric survey."]
["2007-096T00:03:00","003T07:15:00","2007-04-06","CDA","Non-SPASS","Other","DRATESAP","Data volume adjustment","adjust datavolume for E-Ring measurements","E-Ring dust measurements"]
["2007-096T00:33:00","000T21:15:00","2007-04-06","VIMS","SPASS Rider","Saturn","NAURMOV","Saturn north pole movie","Saturn North Aurora Movie UVIS Ridealong","Saturn Global North Aurora Movie- Double Maps in ride-along to UVIS (Bob West design)"]
["2007-098T00:00:01","000T03:40:00","2007-04-08","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SURVEY Campaign","Part of SURVEY MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2007-098T10:30:00","000T04:00:00","2007-04-08","CIRS","SPASS Rider","rings(general)","RDMRSCNMP","Medium resolution radial scan of ring system",null,"rider"]
["2007-098T14:30:00","000T01:00:00","2007-04-08","ISS","SPASS Rider","Dione","DIONE","Dione","Dione limb topography and regional geodesy observa","Do 1x1 NAC (clr and color filters)."]
["2007-099T14:30:14","000T01:59:59","2007-04-09","CDA","SPASS Rider","DustRAM direction","1230SUOUT","Dust survey","Dust survey outside 8 Rs 30.00<lat< 32.50 deg 11.7","Dust survey outside 8 Rs$ 1012.6043$ 1012.6877$ 11.714 to 11.894 Rs lat:-31.215 to -30.205 deg ring-alt: 366258. to 360995.km 001OF002 no ADJ: 79 was:2007-099T15:10:06...2007-099T15:50:22,pointing=CDA to Kepler RAM,rate=200,dataVolume=1.373"]
["2007-100T07:03:01","000T13:54:59","2007-04-10","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SURVEY Campaign","Part of SURVEY MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2007-100T13:58:00","000T03:50:00","2007-04-10","UVIS","Prime","Titan","FIRNADCMP","Far infrared nadir composition map","FUVEUV-type mosaic of Titan","Essentially a mosaic across Titan, like EUVFUV."]
["2007-100T23:58:00","000T01:00:00","2007-04-10","ISS","SPASS Rider","Titan","HIRESNAC","High resolution map","RCI (Ridealong Context Imaging)","high-resolution imaging, 50-200 m/px, special targets, emission angles < 45 prefer IR-polarizer (phase 45-110)"]
["2007-101T02:58:00","000T01:00:00","2007-04-11","ISS","SPASS Rider","Titan","MIRLMBINT","Mid infrared limb integration","RCI (Ridealong Context Imaging)","ISS on, max data rate = 182.784 kbps, number of frames and bits/frame are input parameters, data volume = number of frames x bits/frame, average data rate = data volume/duration."]
["2007-102T17:00:00","000T08:00:00","2007-04-12","RSS","SPASS Rider","Earth","PIM","Periodic Instrument maintenance","RSS Ka-TWTA Maintenance","Ka-TWTA maintenance; Pointing = n/a; No DSN tracking required."]
["2007-103T20:30:00","000T00:30:00","2007-04-13","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 016 TH OBS","Turn to first satellite, take 1 NAC (CL1,CL2). Turn to second satellite take 1 NAC (CL1,CL2), repeat for up to 8 satellites if visible"]
["2007-105T08:17:00","000T06:30:00","2007-04-15","CIRS","Prime","rings(general)","FMONITOR","F ring monitor","Ring FP3/FP4 during F Ring monitoring","FP3/4 integration on the main rings"]
["2007-106T20:41:55","000T00:00:01","2007-04-16","MP","SPASS Note","Saturn","APOAPSE","Apoapse",null,"Apoapse  Per = 15.9 d, inc = 46.8 deg, r = 34.8 Rs, phase = 73 deg"]
["2007-108T19:02:00","000T02:00:00","2007-04-18","ISS","Prime","Iapetus","GLOBCOL",null,"Iapetus global color observation","Turn -Y to Iapetus; do 1x1 NAC mosaic clr + N24 + NP09; turn to WP"]
["2007-111T06:16:00","000T22:00:00","2007-04-21","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_SURVEY","Continuous low-rate magnetospheric survey"]
["2007-112T08:00:00","000T18:35:16","2007-04-22","INMS","Non-SPASS","Saturn","TTORUS","Titan Torus","Titan Torus Campaign Support using Sponge Bits","Memory read out request."]
["2007-113T00:20:13","000T02:09:33","2007-04-23","CDA","SPASS Rider","DustRAM direction","1845SUOUT","Dust survey","Dust survey outside 8 Rs 45.00<lat< 47.50 deg 17.7","Dust survey outside 8 Rs$ 1026.0140$ 1026.1040$ 18.297 to 17.721 Rs lat: 46.671 to 46.476 deg ring-alt: 802982. to 775175.km 002OF006 no ADJ: 0 was:...,pointing=CDA to Kepler RAM,rate=200,dataVolume=1.482"]
["2007-113T20:28:08","000T02:00:00","2007-04-23","CDA","SPASS Rider","DustRAM direction","1238SUOUT","Dust survey","Dust survey outside 8 Rs 37.50<lat< 40.00 deg 11.7","Dust survey outside 8 Rs$ 1026.8529$ 1026.9362$ 12.294 to 11.711 Rs lat: 39.814 to 38.269 deg ring-alt: 474898. to 437571.km 001OF004 no ADJ: 14 was:2007-113T20:35:34...2007-113T22:20:41,pointing=CDA to Kepler RAM,rate=200,dataVolume=1.373"]
["2007-114T14:49:57","000T00:25:03","2007-04-24","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SURVEY Campaign","Part of SURVEY MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2007-114T18:54:56","002T00:38:02","2007-04-24","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey"]
["2007-115T12:20:21","000T00:49:59","2007-04-25","CDA","Non-SPASS","DustRAM direction","1030SUOUT","Dust survey","Dust survey outside 8 Rs 30.00<lat< 32.50 deg 9.70","Dust survey outside 8 Rs$ 1028.5141$ 1028.5489$ 9.709 to 9.882 Rs lat:-30.921 to -30.072 deg ring-alt: 300995. to 298736.km 008OF009 no ADJ: 19 was:2007-115T12:30:14...2007-115T13:00:28,pointing=CDA to Kepler RAM,rate=200,dataVolume=0.572"]
["2007-116T12:32:58","000T04:00:00","2007-04-26","VIMS","Prime","Titan","MEDRESDRK","Medium resolution global mapping","Regional Map","Obtain a 2X2 mosaic of 64X64 images in two integration times if possible, the shot integration time should be double resolution. When Titan fills FOV, obtain one or two 64X64 images. Shot integration time could be double resolution."]
["2007-116T22:32:58","000T01:00:00","2007-04-26","MIMI","SPASS Rider","Titan","T29OUTBND",null,"MAPS 043TI(T29) Campaign","Part of 043TI(T29) MAPS Campaign.   Investigate micro-scale and near aspects of the Titan interaction by observing during about one hour period around an encounter. With -Y pointed toward Titan, when within 30 minutes of the targeted flyby, optimize secondary axis for corotation flow as close to the S/C -X, +/- Z plane as works with the other constraints on pointing. Also, measure Titan exosphere/magnetosphere interaction by imaging in ENA with INCA (when sun is not in INCA FOV)."]
["2007-116T23:32:58","000T20:37:08","2007-04-26","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SURVEY Campaign","Part of SURVEY MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2007-117T11:32:58","000T01:05:00","2007-04-27","VIMS","SPASS Rider","Titan","MIRTEMP","Mid infrared thermal map","Mid IR Temperature Map","Ridealong with CIRS Mid IR Temperature Map. Template A (Modified)"]
["2007-119T06:45:00","000T01:00:00","2007-04-29","ISS","Prime","Titan","1X1PT60","Photopolarimetry","Titan NAC Photopol 60 Phase","Titan NAC Photopol 60 Phase"]
["2007-119T19:15:00","000T01:00:00","2007-04-29","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 022 TH OBS","Turn to first satellite, take 1 NAC (CL1,CL2). Turn to second satellite take 1 NAC (CL1,CL2), repeat for up to 8 satellites if visible"]
["2007-124T06:00:00","000T00:30:00","2007-05-04","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 004 TH OBS","Turn to first satellite, take 1 NAC (CL1,CL2). Turn to second satellite take 1 NAC (CL1,CL2), repeat for up to 8 satellites if visible"]
["2007-124T23:00:00","000T02:00:00","2007-05-04","ISS","Prime","Star","MONITOR",null,"ISS Sensitivity monitor","Periodic standard star image to monitor ISS sensitivity"]
["2007-126T06:00:00","000T13:30:00","2007-05-06","UVIS","SPASS Rider","Janus","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2007-128T03:05:00","002T16:50:00","2007-05-08","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey"]
["2007-129T19:08:09","000T02:00:00","2007-05-09","CDA","Non-SPASS","DustRAM direction","1438SUOUT","Dust survey","Dust survey outside 8 Rs 37.50<lat< 40.00 deg 13.7","Dust survey outside 8 Rs$ 1042.7973$ 1042.8807$ 14.283 to 13.728 Rs lat: 39.013 to 38.926 deg ring-alt: 542427. to 520366.km 004OF011 no ADJ: 25 was:2007-129T19:20:41...2007-129T20:55:36,pointing=CDA to Kepler RAM,rate=200,dataVolume=1.373"]
["2007-130T15:55:50","000T14:00:00","2007-05-10","RPWS","Non-SPASS","Saturn","SEDDF","Saturn Electrical Discharge direction finding","SED Direction-finding","Perform direction-finding on SED to a) verify source in Saturn's atmosphere (or refute this and find source in rings), and b) if source is in atmosphere, use location to characterize the location of thunderstorms.  Need to do this inside 6 RS on at least half of the periapses inside of 6RS.  No pointing requirement"]
["2007-130T22:08:00","000T02:12:00","2007-05-10","CIRS","SPASS Rider","Saturn","LIMBINT","Limb integration","CIRS_044SA_LIMBINT SI","obtain stratospheric thermal structure by means of limb sounding in the mid-IR, latitude coverage.  POINTING: -y to Saturn, z to limb"]
["2007-131T04:05:48","000T14:35:23","2007-05-11","CDA","Non-SPASS","DustRAM direction","0516DUST","Dust survey","Dust survey outside 8 Rs 16.05<lat< 38.71 deg 5.32","Dust survey outside 8 Rs $ 1044.1707 $ 1044.7786 $ 5.320 to 11.358 Rs lat:-38.705 to -16.051 deg ring-alt: 200707. to 189458.km,pointing=CDA to Kepler RAM,rate=200,dataVolume=10.017"]
["2007-131T20:43:17","000T11:45:54","2007-05-11","CDA","Non-SPASS","DustRAM direction","1205DUST","Dust survey","Dust survey outside 8 Rs 5.43<lat< 14.02 deg 12.13","Dust survey outside 8 Rs $ 1044.8634 $ 1045.3536 $ 12.128 to 16.212 Rs lat:-14.018 to -5.433 deg ring-alt: 177227. to 92602.km,pointing=CDA to Kepler RAM,rate=200,dataVolume=8.078"]
["2007-132T19:53:58","000T00:09:00","2007-05-12","RADAR","Prime","Titan","T30INLSAR",null,"Inbound Low Resolution SAR of T30","Low resolution SAR imaging acquired during the inbound leg of the T30 flyby.  REU bits included."]
["2007-132T22:09:58","000T19:11:46","2007-05-12","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2007-133T10:09:58","000T01:19:00","2007-05-13","CIRS","Prime","Titan","MIDIRTMAP","Mid infrared thermal map",null,"Obtain information on the thermal structure of Titan's stratosphere. Slew across disk at 4 microrad/s."]
["2007-133T17:20:00","000T03:53:00","2007-05-13","RPWS","Non-SPASS","Sun","MAGBOUND","MAPS magnetosphere boundary campaign","MAPS MB,C Campaign","Part of MB,C MAPS Campaign.  Observe afternoon magnetospheric boundaries at 35 RS apoapsis distance and a range of inclinations"]
["2007-135T06:43:00","000T01:00:00","2007-05-15","ISS","Prime","Titan","1X1PHOT30","Photopolarimetry","Titan NAC Photopol 30 Phase","Titan NAC Photopol 30 Phase"]
["2007-137T05:15:00","000T05:05:00","2007-05-17","UVIS","SPASS Rider","rings(general)","APOMOSAIC","Apoapsis mosaic"]
["2007-140T05:36:58","000T22:50:02","2007-05-20","INMS","Non-SPASS","Sun","MAGBOUND","MAPS magnetosphere boundary campaign","MAPS","Part of MB,C MAPS Campaign.  Observe afternoon magnetospheric boundaries at 35 RS apoapsis distance and a range of inclinations"]
["2007-141T12:27:00","000T08:00:00","2007-05-21","CIRS","SPASS Rider","InstrumentCalibration","DSCAL07","Deep space calibration","CIRS_045IC_DSCAL07141_RIDER","Calibration rider.  Data Volume will be 115.2 Mb or less."]
["2007-143T04:12:00","001T00:00:00","2007-05-23","MAG","Non-SPASS","Sun","MAGBOUND","MAPS magnetosphere boundary campaign","MAG_MAPS_MB_C_Campaign","Observe_afternoon_magnetospheric_boundaries_at_35_RS_apoapsis_distance_and_a_range_of_inclinations."]
["2007-145T07:39:00","000T03:00:00","2007-05-25","VIMS","Prime","rings(general)","LATPHASE","Latitude phase coverage","latitude-phase coverage: 3x1 mosaic on each ansa","Orbits = 026-064, Cube Size (X,Z) = 64*64, Time per SC pointing (mins) = 60,  Number of SC pointings = 6, Time of observation (hours) = 3.0, Desc = Obtain 3x1 mosaic on one ring ansa on unlit face, or at high phase angle. Distance 20 R_S.   November 23, 2006: Reduced to 3 hrs to accomodate MAG Cals"]
["2007-146T13:35:00","000T06:44:00","2007-05-26","MAG","Non-SPASS","co-rotation","RNGSAT","Ring / Satellite","MAG MAPS RS Campaign","Observe Saturns inner magnetosphere and the interactions between icy satellites rings and the magnetosphere. Measure properties of a statistically significant number of satellite L-shell crossings distributed among the satellites and in longitudinal distance from the satellites."]
["2007-146T20:19:00","000T09:02:00","2007-05-26","MAG","SPASS Rider","Other","INTFLD","MAG Internal field observation","MAG_Internal_Field_Measurements","This request will yield unique observations of Saturns internal magnetic field over a unique orbit track in latitude and longitude space. Times originally were 21:25-03:50 (4Rs)."]
["2007-146T23:00:00","000T03:00:00","2007-05-26","ISS","SPASS Rider","Mimas","MIMASX",null,"Mimas color/polarization: CIRS RIDER","N05 + NP09 done twice over 3 hour observation."]
["2007-147T05:50:00","000T00:30:00","2007-05-27","UVIS","Prime","Mimas","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2007-147T06:50:00","000T01:00:00","2007-05-27","UVIS","Prime","Mimas","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2007-147T12:25:28","000T04:26:07","2007-05-27","CDA","Non-SPASS","DustRAM direction","0812DUST","Dust survey","Dust survey outside 8 Rs 11.52<lat< 15.94 deg 8.32","Dust survey outside 8 Rs $ 1060.5177 $ 1060.7025 $ 8.322 to 10.383 Rs lat:-15.937 to -11.522 deg ring-alt: 137856. to 125126.km,pointing=CDA to Kepler RAM,rate=200,dataVolume=3.045"]
["2007-147T17:45:00","000T00:30:00","2007-05-27","UVIS","SPASS Rider","Rhea","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2007-148T04:42:55","000T04:09:00","2007-05-28","ISS","SPASS Rider","Titan","FIRNADCMP","Far infrared nadir composition map","RCI (Rider Context Imaging)","ISS on, max data rate = 182.784 kbps, number of frames and bits/frame are input parameters, data volume = number of frames x bits/frame, average data rate = data volume/duration."]
["2007-148T14:51:55","000T08:00:00","2007-05-28","MAG","Non-SPASS","Titan","MAGTITAN","MAG Titan observation","T31 flyby","T31 is similar again to the previous encounters except for a flyby at a somewhat larger distance encounter above the northern pole (2458 km) which represents an interesting chance to study the wings in their initial development. The flyby is also unique under magnetosheath and solar wind conditions. Thus the rating is grade one priority.  NOTE: - continuous data rate of 1976bps (32vps)."]
["2007-148T22:51:55","000T01:00:00","2007-05-28","CIRS","Prime","Titan","FIRNADMAP","Far infrared nadir composition map",null,"Obtain information on surface & tropopause temperatures, and on tropospheric CH4. Scan or contiguous steps across disk."]
["2007-149T15:30:00","005T09:53:00","2007-05-29","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS","Part of  MB,C  MAPS Campaign.  Observe afternoon magnetospheric boundaries at 35 RS apoapsis distance and a range of inclinations"]
["2007-149T21:21:00","005T04:00:04","2007-05-29","RPWS","Non-SPASS","Sun","MAGBOUND","MAPS magnetosphere boundary campaign","MAPS MB,C Campaign","Part of MB,C MAPS Campaign.  Observe afternoon magnetospheric boundaries at 35 RS apoapsis distance and a range of inclinations"]
["2007-152T03:41:00","000T00:30:00","2007-06-01","CIRS","SPASS Rider","InstrumentCalibration","DEEPSPACE","Deep space calibration","CIRS_045IC_DEEPSPACE_SP","rider"]
["2007-153T11:41:00","000T07:31:00","2007-06-02","INMS","Non-SPASS","Sun","SPBITS","Data volume adjustment","MAPS Survey","Memory read out request."]
["2007-155T10:45:00","000T06:30:00","2007-06-04","CAPS","Prime","Sun","MAGBNDPTG","MAPS magnetosphere boundary campaign","CAPS Control Pointing during MAG BND Campaign","Part of  MB,C  MAPS Campaign.  Observe dusk-side magnetospheric boundaries at a variety of latitudes"]
["2007-158T04:55:00","000T00:30:00","2007-06-07","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 010 TH OBS","Turn to first satellite, take 1 NAC (CL1,CL2). Turn to second satellite take 1 NAC (CL1,CL2), repeat for up to 8 satellites if visible"]
["2007-159T03:55:00","000T01:50:56","2007-06-08","CAPS","Non-SPASS","Saturn","BURST4K","4 kbps burst","Burst of 4kbps data","Burst of 8 kbps data (which gives uncollapsed ELS data)."]
["2007-160T03:10:00","000T12:30:00","2007-06-09","CAPS","Non-SPASS","Saturn","BURST8K","8 kbps burst","Burst of 8kbps data","Burst of 8 kbps data (which gives uncollapsed ELS data)."]
["2007-161T02:40:00","000T10:45:00","2007-06-10","ISS","Prime","Saturn","WALGTNG11","Lightning search","Northern hemisphere lightning with the WAC.","Alternate between day and night sides every 30 min. Day side in R, G, B, CB3/MT3, CB2/MT2. Night side in CLR(2), RED, HAL(2)."]
["2007-162T05:35:00","000T09:10:00","2007-06-11","CAPS","SPASS Rider","InstrumentCalibration","CALIBRATE","Calibration","CAPS Calibration","CAPS periodic gain test and calibration. The specified rate and data volume are the delta above the CAPS survey rate (1000 bps), and the rate is the average over the entire request (current plans are to conduct the test in two different rates.)"]
["2007-162T18:10:00","000T19:10:00","2007-06-11","RPWS","Non-SPASS","co-rotation","RNGSAT","Ring / Satellite","MAPS RS Campaign","Part of RS MAPS Campaign.  Observe Saturn's inner magnetosphere and the interactions between icy satellites, rings and the magnetosphere. Measure properties of a statistically significant number of satellite L shell crossings distributed amoung the satellites and in longitudinal distance from the satellites."]
["2007-163T01:30:00","000T01:00:00","2007-06-12","VIMS","SPASS Rider","Star","ALPORIOCC","Alpha Orion occultation","VIMS_046ST_ALPORIOCC001_SI occultation ingress","Supp Image for Occultation start within 3 minutes of occ ingress ISS_WAC image (only 1 image on ingress) clear filter 2x2 on-chip summing mode slightly-lossy compression data vol = 0.5 Mbit/image"]
["2007-163T04:30:00","000T08:50:00","2007-06-12","MAG","Non-SPASS","co-rotation","RNGSAT","Ring / Satellite","MAG MAPS RS Campaign","Observe Saturns inner magnetosphere and the interactions between icy satellites rings and the magnetosphere. Measure properties of a statistically significant number of satellite L-shell crossings distributed among the satellites and in longitudinal distance from the satellites."]
["2007-163T15:03:44","000T05:15:22","2007-06-12","CDA","SPASS Rider","DustRAM direction","1005DUST","Dust survey","Dust survey outside 8 Rs 5.24<lat< 7.77 deg 9.70..","Dust survey outside 8 Rs $ 1076.6276 $ 1076.8466 $ 9.700 to 12.076 Rs lat: -7.774 to -5.238 deg ring-alt: 79155. to 66509.km,pointing=CDA to Kepler RAM,rate=200,dataVolume=3.609"]
["2007-164T08:46:11","000T04:00:00","2007-06-13","ISS","SPASS Rider","Titan","MIRLMBMAP","Mid infrared limb map","RCI (Ridealong Context Imaging)","ISS on, max data rate = 182.784 kbps, number of frames and bits/frame are input parameters, data volume = number of frames x bits/frame, average data rate = data volume/duration."]
["2007-164T16:39:11","000T00:24:24","2007-06-13","UVIS","SPASS Rider","Sun","USUNOCC","Solar occultation","USUN_T32I/E rider","This is an ingress/egress solar occultation of Titan.  During this period the spacecraft is transitioning from wheels to thrusters and we have ho option but to stare at the sun with a fixed attitude."]
["2007-164T18:32:11","000T00:16:00","2007-06-13","CIRS","Prime","Titan","FIRLMBINT","Vertical limb sounding",null,"Vertical temperature sounding of Titan's tropopause & stratosphere. Slow radial scans."]
["2007-165T07:46:11","000T02:15:00","2007-06-14","CIRS","Prime","Titan","MIDIRTMAP","Mid infrared thermal map",null,"Obtain information on the thermal structure of Titan's stratosphere. Slew across disk at 4 microrad/s."]
["2007-166T08:00:00","000T08:54:00","2007-06-15","VIMS","Prime","RingG","G45PHASE","G ring observation","G Ring near phase 45","12x12; 1 sec exp; do any 1 of 4 at Priority 1; also any 1 of 4 at Priority 2"]
["2007-167T03:24:00","000T01:00:00","2007-06-16","ISS","Prime","rings(general)","FMONITOR","F ring monitor","F RING TEMPORAL MONITORING","long term temporal monitoring of F ring."]
["2007-171T01:09:30","000T00:00:01","2007-06-20","MP","SPASS Note","Saturn","APOAPSE","Apoapse",null,"Apoapse  Per = 16.0 d, inc = 2.1 deg, r = 38.1 Rs, phase = 54 deg"]
["2007-172T03:00:00","000T00:30:00","2007-06-21","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 004 TH OBS","Turn to first satellite, take 1 NAC (CL1,CL2). Turn to second satellite take 1 NAC (CL1,CL2), repeat for up to 8 satellites if visible"]
["2007-174T03:30:00","000T06:00:00","2007-06-23","MIMI","Prime","Saturn","MAGBNDSAT","MAPS magnetosphere boundary campaign","Magnetospheric Boundary Campaign, Saturn imaging","Pointing for MAGBOUNDARY Campaign, -X to sun, -Y to Saturn"]
["2007-175T18:38:00","000T18:02:00","2007-06-24","CAPS","SPASS Rider","Sun","MAGBOUND","MAPS magnetosphere boundary campaign","MAPS","Part of  MB,C  MAPS Campaign.  Observe afternoon magnetospheric boundaries at 35 RS apoapsis distance and a range of inclinations"]
["2007-176T12:40:00","000T13:28:00","2007-06-25","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_SURVEY","Continuous low-rate magnetospheric survey"]
["2007-178T02:08:00","000T06:02:00","2007-06-27","CDA","Non-SPASS","DustRAM direction","DATA","Data volume adjustment","Dust survey DV (AM)","Dust survey $ 1084.0624 $ 1091.3740 $ 38.111 to 10.707 Rs lat: 0.946 to 2.055 deg ring-alt: 37961. to 23164.km,pointing=CDA to Kepler RAM,rate=150,dataVolume=90.368"]
["2007-178T15:08:46","000T01:10:17","2007-06-27","CDA","Non-SPASS","DustRAM direction","0702DUST","Dust survey","E Ring dense - survey - 2.13<lat< 2.13 deg 6.94...","E Ring dense - survey - $ 1091.6311 $ 1091.6799 $ 7.588 to 6.937 Rs lat: 2.133 to 2.132 deg ring-alt: 17039. to 15570.km,pointing=CDA to Kepler RAM,rate=524,dataVolume=2.107"]
["2007-178T20:00:00","000T00:23:44","2007-06-27","RPWS","Non-SPASS","Tethys","TECA","Tethys closest approach","Tethys closest approach observations","RPWS observations in the immediate vicinity of Tethys, including the characterization of the plasma wave spectrum and search for evidence of pickup ions.  Pointing:  prefer RPWS Langmuir Probe within 90 degrees of plasma ram."]
["2007-179T01:55:00","000T00:15:00","2007-06-28","VIMS","SPASS Rider","Mimas","GLOCOL","Global coverage mapping","Tethys","24x12i2-v3 160 ms, 640 ms sets, assuming ISS is ponting and staring.  (my need to increase cube size for pointing error possibilities. 1.5 mbits, 4 minutes per set,  3 sets in 30 min. 10.5 mbits total  edited by hibbitts, 07/04/03"]
["2007-179T13:30:00","000T04:16:00","2007-06-28","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey."]
["2007-179T15:40:00","000T14:20:00","2007-06-28","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_SURVEY","Continuous low-rate magnetospheric survey"]
["2007-180T05:59:46","000T02:00:00","2007-06-29","RSS","SPASS Rider","Titan","THERMAL","Thermal stabilization period","RSS Titan Mass Thermal Stabilization","A period of thermal stabilization is required immediately prior to any radio science experiment and test using Ka-band or S-band."]
["2007-180T19:01:00","000T16:33:56","2007-06-29","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SURVEY Campaign","Part of SURVEY MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2007-181T04:59:46","000T12:02:36","2007-06-30","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey."]
["2007-182T02:35:00","006T07:17:00","2007-07-01","MAG","Non-SPASS","Sun","MAGBOUND","MAPS magnetosphere boundary campaign","MAG_MAPS_MB_C_Campaign","Observe_afternoon_magnetospheric_boundaries_at_35_RS_apoapsis_distance_and_a_range_of_inclinations."]
["2007-182T10:22:00","000T06:00:00","2007-07-01","ISS","SPASS Rider","RingE","E45PHASE","E ring observation","RIDER ON VIMS E RING OBSERVATION","RIDER ON VIMS E RING OBSERVATION."]
["2007-184T16:37:00","000T09:00:00","2007-07-03","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2007-188T15:52:00","004T09:15:00","2007-07-07","MAG","Non-SPASS","Sun","MAGBOUND","MAPS magnetosphere boundary campaign","MAG_MAPS_MB_C_Campaign","Observe_afternoon_magnetospheric_boundaries_at_35_RS_apoapsis_distance_and_a_range_of_inclinations."]
["2007-190T08:52:00","000T09:00:00","2007-07-09","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2007-192T07:00:00","000T02:59:12","2007-07-11","CAPS","Non-SPASS","Saturn","BURST16K","16 kbps burst","Burst of 16kbps data","Burst of 16 kbps data (which gives uncollapsed ELS data)."]
["2007-193T01:07:01","001T14:58:59","2007-07-12","MIMI","SPASS Rider","Sun","MAGBOUND","MAPS magnetosphere boundary campaign","MAPS MB/C Campaign","Part of MB/C MAPS Campaign.   Observe afternoon magnetospheric boundaries at 35 RS apoapsis distance and a range of inclinations. Set up MIMI for magnetospheric boundaries campaign Pointing: -X to sun and/or corotation, internal B in X, Z plane; or spin about Z."]
["2007-195T18:48:00","001T06:18:00","2007-07-14","INMS","Non-SPASS","Sun","MAGBOUND","MAPS magnetosphere boundary campaign","MAPS","Part of MB,C MAPS Campaign.  Observe afternoon magnetospheric boundaries at 35 RS apoapsis distance and a range of inclinations"]
["2007-197T02:36:00","000T05:24:00","2007-07-16","VIMS","Prime","RingG","G80PHASE","G ring observation","G Ring near phase 80","12x12; 1 sec exp; do any 1 of 9 at Priority 1; also any 1 of 9 at Priority 2"]
["2007-198T18:14:56","000T06:36:04","2007-07-17","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2007-199T11:13:37","000T23:35:23","2007-07-18","CDA","Non-SPASS","DustRAM direction","1700DUST","Dust survey","Dust survey 0.28<lat< 0.29 deg 16.85... 24.23 Rs v","Dust survey $ 1112.4678 $ 1113.4507 $ 24.231 to 16.851 Rs lat: 0.279 to 0.291 deg ring-alt: 7119. to 5163.km,pointing=CDA to Kepler RAM,rate=150,dataVolume=12.148"]
["2007-199T21:41:20","000T00:30:00","2007-07-18","UVIS","Prime","Titan","EUVFUV","UVIS EUV / FUV imaging","EUVFUV Imaging of  Titan","slow scan across Titan's visible hemisphere to form spectral images"]
["2007-200T06:11:20","000T03:36:00","2007-07-19","VIMS","SPASS Rider","Titan","GLOBMAP","Global coverage mapping","Global Map","Ridealong with ISS Global Map. Template H"]
["2007-200T15:36:00","000T09:00:00","2007-07-19","RPWS","Non-SPASS","co-rotation","TINTERACT","MAPS TI/EE Campaign","MAPS TI/EE Campaign","Part of TI/EE MAPS Campaign.  Investigate large-scale and distant aspects of the Titan interaction by observing during entire period around an encounter from 10 to 25 RS"]
["2007-201T00:36:00","000T03:38:56","2007-07-20","RPWS","Non-SPASS","co-rotation","TINTERACT","MAPS TI/EE Campaign","MAPS TI/EE Campaign","Part of TI/EE MAPS Campaign.  Investigate large-scale and distant aspects of the Titan interaction by observing during entire period around an encounter from 10 to 25 RS"]
["2007-201T14:30:00","000T03:00:00","2007-07-20","RADAR","SPASS Rider","Other","WARM4TE","RADAR warmup","Scatterometry/Radiometry of Tethys.","Warmup for scatterometry and simultaneous radiometry of icy satellite."]
["2007-202T02:26:00","000T00:30:00","2007-07-21","VIMS","Prime","Saturn","FEATRACK","Imaging selected lattitudes at a range of emission angles as the planet rotates","Saturn Feature Track #3","New Feature track added 03-08-07, per Barbara Larsen. This is the first of a series, but each of these incorporates different territory."]
["2007-202T10:38:37","000T01:35:46","2007-07-21","CDA","Non-SPASS","DustRAM direction","1000DUST","Dust survey","Ring Margin - survey - 0.20<lat< 0.22 deg 9.69...","Ring Margin - survey - $ 1115.4435 $ 1115.5100 $ 9.685 to 10.331 Rs lat: -0.218 to -0.201 deg ring-alt: 2223. to 2186.km,pointing=CDA to Kepler RAM,rate=524,dataVolume=2.871"]
["2007-203T04:15:00","000T00:30:00","2007-07-22","ISS","Prime","Mimas","238W026PH","Spectrophotometery","Mimas spectrophotometry/ phase coverage","Turn -Y to Mimas; do 1x1 mosaic 3 clear + 4 NAC color + 9 NAC polarizer + 4 WAC polarizer filters; turn to WP"]
["2007-203T06:20:00","000T01:16:00","2007-07-22","CDA","Non-SPASS","Other","ECCSCAN2B","Eccentricity scan","CDA Eccentricity Scan","CDA eccentricity scan: An observation scenario which allows the separation of orbital elements to the greatest degree possible is required. Particle inclinations can be determined having a rolling S/C with a rotation axis parallel to the ring plane (equatorial orbits). However in order to determine particle eccentricities the CDA boresight must rotate in the ring plane. This observation mode requires a CDA prime observation and cannot easily be combined with ORS, RADAR or D/L observations. During the proposed observation CDA will perform a rock about the x axis which will be aligned perpendicular to the ring plane. This allows scan through the dust RAM direction without violating flight rules."]
["2007-204T01:06:00","000T08:15:00","2007-07-23","CIRS","SPASS Rider","rings(general)","RPX10PH","Ring plane crossing","Rider on VIMS RPX10PH","Rider on VIMS RPX10PH. Stare at rings"]
["2007-205T00:21:04","000T14:59:51","2007-07-24","RPWS","Non-SPASS","Saturn","HIRATE","High rate mode","MAPS MB,A Campaign","null"]
["2007-207T16:06:00","000T08:00:00","2007-07-26","CIRS","SPASS Rider","InstrumentCalibration","DSCAL07","Deep space calibration","CIRS_048IC_DSCAL07207_RIDER","Calibration rider."]
["2007-209T16:51:04","000T22:29:51","2007-07-28","RPWS","Non-SPASS","Saturn","HIRATE","High rate mode","MAPS MB,A Campaign","null"]
["2007-213T01:20:00","000T03:30:00","2007-08-01","CIRS","SPASS Rider","InstrumentCalibration","MOS48APO","Apoapsis mosaic","CIRS_048IC_MOS48APO009_UVIS","Calibration rider.  Data Volume will be 50.4 Mb or less."]
["2007-213T04:50:00","000T09:30:00","2007-08-01","ISS","Prime","Saturn","APOMOVIEA","Apoapsis movie","NAC Southern Hemisphere Saturn movie","4x4 BOTSIM mosaic in 2 filters of the Southern Hemisphere for one rotation; pickets of 1:10 duration, 6 repetitions with 1:40 spacing."]
["2007-215T13:35:00","000T01:00:00","2007-08-03","UVIS","Prime","Saturn","MOS48APO","Apoapsis mosaic","MOSAIC_APO_48_11","Mosaic of Saturn inner magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with the Saturn spin axis. 1) Drift at a rate of .1084 mrad/sec about the Z-axis for 3000s toward +MOS Orb. 2) Slew back to Saturn center and reset pointing. MOS orb (+/-range): 433.44mrad"]
["2007-219T02:55:00","000T01:30:00","2007-08-07","CIRS","SPASS Rider","InstrumentCalibration","MOS48APOA","Apoapsis mosaic","CIRS_048IC_MOS48APOA015_UVIS","Calibration rider.  Data Volume will be 21.6 Mb or less."]
["2007-221T01:05:00","000T03:15:00","2007-08-09","CIRS","SPASS Rider","InstrumentCalibration","MOS48APO","Apoapsis mosaic","CIRS_048IC_MOS48APO017_UVIS","Calibration rider.  Data Volume will be 46.8 Mb or less."]
["2007-221T23:50:00","000T04:30:00","2007-08-09","UVIS","Prime","Saturn","MOS48APO","Apoapsis mosaic","MOSAIC_APO_48_18","Mosaic of Saturn inner magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with the Saturn spin axis. 1) Slew about the Z-axis from Saturn Center to -MOS Orb. Rotate +64mrad in the YZ plane.  2) Drift at a rate of .1017 mrad/sec about the Z-axis for 8000s to +MOS. 3) Drift at indicated rate about the Z-axis for 6000s toward -MOS Orb. 4) Slew back to Saturn center and reset pointing. Stare for remaining observation time. Orb MOS orb (+/-range): 407.13mrad"]
["2007-223T04:20:00","000T09:30:00","2007-08-11","UVIS","SPASS Rider","Saturn","APOMOVIEA","Apoapsis movie","DAYGLOW OBSERVATION"]
["2007-226T04:05:00","000T09:30:00","2007-08-14","ISS","Prime","Saturn","APOMOVIEA","Apoapsis movie","NAC Southern Hemisphere Saturn movie","4x4 BOTSIM mosaic in 2 filters of the Southern Hemisphere for one rotation; pickets of 1:10 duration, 6 repetitions with 1:40 spacing."]
["2007-227T04:05:00","000T09:30:00","2007-08-15","ISS","Prime","Saturn","APOMOVIEA","Apoapsis movie","NAC Southern Hemisphere Saturn movie","4x4 BOTSIM mosaic in 2 filters of the Southern Hemisphere for one rotation; pickets of 1:10 duration, 6 repetitions with 1:40 spacing."]
["2007-229T07:20:00","000T08:00:00","2007-08-17","CIRS","SPASS Rider","InstrumentCalibration","DSCAL07","Deep space calibration","Deep Space Calibration","Deep space obervations for calibration."]
["2007-238T13:20:00","000T09:00:00","2007-08-26","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2007-240T13:50:00","000T07:55:52","2007-08-28","CAPS","Non-SPASS","Earth","BURST8K","8 kbps burst","Burst of 8kbps data","Burst of 16 kbps data (which gives uncollapsed ELS data)."]
["2007-241T10:15:00","000T00:45:00","2007-08-29","VIMS","SPASS Rider","Tethys","TETHYS","Tethys","Tethys","64x64i2-v1 160ms, 320ms follow cirs tethys phase ~110 deg, size~41 pixels"]
["2007-241T13:40:00","000T01:00:00","2007-08-29","CIRS","SPASS Rider","Tethys","TETHYS","Tethys","VIMS rider on Tethys","VIMS Tethys rider for high spectral resolution and for phase angle coverage. Phase=65, Local time=7.7, sub S/C=(-2, 111), AD=16.8 mrad.  Duration: 01:00.  CIRS: 96 RTI (2.85 cm-1, 12 sec/frame), FP1+FP3 only, blink.  Shutter closed 00:10 to 00:16, 00:44 to 00:50."]
["2007-241T16:40:00","000T00:15:00","2007-08-29","UVIS","SPASS Rider","Tethys","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2007-241T22:33:55","000T00:45:00","2007-08-29","UVIS","SPASS Rider","Rhea","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2007-242T02:18:55","000T00:45:00","2007-08-30","UVIS","Prime","Rhea","ICYMAP","Icy satellite surface map","ICYMAP:  UV Surface Map of Rhea and Limb Drifts","Map surface albedo of Rhea in UV.  Limb drifts to determine atmospheric scattering.  Slew from Rhea center to FUV positioned just off north polar limb.  Carry out one north-south scan at ~26 urad/sec slew rate to FUV positioned one field-of-view width off the south polar limb.  Return to Rhea center."]
["2007-242T07:34:00","000T09:00:00","2007-08-30","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2007-242T16:34:00","000T00:41:00","2007-08-30","RPWS","Non-SPASS","Saturn","INSURVEY","Inner magnetosphere survey","RPWS Inner Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2007-243T05:32:34","000T02:00:00","2007-08-31","MIMI","SPASS Rider","Titan","T35CLOSE",null,"MAPS 049TI(T35) Campaign","Part of 049TI(T35) MAPS Campaign.   Investigate micro-scale and near aspects of the Titan interaction by observing during about one hour period around an encounter. With -Y pointed toward Titan, when within 30 minutes of the targeted flyby, optimize secondary axis for corotation flow as close to the S/C -X, +/- Z plane as works with the other constraints on pointing. Also, measure Titan exosphere/magnetosphere interaction by imaging in ENA with INCA (when sun is not in INCA FOV)."]
["2007-243T11:32:34","000T03:36:00","2007-08-31","CIRS","SPASS Rider","Titan","GLOBMAP","Global coverage mapping",null,"Obtain information on CO, HCN, CH4. Integrate on disk at airmass 1.5--2.0."]
["2007-246T10:45:00","000T01:45:00","2007-09-03","ISS","Prime","Iapetus","LIMBTOPOA","Limb topography and geodesy observation","Iapetus limb topography, geodesy , and graylight o","Turn CIRS_FP3 to Iapetus; turn CIRS_FP1 to Iapetus; turn UVIS_FUV to Iapetus; turn to WP."]
["2007-249T05:20:00","000T09:00:00","2007-09-06","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2007-249T19:30:00","000T01:20:00","2007-09-06","ISS","SPASS Rider","rings(general)","FMONITOR","F ring monitor","F ring imaging on each ansa","One WAC each ansa at beginning or end"]
["2007-250T22:20:00","000T05:30:00","2007-09-07","ISS","SPASS Rider","Iapetus","IAPETUS","Iapetus observation","Iapetus limb topography, geodesy, and graylight ob","Do 1x1 mosaics at start and end of observation"]
["2007-251T11:50:00","000T00:30:00","2007-09-08","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 074 TH OBS","Turn to first satellite, take 1 NAC (CL1,CL2). Turn to second satellite take 1 NAC (CL1,CL2), repeat for up to 8 satellites if visible"]
["2007-252T22:25:00","000T01:30:00","2007-09-09","CIRS","SPASS Rider","Iapetus","NITPOLRIZ",null,"4 WACs to support polarization pointing","4 compressed WAC images (0.5 Mb each) for pointing verification.  Frame at 2007-252T22:44, 2007-252T22:53, 2007-252T23:14, and 2007-252T23:23."]
["2007-253T12:30:40","000T00:01:00","2007-09-10","ISS","Prime","Iapetus","CASSREG",null,"Iapetus I49 targeted flyby imaging","Do BOTSIM over +2/130."]
["2007-253T17:15:40","000T02:00:00","2007-09-10","CIRS","Prime","Iapetus","FP1DAYMAP","CIRS FP1 daytime map","Outgoing dayside FP1 map","PREVIOUS REMARKS:  Shortened 20 minutes to 01:10; must redesign.    7/18/04.         Outgoing dayside FP1 map.  AD=52-36 mrad, phase=31, sub-s/c=(-12, 243)= Roncevaux Terra, LT=10.1.  Duration=01:30  CIRS 38 RTI (15.67 cm-1, 4.75 sec./scan) Nyquist-sampled FP1 map of disk; construct to cover as much as possible (if any extra time, use it for integration at center of disk at END of observation).  FP1 and FP3 only; for FP3: center detectors, shutter closed 00:10-00:15 and 01:20-01:25  NEW DESIGN REQUIREMENTS (3/19/07):   First 30 min FP3, then FP1 map; last 30 min FP3 (time extended from 01:10 to 02:00).  Include FP4, so use all focal planes."]
["2007-253T19:15:40","000T00:44:00","2007-09-10","UVIS","SPASS Rider","Iapetus","ICYMAP","Icy satellite surface map","ICYMAP:  Iapetus UV Map, Rider on ORS","UV albedo of Iapetus' surface"]
["2007-254T20:45:00","000T02:15:00","2007-09-11","ISS","SPASS Rider","Iapetus","IAPETUS","Iapetus observation","Iapetus global color observation","Do NAC 1x1 multi-color imaging."]
["2007-257T11:43:07","008T09:07:53","2007-09-14","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2007-259T02:21:00","000T09:30:00","2007-09-16","ISS","Prime","Saturn","APOMOVIEA","Apoapsis movie","NAC Southern Hemisphere Saturn movie","4x4 BOTSIM mosaic in 2 filters of the Southern Hemisphere for one rotation; pickets of 1:10 duration, 6 repetitions with 1:40 spacing."]
["2007-260T22:01:00","000T01:30:00","2007-09-17","UVIS","Prime","Saturn","MOS49APO","Saturn inner magnetosphere mosaic","MOSAIC_APO_49_24","Mosaic of Saturn inner magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with the Saturn Spin axis. 1) Rotate -64mrad in the YZ plane from Saturn Center. Slew about the Z-axis to -MOS Orb. 2) Drift at a rate of .1192mrad/s about the Z-axis for 4000s toward +MOS Orb. 3) Slew back to Saturn Center and reset pointing. MOS Orb (+/-Range): 476.662mrad"]
["2007-264T04:06:00","000T07:30:00","2007-09-21","UVIS","Prime","Saturn","MOS49APO","Saturn inner magnetosphere mosaic","MOSAIC_APO_49_28","Mosaic of Saturn inner magnetosphere.  EUV and FUV low resolution slits on, aligned parallel with the Saturn spin axis. 1) Rotate +128mrad in the YZ plane from Saturn Center. Slew about the Z-axis to -MOS Orb. 2) Drift at a rate of .1292mrad/s about the Z-axis for 8000s to +MOS Orb. 3) Drift at indicated rate about the Z-axis for 8000s to -MOS Orb. 4) Drift at indicated rate about the Z-axis for 8000s to +MOS Orb. 5) Drift at indicated rate about the Z-axis for 1000s toward -MOS Orb. 6) Slew back to Saturn center and reset pointing. MOS orb (+/-range): 516.792mrad."]
["2007-265T21:21:00","000T05:30:00","2007-09-22","ISS","Prime","Star","CALSTAR1","Stellar Calibration","ISS Photometric Calibration Star 1","Photometric Calibration Star 1 (Vega)"]
["2007-266T04:21:00","000T09:00:00","2007-09-23","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2007-270T05:21:00","000T04:15:00","2007-09-27","ISS","SPASS Rider","rings(general)","FMONITOR","F ring monitor","F ring imaging on each ansa","One WAC each ansa at beginning and then at 2-hr intervals"]
["2007-272T03:30:00","000T00:36:00","2007-09-29","CIRS","SPASS Rider","InstrumentCalibration","DEEPSPACE","Deep space calibration",null,"rider"]
["2007-272T13:30:00","000T05:00:00","2007-09-29","UVIS","SPASS Rider","RingA","COMP001","Sit and stare to derive composition","Ring Rider"]
["2007-273T07:45:00","000T01:05:00","2007-09-30","VIMS","SPASS Rider","Saturn","SOLAROCC","Solar occultation","solar planet occultation","Egress Rev 50 Nicholson Addition"]
["2007-273T10:50:00","000T00:55:00","2007-09-30","VIMS","SPASS Rider","Enceladus","COLORF","Color image","Enceladus","Follow ISS, probably 12x24 double res IR phase ~20 deg, size ~ 11 pixels If ISS stare, do slightly bigger frames ideally alternate 160ms, 640ms frames   edited time hibbitts 10/01/03"]
["2007-273T12:40:00","000T00:50:00","2007-09-30","VIMS","SPASS Rider","Enceladus","PHOTOM","Photometry","Enceladus","Follow ISS, probably 12x24 double res IR phase ~10 deg, size ~ 10 pixels If ISS stare, do slightly bigger frames ideally alternate 160ms, 640ms frames"]
["2007-273T22:33:44","000T05:23:00","2007-09-30","CDA","Non-SPASS","DustRAM direction","0803DUST","Dust survey","Ring Margin - survey - 2.68<lat< 4.16 deg 8.00...","Ring Margin - survey - $ 1186.9401 $ 1187.1644 $ 7.998 to 10.346 Rs lat: 4.160 to 2.682 deg ring-alt: 35003. to 29207.km,pointing=CDA to Kepler RAM,rate=524,dataVolume=9.684"]
["2007-274T18:42:43","000T01:00:00","2007-10-01","ISS","Prime","Titan","PHOTOMWAC","Photometry map","WPH (WAC Photometry)","particle properties, vertical distributions ~6 km/px.  0.6 Mbit/frame with 2x2 summing. special S/C orientation requested."]
["2007-275T05:27:43","000T01:15:00","2007-10-02","CAPS","SPASS Rider","Titan","T36OUTBND",null,"MAPS 050TI(T36) Campaign","Part of 050TI(T36) MAPS Campaign.  Outbound approach observations and context for the interaction between Titan and Saturn's magnetosphere"]
["2007-275T15:42:43","000T02:00:00","2007-10-02","VIMS","SPASS Rider","Titan","MONITORNA","Monitoring of surface and atmosphere","MOSAIC","Ridealong with ISS Mosaic map. Template D"]
["2007-276T02:12:00","000T12:07:00","2007-10-03","RSS","SPASS Rider","Saturn","OCCORT","Operations Readiness Test to demonstrate DSN and RSSG preparedness to support upcoming occultations","RSS Operational Readiness Test","RSS Operations Readiness Test (ORT), to demonstrate DSN and RSSG preparedness to support the Rings/Saturn Occultation experiment on DOY 297."]
["2007-278T20:22:00","000T23:45:00","2007-10-05","INMS","Non-SPASS","Saturn","PTOTM131","MAPS survey","MAPS Survey","MAPS magnetospheric survey."]
["2007-293T07:53:00","000T00:30:00","2007-10-20","ISS","Prime","Hyperion","ROTCOL","Satellite rotation and color imaging","HYPERION Rotation and Color","0; Hyperion rotation and color, N09"]
["2007-294T08:23:00","000T01:30:00","2007-10-21","ISS","Prime","rings(general)","WNL4P5UN","Ring photometry","Rev 51 (formerly 50) low-tilt ring photometry","TWT X-DIS  Range 28.27  B 4.5  Phase (start) 66.31-59.28  Phase (end) 66.62-59.53  NAC pixel (ansa, sub-sc) 10.23-130.43"]
["2007-295T19:23:01","001T07:37:58","2007-10-22","MIMI","SPASS Rider","Saturn","MAGDYN","MAPS magnetosphere dynamics campaign","MIMI Magnetospheric Dynamics Imaging Campaign","MIMI Magnetospheric Dynamics Imaging"]
["2007-296T17:00:00","000T01:00:00","2007-10-23","ISS","Prime","rings(general)","PHOTOMDRK","Photometry map","Ring photometry","WAC 1x3 mosaic on left ansa in multi-colors"]
["2007-296T17:00:00","000T01:00:00","2007-10-23","CIRS","SPASS Rider","rings(general)","PHOTOMDRK","Photometry map",null,"rider"]
["2007-297T07:56:22","000T00:00:01","2007-10-24","MP","SPASS Note","Saturn","PERIAPSE","Periapse",null,"Periapse R = 3.8 Rs, lat = -3 deg, phase = 145 deg"]
["2007-298T00:00:00","000T02:00:00","2007-10-25","CIRS","SPASS Rider","rings(general)","RADSCAN",null,null,"rider"]
["2007-298T20:25:08","000T02:00:00","2007-10-25","CDA","Non-SPASS","rings(general)","1800RINGM","Ring margin","Ring Margin 0.00<lat< 1.00 deg 18.40... 18.60 Rs v","Ring Margin$ 1211.8508$ 1211.9341$ 18.422 to 18.589 Rs lat: -0.626 to -0.598 deg ring-alt: 12142. to 11705.km 028OF029 no ADJ: 89 was:2007-298T21:10:01...2007-298T21:40:15,pointing=CDA to Kepler RAM,rate=524,dataVolume=3.598"]
["2007-299T00:00:00","000T01:00:00","2007-10-26","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 030 TH OBS","Turn to first satellite, take 1 NAC (CL1,CL2). Turn to second satellite take 1 NAC (CL1,CL2), repeat for up to 8 satellites if visible"]
["2007-299T12:25:00","000T00:25:00","2007-10-26","ISS","Prime","Enceladus","022W010PH","Spectrophotometery","Enceladus spectrophotometry/ phase coverage","Turn -Y to Enceladus; do 1x1 mosaic; turn to WP"]
["2007-300T10:15:00","000T01:00:00","2007-10-27","RADAR","Prime","Titan","PHASE1CAL","Distant Titan observation","Distant Titan Phase Study Group","Obtain distant Titan radiometer science and calibration data. Near zero titan sub-spacecraft latitudes, near zero sub-spacecraft longitudes.  One of a set with varying phase angle."]
["2007-300T16:45:04","000T17:24:56","2007-10-27","RPWS","Non-SPASS","Saturn","SWAURORA","Solar wind campaign","MAPS SW2 Campaign","Part of SW2 MAPS Campaign.  Monitor the solar wind while Cassini is well upstream of Saturn's bow shock in coordination with RPWS and Earth based observations of Saturn's aurora"]
["2007-301T10:10:00","000T09:00:00","2007-10-28","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2007-303T18:10:00","000T01:00:00","2007-10-30","UVIS","SPASS Rider","Dione","022W025PH","Spectrophotometery"]
["2007-306T18:40:00","002T13:27:46","2007-11-02","INMS","Non-SPASS","Saturn","PTOTM132B","MAPS survey","MAPS Survey","MAPS magnetospheric survey."]
["2007-310T01:55:00","000T09:00:00","2007-11-06","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2007-313T18:11:00","000T22:29:00","2007-11-09","CAPS","SPASS Rider","Saturn","SWAURORA","Solar wind campaign","MAPS SW2 Campaign","Part of SW2 MAPS Campaign.  Monitor the solar wind while Cassini is well upstream of Saturn's bow shock in coordination with RPWS and Earth based observations of Saturn's aurora"]
["2007-316T19:26:00","000T13:00:00","2007-11-12","UVIS","Prime","Saturn","EUVFUV","UVIS EUV / FUV imaging","EUVFUV Imaging of Saturn","Several slow scans across Saturn's visible hemisphere to form spectral images. Distance to Saturn -s 2 million Km.  Phase is 0-145"]
["2007-318T18:30:00","000T10:00:00","2007-11-14","RADAR","Prime","rings(general)","PO8RINGS","Ring observation","Prioritized Ring Observation Number 8","Image rings via radiometry at low inclination and low resolution."]
["2007-320T07:25:00","000T00:20:00","2007-11-16","CIRS","SPASS Rider","co-rotation","DTORUSPTG",null,"Rider for deep space calibration","rider for deep space.  38 RTI, blink."]
["2007-320T10:30:00","000T00:40:00","2007-11-16","VIMS","SPASS Rider","Rhea","REGGODB","Regional geodesy","Rhea","tbd Frame at 160ms, 640 pairs, 6 kbps average."]
["2007-320T17:41:00","000T11:24:00","2007-11-16","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_SURVEY","Continuous low-rate magnetospheric survey"]
["2007-321T04:24:28","000T00:50:00","2007-11-17","VIMS","SPASS Rider","Saturn","SOLOCC","Solar occultation","Solar Occultation","Solar Occultation by Saturn. Ride with UVIS."]
["2007-321T11:20:00","000T12:30:08","2007-11-17","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_SURVEY","Continuous low-rate magnetospheric survey"]
["2007-322T10:12:00","000T13:50:25","2007-11-18","CAPS","SPASS Rider","Titan","T37EXTINB",null,"MAPS TI/EE Campaign","Part of TI/EE MAPS Campaign.  Investigate large-scale and distant aspects of the Titan interaction by observing during entire period around an encounter from 10 to 25 RS"]
["2007-322T22:47:25","000T00:21:00","2007-11-18","CIRS","Prime","Titan","FIRLMBINT","Vertical limb sounding",null,"Vertical sounding of stratospheric compounds on Titan, including H2O. Integrations at 2 locations on the limb displaced vertically."]
["2007-323T01:08:25","000T00:23:00","2007-11-19","CIRS","SPASS Rider","Titan","FIRLMBT","Far Infrared limb tracking",null,"Vertical temperature sounding of Titan's tropopause & stratosphere. Slow radial scans."]
["2007-323T01:31:25","000T01:16:00","2007-11-19","CIRS","SPASS Rider","Titan","HIRESNAC","High resolution map",null,"Vertical sounding of stratospheric compounds on Titan, including H2O. Integrations at 2 locations on the limb displaced vertically."]
["2007-323T13:14:24","000T20:43:36","2007-11-19","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_SURVEY","Continuous low-rate magnetospheric survey"]
["2007-325T00:57:00","000T09:00:00","2007-11-21","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2007-328T08:13:00","000T09:00:00","2007-11-24","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2007-329T08:13:00","000T09:00:00","2007-11-25","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2007-330T20:45:00","000T03:15:00","2007-11-26","CAPS","Prime","Sun","SWAURPTG","MAPS aurora campaign","CAPS Control Pointing during Ring Sat Campaign","Part of  MB,C  MAPS Campaign.  Observe dusk-side magnetospheric boundaries at a variety of latitudes"]
["2007-334T06:30:00","000T01:00:00","2007-11-30","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 014 TH OBS","Turn to first satellite, take 1 NAC (CL1,CL2). Turn to second satellite take 1 NAC (CL1,CL2), repeat for up to 8 satellites if visible"]
["2007-335T08:30:00","000T01:28:00","2007-12-01","CIRS","SPASS Rider","InstrumentCalibration","DEEPSPACE","Deep space calibration",null,"rider"]
["2007-336T18:14:00","000T01:31:00","2007-12-02","ISS","Prime","Mimas","PHOTOM","Photometry","MIMAS Color Photometry/Polarization","92.023; Leading Side; NP09 + N05, Done twice."]
["2007-337T06:19:49","000T00:49:00","2007-12-03","CIRS","SPASS Rider","InstrumentCalibration","ERNX","E ring plane crossing","CIRS_053IC_ERNX001_CDA","Calibration rider.  Data Volume will be 11.76 Mb or less."]
["2007-337T07:54:49","000T00:39:00","2007-12-03","CIRS","SPASS Rider","Epimetheus","GEOLOG","Geologic study","FP3 ISS rider (5.1-3.3 mrad, ph=67-63, (-46,307) )","Epimetheus ISS rider.  AD=5.1-3.3, phase=67-63, (-46, 307), duration 00:39.  CIRS:  blink, 38 RTI (15.5 cm-1 res.), shutter closed 00:05 - 00:10 and 00:30 - 00:35."]
["2007-337T20:05:01","000T04:01:59","2007-12-03","MIMI","SPASS Rider","Saturn","MAGDYN","MAPS magnetosphere dynamics campaign","MAPS IM/DYN Campaign","Part of IM/DYN MAPS Campaign.   Image the dynamics of the inner magnetosphere in ENA with MIMI/INCA. With -Y pointed toward Saturn, corotation as close to the S/C -X, +/- Z plane as possible."]
["2007-338T20:06:50","000T08:00:00","2007-12-04","MAG","Non-SPASS","Titan","MAGTITAN","MAG Titan observation","T38 flyby","T38 is a southern polar flyby at a close flyby distance of 1300 km. It is at the transition from the southern wing/outer flank region. We assign grade one priority.  NOTE: - continuous data rate of 1976bps (32vps)."]
["2007-338T23:16:50","000T00:35:00","2007-12-04","CIRS","SPASS Rider","Titan","FIRLMBT","Far Infrared limb tracking","ISS_PHOT_1x1","ISS WAC support imaging, 2 images per integration (3 integrations total = 6 frames, 0.5 Mb/frame)"]
["2007-339T02:06:50","000T21:59:23","2007-12-05","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SURVEY Campaign","Part of SURVEY MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2007-340T09:29:00","000T14:45:56","2007-12-06","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_SURVEY","Continuous low-rate magnetospheric survey"]
["2007-341T11:00:00","000T10:30:00","2007-12-07","CAPS","Prime","Sun","SWAURPTG","MAPS aurora campaign","CAPS Control Pointing during Ring Sat Campaign","Part of  MB,C  MAPS Campaign.  Observe dusk-side magnetospheric boundaries at a variety of latitudes"]
["2007-341T22:00:00","000T01:30:00","2007-12-07","ISS","Prime","rings(general)","PHOTOMDRK","Photometry map","Ring photometry","WAC 1x3 mosaic of entire ring system in multi-colors"]
["2007-344T19:45:00","000T03:15:00","2007-12-10","UVIS","SPASS Rider","rings(general)","APOMOSAIC","Apoapsis mosaic"]
["2007-347T16:25:00","000T01:00:00","2007-12-13","RSS","Prime","Earth","BORESIGHT","HGA boresight calibration","HGA Boresight Calibration","HGA Boresight Calibration; Pointing=XBAND to Earth + crosshair maneuver. Last hour (crosshair maneuver) required to be tracked at DSS-25 in 1-way mode. Playback of telemetry required afterwards for C-Kernel generation."]
["2007-350T07:01:00","000T03:00:00","2007-12-16","RSS","SPASS Rider","Saturn","OCCORT","Operations Readiness Test to demonstrate DSN and RSSG preparedness to support upcoming occultations","RSS Operational Readiness Test","RSS Operations Readiness Test (ORT), to demonstrate DSN and RSSG preparedness to support the Rings/Saturn Occultation experiment on DOY 353."]
["2007-351T21:46:00","000T01:00:00","2007-12-17","ISS","Prime","Rhea","REGGEOD","Regional geodesy","Rhea regional geodesy","Turn -Y to Rhea; Do 1x1 mosaic in NAC clear filter twice."]
["2007-352T17:55:00","000T06:40:00","2007-12-18","MAG","Non-SPASS","co-rotation","RNGSAT","Ring / Satellite","MAG MAPS RS Campaign","Observe Saturns inner magnetosphere and the interactions between icy satellites rings and the magnetosphere. Measure properties of a statistically significant number of satellite L-shell crossings distributed among the satellites and in longitudinal distance from the satellites."]
["2007-353T00:31:00","000T00:55:00","2007-12-19","VIMS","SPASS Rider","Rhea","FP1FAZ0P5","CIRS FP1 phase coverage","Rhea CIRS FP1","VIMS ride with CIRS FP1.  specfiics TBD assume 55 min ar ~6 kbits/sec ~  21 Mbits for a full FOV long+short integration"]
["2007-353T05:25:00","000T01:11:00","2007-12-19","CIRS","SPASS Rider","Saturn","OCCLIMB","Occultation","CIRS_054SA_OCCLIMB SI","obtain stratospheric thermal structure by means of limb sounding in the mid-IR, latitude coverage.  POINTING: -y to Saturn, z to limb"]
["2007-353T20:16:00","000T05:30:00","2007-12-19","UVIS","SPASS Rider","rings(general)","SUBML08LP","Ring radial scan"]
["2007-354T20:57:55","000T01:00:00","2007-12-20","CAPS","SPASS Rider","Titan","T39INBND",null,"MAPS 054TI(T39) Campaign","Part of 054TI(T39) MAPS Campaign.  Inbound approach observations and context for the interaction between Titan and Saturn's magnetosphere"]
["2007-355T04:02:55","000T03:55:00","2007-12-21","VIMS","SPASS Rider","Titan","MIRLMBINT","Mid infrared limb integration","Limb Map","Ridealong with CIRS Limb Map Template F"]
["2007-355T09:57:55","000T02:00:00","2007-12-21","ISS","Prime","Titan","MONITORNA","Monitoring of surface and atmosphere","NMA (NAC Monitoring of Surface and Atmosphere)","monitoring for surface/atmosphere changes; attempt to see surface color variations; monitor limb hazes, 1-3 km/px"]
["2007-356T08:57:00","003T06:20:00","2007-12-22","MAG","Non-SPASS","Sun","MAGBOUND","MAPS magnetosphere boundary campaign","MAG MAPS MB D Campaign","Observer magnetospheric boundaries near noon on highly inclined orbits. (MB D-assigned to MAPS)"]
["2007-359T15:47:00","000T11:00:00","2007-12-25","VIMS","SPASS Rider","Saturn","MIRMAP","Mid infrared map","Saturn Feature Track","Saturn Global Map and Feature Track, rider with CIRS MIRMAP"]
["2007-361T01:27:43","001T13:49:17","2007-12-27","RPWS","Non-SPASS","Sun","MAGBOUND","MAPS magnetosphere boundary campaign","MAPS MB,D Campaign","Part of MB,D MAPS Campaign.  Observe magnetospheric boundaries near noon on highly inclined orbits"]
["2007-362T06:17:00","000T09:00:00","2007-12-28","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2007-364T14:50:00","001T15:05:00","2007-12-30","MAG","Non-SPASS","Sun","MAGBOUND","MAPS magnetosphere boundary campaign","MAG MAPS MB D Campaign","Observer magnetospheric boundaries near noon on highly inclined orbits. (MB D-assigned to MAPS)"]
["2008-001T15:33:00","000T02:45:00","2008-01-01","CIRS","Prime","rings(general)","TEMPU33MP","Thermal map","CIRS_055RI_TEMPU33MP","Radial scan of main rings to obtain temperature measurement of rings at a variety of geometries.  -Y to rings, Z perp to rings"]
["2008-002T03:02:00","001T18:35:59","2008-01-02","MIMI","SPASS Rider","Saturn","MAGDYN","MAPS magnetosphere dynamics campaign","MAPS IM/DYN Campaign","Part of IM/DYN MAPS Campaign.   Image the dynamics of the inner magnetosphere in ENA with MIMI/INCA. With -Y pointed toward Saturn, corotation as close to the S/C -X, +/- Z plane as possible."]
["2008-003T16:47:26","000T00:40:00","2008-01-03","CDA","Non-SPASS","DustRAM direction","0623SURIN","Dust survey","Dust survey inside 8 Rs 22.50<lat< 25.00 deg 6.20.","Dust survey inside 8 Rs$ 1281.6996$ 1281.7274$ 6.289 to 6.253 Rs lat: 24.944 to 24.703 deg ring-alt: 160023. to 157644.km 004OF005 yes ADJ: 35 was:2008-003T17:05:20...2008-003T17:09:33,pointing=CDA to Kepler RAM,rate=200,dataVolume=0.457"]
["2008-003T22:05:00","000T07:00:00","2008-01-03","MAG","SPASS Rider","Other","INTFLD","MAG Internal field observation","MAG_Internal_Field_Measurements","This request will yield unique observations of Saturns internal magnetic field over a unique orbit track in latitude and longitude space."]
["2008-004T03:15:00","000T00:38:40","2008-01-04","CIRS","SPASS Rider","InstrumentCalibration","INMAGCOMP","Inner magnetospheric composition","CIRS_055IC_INMAGCOMP001_INMS","Calibration rider.  Data Volume will be 9.28 Mb or less."]
["2008-005T11:30:20","000T01:00:00","2008-01-05","ISS","Prime","Titan","PHOTOMWAC","Photometry map","WPH (WAC Photometry)","particle properties, vertical distributions ~6 km/px.  0.6 Mbit/frame with 2x2 summing. special S/C orientation requested."]
["2008-005T18:30:20","000T01:00:00","2008-01-05","CIRS","SPASS Rider","Titan","NIGHTWAC","ISS lightning / aurora observation",null,"Obtain information on CO, HCN, CH4. Integrate on disk at airmass 1.5--2.0."]
["2008-005T20:30:20","000T02:00:00","2008-01-05","MIMI","SPASS Rider","Titan","T40CLOSE",null,"MAPS 055TI(T40) Campaign","Part of 055TI(T40) MAPS Campaign.   Investigate micro-scale and near aspects of the Titan interaction by observing during about one hour period around an encounter. With -Y pointed toward Titan, when within 30 minutes of the targeted flyby, optimize secondary axis for corotation flow as close to the S/C -X, +/- Z plane as works with the other constraints on pointing. Also, measure Titan exosphere/magnetosphere interaction by imaging in ENA with INCA (when sun is not in INCA FOV)."]
["2008-005T22:30:20","000T11:00:00","2008-01-05","INMS","Non-SPASS","Titan","T40OUTBD",null,"MAPS TOST Campaign","Part of the MAPS/TOST Campaign. Determine atmospheric and ionospheric thermal structure."]
["2008-006T09:25:11","000T12:03:49","2008-01-06","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey."]
["2008-008T05:33:00","000T09:00:00","2008-01-08","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2008-008T15:03:00","000T01:12:00","2008-01-08","UVIS","SPASS Rider","Rhea","ICYLON","Icy satellite longitudinal coverage","ICYLON rider"]
["2008-010T20:49:00","000T07:00:00","2008-01-10","CIRS","SPASS Rider","rings(general)","APOMOSAIC","Apoapsis mosaic","CIRS_056RI_APOMOSAIC001","null"]
["2008-012T20:30:00","000T17:34:00","2008-01-12","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2008-014T01:05:00","000T00:30:00","2008-01-14","VIMS","SPASS Rider","Saturn","POLRMOV01","Saturn polar movie","TBD","TBD"]
["2008-014T17:05:00","000T00:30:00","2008-01-14","VIMS","SPASS Rider","Saturn","POLRMOV02","Saturn polar movie","TBD","TBD"]
["2008-015T07:05:00","000T02:55:00","2008-01-15","CIRS","Prime","rings(general)","TEMPU45MP","Thermal map","CIRS_056RI_TempU45MP","Afternoon radial scan of main rings to obtain thermal measurement of rings.  -Y to rings, Z perp to rings"]
["2008-015T19:54:00","000T01:00:00","2008-01-15","RPWS","Non-SPASS","rings(general)","RPXING","Measurements of dust flux, scale height and plasma waves at the magnetic equator during ring plane crossing","RPWS Ring Plane Crossing","Determine the equatorial dust flux and scale height as a function of radial distance.  Obtain high resolution of plasma waves at the magnetic equator."]
["2008-015T20:25:22","000T00:07:54","2008-01-15","CDA","Non-SPASS","DustRAM direction","0302DUST","Dust survey","E Ring dense - survey - 1.50<lat< 2.59 deg 3.41...","E Ring dense - survey - $ 1293.8517 $ 1293.8557 $ 3.432 to 3.413 Rs lat: -1.502 to -2.585 deg ring-alt: 5427. to 9288.km,pointing=CDA to Kepler RAM,rate=524,dataVolume=0.172"]
["2008-016T06:08:46","000T02:25:10","2008-01-16","CDA","Non-SPASS","DustRAM direction","0631DUST","Dust survey","Dust survey inside 8 Rs 31.09<lat< 36.95 deg 6.40.","Dust survey inside 8 Rs $ 1294.2561 $ 1294.3569 $ 6.400 to 7.574 Rs lat:-36.951 to -31.087 deg ring-alt: 232091. to 235936.km,pointing=CDA to Kepler RAM,rate=200,dataVolume=1.661"]
["2008-017T07:50:00","000T01:30:00","2008-01-17","ISS","Prime","rings(general)","PHOTOMLIT","Ring photometry","Ring photometry","WAC 1x5 mosaic of the entire system in multi-colors."]
["2008-017T20:45:00","000T00:35:00","2008-01-17","ISS","Prime","Janus","MUTUALEVE","Mutual event satellite transit observation","MUTUAL EVENTS, TRANSIT OF Janus     ACROSS Dione","Turn to satellite, take 1 NAC every ~ minute for duration of event while tracking satellite"]
["2008-017T23:30:00","000T04:20:00","2008-01-17","CIRS","SPASS Rider","rings(general)","DIFFRINGS","Diffuse ring observation","CIRS_056RI_DIFFRINGS001","null"]
["2008-019T01:20:00","000T00:30:00","2008-01-19","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 016 TH OBS","Turn to first satellite, take 1 NAC (CL1,CL2). Turn to second satellite take 1 NAC (CL1,CL2), repeat for up to 8 satellites if visible"]
["2008-022T00:05:00","000T03:00:00","2008-01-22","RADAR","SPASS Rider","Other","NORTHWARM","Distant Titan latitude study warmup","Distant Titan Latitude Study, Northern Latitudes","Warmup for calibration and science data collection."]
["2008-022T13:40:00","000T00:02:00","2008-01-22","CIRS","Non-SPASS","InstrumentCalibration","SEQSETUP","CIRS sequence setup activity","CIRS S37 Sequence Setup","Enforce CIRS science no-data state, load tables (IEBs) from the SSR, set the focal plane assembly set point"]
["2008-024T13:20:00","000T05:25:04","2008-01-24","MAG","Non-SPASS","Sun","MAGBOUND","MAPS magnetosphere boundary campaign","MAG MAPS MB D Campaign","Observer magnetospheric boundaries near noon on highly inclined orbits."]
["2008-026T13:20:00","000T01:10:00","2008-01-26","UVIS","SPASS Rider","Star","URNUCEN","Stellar occultation","Support Imaging","NAC and WAC images at the following times: (TIMES TBD, desired when star is on either side of F ring, and behind  F ring core.)"]
["2008-026T15:30:00","000T01:30:00","2008-01-26","UVIS","Prime","Star","URIOTCEN","Stellar occultation","URSTAR","3rd in series of 8 stellar occs. Turn to this star directly from previous star (SAO 205839). Turn directly to next star, not the waypoint, after this occ."]
["2008-027T05:35:00","000T07:18:58","2008-01-27","RPWS","Non-SPASS","Saturn","INSURVEY","Inner magnetosphere survey","RPWS Inner Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2008-027T19:13:10","000T00:45:21","2008-01-27","CDA","Non-SPASS","DustRAM direction","0305DUST","Dust survey","E-Ring Margin - survey - 5.19<lat< 15.39 deg 3.28.","E-Ring Margin - survey - $ 1305.8015 $ 1305.8323 $ 3.376 to 3.280 Rs lat: -5.192 to -15.389 deg ring-alt: 18430. to 52506.km,pointing=CDA to Kepler RAM,rate=524,dataVolume=1.330"]
["2008-027T22:20:00","000T02:55:00","2008-01-27","VIMS","Prime","Star","ALPAUROCC","Alpha Aur occultation","alpAur","Alp Aur Ring occ and Saturn occ; duration = 2:30 + 0:45 = 3:15"]
["2008-028T07:51:00","000T08:25:27","2008-01-28","CDA","Non-SPASS","DustRAM direction","0817DUST","Dust survey","Dust survey outside 8 Rs 16.66<lat< 29.17 deg 7.98","Dust survey outside 8 Rs $ 1306.3271 $ 1306.6781 $ 7.979 to 11.597 Rs lat:-29.174 to -16.664 deg ring-alt: 234656. to 200625.km,pointing=CDA to Kepler RAM,rate=200,dataVolume=5.784"]
["2008-030T04:05:00","000T09:00:00","2008-01-30","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2008-031T15:00:00","000T11:45:00","2008-01-31","CIRS","SPASS Rider","InstrumentCalibration","MAGBNDPTG","MAPS magnetosphere boundary campaign","CIRS_057IC_MAGBNDPTG001_CAPS","Calibration rider.  Data Volume will be 169.2 Mb or less."]
["2008-033T02:45:00","000T00:30:00","2008-02-02","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 022 TH OBS","Turn to first satellite, take 1 NAC (CL1,CL2). Turn to second satellite take 1 NAC (CL1,CL2), repeat for up to 8 satellites if visible"]
["2008-034T21:21:00","000T02:40:00","2008-02-03","CAPS","Prime","Sun","MAGBNDPTG","MAPS magnetosphere boundary campaign","CAPS Control Pointing during MAG BND Campaign","Part of  MB,C  MAPS Campaign.  Observe dusk-side magnetospheric boundaries at a variety of latitudes"]
["2008-037T05:36:00","000T13:00:00","2008-02-06","UVIS","Prime","Saturn","NAURMOV","Saturn north pole movie","North Auroral Movie","Repeated UVIS scans across the north polar region of Saturn to produce an auroral movie"]
["2008-039T05:21:00","000T10:04:00","2008-02-08","CIRS","SPASS Rider","rings(general)","SUBRADARU","Ring radial scan","CIRS_058RI_SUBRADARU001_SI"]
["2008-039T17:28:03","000T00:10:12","2008-02-08","CDA","Non-SPASS","RingE","0300ERNGX","Ring plane crossing","E Ring Xing 0.00<lat< 1.00 deg 3.38... 3.62 Rs v2.","E Ring Xing$ 1317.7314$ 1317.7349$ 3.436 to 3.436 Rs lat: -0.022 to -0.022 deg ring-alt: 80. to 80.km 010OF011 yes ADJ: 4 was:2008-039T17:35:34...2008-039T17:35:58,pointing=CDA to Kepler RAM,rate=524,dataVolume=0.149"]
["2008-039T19:14:00","000T01:01:00","2008-02-08","VIMS","Prime","Dione","DIONE","Dione","Dione","42i2-63v3 80ms, 640 ms (13 min/cycle) repeat 4 times."]
["2008-039T21:45:00","000T08:52:28","2008-02-08","INMS","Non-SPASS","Saturn","INMAGSURV","Observing neutral molecules in the inner magnetosphere","MAPS Survey","MAPS magnetospheric survey."]
["2008-041T04:36:00","000T15:17:20","2008-02-10","CAPS","Non-SPASS","Saturn","BURST4K","4 kbps burst","Burst of 4kbps data","Burst of 16 kbps data (which gives uncollapsed ELS data). 32 B cycles duration. Data is in addition to 1000 bps from SWSKR."]
["2008-041T18:24:59","000T02:00:00","2008-02-10","CDA","Non-SPASS","Titan","2000TIORX","Titan orbit crossing","Titan Orbit Xing 0.00<lat< 0.60 deg 20.12... 20.42","Titan Orbit Xing$ 1319.7674$ 1319.8507$ 20.124 to 20.399 Rs lat: 0.086 to 0.521 deg ring-alt: 1822. to 11190.km 028OF031 no ADJ: 50 was:2008-041T18:50:27...2008-041T19:59:32,pointing=CDA to Kepler RAM,rate=200,dataVolume=1.373"]
["2008-043T12:06:00","000T07:30:00","2008-02-12","MAG","Non-SPASS","Sun","MAGBOUND","MAPS magnetosphere boundary campaign","MAG MAPS MB D Campaign","Observer magnetospheric boundaries near noon on highly inclined orbits."]
["2008-046T12:51:00","000T13:30:00","2008-02-15","UVIS","Prime","Saturn","MOS59APO","Saturn inner magnetosphere mosaic","MOSAIC_APO_59_59","Mosaic of Saturn inner magnetosphere.  EUV and FUV low resolution slits on, perpendicular to the orbital plane. 1) Slew about the Z-axis from Saturn Center to -MOS Orb. Rotate +300mrad in the YZ Plane. 2) Drift at a rate of .1913 mrad/s about the Z-axis for 5650s to +MOS Orba. 3) Rotate -300mrad in the YZ plane. Drift at indicated rate about the Z-axis for 5650s to -MOS Orb. 4) Rotate -300mrad in the YZ plane. Drift at indicated rate about the Z-axis for 5650s to +MOS Orba. 5) Drift at indicated rate about the Z-axis for 5650s to -MOS Orb. 6) Rotate +300mrad in the YZ plane. Drift at indicated rate about the Z-axis for 5650s to +MOS Orba. 7) Rotate +300mrad in the YZ plane. Drift at indicated rate about the Z-axis for 5650s to -MOS Orb. 8) Drift at indicated rate about the Z-axis for 5650s to +MOS Orba. 9) Rotate -300mrad in the YZ plane. Drift at indicated rate about the Z-axis for 5650s to -MOS Orb. 10) Drift at indicated rate about the Z-axis for 1650s toward +MOS Orba. 11) Slew back to Saturn Center and reset pointing. Stare for remaining observation time.  -MOS orb (-range): -784.41mrad, +MOS Orb (+range): 296.70mrad."]
["2008-047T11:51:00","001T07:03:56","2008-02-16","MIMI","SPASS Rider","Sun","MAGBOUND","MAPS magnetosphere boundary campaign","MAPS MB/D Campaign","Part of MB/D MAPS Campaign.   Observer magnetospheric boundaries near noon on highly inclined orbits. Set up MIMI for magnetospheric boundaries campaign Pointing: -X to sun and/or corotation, internal B in X, Z plane; or spin about Z."]
["2008-048T12:21:00","000T13:45:00","2008-02-17","ISS","SPASS Rider","RingF","FMOVIE","F ring movie","F RING OBSERVATION RIDING ALONG WITH VIMS","F ring rider observation"]
["2008-050T12:06:00","000T08:30:00","2008-02-19","UVIS","SPASS Rider","Saturn","POLRMOV04","Saturn polar movie"]
["2008-051T14:49:58","000T01:42:01","2008-02-20","CDA","Non-SPASS","DustRAM direction","0409DUST","Dust survey","Dust survey inside 8 Rs 8.73<lat< 30.15 deg 3.64..","Dust survey inside 8 Rs $ 1329.6187 $ 1329.7250 $ 4.673 to 3.636 Rs lat: 30.150 to 8.725 deg ring-alt: 141593. to 33278.km,pointing=CDA to Kepler RAM,rate=200,dataVolume=1.751"]
["2008-051T18:40:00","000T00:15:00","2008-02-20","RPWS","Non-SPASS","Saturn","WHISTLER","RPWS lightning search","Obtain wideband examples of lightning whistlers","Obtain wideband evidence of lightning whistlers.  These would verify the existence of lightning already suspected from Saturn Electrostatic Discharges (SED) and would provide information on the electron density along the field line to the source.  No pointing requirement."]
["2008-052T07:08:32","000T03:27:57","2008-02-21","CDA","Non-SPASS","DustRAM direction","0823DUST","Dust survey","Dust survey outside 8 Rs 23.30<lat< 29.51 deg 7.99","Dust survey outside 8 Rs $ 1330.2976 $ 1330.4420 $ 7.995 to 9.583 Rs lat:-29.509 to -23.297 deg ring-alt: 237574. to 228643.km,pointing=CDA to Kepler RAM,rate=200,dataVolume=2.379"]
["2008-053T03:51:01","000T11:41:06","2008-02-22","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SURVEY Campaign","Part of SURVEY MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2008-053T07:32:07","000T01:00:00","2008-02-22","VIMS","SPASS Rider","Titan","PHOTMAP","Photometry map","Photometry Map","Ridealong with ISS Photometry Map Template N"]
["2008-053T18:55:07","000T00:23:00","2008-02-22","UVIS","SPASS Rider","SpacecraftActivity","DFPWBIAS0",null,"Titan Occults  ETA CMa","UVIS FUV Occultation slit boresite on star for the entire time.  Note:  Start time may change depending on trajectory updates. duration includes half hour turns on each end."]
["2008-054T04:32:07","000T02:00:00","2008-02-23","CIRS","SPASS Rider","Titan","MONITORNA","Monitoring of surface and atmosphere",null,"Obtain information on the thermal structure of Titan's stratosphere. Slew across disk at 4 microrad/s."]
["2008-054T23:42:07","000T01:45:00","2008-02-23","ISS","SPASS Rider","Titan","TEMPMAP","Thermal map","RCI (Ridealong context Imaging)","ISS on, max data rate = 182.784 kbps, number of frames and bits/frame are input parameters, data volume = number of frames x bits/frame, average data rate = data volume/duration."]
["2008-056T11:06:00","000T00:30:00","2008-02-25","CIRS","SPASS Rider","InstrumentCalibration","DEEPSPACE","Deep space calibration",null,"rider"]
["2008-056T22:23:38","004T20:16:22","2008-02-25","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey"]
["2008-059T01:21:00","000T00:30:00","2008-02-28","CIRS","SPASS Rider","InstrumentCalibration","DEEPSPACE","Deep space calibration",null,"rider"]
["2008-059T15:21:00","000T04:33:04","2008-02-28","CAPS","Non-SPASS","Saturn","BURST16K","16 kbps burst","Burst of 16kbps data","Burst of 16kbps data"]
["2008-061T10:51:00","000T07:49:00","2008-03-01","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_SURVEY","Continuous low-rate magnetospheric survey"]
["2008-061T18:17:00","000T06:15:00","2008-03-01","RPWS","Non-SPASS","Saturn","AURXNG","Aurora and Saturn Kilometric Radiation","MAPS AS Campaign","Part of AS MAPS Campaign.  Observe the auroral magnetosphere (e.g. the acceleration region) and SKR source regions"]
["2008-062T01:56:00","000T00:54:00","2008-03-02","INMS","Non-SPASS","Saturn","PTOTM146","MAPS survey","MAPS Survey","MAPS magnetospheric survey."]
["2008-062T03:38:53","000T00:11:56","2008-03-02","CDA","Non-SPASS","Enceladus","0400ENORX","Enceladus orbit crossing","Enceladus Orbit Xing 0.00<lat< 0.50 deg 3.85... 4.","Enceladus Orbit Xing$ 1340.1527$ 1340.1596$ 3.920 to 3.920 Rs lat: -0.430 to -0.430 deg ring-alt: 1775. to 1775.km 019OF020 yes ADJ: 9 was:2008-062T03:44:39...2008-062T03:45:03,pointing=CDA to Kepler RAM,rate=524,dataVolume=0.299"]
["2008-062T08:10:00","000T02:30:00","2008-03-02","CAPS","SPASS Rider","Saturn","AURXNG","Aurora and Saturn Kilometric Radiation","MAPS AS Campaign","Part of AS MAPS Campaign.  Observe the auroral magnetosphere (e.g. the acceleration region) and SKR source regions"]
["2008-063T10:36:00","002T07:14:13","2008-03-03","INMS","Non-SPASS","co-rotation","PTOTM146B","MAPS survey","MAPS TI/DT Campaign","Part of TI/DT MAPS Campaign.  Measure the properties of the Titan torus and Titan interaction at large distances from Titan"]
["2008-064T11:15:00","000T00:30:00","2008-03-04","CIRS","SPASS Rider","Other","SATELLORB","Satellite orbit campaign",null,"rider"]
["2008-066T01:21:00","000T09:00:00","2008-03-06","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2008-066T10:21:00","001T02:38:52","2008-03-06","CDA","Non-SPASS","DustRAM direction","2001DUST","Dust survey","Dust survey 0.94<lat< 22.91 deg 20.37... 27.20 Rs","Dust survey $ 1342.4539 $ 1345.5416 $ 20.374 to 27.201 Rs lat: 0.942 to 22.907 deg ring-alt: 20208. to 638753.km,pointing=CDA to Kepler RAM,rate=150,dataVolume=38.162"]
["2008-067T16:51:00","000T07:00:00","2008-03-07","CIRS","SPASS Rider","rings(general)","APOMOSAIC","Apoapsis mosaic",null,"rider"]
["2008-070T23:36:00","001T03:00:00","2008-03-10","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_SURVEY","Continuous low-rate magnetospheric survey"]
["2008-071T17:35:00","000T01:31:00","2008-03-11","CIRS","SPASS Rider","InstrumentCalibration","DEEPSPACE","Deep space calibration",null,"rider"]
["2008-072T12:26:12","000T02:10:00","2008-03-12","VIMS","SPASS Rider","Enceladus","ENCELADUS","Enceladus","Enceladus targeted","16x16i2v3 160ms, 640 ms (5 min/cycle) repeat 12 each hour."]
["2008-072T18:44:42","000T00:26:30","2008-03-12","CAPS","Prime","Enceladus","ENCLDSPTG",null,"CAPS control of pointing near Enceladus c/a","CAPS control of spacecraft pointing from -19 to +5 min. This request is in addition to the EN_ENCOUNTER request which covers the CAPS data volume"]
["2008-072T18:44:42","000T00:26:30","2008-03-12","CIRS","SPASS Rider","Enceladus","DRAGCIRS","ORS drag secondary axis","Drag CIRS FOVs across disk at closest approach.","CIRS will take data during closest approach when S/C cannot track Enceladus, provided that the INMS orientation permits it.  CIRS to operate all focal planes; 38 RTI (15.5 cm-1 resolution, 4.75 sec frame time). Blink."]
["2008-072T20:56:48","000T00:00:01","2008-03-12","MP","SPASS Note","Saturn","PERIAPSE","Periapse",null,"Periapse R = 3.751 Rs, lat = -23 deg, phase = 149 deg"]
["2008-073T10:20:00","000T00:41:55","2008-03-13","INMS","Prime","Saturn","INMAGCOMP","Inner magnetospheric composition","INMS Inner Magnetospheric Composition","Acceptable time range - Start time 072T13:27:29 to end time 073T04:22:17"]
["2008-074T08:55:00","000T12:05:00","2008-03-14","CIRS","SPASS Rider","rings(general)","LPHRLFMOV","Ansa movie",null,"rider"]
["2008-075T09:51:00","000T15:00:00","2008-03-15","ISS","Prime","rings(general)","LPMRDFMOV","Ansa movie","Ansa movie: low phase med res dark face","Ansa movie F ring.  Point to F ring and dwell for duration."]
["2008-078T09:35:00","001T00:00:00","2008-03-18","INMS","Non-SPASS","Saturn","PTOTM150","MAPS survey","MAPS Survey","MAPS magnetospheric survey."]
["2008-080T09:50:00","000T04:00:00","2008-03-20","UVIS","SPASS Rider","rings(general)","TEMPU47MP","Thermal map","UV Ring Spectroscopy"]
["2008-081T09:50:00","000T13:15:00","2008-03-21","CIRS","SPASS Rider","RingB","VERTULMP","Unlit face radial scan observation","CIRS_062RB_VERTULMP001_SI"]
["2008-082T11:10:00","000T05:10:00","2008-03-22","UVIS","Prime","Star","URZETCEN","Stellar ring occultation","URSTAR"]
["2008-083T04:24:54","000T02:24:58","2008-03-23","CDA","Non-SPASS","DustRAM direction","0534DUST","Dust survey","Dust survey inside 8 Rs 33.76<lat< 44.91 deg 5.19.","Dust survey inside 8 Rs $ 1361.1847 $ 1361.2839 $ 6.195 to 5.187 Rs lat: 44.913 to 33.755 deg ring-alt: 263876. to 173869.km,pointing=CDA to Kepler RAM,rate=200,dataVolume=1.634"]
["2008-083T12:21:18","000T00:12:06","2008-03-23","CDA","Non-SPASS","DustRAM direction","0323SURIN","Dust survey","Dust survey inside 8 Rs 22.50<lat< 25.00 deg 3.20.","Dust survey inside 8 Rs$ 1361.5155$ 1361.5225$ 3.730 to 3.731 Rs lat:-23.022 to -24.075 deg ring-alt: 88018. to 91819.km 009OF013 yes ADJ: 4 was:2008-083T12:24:26...2008-083T12:30:14,pointing=CDA to Kepler RAM,rate=200,dataVolume=0.114"]
["2008-083T18:20:00","000T05:30:00","2008-03-23","CIRS","SPASS Rider","RingB","SHADLLP","Saturn ring shadow observation","CIRS_062RB_SHADLLP001_SI"]
["2008-083T23:54:32","000T00:56:52","2008-03-23","CDA","Non-SPASS","DustRAM direction","0838SURVY","Dust survey","Dust survey 37.50<lat< 40.00 deg 7.70... 8.30 Rs v","Dust survey$ 1361.9969$ 1362.0350$ 7.773 to 8.168 Rs lat:-39.951 to -37.704 deg ring-alt: 301117. to 301371.km 005OF006 no ADJ: 0 was:...,pointing=CDA to Kepler RAM,rate=100,dataVolume=0.313"]
["2008-084T19:20:00","000T06:15:00","2008-03-24","CIRS","SPASS Rider","InstrumentCalibration","DSCAL08","Deep space calibration","CIRS_062IC_DSCAL08484_SP","rider"]
["2008-085T13:37:48","000T00:29:00","2008-03-25","CIRS","SPASS Rider","Titan","FIRLMBT","Far Infrared limb tracking","ISS_PHOT_1x1","ISS WAC support imaging, 2 images per integration (1 integrations total = 2 frames, 0.5 Mb/frame)"]
["2008-085T15:27:48","000T11:00:00","2008-03-25","INMS","Non-SPASS","Titan","T42OUTBD",null,"MAPS TOST Campaign","Part of the MAPS/TOST Campaign. Determine atmospheric and ionospheric thermal structure."]
["2008-085T19:27:48","000T04:00:00","2008-03-25","ISS","SPASS Rider","Titan","MIRLMBMAP","Mid infrared limb map","WPH/NGM/RCI (WAC Photometry,  NAC Global Mapping,","particle properties, vertical distributions ~6 km/px.  0.6 Mbit/frame with 2x2 summing. special S/C orientation requested."]
["2008-086T02:27:48","000T11:59:52","2008-03-26","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey."]
["2008-088T01:28:00","002T20:31:10","2008-03-28","CDA","Non-SPASS","DustRAM direction","1823DUST","Dust survey","Dust survey 23.12<lat< 49.63 deg 17.98... 24.54 Rs","Dust survey $ 1366.0794 $ 1368.9161 $ 24.537 to 17.976 Rs lat: 23.118 to 49.632 deg ring-alt: 581205. to 826261.km,pointing=CDA to Kepler RAM,rate=150,dataVolume=35.060"]
["2008-089T09:20:00","000T14:00:00","2008-03-29","CIRS","SPASS Rider","Saturn","POLRMOV01","Saturn polar movie",null,"rider"]
["2008-091T08:34:00","001T08:51:04","2008-03-31","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_SURVEY","Continuous low-rate magnetospheric survey"]
["2008-092T08:07:00","000T04:28:00","2008-04-01","INMS","Non-SPASS","Saturn","INMAGSURV","Observing neutral molecules in the inner magnetosphere","MAPS Survey","MAPS magnetospheric survey."]
["2008-092T13:50:00","000T05:15:14","2008-04-01","INMS","Non-SPASS","co-rotation","IMVP5M","Inner Magnetosphere vertical profile","MAPS IM/VP Campaign","Part of IM/VP MAPS Campaign.   Measure the vertical structure and dynamics of the inner magnetosphere on orbits nearly tangent to L shells, at a variety of local times and L shells"]
["2008-093T06:05:00","000T02:00:00","2008-04-02","CIRS","SPASS Rider","rings(general)","SPOKE","Ring spoke movie",null,"rider"]
["2008-094T01:35:00","000T04:30:00","2008-04-03","MAG","Prime","Sun","CALROLL","MAG calibration roll","MAG Calibration Rolls","Roll about axis other than Z for determination of sensor offsets, actual roll axis is not important - selected axis is usually suitable for MAPS.  Preferably calibrations should be made every 15-20 days in areas where field conditions are suitable.  Suitable periods for S39 are from : Preferred times (high probability of good calibration) **************************************** None ****************************************  Relaxed Times (lower probability of good calibration) **************************************** START POSSIBLE CALROLL PERIOD 23 : 2008-084T15:00:00 END POSSIBLE CALROLL PERIOD: 23 : 2008-084T21:00:00 **************************************** START POSSIBLE CALROLL PERIOD 24 : 2008-094T00:00:00 END POSSIBLE CALROLL PERIOD: 24 : 2008-094T09:00:00 **************************************** START POSSIBLE CALROLL PERIOD 25 : 2008-103T15:00:00 END POSSIBLE CALROLL PERIOD: 25 : 2008-104T00:00:00 ****************************************  Note: periods of suitable data are defined as follows; 1) More distant than 15 RS from Saturn's axis (to try and get into the more uniform part of the internal+sheet field). 2) Inside the magnetopause (more specifically inside a most compressed model MP). 3) More distant than 3 RS from the current sheet. Using a 'hinged' sheet model which departs from Saturn's equatorial plane at about 15 RS and then follows the anti-solar direction on the nightside. This means that, even though its orbit is equtorial, if the spacecraft is situated far enough away from the planet, it should see the nightside current sheet divert northwards away from it (using Saturn axis tilted 17 deg away from Sun).  Apart from possible injection events, sheet disruptions etc the resultant periods should have a reasonable probability of seeing a 'quiescent' 'lobe-like' or 'disk-like' field. We would prefer as far downtail as possible so the field has more chance of pointing in a single direction over larger length scales."]
["2008-094T13:33:18","000T07:08:16","2008-04-03","CDA","Non-SPASS","DustRAM direction","1705DUST","Dust survey","Dust survey outside 8 Rs 4.84<lat< 9.68 deg 16.75.","Dust survey outside 8 Rs $ 1372.5648 $ 1372.8622 $ 16.747 to 18.296 Rs lat: -9.683 to -4.840 deg ring-alt: 169934. to 93133.km,pointing=CDA to Kepler RAM,rate=200,dataVolume=4.901"]
["2008-095T11:20:00","000T01:00:00","2008-04-04","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 007 TH OBS","Turn to first satellite, take 1 NAC (CL1,CL2). Turn to second satellite take 1 NAC (CL1,CL2), repeat for up to 8 satellites if visible"]
["2008-096T21:40:00","000T01:08:16","2008-04-05","CAPS","Non-SPASS","Saturn","BURST4K","4 kbps burst","Burst of 4kbps data","Burst of 4 kbps data (which gives uncollapsed ELS data). 110 B cycles duration. Data is in addition to 1000 bps from SWSKR."]
["2008-098T00:04:00","000T08:00:00","2008-04-07","CIRS","SPASS Rider","InstrumentCalibration","DSCAL08","Deep space calibration","CIRS_064IC_DSCAL08098_SP","rider"]
["2008-098T08:04:00","000T00:30:00","2008-04-07","CIRS","SPASS Rider","InstrumentCalibration","DEEPSPACE","Deep space calibration",null,"rider"]
["2008-099T18:34:00","000T04:00:00","2008-04-08","CIRS","SPASS Rider","Saturn","1X2WPH60","Photopolarimetry",null,"rider"]
["2008-100T23:04:00","000T09:00:00","2008-04-09","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2008-101T19:04:00","000T09:00:00","2008-04-10","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2008-102T14:10:00","000T07:10:00","2008-04-11","CIRS","SPASS Rider","rings(general)","AZSCAN","Azimuthal ring scan",null,"rider, FP1 and FP3 only"]
["2008-103T07:48:00","000T00:32:00","2008-04-12","CIRS","SPASS Rider","InstrumentCalibration","DEEPSPACE","Deep space calibration",null,"rider"]
["2008-103T08:20:00","000T01:30:00","2008-04-12","VIMS","SPASS Rider","Rhea","RHEA","Rhea","Rhea","36i2-54v3 80ms, 640 ms (10 min/cycle) repeat"]
["2008-104T12:48:05","002T16:17:55","2008-04-13","CDA","Non-SPASS","DustRAM direction","1904DUST","Dust survey","Dust survey 3.56<lat< 22.94 deg 18.67... 24.48 Rs","Dust survey $ 1382.5334 $ 1385.2116 $ 18.675 to 24.482 Rs lat: -3.562 to 22.944 deg ring-alt: 69997. to 575771.km,pointing=CDA to Kepler RAM,rate=150,dataVolume=33.101"]
["2008-107T04:56:04","000T00:00:01","2008-04-16","MP","SPASS Note","Saturn","APOAPSE","Apoapse",null,"Apoapse  Per = 9.6 d, inc = 63.1 deg, r = 24.493 Rs, phase = 30 deg"]
["2008-109T22:18:00","000T09:00:00","2008-04-18","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2008-110T08:39:00","000T00:58:45","2008-04-19","INMS","Non-SPASS","Saturn","FLRATESCN","Full rate scan","MAPS Survey","Startup sequence. Load FSW, MRO, Load IEB from SSR's, MRO"]
["2008-111T00:17:00","000T07:00:00","2008-04-20","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2008-111T16:58:36","000T03:46:24","2008-04-20","RPWS","Non-SPASS","Saturn","SEDDF","Saturn Electrical Discharge direction finding","SED Direction-finding","Perform direction-finding on SED to a) verify source in Saturn's atmosphere (or refute this and find source in rings), and b) if source is in atmosphere, use location to characterize the location of thunderstorms.  Need to do this inside 6 RS on at least half of the periapses inside of 6RS.  No pointing requirement"]
["2008-111T22:15:00","000T01:50:00","2008-04-20","CIRS","SPASS Rider","RingB","SPOKEHIPH","High phase ring spoke observation",null,"rider"]
["2008-112T12:00:00","000T02:30:00","2008-04-21","ISS","Prime","Other","RETARGEMR","Retargetable observation","DETERMINING THE ORBITS OF NEWLY DISCOVERED RING GA","Need several 0.5 hr blocks out of the nominal 8 hr request. Each observation is turn to satellite, take 3x1 BOTSIM mosaic(6 images 24 Mbits each)"]
["2008-113T23:02:00","000T08:00:00","2008-04-22","CIRS","SPASS Rider","InstrumentCalibration","DSCAL08","Deep space calibration","CIRS_065IC_DSCAL08113_SP","rider"]
["2008-115T16:32:00","000T03:59:00","2008-04-24","UVIS","SPASS Rider","rings(general)","TEMPU15LP","Thermal map","UV Ring Spectroscopy"]
["2008-116T08:32:00","000T04:00:00","2008-04-25","ISS","Prime","rings(general)","SILHDFLPH","Ring limb observation","OBS OF THE RING AGAINST THE LIMB AT LOW PHASE","A 1x10 MOSAIC OF RING AGAINST LIMB AT LOW PHASE, 6 COLOUR"]
["2008-117T06:47:00","000T00:30:00","2008-04-26","CIRS","SPASS Rider","InstrumentCalibration","DEEPSPACE","Deep space calibration",null,"rider"]
["2008-119T16:30:14","001T11:39:46","2008-04-28","CDA","Non-SPASS","DustRAM direction","0748DUST","Dust survey","Dust survey outside 8 Rs 47.59<lat< 50.67 deg 6.61","Dust survey outside 8 Rs $ 1397.6884 $ 1399.1729 $ 17.521 to 6.614 Rs lat: 50.673 to 47.591 deg ring-alt: 817645. to 294633.km,pointing=CDA to Kepler RAM,rate=200,dataVolume=24.463"]
["2008-121T00:00:00","000T09:00:00","2008-04-30","RPWS","Non-SPASS","Saturn","AURXNGIN","Aurora and Saturn Kilometric Radiation","Auroral Campaign","Observe the auroral magnetosphere (e.g. the acceleration region) and SKR source regions"]
["2008-121T10:20:00","000T01:10:00","2008-04-30","MIMI","SPASS Rider","DustRAM direction","INCADUST","MIMI INCA dust observation","MAPS RS Campaign","Part of RS MAPS Campaign.   Spacecraft must be pointed such that the dust ram is not entering the INCA FOV. Required to satisfy FR76C3. This means INCA boresight (in S/C X, Y plane, 9.5 deg toward +X from -Y) >70 deg from dust ram."]
["2008-122T08:30:00","000T05:00:00","2008-05-01","CIRS","SPASS Rider","rings(general)","SPKHRLPLF","Ring spoke campaign",null,"rider"]
["2008-123T14:40:00","000T05:05:00","2008-05-02","CIRS","SPASS Rider","rings(general)","SPKSTFORM","Ring spoke campaign",null,"rider"]
["2008-124T06:16:00","000T00:30:00","2008-05-03","CIRS","SPASS Rider","InstrumentCalibration","DEEPSPACE","Deep space calibration",null,"rider"]
["2008-126T07:42:09","002T09:04:51","2008-05-05","MIMI","SPASS Rider","Saturn","MAGDYN","MAPS magnetosphere dynamics campaign","MAPS IM/DYN Campaign","Part of IM/DYN MAPS Campaign.   Image the dynamics of the inner magnetosphere in ENA with MIMI/INCA. With -Y pointed toward Saturn, corotation as close to the S/C -X, +/- Z plane as possible."]
["2008-127T23:00:00","000T21:30:00","2008-05-06","UVIS","SPASS Rider","Saturn","POLEMOV01","Saturn polar movie","ISS Saturn Rider","UVIS EUV and FUV riding along with ISS observation"]
["2008-129T06:00:00","000T10:20:00","2008-05-08","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Inner Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2008-130T18:02:41","000T03:12:34","2008-05-09","CDA","Non-SPASS","DustRAM direction","0526DUST","Dust survey","Dust survey inside 8 Rs 26.31<lat< 44.78 deg 5.23.","Dust survey inside 8 Rs $ 1408.7526 $ 1408.8849 $ 6.360 to 5.232 Rs lat: 44.782 to 26.312 deg ring-alt: 270265. to 139920.km,pointing=CDA to Kepler RAM,rate=200,dataVolume=2.180"]
["2008-131T03:05:00","000T03:15:00","2008-05-10","ISS","Prime","rings(general)","RDHRSSCHP","High resolution radial scan of ring system","High res radial scan of the main rings","HI RES RAD SCAN OF MAIN RINGS"]
["2008-131T16:20:00","000T01:00:00","2008-05-10","UVIS","SPASS Rider","Tethys","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2008-132T17:16:56","000T02:01:58","2008-05-11","CDA","Non-SPASS","DustRAM direction","1610SUOUT","Dust survey","Dust survey outside 8 Rs 10.00<lat< 11.30 deg 16.4","Dust survey outside 8 Rs$ 1410.7208$ 1410.8041$ 16.413 to 16.590 Rs lat:-10.599 to -10.029 deg ring-alt: 182133. to 174301.km 010OF013 no ADJ: 75 was:2008-132T17:55:36...2008-132T18:40:15,pointing=CDA to Kepler RAM,rate=200,dataVolume=1.373"]
["2008-133T09:01:58","000T02:00:00","2008-05-12","INMS","Non-SPASS","Titan","T43CLOSE",null,"MAPS TOST Campaign","Part of the MAPS/TOST Campaign. Determine atmospheric and ionospheric composition and thermal structure."]
["2008-133T15:01:58","000T04:00:00","2008-05-12","CIRS","SPASS Rider","Titan","MIRLMBINT","Mid infrared limb integration","ISS_PHOT_1x1","ISS WAC support imaging, 2 images per integration (4 integrations total = 8 frames, 0.5 Mb/frame)"]
["2008-134T22:14:00","000T01:59:05","2008-05-13","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2008-135T00:13:53","002T23:46:07","2008-05-14","MIMI","SPASS Rider","Saturn","MAGDYN","MAPS magnetosphere dynamics campaign","MAPS IM/DYN Campaign","Part of IM/DYN MAPS Campaign.   Image the dynamics of the inner magnetosphere in ENA with MIMI/INCA. With -Y pointed toward Saturn, corotation as close to the S/C -X, +/- Z plane as possible."]
["2008-136T05:59:00","000T06:00:00","2008-05-15","VIMS","SPASS Rider","rings(general)","SUBMU33LP","Ring radial scan","Slow radial scan, low phase, dark face","Cube Size (X,Z) = 64*12 hires,  IRInt = 640 msec.   Desc = Either 1 slow scan across an entire ring ansa, or  3 shorter scans across A,B, and C rings with interleaved dark skies.   Medium phase, dark side of rings, 7 hi-res cubes = 11.4 Mbit/hour"]
["2008-138T05:29:00","000T07:15:00","2008-05-17","RPWS","Non-SPASS","Saturn","INSURVEY","Inner magnetosphere survey","RPWS Inner Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2008-138T21:22:20","000T00:41:40","2008-05-17","CDA","Non-SPASS","DustRAM direction","0323SURA","Dust survey","Dust survey inside 8 Rs 22.50<lat< 25.00 deg 3.20.","Dust survey inside 8 Rs$ 1416.8905$ 1416.8975$ 3.676 to 3.650 Rs lat: 24.660 to 23.483 deg ring-alt: 92526. to 87735.km 010OF013 yes ADJ: 4 was:2008-138T21:24:26...2008-138T21:30:14,pointing=CDA to Kepler RAM,rate=200,dataVolume=0.114"]
["2008-139T02:05:20","000T10:24:53","2008-05-18","CDA","Non-SPASS","DustRAM direction","0447DUSTA","Dust survey","Dust survey inside 8 Rs 47.46<lat< 53.04 deg 3.64.","Dust survey inside 8 Rs $ 1417.0877 $ 1417.4853 $ 3.643 to 7.823 Rs lat:-53.038 to -47.460 deg ring-alt: 175591. to 347762.km,pointing=CDA to Kepler RAM,rate=200,dataVolume=6.552"]
["2008-139T12:14:00","000T01:00:00","2008-05-18","VIMS","SPASS Rider","Tethys","TETHYS","Tethys","Tethys","12x12 hi/hi 640ms 35 reps 1mrad, 60deg phase"]
["2008-144T05:28:00","000T06:00:00","2008-05-23","VIMS","SPASS Rider","Saturn","NAURMOV","Saturn north pole movie","Saturn North Aurorae Movie UVIS Ridealong","Saturn North Auroral Movie ridealong with UVIS."]
["2008-145T20:58:00","000T08:00:00","2008-05-24","CIRS","SPASS Rider","InstrumentCalibration","DSCAL08","Deep space calibration","CIRS_069IC_DSCAL08145_SP","rider"]
["2008-146T23:14:00","000T02:56:00","2008-05-25","ISS","Prime","Janus","COLORF","Color image","JANUS Color","N09 + 2 WAC GRN (repeat 3 times)"]
["2008-147T14:28:00","000T00:45:00","2008-05-26","UVIS","SPASS Rider","Enceladus","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2008-148T17:24:32","000T02:00:00","2008-05-27","ISS","SPASS Rider","Titan","FIRNADCMP","Far infrared nadir composition map","RCI (Ridealong Context Imaging)","ISS on, max data rate = 182.784 kbps, number of frames and bits/frame are input parameters, data volume = number of frames x bits/frame, average data rate = data volume/duration."]
["2008-149T06:39:32","000T01:15:00","2008-05-28","CAPS","SPASS Rider","Titan","T44INBDN",null,"MAPS Titan inbound period","Part of TI/EE MAPS Campaign.  Investigate large-scale and distant aspects of the Titan interaction by observing during entire period around an encounter from 10 to 25 RS"]
["2008-149T08:09:32","000T00:08:00","2008-05-28","RADAR","Prime","Titan","T44INLSAR",null,"T44 inbound low rate SAR","Inbound low rate SAR of Titan. REU bits included"]
["2008-149T21:24:32","000T01:00:00","2008-05-28","ISS","SPASS Rider","Titan","GLOBMAP","Global coverage mapping","RCI (Ridealong Context Imaging)","ISS on, max data rate = 182.784 kbps, number of frames and bits/frame are input parameters, data volume = number of frames x bits/frame, average data rate = data volume/duration."]
["2008-150T13:12:00","000T08:00:00","2008-05-29","CIRS","SPASS Rider","InstrumentCalibration","DSCAL08","Deep space calibration","CIRS_070IC_DSCAL08550_SP","rider"]
["2008-151T06:42:00","000T20:23:04","2008-05-30","MIMI","SPASS Rider","Titan","TINTERACT","MAPS TI/EE Campaign","MAPS TI/EE Campaign","Part of TI/EE MAPS Campaign.   Investigate large-scale and distant aspects of the Titan interaction by observing during entire period around an encounter from 10 to 25 RS. With -Y pointed toward Titan, when far from Titan (more than 30 minutes to either side of a targeted flyby), measure Titan exosphere/magnetosphere interaction by imaging in ENA with INCA (when sun is not in INCA FOV). Also, optimize secondary axis for corotation flow as close to the S/C -X, +/- Z plane as works with the other constraints on pointing."]
["2008-152T04:27:00","000T00:43:00","2008-05-31","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","Startup sequence. Load FSW, MRO, Load IEB from SSR's, MRO"]
["2008-153T14:42:00","000T01:32:56","2008-06-01","CAPS","SPASS Rider","Saturn","AURXNG3N","Aurora and Saturn Kilometric Radiation","MAPS AS Campaign","Part of AS MAPS Campaign.  Observe the auroral magnetosphere (e.g. the acceleration region) and SKR source regions"]
["2008-153T19:15:00","000T00:44:00","2008-06-01","CIRS","Prime","Saturn","OCCLIMB","Occultation","CIRS_070SA_OCCLIMB005_PRIME;","obtain stratospheric thermal structure at the RSS occultation points.  POINTING: -y to Saturn, z to limb.  Using MAG 2nd of Neg_X to Sun!"]
["2008-154T00:05:04","000T05:27:56","2008-06-02","CAPS","SPASS Rider","Saturn","AURXNG3S","Aurora and Saturn Kilometric Radiation","MAPS AS Campaign","Part of AS MAPS Campaign.  Observe the auroral magnetosphere (e.g. the acceleration region) and SKR source regions"]
["2008-155T17:30:00","000T01:41:00","2008-06-03","CIRS","SPASS Rider","InstrumentCalibration","DEEPSPACE","Deep space calibration",null,"rider"]
["2008-156T12:41:00","003T14:04:00","2008-06-04","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_SURVEY","Continuous low-rate magnetospheric survey"]
["2008-157T20:00:00","000T08:00:00","2008-06-05","CIRS","SPASS Rider","InstrumentCalibration","DSCAL08","Deep space calibration","Deep Space Calibration","Deep space obervations for calibration."]
["2008-158T19:11:00","000T09:00:00","2008-06-06","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2008-160T06:45:00","000T01:05:00","2008-06-08","ISS","Prime","Saturn","AURMOV","Saturn aurora movie","Auroral WAC movie","Auroral WAC movie. one picket in a 2x2 mosaic in five filters. Space pickets evenly."]
["2008-160T18:15:00","000T13:12:00","2008-06-08","MAG","Non-SPASS","Other","INTFLD","MAG Internal field observation","MAG_Internal_Field_Measurements","This request will yield unique observations of Saturns internal magnetic field over a unique orbit track in latitude and longitude space."]
["2008-161T05:45:00","000T05:45:00","2008-06-09","CIRS","SPASS Rider","rings(general)","PAZSCN","Azimuthal ring scan",null,"rider"]
["2008-162T03:20:00","000T00:30:00","2008-06-10","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT DETERMINATION CAMPAIGN, 004 TH OBS","Turn to first satellite, take 1 NAC (CL1,CL2). Turn to second satellite take 1 NAC (CL1,CL2), repeat for up to 8 satellites if visible"]
["2008-162T09:00:00","000T03:30:00","2008-06-10","CIRS","SPASS Rider","rings(general)","SPKFRMMOV","Ring spoke movie",null,"rider"]
["2008-163T04:26:00","000T07:00:00","2008-06-11","CIRS","SPASS Rider","InstrumentCalibration","HSPDARK","Dark sky calibration",null,"rider"]
["2008-164T11:10:00","000T09:00:00","2008-06-12","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2008-166T03:40:00","000T01:30:00","2008-06-14","CIRS","SPASS Rider","InstrumentCalibration","DEEPSPACE","Deep space calibration",null,"rider"]
["2008-167T15:38:00","000T01:07:04","2008-06-15","INMS","Non-SPASS","Saturn","INMAGSURV","Observing neutral molecules in the inner magnetosphere","MAPS Survey","MAPS magnetospheric survey."]
["2008-168T00:30:00","000T04:44:56","2008-06-16","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey"]
["2008-168T06:10:00","000T00:40:00","2008-06-16","CIRS","Prime","Saturn","OCCLIMB","Occultation","CIRS_072SA_OCCLIMB006","obtain stratospheric thermal structure at the RSS occultation points.  POINTING: -y to Saturn, z to limb"]
["2008-170T04:25:00","000T09:00:00","2008-06-18","ISS","Prime","Saturn","ATMOPHASE",null,"Atmospheric Phase behavior using NAC and WAC.","WAC 1X2 and BOTSIMS covering north and south hemispheres and the bright limb of Saturn.  One image in the north and one in the south with 6 mrad overlap.  Left edge of 1X2 WAC should include the sub-spacecraft meridian."]
["2008-170T19:15:00","000T08:00:00","2008-06-18","CIRS","SPASS Rider","InstrumentCalibration","DSCAL08","Deep space calibration","Deep Space Calibration","Deep space obervations for calibration."]
["2008-172T17:09:00","000T01:00:00","2008-06-20","CIRS","SPASS Rider","InstrumentCalibration","DEEPSPACE","Deep space calibration",null,"rider"]
["2008-174T04:39:00","000T07:31:00","2008-06-22","CIRS","Prime","rings(general)","VERTULMP","Unlit face radial scan observation",null,"Radial scans at different local times, unlit face, mid phase -Y to ring, +Z perpendicular to rings"]
["2008-174T14:15:00","000T03:40:00","2008-06-22","VIMS","Prime","Star","GAMCRUOCC","Gamma Cru occultation","gamCru","ingress, same as 70, Phase=0, Dist=0(10^6km)"]
["2008-175T06:17:00","000T00:15:00","2008-06-23","RPWS","Non-SPASS","Saturn","WHISTLER","RPWS lightning search","Obtain wideband examples of lightning whistlers","Obtain wideband evidence of lightning whistlers.  These would verify the existence of lightning already suspected from Saturn Electrostatic Discharges (SED) and would provide information on the electron density along the field line to the source.  No pointing requirement."]
["2008-176T03:39:00","000T09:00:00","2008-06-24","CIRS","SPASS Rider","rings(general)","SUBML25LP","Ring radial scan","CIRS_073RI_SUBML25LP001_SI"]
["2008-177T14:55:00","000T00:34:00","2008-06-25","ISS","Prime","Dione","LOWPHASEX","Low phase imaging","Dione low phase observation","Turn -Y to Dione; Do 1x1 mosaic 5 NAC color + 9 NAC polarizer"]
["2008-178T15:00:00","000T00:30:00","2008-06-26","UVIS","SPASS Rider","Enceladus","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2008-181T04:45:00","000T04:23:00","2008-06-29","VIMS","Prime","Saturn","CYLMAP","Saturn cylindrical map","Saturn Cylindical Map (Third of three).","Saturn Cylindrical Map, third of three."]
["2008-182T01:41:00","000T13:13:00","2008-06-30","MAG","Non-SPASS","Other","INTFLD","MAG Internal field observation","MAG_Internal_Field_Measurements","This request will yield unique observations of Saturns internal magnetic field over a unique orbit track in latitude and longitude space."]
["2008-182T05:25:04","000T04:44:56","2008-06-30","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SURVEY Campaign","Part of SURVEY MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2008-182T10:10:00","000T08:44:56","2008-06-30","INMS","Non-SPASS","Saturn","AURXNG3S","Aurora and Saturn Kilometric Radiation","MAPS AS Campaign","Part of AS MAPS Campaign.  Observe the auroral magnetosphere (e.g. the acceleration region) and SKR source regions"]
["2008-183T11:00:00","000T08:00:00","2008-07-01","CIRS","SPASS Rider","InstrumentCalibration","DSCAL08","Deep space calibration","Deep Space Calibration","rider"]
["2008-185T02:38:00","000T00:32:00","2008-07-03","CIRS","SPASS Rider","InstrumentCalibration","DEEPSPACE","Deep space calibration","CIRS_074IC_DEEPSPACE185_SP","rider"]
["2008-186T02:55:00","000T08:00:00","2008-07-04","CIRS","Prime","rings(general)","SUBMU14LP",null,"CIRS_075RI_SUBMU14LP001_PRIME;","null"]
["2008-187T00:55:00","000T16:00:00","2008-07-05","ISS","SPASS Rider","RingF","FMOVIE","F ring movie","F RING OBSERVATION RIDING ALONG WITH VIMS","F ring rider observation"]
["2008-188T10:37:00","000T07:15:00","2008-07-06","CIRS","SPASS Rider","InstrumentCalibration","DSCAL08","Deep space calibration","CIRS_075IC_DSCAL08188_RIDER","Calibration rider.  Data Volume will be 115.2 Mb or less."]
["2008-189T11:30:00","000T09:15:00","2008-07-07","CAPS","SPASS Rider","Saturn","AURXNG3S","Aurora and Saturn Kilometric Radiation","MAPS AS Campaign","Part of AS MAPS Campaign.  Observe the auroral magnetosphere (e.g. the acceleration region) and SKR source regions"]
["2008-190T00:05:00","000T03:00:00","2008-07-08","VIMS","Prime","rings(general)","COMPLOLIT","Low phase sunlit ring radial scan","radial scan, low phase, lit face.","Cube Size (X,Z) = 64*12 hires, 80 msec, + 320 msec, Time per SC pointing (mins) = 5, Number of SC pointings = 30?  Time of observation (hours) = 3.0"]
["2008-191T17:52:00","000T08:00:00","2008-07-09","CIRS","SPASS Rider","InstrumentCalibration","DSCAL08","Deep space calibration","CIRS_075IC_DSCAL08191_RIDER","Calibration rider.  Data Volume will be 115.2 Mb or less."]
["2008-194T02:22:00","000T11:00:00","2008-07-12","CIRS","Prime","Saturn","FIRMAPC",null,"Far-IR map","Far-IR maps - 3 rotations required, requested as 1st priority (1 of each hemisphere), as discussed at Oct '03 PSG. N. hemisphere, can be split into 11-hr segs., as needed"]
["2008-195T02:20:00","000T21:40:00","2008-07-13","RPWS","Non-SPASS","Saturn","INSURVEY","Inner magnetosphere survey","RPWS Inner Survey","Setup RPWS for inner magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2008-196T05:02:00","000T03:18:00","2008-07-14","CAPS","SPASS Rider","Saturn","AURXNG3N","Aurora and Saturn Kilometric Radiation","MAPS AS Campaign","Part of AS MAPS Campaign.  Observe the auroral magnetosphere (e.g. the acceleration region) and SKR source regions"]
["2008-196T12:12:00","000T04:48:00","2008-07-14","CIRS","Prime","Mimas","ORSSECLN",null,"Mimas ORS and solar eclipse entry FP1SECLN","Combined ORS and eclipse observations.  FP1 observation of Mimas solar eclipse entry.  Duration 06:01.  Begin 10:59:00, eclipse entry 15:46:38 (iDigit), end 17:00:00.  AD=1.81-1.85-1.06, phase=137-54, (-12, 46)-(-48, 19).  FP1+FP3 only.  ________________________ Previous design, comments: Combined ORS and eclipse observations.  FP1 observation of Mimas solar eclipse entry and exit.  Eclipse observation needed because only one other complete Mimas eclipse in Tour.   Entry at 15:47; exit at 18:04.  At entry: AD=1.2 mrad, phase= 54, Local time= , sub S/C=(-50, 19); at exit: AD=1.0 mrad, phase= 44, sub S/C=(-47, 31).  Full duration of ORS+eclipse 08:05.  Request four WAC SI: one in daylight at 15:30, another in eclipse (exposed for grey light or star field) at 16:40, another in eclipse at 17:50, and a final one in daylight at 19:00.  CIRS: center detectors, 38 RTI, shutter closed 16:00 to 16:10, and 17:40 to 17:50 (and early and late...)."]
["2008-197T03:05:00","000T07:55:00","2008-07-15","ISS","SPASS Rider","Saturn","AURORA","Saturn aurora","ISS AURORAL Rider","Image Saturn - auroral rider"]
["2008-199T02:06:00","000T14:00:00","2008-07-17","CIRS","Prime","Saturn","FIRMAPB","Far Infrared map","Far-IR map","Far-IR maps - 3 rotations required, requested as 1st priority (1 of each hemisphere), as discussed at Oct. '03 PSG. S. hemisphere, can be split into 11 hr segs., as needed"]
["2008-202T04:50:00","000T03:45:00","2008-07-20","CIRS","SPASS Rider","rings(general)","VTMPU37MP",null,"CIRS_077RI_VTMPU37MP001_SI"]
["2008-203T04:10:00","000T03:55:00","2008-07-21","CIRS","SPASS Rider","Star","URBETCEN","Stellar occultation","CIRS_077ST_URBETCEN002_UVIS","rider"]
["2008-203T09:05:00","000T01:35:00","2008-07-21","ISS","Prime","RingF","HIRESFRNG","High resolution F ring image","HIGH RES F RING IMAGING","High resolution imaging of the F ring at ~4 to 1.5 RS."]
["2008-203T22:25:00","002T03:05:00","2008-07-21","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_SURVEY","Continuous low-rate magnetospheric survey"]
["2008-205T09:35:00","000T02:10:00","2008-07-23","ISS","Prime","Other","RETARG","Retargetable observation",null,"ISS on, max data rate = 182.784 kbps, number of frames and bits/frame are input parameters, data volume = number of frames x bits/frame, average data rate = data volume/duration."]
["2008-206T01:30:00","003T00:00:00","2008-07-24","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG_MAPS_SURVEY","Continuous low-rate magnetospheric survey"]
["2008-207T15:06:00","000T05:00:00","2008-07-25","RSS","SPASS Rider","Earth","BORESIGHT","HGA boresight calibration","HGA Boresight Calibration","HGA Boresight Calibration; Pointing=XBAND to Earth + crosshair maneuver. Last hour (crosshair maneuver) required to be tracked at DSS-25 in 1-way mode. Playback of telemetry required afterwards for C-Kernel generation."]
["2008-209T22:40:00","000T05:20:00","2008-07-27","VIMS","SPASS Rider","rings(general)","ETACAROCC",null,"eta Carina ring occ.","Eta Carina Ring occultation. tau_IR=80 msec, IR_only. Stellar_occ mode. no spectral summing."]
["2008-210T05:53:00","000T13:12:00","2008-07-28","MAG","SPASS Rider","Other","INTFLD","MAG Internal field observation","MAG_Internal_Field_Measurements","This request will yield unique observations of Saturns internal magnetic field over a unique orbit track in latitude and longitude space."]
["2008-210T13:00:00","000T00:50:00","2008-07-28","CIRS","SPASS Rider","rings(general)","RETARGHR","Retargetable observation","CIRS_078RI_RETARGHR001_ISS","rider"]
["2008-211T20:40:00","000T04:20:00","2008-07-29","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2008-213T01:13:11","000T02:00:00","2008-07-31","RPWS","Non-SPASS","Titan","TICA","Titan closest approach","Titan closest approach observations","RPWS observations in the immediate vicinity of Titan, including thermal plasma density and temperature measurements with the Langmuir probe, search for lightning and other radio emissions, characterization of plasma wave spectrum, search for evidence of pickup ions.  Langmuir  probe within 90 degrees of spacecraft ram at closest approach, corotational ram outside of +/- 15 minutes."]
["2008-213T06:58:11","000T03:30:00","2008-07-31","CIRS","SPASS Rider","Titan","MIRLMBMAP","Mid infrared limb map","ISS_PHOT_1x1","ISS WAC support imaging, 2 images per integration (4 integrations total = 8 frames, 0.5 Mb/frame)"]
["2008-214T13:50:00","000T00:30:00","2008-08-01","CIRS","SPASS Rider","Other","SATELLORB","Satellite orbit campaign","CIRS_079OT_SATELLORB003_ISS","rider"]
["2008-216T02:05:00","000T08:55:00","2008-08-03","CIRS","SPASS Rider","RingF","FRINGMRDF",null,"CIRS_079RF_FRINGMRDF002_ISS","rider"]
["2008-217T01:15:00","000T00:30:00","2008-08-04","CIRS","SPASS Rider","InstrumentCalibration","DEEPSPACE","Deep space calibration","CIRS_079IC_DEEPSPACE217_RIDER","rider"]
["2008-217T14:25:00","000T09:40:00","2008-08-04","MIMI","Non-SPASS","Saturn","AURXNG4S",null,"MAPS AS Campaign","Part of AS MAPS Campaign.  Observe the auroral magnetosphere (e.g. the acceleration region) and SKR source regions"]
["2008-218T08:50:00","000T08:00:00","2008-08-05","CIRS","SPASS Rider","InstrumentCalibration","DSCAL08","Deep space calibration","CIRS Deep Space Calibration","null"]
["2008-219T11:05:00","000T01:30:00","2008-08-06","ISS","Prime","Rhea","060W005PH",null,"Rhea lon/phase observation","Turn UVIS_FUV to Rhea; do ftprt with (0,0,-1.03 mrad) offset for CIRS; do ftprt with (0,0,0) mrad offset for UVIS; turn to WP."]
["2008-220T08:00:00","000T02:00:00","2008-08-07","UVIS","SPASS Rider","Tethys","ICYLON","Icy satellite longitudinal coverage"]
["2008-221T08:50:00","000T06:00:00","2008-08-08","UVIS","SPASS Rider","rings(general)","TEMPN10LP"]
["2008-223T08:50:00","000T06:00:00","2008-08-10","UVIS","SPASS Rider","rings(general)","TEMPN45LP"]
["2008-224T05:40:19","000T06:26:00","2008-08-11","CIRS","SPASS Rider","Enceladus","PLUME001",null,"Rider on ISS plume observation","FP1+FP3 only."]
["2008-224T16:06:19","000T03:30:00","2008-08-11","CIRS","SPASS Rider","Enceladus","ENCEL","Enceladus","Rider on VIMS distant N. hemisphere observation","FP1+FP3 only."]
["2008-224T20:36:25","000T01:00:00","2008-08-11","CAPS","SPASS Rider","Enceladus","ENCOUNTER","MAPS Campaign","MAPS 080EN Campaign","Part of 080EN MAPS Campaign. Observe interaction between Enceladus and Saturn's magn"]
["2008-225T15:04:00","000T09:00:00","2008-08-12","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2008-227T00:44:00","000T06:00:00","2008-08-14","VIMS","SPASS Rider","rings(general)","TEMPS10LP",null,"Slow radial scan, low phase, lit side.","Cube Size (X,Z) = 64*12 hires,  IRInt = 320 msec.   Low phase, lit side of rings."]
["2008-228T03:10:00","000T02:00:00","2008-08-15","CAPS","Prime","Saturn","SURVEYPTG","MAPS survey/Prime pointing","MAPS Survey w/ prime pointing","null"]
["2008-230T04:00:00","001T14:40:00","2008-08-17","MIMI","Non-SPASS","Saturn","MAGDYN","MAPS magnetosphere dynamics campaign","MIMI Magnetospheric Dymanics","Setup MIMI for magnetospheric dynamics observations, INCA imaging, any OPMODE or TLM mode."]
["2008-232T00:30:00","003T08:35:00","2008-08-19","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","Survey","Ridealong, survey of outer mag at high latitudes"]
["2008-232T05:05:00","000T00:21:00","2008-08-19","CDA","Non-SPASS","Other","RATE080","Dust survey","Data rate","Range enter= 4.0048274 Rs exit= 3.9676038 Range altitude= 39223.876 km ... 20438.900"]
["2008-233T00:30:00","000T13:24:00","2008-08-20","VIMS","Prime","rings(general)","FMOVIE","F ring movie","F Ring movie","Do about 5 of 50."]
["2008-234T12:29:00","000T11:05:00","2008-08-21","RSS","SPASS Rider","Earth","SCE5",null,"Solar Conjunction Experiment (SCE) #5","Characterize the solar corona at 2 frequency bands (X and Ka1), and assess the electron content and possible Faraday rotation, during the solar conjunction period."]
["2008-235T04:40:00","000T03:20:00","2008-08-22","VIMS","SPASS Rider","rings(general)","GRINGARC",null,"G Ring arc observation","null"]
["2008-238T06:29:00","000T07:21:00","2008-08-25","UVIS","Prime","Saturn","NPOLECAM",null,"Saturn North Pole Campaign","UVIS/VIMS/ISS/CIRS North Pole Campaign end time set by VIMS GamCru Occ that follows"]
["2008-239T09:18:00","000T12:06:00","2008-08-26","MAG","Non-SPASS","Other","INTFLD","MAG Internal field observation","MAG_Internal_Field_Measurements","This request will yield unique observations of Saturns internal magnetic field over a unique orbit track in latitude and longitude space."]
["2008-239T14:25:00","000T00:30:00","2008-08-26","MIMI","Non-SPASS","Saturn","IMVP3",null,"MIMI Inner Magnetosphere Vertical Profile","Setup MIMI for inner magnetosphere vertical equatorial plane crossing observations, any OPMODE or TLM mode."]
["2008-240T14:19:00","000T09:00:00","2008-08-27","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2008-243T07:40:00","003T15:07:00","2008-08-30","CDA","Non-SPASS","Other","RATE010","Dust survey","Data rate Enter:SApo","Range enter= 3.9590757 Rs exit= 4.0382403 Range altitude= -40739.811 km ... 40519.964"]
["2008-245T00:50:00","000T01:00:00","2008-09-01","ISS","Prime","rings(general)","FMONITOR","F ring monitor","F RING TEMPORAL MONITORING","Long term temporal monitoring of F ring. Observation in collaboration with Jeff Cuzzi. The time isn't critical so the obs can be put anywhere in the same ~14 hr period between downlinks."]
["2008-246T23:15:00","000T00:40:00","2008-09-02","MIMI","Non-SPASS","Saturn","IMVP3",null,"MIMI Inner Magnetosphere Vertical Profile","Setup MIMI for inner magnetosphere vertical equatorial plane crossing observations, any OPMODE or TLM mode."]
["2008-251T03:59:00","000T11:05:00","2008-09-07","RSS","SPASS Rider","Earth","SCE5",null,"Solar Conjunction Experiment (SCE) #5","Characterize the solar corona at 2 frequency bands (X and Ka1), and assess the electron content and possible Faraday rotation, during the solar conjunction period."]
["2008-252T03:49:00","000T01:00:00","2008-09-08","ISS","Prime","rings(general)","FMONITOR","F ring monitor","F RING TEMPORAL MONITORING","Long term temporal monitoring of F ring. Observation in collaboration with Jeff Cuzzi. The time isn't critical so the obs can be put anywhere in the same ~14 hr period between downlinks."]
["2008-254T02:15:00","000T04:22:00","2008-09-10","CAPS","Prime","Saturn","AURXNGPTG","Aurora and Saturn Kilometric Radiation","MAPS AS Campaign","Prime pointing during AS MAPS Campaign. Observe the auroral magnetosphere (e.g. the acceleration region) and SKR source region"]
["2008-254T20:45:00","003T01:34:00","2008-09-10","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magn"]
["2008-256T20:45:00","000T04:00:00","2008-09-12","CIRS","SPASS Rider","Enceladus","PLMLP","Low phas plume imaging","CIRS_084EN_PLMLP001_ISS","rider"]
["2008-257T12:00:00","000T02:00:00","2008-09-13","INMS","Non-SPASS","Titan","TTNTORUS","Titan torus observation","Titan Torus observation","Ridealong, full rate inner mag composition measurement"]
["2008-258T01:24:00","003T15:06:00","2008-09-14","CDA","Non-SPASS","Other","RATE010","Dust survey","Data rate Enter:SApo","Range enter= 3.9497233 Rs exit= 4.0346349 Range altitude= -40731.080 km ... 40683.727"]
["2008-260T13:49:00","000T07:45:00","2008-09-16","CIRS","SPASS Rider","InstrumentCalibration","DSCAL08","Deep space calibration","CIRS Deep Space Calibration","null"]
["2008-261T08:00:00","000T06:20:00","2008-09-17","UVIS","Prime","Star","URALPARA","Alpha Ara occultation","URSTAR"]
["2008-261T17:42:00","000T11:48:00","2008-09-17","RPWS","Non-SPASS","Saturn","AURXNGSIN","Aurora and Saturn Kilometric Radiation","MAPS AS Campaign","Part of AS MAPS Campaign.  Observe the auroral magnetosphere (e.g. the acceleration region) and SKR source regions"]
["2008-263T06:09:00","000T08:25:00","2008-09-19","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2008-263T15:05:00","000T04:10:00","2008-09-19","CIRS","Prime","rings(general)","TMAPS10LP",null,null,"Priority: M/N~1/2; other opps exist unless otherwise noted."]
["2008-265T00:25:00","000T00:30:00","2008-09-21","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT CAMPAIGN, 013 TH OBS SET IN REV 08","Turn to first satellite, take 1 NAC (CL1,CL2). Turn to second satellite take 1 NAC (CL1,CL2), repeat for up to 8 satellites if visible"]
["2008-267T02:45:00","000T02:00:00","2008-09-23","CAPS","Prime","Saturn","SURVEYPTG","MAPS survey/Prime pointing","MAPS Survey w/ prime pointing","null"]
["2008-268T16:45:00","000T06:30:00","2008-09-24","UVIS","Prime","Star","URALPARA","Alpha Ara occultation","URSTAR"]
["2008-269T01:41:00","000T00:43:00","2008-09-25","CDA","Non-SPASS","Other","RATE320",null,"Data rate","Range enter= 3.9915572 Rs exit= 3.9502287 Range altitude= 19642.573 km ... -19845.477"]
["2008-270T08:05:00","000T00:30:00","2008-09-26","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT CAMPAIGN, 007 TH OBS SET IN REV 08","Turn to first satellite, take 1 NAC (CL1,CL2). Turn to second satellite take 1 NAC (CL1,CL2), repeat for up to 8 satellites if visible"]
["2008-271T23:15:00","000T06:55:00","2008-09-27","ISS","Prime","rings(general)","FNTLPLE",null,"Phase Curve and color measurements of faint rings","Low res, low elev., high-phase of E ring, need 3 of 20 opportunities"]
["2008-272T10:10:00","000T00:40:00","2008-09-28","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT CAMPAIGN, 013 TH OBS SET IN REV 08","Turn to first satellite, take 1 NAC (CL1,CL2). Turn to second satellite take 1 NAC (CL1,CL2), repeat for up to 8 satellites if visible"]
["2008-274T09:30:00","000T19:20:00","2008-09-30","MIMI","Non-SPASS","Saturn","MAGDYN","MAPS magnetosphere dynamics campaign","MIMI Magnetospheric Dymanics","Setup MIMI for magnetospheric dynamics observations, INCA imaging, any OPMODE or TLM mode."]
["2008-276T04:19:00","000T01:12:00","2008-10-02","MAG","Non-SPASS","Saturn","AURXNG","Aurora and Saturn Kilometric Radiation","MAG MAPS AS Campaign","Observe the auroral magnetosphere (e.g. the acceleration region) and SKR source regions.   AURXNG are L>4, r<7.5"]
["2008-276T09:52:29","000T02:00:00","2008-10-02","CDA","SPASS Rider","DustRAM direction","RPX0060",null,"CDA RPXing 2008-276T10:52:29 NTH","Nice to have - variation of angular distance to source (longitude)"]
["2008-277T14:15:00","000T08:52:00","2008-10-03","CIRS","SPASS Rider","rings(general)","RSCNCOCC",null,"CIRS_087RI_RSCNCOCC203_VIMS","rider"]
["2008-278T14:15:00","000T04:00:00","2008-10-04","VIMS","SPASS Rider","rings(general)","TMAPS10LP",null,null,"null"]
["2008-279T07:05:00","000T04:00:00","2008-10-05","INMS","SPASS Rider","Titan","TTNTORUS","Titan torus observation","Titan Torus region full rate ridealong","Ridealong, survey of outer mag at high latitudes"]
["2008-280T03:35:03","000T00:00:01","2008-10-06","MP","SPASS Note","Saturn","APOAPSE","Apoapse",null,"Apoapse  Per = 7.3 d, inc = 74.5 deg, r = 20.212 Rs, phase = 23 deg"]
["2008-282T21:35:00","000T01:15:00","2008-10-08","UVIS","SPASS Rider","Titan","TITAN","Titan observation","Rider for Titan Monitoring Campaign","UVIS will be riding with the design determined by the prime instrument, ISS"]
["2008-283T14:06:40","000T03:00:00","2008-10-09","CIRS","Prime","Enceladus","ENCEL","Enceladus","CIRS_088EN_ENCEL001_PRIME;","null"]
["2008-283T19:49:40","000T00:46:00","2008-10-09","CIRS","Prime","Enceladus","SECLNX",null,"CIRS_088EN_SECLNX001_PRIME;","(E5)  FP3 Polar thermal output integration; 11-3, high S lat.; begins C/A+00:46.  SOST. N283T19:52:09, X283T22:23:05."]
["2008-283T20:35:40","000T00:22:00","2008-10-09","ISS","SPASS Rider","SpacecraftActivity","DFPWBIAS",null,"Enceladus","SPT in eclipse to detect non-thermal emission"]
["2008-284T11:00:00","000T02:00:00","2008-10-10","INMS","Non-SPASS","Saturn","INNERMAG","Observing neutral molecules in the inner magnetosphere","MAPS Survey","Startup sequence. Load FSW, MRO, Load IEB from SSR's, MRO"]
["2008-285T22:25:00","000T12:15:00","2008-10-11","CIRS","SPASS Rider","rings(general)","SPKMVLFLP",null,"CIRS_088RI_SPKMVLFLP001_ISS","rider"]
["2008-287T03:30:00","000T02:00:00","2008-10-13","ISS","Prime","Rhea","044W009PH",null,"Rhea lon/phase angle observation","Turn UVIS_FUV to Rhea; do ftprt with (0,0,-1.03 mrad) offset for CIRS; do ftprt with (0,0,0) mrad offset for UVIS; turn to WP."]
["2008-287T11:41:31","000T00:00:01","2008-10-13","MP","SPASS Note","Saturn","APOAPSE","Apoapse",null,"Apoapse  Per = 7.3 d, inc = 74.5 deg, r = 20.184 Rs, phase = 23 deg"]
["2008-288T22:25:00","000T12:25:00","2008-10-14","ISS","Prime","RingF","FMOVIE","F ring movie","Long Medium Res F Ring Movie","Medium Resolution F Ring Movie. There is often some flexibility in placement - can often be the day before or day after. Want at least 12 during XM. 6 of 61 priority 1, 6 of 61 priority 2"]
["2008-291T02:25:00","000T00:45:00","2008-10-17","CDA","Non-SPASS","Other","RATE320",null,"Data rate","Range enter= 3.9850771 Rs exit= 3.9443173 Range altitude= 19981.102 km ... -19531.865"]
["2008-291T03:31:00","000T07:54:00","2008-10-17","RPWS","Non-SPASS","Saturn","AURXNGSIN","Aurora and Saturn Kilometric Radiation","MAPS AS Campaign","Part of AS MAPS Campaign.  Observe the auroral magnetosphere (e.g. the acceleration region) and SKR source regions"]
["2008-292T11:36:00","000T08:45:00","2008-10-18","MAG","Non-SPASS","Other","R1DLROLL","MAG downlink roll calibration","MAG_R1_DLROLL_CAL","Rider on rolling downlink with MAG FGM in range 1. Used for calibration of range 1. Rides on current MAG activities - no additional power or datavolume used."]
["2008-293T11:06:00","000T09:00:00","2008-10-19","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2008-294T00:40:00","000T02:00:00","2008-10-20","ISS","Prime","Tethys","091W009PH",null,"Tethys lon/phase angle observation","Turn UVIS_FUV to Tethys; do ftprt with (0,0,-1.03 mrad) offset for CIRS; do ftprt with (0,0,0) mrad offset for UVIS; turn to WP."]
["2008-296T00:06:00","000T02:00:00","2008-10-22","CIRS","SPASS Rider","rings(general)","SURVEYPTG","MAPS survey/Prime pointing","CIRS_090RI_SURVEYPTG002_CAPS","rider"]
["2008-297T06:01:00","000T04:10:00","2008-10-23","ISS","Prime","rings(general)","SHRTMOV",null,"Short movies of select features","Short movies of select features"]
["2008-297T22:55:00","000T10:55:00","2008-10-23","MIMI","Non-SPASS","Saturn","AURXNG","Aurora and Saturn Kilometric Radiation","MAPS AS Campaign","Part of AS MAPS Campaign.  Observe the auroral magnetosphere (e.g. the acceleration region) and SKR source regions"]
["2008-298T10:26:00","000T00:21:00","2008-10-24","CDA","Non-SPASS","Other","RATE080","Dust survey","Data rate","Range enter= 3.9543472 Rs exit= 3.9521724 Range altitude= -20520.993 km ... -39212.235"]
["2008-300T13:02:00","000T00:43:00","2008-10-26","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT CAMPAIGN, 009 TH OBS SET IN REV 09","Turn to first satellite, take 1 NAC (CL1,CL2). Turn to second satellite take 1 NAC (CL1,CL2), repeat for up to 8 satellites if visible"]
["2008-301T18:45:00","000T07:30:00","2008-10-27","INMS","Non-SPASS","Saturn","SURVEYREV",null,"MAPS TOST Campaign","Part of the MAPS/TOST Campaign. Determine atmospheric and ionospheric thermal structure."]
["2008-302T00:17:00","000T02:00:00","2008-10-28","CAPS","Prime","Saturn","SURVEYPTG","MAPS survey/Prime pointing","MAPS Survey w/ prime pointing","null"]
["2008-303T20:17:00","000T12:50:00","2008-10-29","CIRS","SPASS Rider","RingF","FMOVIE","F ring movie","CIRS_091RF_FMOVIE003_ISS","rider"]
["2008-305T06:05:00","000T10:39:51","2008-10-31","RPWS","Non-SPASS","Saturn","AURXNGOUT","Aurora and Saturn Kilometric Radiation","MAPS AS Campaign","Part of AS MAPS Campaign.  Observe the auroral magnetosphere (e.g. the acceleration region) and SKR source regions"]
["2008-305T17:34:51","000T00:40:00","2008-10-31","INMS","Non-SPASS","Enceladus","ENCEL6",null,"Enceladus encounter"]
["2008-305T18:14:51","002T01:07:06","2008-10-31","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS TOST Campaign","Part of the MAPS/TOST Campaign. Determine atmospheric and ionospheric thermal structure."]
["2008-306T06:15:00","000T03:22:00","2008-11-01","CIRS","SPASS Rider","Enceladus","ICYATM","Icy satellite system volatile map","CIRS_091EN_ICYATM003_UVIS","rider"]
["2008-306T20:37:00","000T13:00:00","2008-11-01","UVIS","SPASS Rider","rings(general)","APOMOS","Apoapsis mosaic"]
["2008-308T12:35:23","000T01:30:00","2008-11-03","CIRS","SPASS Rider","Titan","REGMAP","Regional mapping",null,"Obtain information on CO, HCN, CH4. Integrate on disk at airmass 1.5--2.0."]
["2008-308T19:27:23","000T07:08:00","2008-11-03","CIRS","SPASS Rider","Titan","EUVFUV","UVIS EUV / FUV imaging",null,"Obtain information on surface & tropopause temperatures, and on tropospheric CH4. Scan or contiguous steps across disk."]
["2008-309T20:23:00","000T03:00:00","2008-11-04","CIRS","SPASS Rider","rings(general)","ALPVIR","Alpha Virginis occultation","CIRS_091RI_ALPVIR001_UVIS","rider"]
["2008-310T19:48:00","000T06:10:00","2008-11-05","CIRS","SPASS Rider","rings(general)","TMAPN30LP",null,"CIRS_092RI_TMAPN30LP001_SI"]
["2008-311T12:18:00","000T01:15:00","2008-11-06","CIRS","SPASS Rider","Titan","MR1CLD",null,"Rider for Titan Monitoring Campaign","Rider to ISS Titan cloud monitor"]
["2008-312T10:00:00","003T00:55:00","2008-11-07","RPWS","Non-SPASS","Saturn","INSURVEY","Inner magnetosphere survey","RPWS Inner Survey","Setup RPWS for inner magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2008-314T01:23:00","000T17:30:00","2008-11-09","INMS","Non-SPASS","Saturn","SURVPOTM","MAPS survey","Post OTM request to trigger nominal science mode","Ridealong, survey of outer mag at high latitudes"]
["2008-314T22:48:00","000T01:12:00","2008-11-09","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT CAMPAIGN, 008 TH OBS SET IN REV 09","Turn to first satellite, take 1 NAC (CL1,CL2). Turn to second satellite take 1 NAC (CL1,CL2), repeat for up to 8 satellites if visible"]
["2008-316T04:44:00","000T00:30:00","2008-11-11","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT CAMPAIGN, 010 TH OBS SET IN REV 09","Turn to first satellite, take 1 NAC (CL1,CL2). Turn to second satellite take 1 NAC (CL1,CL2), repeat for up to 8 satellites if visible"]
["2008-317T22:30:00","001T07:30:00","2008-11-12","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SURVEY Campaign","Part of SURVEY MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2008-318T03:04:00","000T02:00:00","2008-11-13","CAPS","Prime","Saturn","SURVEYPTG","MAPS survey/Prime pointing","MAPS Survey w/ prime pointing","null"]
["2008-320T19:42:00","000T05:47:00","2008-11-15","VIMS","Prime","Saturn","NPOLEAUR",null,"North Pole aurora mosaic 2","3x3 North Polar mosaic.   1 sec integration/pixel.  Each frame takes approx 70 min."]
["2008-322T01:20:00","000T08:40:00","2008-11-17","CAPS","SPASS Rider","Saturn","AURXNG","Aurora and Saturn Kilometric Radiation","MAPS AS Campaign","Part of AS MAPS Campaign. Observe the auroral magnetosphere (e.g. the acceleration region) and SKR source region"]
["2008-323T09:24:00","000T09:00:00","2008-11-18","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2008-324T06:56:28","000T01:00:00","2008-11-19","CIRS","SPASS Rider","Titan","GLOBMAP","Global coverage mapping",null,"Ride along with ISS."]
["2008-324T16:58:28","000T00:58:00","2008-11-19","VIMS","SPASS Rider","Titan","GLOBMAP","Global coverage mapping","Map of Titan","Map of Titan with CIRS ride-along"]
["2008-325T00:56:28","000T01:00:00","2008-11-20","ISS","Prime","Titan","PHOTOMWAC","Photometry map","PHW (WAC Photometry)","monitoring for surface/atmosphere changes; attempt to see surface color variations; monitor limb hazes, 1-3 km/px"]
["2008-325T05:56:28","000T02:00:00","2008-11-20","CIRS","SPASS Rider","Titan","MIDIRTMAP","Mid infrared thermal map","ISS_PHOT_1x1","ISS WAC support imaging, 2 images per integration (3 integrations total = 6 frames, 0.5 Mb/frame)"]
["2008-326T18:50:00","000T00:30:00","2008-11-21","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT CAMPAIGN, 003 TH OBS SET IN REV 09","Turn to first satellite, take 1 NAC (CL1,CL2). Turn to second satellite take 1 NAC (CL1,CL2), repeat for up to 8 satellites if visible"]
["2008-328T22:25:00","000T23:00:00","2008-11-23","CAPS","SPASS Rider","Saturn","AURXNG","Aurora and Saturn Kilometric Radiation","MAPS AS Campaign","Part of AS MAPS Campaign. Observe the auroral magnetosphere (e.g. the acceleration region) and SKR source region"]
["2008-329T11:30:00","000T03:15:00","2008-11-24","CIRS","Prime","rings(general)","TDIFS45HP",null,null,"Priority: M/N~1/2; other opps exist unless otherwise noted."]
["2008-330T21:50:00","000T10:25:00","2008-11-25","CIRS","SPASS Rider","rings(general)","SPKMVLFLP",null,"CIRS_094RI_SPKMVLFLP001_ISS","rider"]
["2008-331T17:55:00","001T15:36:00","2008-11-26","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SURVEY Campaign","Part of SURVEY MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2008-332T16:10:00","000T08:00:00","2008-11-27","CIRS","SPASS Rider","InstrumentCalibration","DSCAL08","Deep space calibration","CIRS_094IC_DSCAL08332_SP","rider"]
["2008-333T09:31:00","000T08:25:00","2008-11-28","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2008-337T00:00:00","000T07:06:59","2008-12-02","CDA","Non-SPASS","Other","RATE010B",null,"Data rate Enter:SApo","Range enter= 5.2183240 Rs exit= 5.3162577 Range altitude= -40718.264 km ... 40211.656"]
["2008-337T11:00:00","000T21:26:00","2008-12-02","CDA","Non-SPASS","Other","RATE010B",null,"Data rate End:SApo","Range enter= 5.2181937 Rs exit= 5.7969554 Range altitude= -40682.716 km ... 40468.733"]
["2008-339T10:46:00","000T06:40:00","2008-12-04","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG MAPS Survey","Continuous low-rate magnetospheric survey"]
["2008-339T12:11:00","000T05:15:00","2008-12-04","CIRS","SPASS Rider","InstrumentCalibration","DSCAL08","Deep space calibration","CIRS_095IC_DSCAL08339_SP","rider"]
["2008-340T12:25:00","000T01:00:00","2008-12-05","MIMI","SPASS Rider","Titan","TITANIN",null,"MAPS TI Campaign","Part of TI MAPS Campaign.   Investigate micro-scale and near aspects of the Titan interaction by observing during about one hour period around an encounter. With -Y pointed toward Titan, when within 30 minutes of the targeted flyby, optimize secondary axis for corotation flow as close to the S/C -X, +/- Z plane as works with the other constraints on pointing. Also, measure Titan exosphere/magnetosphere interaction by imaging in ENA with INCA (when sun is not in INCA FOV)."]
["2008-340T15:25:45","000T02:56:15","2008-12-05","INMS","Non-SPASS","Saturn","SURVEYREV",null,"Survey","Part of the MAPS/TOST Campaign. Determine atmospheric and ionospheric thermal structure."]
["2008-341T03:25:45","000T01:00:00","2008-12-06","ISS","Prime","Titan","NIGHTNAC","ISS lightning / aurora observation","NNA (Night NAC)","monitoring for surface/atmosphere changes; attempt to see surface color variations; monitor limb hazes, 1-3 km/px"]
["2008-341T22:07:00","000T06:55:00","2008-12-06","CIRS","SPASS Rider","rings(general)","TMAPN20LP",null,"CIRS_096RI_TMAPN20LP001_SI"]
["2008-343T10:08:00","000T04:28:00","2008-12-08","VIMS","Prime","rings(general)","GAMCRUOCC","Gamma Cru occultation","Ring stellar occ - gamCru","F-D Rings, do 9 of 17. Priority 1., tau=20 ms"]
["2008-344T12:00:00","000T11:30:00","2008-12-09","CAPS","SPASS Rider","Saturn","AURXNG","Aurora and Saturn Kilometric Radiation","MAPS AS Campaign","Part of AS MAPS Campaign. Observe the auroral magnetosphere (e.g. the acceleration region) and SKR source region"]
["2008-345T17:12:00","001T03:48:00","2008-12-10","MIMI","Non-SPASS","Saturn","MAGDYN","MAPS magnetosphere dynamics campaign","MIMI Magnetospheric Dymanics","Setup MIMI for magnetospheric dynamics observations, INCA imaging, any OPMODE or TLM mode."]
["2008-346T23:17:00","000T08:00:00","2008-12-11","UVIS","SPASS Rider","rings(general)","APOMOSL"]
["2008-348T05:22:00","000T03:00:00","2008-12-13","CIRS","SPASS Rider","rings(general)","FMONITOR","F ring monitor","CIRS_096RI_FMONITOR002_ISS","rider"]
["2008-350T23:48:00","000T09:00:00","2008-12-15","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2008-352T06:30:00","000T21:55:00","2008-12-17","MAG","Non-SPASS","Saturn","AURXNG","Aurora and Saturn Kilometric Radiation","MAG MAPS AS Campaign","Observe the auroral magnetosphere (e.g. the acceleration region) and SKR source regions.   AURXNG are L>4, r<7.5"]
["2008-352T11:43:00","000T00:45:00","2008-12-17","ISS","Prime","Saturn","LIMBSCAN","Limb scan","Saturn Limb Scan","Rings behind Saturn nightside limb"]
["2008-353T15:00:00","000T02:00:00","2008-12-18","INMS","Non-SPASS","Saturn","INNERMAG","Observing neutral molecules in the inner magnetosphere","Inner Mag Survey","Startup sequence. Load FSW, MRO, Load IEB from SSR's, MRO"]
["2008-355T23:59:52","000T04:00:00","2008-12-20","CIRS","SPASS Rider","Titan","FIRNADCMP","Far infrared nadir composition map","ISS_PHOT_1x1","ISS WAC support imaging, 2 images per integration (4 integrations total = 8 frames, 0.5 Mb/frame)"]
["2008-356T12:39:52","000T00:40:00","2008-12-21","INMS","Non-SPASS","Titan","TITAN49",null,"Titan Flyby","Titan observation"]
["2008-356T15:00:00","001T13:15:00","2008-12-21","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SURVEY Campaign","Part of SURVEY MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2008-357T02:29:52","000T03:30:00","2008-12-22","CIRS","SPASS Rider","Titan","MIDIRTMAP","Mid infrared thermal map","ISS_PHOT_1x1","ISS WAC support imaging, 2 images per integration (4 integrations total = 8 frames, 0.5 Mb/frame)"]
["2008-357T22:54:00","000T07:40:00","2008-12-22","ISS","SPASS Rider","rings(general)","TMAPN30LP",null,"Spoke Periodicity Monitoring","One WAC every 20 minutes"]
["2008-359T01:15:00","000T04:00:00","2008-12-24","CAPS","SPASS Rider","Saturn","HLCUSP",null,"MAPS high latitude cusp campaign","MAPS campaign"]
["2008-360T20:36:00","000T05:00:00","2008-12-25","CIRS","Prime","rings(general)","TDIFN20HP",null,"CIRS_098RI_TDIFN20HP001_PRIME;","Priority: M/N~1/2; other opps exist unless otherwise noted."]
["2008-361T07:09:59","004T17:01:01","2008-12-26","CDA","Non-SPASS","Other","RATE010","Dust survey","Data rate End:SApo","Range enter= 9.1232878 Rs exit= 9.1118652 Range altitude= -40119.316 km ... 40456.992"]
["2008-363T18:15:00","000T01:15:00","2008-12-28","ISS","Prime","Titan","MR3CLD",null,"Titan Monitoring Campaign","Titan Monitoring Campaign, phase 20.3 range 1.6 Mkm"]
["2008-364T03:45:00","004T11:20:00","2008-12-29","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG MAPS Survey","Continuous low-rate magnetospheric survey"]
["2008-366T04:05:00","000T02:00:00","2008-12-31","ISS","Prime","Dione","088W008PH",null,"Dione lon/phase angle observation","Turn UVIS_FUV to Dione; do ftprt with (0,0,-1.03 mrad) offset for CIRS; do ftprt with (0,0,0) mrad offset for UVIS; turn to WP."]
["2009-002T19:05:00","001T20:20:00","2009-01-02","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magn"]
["2009-004T15:25:00","000T08:40:00","2009-01-04","CAPS","Prime","Saturn","IMVP9PTG",null,"MAPS IMVP Campaign","Prime pointing during IMVP MAPS Campaign (Inner magn"]
["2009-005T00:05:00","000T11:00:00","2009-01-05","UVIS","SPASS Rider","Saturn","SPOLEDYN",null,"Saturn Aurora","Rider on VIMS SPOLEDYN observations"]
["2009-006T16:11:00","000T01:15:00","2009-01-06","CIRS","SPASS Rider","Titan","MR2HAZ",null,"Rider for Titan Monitoring Campaign","Rider to ISS Titan cloud monitor"]
["2009-008T15:16:00","000T22:42:00","2009-01-08","CDA","Non-SPASS","Other","RATE010","Dust survey","Data rate End:SApo Enter: S S47","Range enter= 9.1277862 Rs exit= 9.1101179 Range altitude= -40095.167 km ... 40518.247"]
["2009-009T15:55:00","000T01:15:00","2009-01-09","CIRS","SPASS Rider","Titan","MR2CLD",null,"Rider for Titan Monitoring Campaign","Rider to ISS Titan cloud monitor"]
["2009-011T10:35:00","000T11:25:00","2009-01-11","ISS","Prime","RingF","FMOVIE","F ring movie","Long Medium Res F Ring Movie","Medium Resolution F Ring Movie. There is often some flexibility in placement - can often be the day before or day after. Want at least 12 during XM. 6 of 61 priority 1, 6 of 61 priority 2"]
["2009-013T02:10:00","000T09:30:00","2009-01-13","VIMS","Prime","rings(general)","ALPTRAOCC","Alpha TrA occultation","Ring stellar occ - alpTrA","B ring, region 1; do one at priority 2, tau=80 ms"]
["2009-013T21:50:00","000T07:15:00","2009-01-13","VIMS","SPASS Rider","rings(general)","FMOVIE","F ring movie","F Ring movie","null"]
["2009-014T13:50:00","004T13:54:00","2009-01-14","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magn"]
["2009-016T14:35:00","000T08:00:00","2009-01-16","VIMS","SPASS Rider","rings(general)","TMAPS45LP",null,"VIMS rider on CIRS","CIRS scan of rings"]
["2009-017T16:00:00","000T12:02:00","2009-01-17","VIMS","SPASS Rider","rings(general)","SUBMS20LP",null,"VIMS rider on CIRS","VIMS ridealong with CIRS"]
["2009-019T02:52:00","000T02:00:00","2009-01-19","CIRS","SPASS Rider","Dione","089W008PH",null,"CIRS_100DI_089W008PH001_ISS","rider"]
["2009-021T18:35:00","000T04:00:00","2009-01-21","CAPS","SPASS Rider","Saturn","HLCUSP",null,"MAPS high latitude cusp campaign","MAPS campaign"]
["2009-022T22:18:00","000T08:23:28","2009-01-22","CAPS","Non-SPASS","Saturn","BURST4K","4 kbps burst","Burst of 4kbps data","Burst of 4kbps data"]
["2009-023T07:28:00","000T06:47:00","2009-01-23","ISS","SPASS Rider","Saturn","AURORA","Saturn aurora","Auroral WAC 2X2 movie + lightning search. North.","Auroral WAC movie. 6 time steps  in a 1x2 mosaic in clear, HAL and IR2 filters. Space pickets one hour apart."]
["2009-024T07:28:00","000T13:40:00","2009-01-24","UVIS","SPASS Rider","Saturn","SPOLEDYN",null,"Saturn Aurora","Rider on VIMS SPOLEDYN observations"]
["2009-027T14:43:00","000T13:10:00","2009-01-27","UVIS","Prime","Saturn","AURORA","Saturn aurora","Saturn Aurora","Target Saturn's auroral zone at high latitude.  Make repeated slow continuous slews across the auroral zone, with a flyback between slow slews."]
["2009-028T17:00:00","000T01:15:00","2009-01-28","CIRS","SPASS Rider","Titan","M60R3CLD",null,"Rider for Titan Monitoring Campaign","Rider to ISS Titan cloud monitor"]
["2009-030T21:18:00","000T09:00:00","2009-01-30","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2009-031T11:35:00","001T20:30:00","2009-01-31","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG MAPS Survey","Continuous low-rate magnetospheric survey"]
["2009-031T23:00:00","000T06:07:00","2009-01-31","ISS","Prime","rings(general)","PHOTDRKBK",null,"high-latitude, dark-face ring photometry","high latitude unlit #3: B ~ 65, phase ~ 70, B = -2.9"]
["2009-033T07:10:00","000T01:00:00","2009-02-02","UVIS","Prime","Rhea","ICYMAP","Icy satellite surface map","ICYMAP:  UV Surface Map","Map surface albedo in UV.  Limb drifts to determine atmospheric scattering."]
["2009-033T14:15:00","000T02:25:00","2009-02-02","VIMS","SPASS Rider","Rhea","ECLIPSE",null,"spectral cubes","eclipse"]
["2009-035T13:34:00","000T23:45:00","2009-02-04","INMS","Non-SPASS","Saturn","SURVPOTM","MAPS survey","Post OTM request to trigger nominal science mode","Ridealong, survey of outer mag at high latitudes"]
["2009-036T16:29:00","000T09:20:00","2009-02-05","CIRS","SPASS Rider","rings(general)","SPKMVLFLP",null,null,"spoke movie rider"]
["2009-037T13:19:00","001T13:17:00","2009-02-06","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2009-038T06:50:51","000T01:30:00","2009-02-07","RPWS","Non-SPASS","Titan","TIINTRMED","Titan magnetosphere interaction","Titan Interaction - Intermediate","Study the interaction of the magnetosphere with Titan at intermediate distances for evidence of ion pickup, radio emissions, density profiles, and the general wave environment.  Prefer Langmuir probe within 90 degrees of plasma ram."]
["2009-038T22:20:51","000T04:30:00","2009-02-07","CIRS","Prime","Titan","MIDIRTMAP","Mid infrared thermal map",null,"Obtain information on the thermal structure of Titan's stratosphere. Slew across disk at 4 microrad/s."]
["2009-039T02:50:51","000T00:30:00","2009-02-08","ISS","Prime","Titan","LRMONITOR","Long range monitor","LRM (Long Range Monitor)","monitoring for surface/atmosphere changes; attempt to see surface color variations; monitor limb hazes, 1-3 km/px"]
["2009-040T16:14:00","000T11:10:00","2009-02-09","CIRS","SPASS Rider","RingF","FRSTRCHAN","F ring streamer movie","CIRS_103RF_FRSTRCHAN001_ISS","rider"]
["2009-043T05:05:00","000T08:00:00","2009-02-12","CIRS","SPASS Rider","InstrumentCalibration","DSCAL09","Deep space calibration","CIRS_103IC_DSCAL09043_SP","rider"]
["2009-045T20:20:00","000T09:00:00","2009-02-14","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2009-046T06:00:00","000T09:15:00","2009-02-15","CIRS","SPASS Rider","Titan","CLOUD",null,null,"Cloud monitor"]
["2009-048T18:15:00","000T08:40:00","2009-02-17","CIRS","Prime","rings(general)","TMAPS30LP",null,null,"Priority: M/N~1/2; other opps exist unless otherwise noted."]
["2009-051T01:01:50","000T00:00:01","2009-02-20","MP","SPASS Note","Saturn","APOAPSE","Apoapse",null,"Apoapse  Per = 11.9 d, inc = 65.3 deg, r = 19.825 Rs, phase = 26 deg"]
["2009-051T18:00:00","000T01:10:00","2009-02-20","RADAR","Prime","Titan","NEQUACAL",null,"Distant Titan Radiometry, South Equatorial Latitud","Obtain distant Titan radiometer science and calibration data."]
["2009-054T15:00:00","000T11:00:00","2009-02-23","UVIS","SPASS Rider","rings(general)","VTMPN60MP",null,"URSTAR"]
["2009-056T02:45:00","000T00:35:00","2009-02-25","CIRS","SPASS Rider","rings(general)","DEEPSPACE","Deep space calibration","CIRS_104RI_DEEPSPACE056_SP","rider"]
["2009-056T15:00:00","000T02:00:00","2009-02-25","CDA","Prime","DustRAM direction","RPX0010",null,"CDA RPXing 2009-056T16:13:00 NtH","RPXing at 13.672008 Rs, large ring extention, small/medium inclintn"]
["2009-057T19:35:00","000T09:00:00","2009-02-26","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2009-059T21:00:00","000T01:10:00","2009-02-28","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT CAMPAIGN, 016 TH OBS SET IN REV 10","Turn to first satellite, take 1 NAC (CL1,CL2). Turn to second satellite take 1 NAC (CL1,CL2), repeat for up to 8 satellites if visible"]
["2009-061T08:45:00","000T09:00:00","2009-03-02","CIRS","SPASS Rider","rings(general)","RADMRLPLF",null,"CIRS_104RI_RADMRLPLF001_ISS","rider"]
["2009-061T18:20:00","000T08:25:00","2009-03-02","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2009-064T04:45:00","000T01:15:00","2009-03-05","CIRS","SPASS Rider","Titan","M30R3CLD",null,"Rider for Titan Monitoring Campaign","Rider to ISS Titan cloud monitor"]
["2009-065T00:00:00","000T22:42:00","2009-03-06","MAG","Non-SPASS","Saturn","HLCUSP",null,"MAG MAPS HL Cusp Campaign","Observe the cusp region from high latitude.   HLCUSP are 9>local time>15, |lat| > 50, r > 15"]
["2009-066T08:49:40","001T11:39:55","2009-03-07","MIMI","Non-SPASS","Saturn","MAGDYN","MAPS magnetosphere dynamics campaign","MIMI Magnetospheric Dymanics","Setup MIMI for magnetospheric dynamics observations, INCA imaging, any OPMODE or TLM mode."]
["2009-068T16:48:00","006T06:30:00","2009-03-09","CDA","Non-SPASS","Other","RATE010","Dust survey","Data rate End:SApo","Range enter= 13.645780 Rs exit= 13.693648 Range altitude= -40595.334 km ... 40599.829"]
["2009-069T18:10:00","000T06:40:00","2009-03-10","VIMS","SPASS Rider","Rhea","ECLIPSE",null,null,"null"]
["2009-072T18:45:00","000T06:25:00","2009-03-13","ISS","Prime","rings(general)","SPKMVLFLP",null,"Lit Face Low Phase Spoke Movie","Spoke Movie to search for periodicities"]
["2009-073T02:50:00","000T08:00:00","2009-03-14","CIRS","SPASS Rider","InstrumentCalibration","DSCAL09","Deep space calibration","CIRS_105IC_DSCAL09073_SP","rider"]
["2009-075T07:45:00","000T10:00:00","2009-03-16","UVIS","SPASS Rider","rings(general)","TMAPN20LP",null,"URSTAR"]
["2009-077T16:20:00","000T08:00:00","2009-03-18","CIRS","Prime","rings(general)","VTMPN60MP",null,null,"Priority: M/N~1/2; other opps exist unless otherwise noted."]
["2009-079T03:00:00","000T04:33:04","2009-03-20","CAPS","Non-SPASS","Saturn","BURST16K","16 kbps burst","Burst of 16kbps data","Burst of 16 kbps data (which gives uncollapsed ELS data). 32 B cycles duration. Data is in addition to 1000 bps from SWSKR."]
["2009-080T00:00:00","000T00:34:00","2009-03-21","CAPS","Non-SPASS","InstrumentCalibration","ELSCAL","CAPS Electron Spectrometer calibration","ELS calibration","ELS calibration"]
["2009-080T19:30:00","000T04:20:00","2009-03-21","VIMS","SPASS Rider","rings(general)","TDIFS20HP",null,null,"null"]
["2009-085T01:05:00","000T09:00:00","2009-03-26","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2009-085T10:48:00","000T00:05:00","2009-03-26","INMS","Non-SPASS","Saturn","IEBLOAD","INMS IEB Load","IEB Load","Startup sequence. Load FSW, MRO, Load IEB from SSR's, MRO"]
["2009-086T00:43:36","000T08:00:00","2009-03-27","MAG","Non-SPASS","Titan","MAGTITAN","MAG Titan observation","MAPS_Titan_Flyby","T051 is another near-noon (10.5 h SLT), upstream flank-out flyby, with a minimum altitude of 1000 km, which is almost parallel to T050.   Therefore, the measurements will be complementary to T050, providing a description of the draping and the pileup of the external magnetic field around Titan on the dayside hemisphere.   As in the previous flybys, Titan could be found in the magnetosheath during T051.  We assign grade one priority. Data rate: 1976bps (32vps)."]
["2009-086T04:58:36","000T01:13:00","2009-03-27","CIRS","SPASS Rider","Titan","BISTATOUT","RSS Bistatic egress observation",null,"Cloud monitor"]
["2009-086T06:35:36","000T03:08:00","2009-03-27","VIMS","SPASS Rider","Titan","FIRNADCMP","Far infrared nadir composition map","Global mapping","VIMS ridealong with CIRS."]
["2009-086T18:13:36","000T05:12:00","2009-03-27","CIRS","SPASS Rider","Titan","MIDIRTMAP","Mid infrared thermal map","ISS_PHOT_1x1","ISS WAC support imaging, 2 images per integration (3 integrations total = 6 frames, 0.5 Mb/frame)"]
["2009-089T01:50:00","000T08:00:00","2009-03-30","CIRS","SPASS Rider","InstrumentCalibration","DSCAL09","Deep space calibration","CIRS_107IC_DSCAL09089_SP","rider"]
["2009-089T20:30:00","001T13:05:00","2009-03-30","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","Survey","Part of the MAPS/TOST Campaign. Determine atmospheric and ionospheric thermal structure."]
["2009-091T18:05:00","000T08:00:00","2009-04-01","CIRS","SPASS Rider","InstrumentCalibration","DSCAL09","Deep space calibration","CIRS_107IC_DSCAL09491_SP","rider"]
["2009-093T12:47:47","000T04:00:00","2009-04-03","CIRS","SPASS Rider","Titan","CLOUDMAP","Cloud map",null,"Ride with VIMS."]
["2009-094T01:27:47","000T00:40:00","2009-04-04","INMS","Non-SPASS","Titan","TITAN52",null,"Titan Flyby","Titan observation"]
["2009-094T01:59:47","000T01:16:00","2009-04-04","RSS","Prime","Titan","BISTATOUT","RSS Bistatic egress observation","RSS Bistatic Obs of Titan T52 (egress)","Bistatic scattering measurments at three radio wavelengths to determine the physical properties of Titan's surface, including reflectivity, dielectric constant, and roughness."]
["2009-094T13:47:47","000T02:00:00","2009-04-04","CIRS","SPASS Rider","Titan","MONITORNA","Monitoring of surface and atmosphere",null,"Ride with ISS."]
["2009-095T15:30:00","001T17:49:00","2009-04-05","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","Survey","Part of the MAPS/TOST Campaign. Determine atmospheric and ionospheric thermal structure."]
["2009-098T20:19:00","000T03:05:00","2009-04-08","ISS","Prime","rings(general)","MNRNGSHAD",null,"Moon Shadows on Rings","Moon Shadows on Rings.  Actual start time and duration will be determined by ultimate purpose of observation: measurements, high res photo ops, low res photo ops, movies, etc.  Need 50, want 70.  40-minute turns included, cannot be shifted."]
["2009-100T01:04:00","000T08:00:00","2009-04-10","CIRS","SPASS Rider","InstrumentCalibration","DSCAL09","Deep space calibration","CIRS_108IC_DSCAL09100_SP","rider"]
["2009-103T00:49:00","000T08:00:00","2009-04-13","CIRS","SPASS Rider","InstrumentCalibration","DSCAL09","Deep space calibration","CIRS_108IC_DSCAL09103_SP","rider"]
["2009-104T00:57:00","001T01:45:00","2009-04-14","MAG","Non-SPASS","Saturn","HLCUSP",null,"MAG MAPS HL Cusp Campaign","Observe the cusp region from high latitude.   HLCUSP are 9>local time>15, |lat| > 50, r > 15"]
["2009-106T10:28:00","000T10:05:00","2009-04-16","ISS","Prime","RingF","FMOVIE","F ring movie","Long Medium Res F Ring Movie","Medium Resolution F Ring Movie. There is often some flexibility in placement - can often be the day before or day after. Want at least 12 during XM. 6 of 61 priority 1, 6 of 61 priority 2"]
["2009-108T12:32:00","001T09:48:45","2009-04-18","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","MAPS magnetospheric survey"]
["2009-109T09:13:42","000T05:07:03","2009-04-19","ISS","SPASS Rider","Titan","FIRNADCMP","Far infrared nadir composition map","RCI (Ridealong Context Imaging)","global map"]
["2009-109T21:20:45","000T01:25:00","2009-04-19","UVIS","Prime","Star","ALPERITI",null,"Titan Occults  Alpha Eri","UVIS FUV Occultation slit boresite on star for the entire time.  Note:  Start time may change depending on trajectory updates."]
["2009-110T01:55:45","000T00:25:00","2009-04-20","ISS","SPASS Rider","Titan","HIRES","High resolution image","RCI (Ridealong Context Imaging)","global map"]
["2009-110T23:18:00","000T13:10:26","2009-04-20","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SURVEY Campaign","Part of SURVEY MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2009-111T10:18:00","001T21:45:00","2009-04-21","INMS","Non-SPASS","Saturn","SURVEYSEG","Campaign to determine atmospheric and ionospheric thermal structure","Segment Boundary Survey","Part of the MAPS/TOST Campaign. Determine atmospheric and ionospheric thermal structure."]
["2009-113T08:03:00","001T00:00:00","2009-04-23","INMS","Non-SPASS","Saturn","SURVPOTM","MAPS survey","Post OTM Survey","MAPS magnetospheric survey"]
["2009-115T08:40:00","000T06:15:00","2009-04-25","CIRS","Prime","rings(general)","TMAPS20LP",null,"CIRS_109RI_TMAPS20LP001_PRIME;","Priority: M/N~1/2; other opps exist unless otherwise noted."]
["2009-116T00:33:00","002T13:29:00","2009-04-26","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG MAPS Survey","Continuous low-rate magnetospheric survey"]
["2009-117T08:27:00","000T15:46:00","2009-04-27","ISS","Prime","Titan","CLOUD",null,"Titan cloud monitoring and gap filling (TCM)","Cloud monitoring"]
["2009-119T14:02:00","002T11:36:00","2009-04-29","INMS","Non-SPASS","Saturn","SURVBOTM","MAPS survey","Post OTM Survey","MAPS magnetospheric survey"]
["2009-120T12:27:00","000T01:55:00","2009-04-30","ISS","Prime","rings(general)","MNRNGSHAD",null,"Moon Shadows on Rings","Moon Shadows on Rings.  Actual start time and duration will be determined by ultimate purpose of observation: measurements, high res photo ops, low res photo ops, movies, etc.  Need 50, want 70.  40-minute turns included, cannot be shifted."]
["2009-122T01:38:00","000T22:24:00","2009-05-02","INMS","Non-SPASS","Saturn","SURVEYREV",null,"Orbit Boundary Survey","Part of the MAPS/TOST Campaign. Determine atmospheric and ionospheric thermal structure."]
["2009-124T10:42:00","000T20:34:00","2009-05-04","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG MAPS Survey","Continuous low-rate magnetospheric survey"]
["2009-125T12:54:16","000T01:00:00","2009-05-05","ISS","Prime","Titan","PHOTOMWAC","Photometry map","WPH (WAC Photometry)","monitoring for surface/atmosphere changes; attempt to see surface color variations; monitor limb hazes, 1-3 km/px"]
["2009-125T13:54:16","000T03:50:00","2009-05-05","UVIS","SPASS Rider","Titan","MIRLMBMAP","Mid infrared limb map","UVIS Rider to CIRS MIRLMBMAP","UVIS Rider to CIRS Mid IR Limb observation"]
["2009-125T22:34:16","000T00:40:00","2009-05-05","INMS","Non-SPASS","Titan","TITAN54",null,"Titan Flyby","Titan observation"]
["2009-126T07:54:16","000T05:00:00","2009-05-06","CIRS","SPASS Rider","Titan","FIRNADCMP","Far infrared nadir composition map","ISS_PHOT_1x1","ISS WAC support imaging, 2 images per integration (5 integrations total = 10 frames, 0.5 Mb/frame)"]
["2009-127T07:16:00","000T04:14:00","2009-05-07","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG MAPS Survey","Continuous low-rate magnetospheric survey"]
["2009-130T07:01:00","004T05:59:00","2009-05-10","INMS","Non-SPASS","Saturn","SURVBOTM","MAPS survey","Post OTM Survey","MAPS magnetospheric survey"]
["2009-131T17:06:00","000T02:00:00","2009-05-11","CAPS","Prime","Saturn","SURVEYPTG","MAPS survey/Prime pointing","MAPS Survey w/ prime pointing","MAPS Survey w/ prime pointing"]
["2009-132T22:45:00","000T08:00:00","2009-05-12","CIRS","SPASS Rider","InstrumentCalibration","DSCAL09","Deep space calibration","CIRS_110IC_DSCAL09132_SP","rider"]
["2009-135T04:45:00","000T08:00:00","2009-05-15","CIRS","SPASS Rider","InstrumentCalibration","DSCAL09","Deep space calibration","CIRS_110IC_DSCAL09135_SP","rider"]
["2009-138T13:45:00","000T09:00:00","2009-05-18","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2009-140T22:14:00","000T08:00:00","2009-05-20","CIRS","SPASS Rider","InstrumentCalibration","DSCAL09","Deep space calibration","CIRS_111IC_DSCAL09140_SP","rider"]
["2009-141T20:26:41","000T00:40:00","2009-05-21","INMS","Non-SPASS","Titan","TITAN55",null,"Titan Flyby","Titan observation"]
["2009-141T21:56:41","000T01:30:00","2009-05-21","RPWS","Non-SPASS","Titan","TIINTRMED","Titan magnetosphere interaction","Titan Interaction - Intermediate","Study the interaction of the magnetosphere with Titan at intermediate distances for evidence of ion pickup, radio emissions, density profiles, and the general wave environment.  Prefer Langmuir probe within 90 degrees of plasma ram."]
["2009-142T02:26:41","000T04:00:00","2009-05-22","VIMS","SPASS Rider","Titan","MIRLMBMAP","Mid infrared limb map","Limb Mapping","VIMS ridealong with CIRS.  Stare at Titan.  64x64 cubes at 80ms, 2x2 mosaics at 80, 160, 500 ms.  Phase = 53 deg, Lat/Lon = 50S/310 deg."]
["2009-143T21:59:00","000T08:00:00","2009-05-23","CIRS","SPASS Rider","InstrumentCalibration","DSCAL09","Deep space calibration","CIRS_111IC_DSCAL09543_SP","rider"]
["2009-145T07:54:00","000T04:00:00","2009-05-25","CIRS","SPASS Rider","rings(general)","TMAPS45MP",null,"CIRS_111RI_TMAPS45MP001_SI","Priority: M/N~1/2; other opps exist unless otherwise noted."]
["2009-147T17:29:00","000T02:34:00","2009-05-27","ISS","Prime","rings(general)","MNRNGSHAD",null,"Moon Shadows on Rings","Moon Shadows on Rings.  Actual start time and duration will be determined by ultimate purpose of observation: measurements, high res photo ops, low res photo ops, movies, etc.  Need 50, want 70.  40-minute turns included, cannot be shifted."]
["2009-150T11:58:00","001T10:00:00","2009-05-30","INMS","Non-SPASS","Saturn","SURVPOTM","MAPS survey","Post OTM Survey","MAPS magnetospheric survey"]
["2009-150T11:58:00","001T01:00:00","2009-05-30","RPWS","Non-SPASS","Sun","MAGBOUND","MAPS magnetosphere boundary campaign","MAPS MB,D Campaign","Part of MB,D MAPS Campaign.  Observe magnetospheric boundaries near noon on highly inclined orbits"]
["2009-153T00:44:00","000T12:14:00","2009-06-02","RPWS","Non-SPASS","Sun","MAGBOUND","MAPS magnetosphere boundary campaign","MAPS MB,D Campaign","Part of MB,D MAPS Campaign.  Observe magnetospheric boundaries near noon on highly inclined orbits"]
["2009-156T05:52:00","000T00:35:00","2009-06-05","MIMI","SPASS Rider","Saturn","DUSKMSPH",null,"MIMI Magnetospheric Dymanics","Part of Dusk Magnetosphere MAPS Campaign. Set up MIMI for with corotation pointing. Pointing: -X to corotation, Saturn B in X, Z plane; or spin about Z. Observe dusk-side magnetosphere at a variety of radial distances."]
["2009-157T06:07:49","000T03:52:12","2009-06-06","UVIS","SPASS Rider","Titan","FIRNADCMP","Far infrared nadir composition map","Rider to CIRS FIRNADCMP","Rider to CIRS FIRNADCMP"]
["2009-157T18:00:01","000T00:48:00","2009-06-06","RADAR","Prime","Titan","T56INSCAT",null,"T56 Inbound Scatterometry"]
["2009-158T10:00:01","000T09:02:48","2009-06-07","CIRS","SPASS Rider","Titan","GLOBMAP","Global coverage mapping",null,"Ride along with ISS"]
["2009-159T07:35:00","000T07:00:00","2009-06-08","VIMS","SPASS Rider","rings(general)","EQLBS",null,"radial scan, low phase, lit side","160 ms, 64*12 cubes?"]
["2009-160T06:45:00","000T01:35:00","2009-06-09","ISS","Prime","RingF","FRINGHRLF",null,"High Resolution F Ring Scan","Complete high resolution (0-10Rs) longitudinal scan of the F ring. Lit face. Need at least 3 during XM. 2 of 27 as priority 1 and 1 as priority 2."]
["2009-161T09:37:59","002T19:03:01","2009-06-10","CDA","Non-SPASS","Other","RATE010","Dust survey","Data rate End:SApo End: S S51","Range enter= 11.502431 Rs exit= 8.0284280 Range altitude= 40146.334 km ... -40576.483"]
["2009-163T09:35:00","000T06:34:00","2009-06-12","UVIS","Prime","Star","URZETCEN","Stellar ring occultation","URSTAR"]
["2009-164T06:42:00","000T10:00:00","2009-06-13","CIRS","Prime","Saturn","COMPSIT","Sit and stare at one location to derive composition","CIRS_112SA_COMPSIT002","Measure oxygen compounds (H2O, CO2) in  stratosphere as a function of latitude. POINTING: -Y to Saturn, Z to pole Northern hemisphere"]
["2009-165T20:26:00","000T06:00:00","2009-06-14","CIRS","SPASS Rider","InstrumentCalibration","DSCAL09","Deep space calibration","CIRS_112IC_DSCAL09165_SP","rider"]
["2009-166T19:26:00","000T09:00:00","2009-06-15","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2009-168T14:08:00","007T23:35:59","2009-06-17","CDA","Non-SPASS","Other","RATE010","Dust survey","Data rate Enter:SApo","Range enter= 11.502431 Rs exit= 8.0284280 Range altitude= 40146.334 km ... -40576.483"]
["2009-169T22:30:00","000T01:30:00","2009-06-18","RADAR","Prime","Titan","NMIDLCAL",null,"Distant Titan Radiometry, North Mid Latitudes","Obtain distant Titan radiometer science and calibration data."]
["2009-172T19:10:00","000T09:00:00","2009-06-21","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2009-173T16:17:35","000T01:05:00","2009-06-22","CIRS","SPASS Rider","Titan","FIRLMBINT","Vertical limb sounding","ISS_PHOT_1x1","ISS WAC support imaging, 2 images per integration (2 integrations total = 4 frames, 0.5 Mb/frame)"]
["2009-173T17:32:35","000T02:00:00","2009-06-22","CAPS","SPASS Rider","Titan","T57CLOSE",null,"Closest Approach 113TI (T57)","Closest Approach 113TI (T57)"]
["2009-174T03:02:35","000T00:30:00","2009-06-23","CIRS","SPASS Rider","Titan","PHOTOMWAC","Photometry map",null,"Ride along with ISS"]
["2009-175T12:20:00","000T06:00:00","2009-06-24","ISS","Prime","rings(general)","EQXSHADOW",null,"Equinox shadow","looking for the shadow of vertical features in the rings during the equinox period"]
["2009-176T18:05:00","000T02:00:00","2009-06-25","VIMS","SPASS Rider","Mimas","063W011PH",null,null,"null"]
["2009-178T01:09:00","000T09:00:00","2009-06-27","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2009-178T14:07:00","001T01:25:00","2009-06-27","MIMI","Non-SPASS","Saturn","MAGDYN","MAPS magnetosphere dynamics campaign","MIMI Magnetospheric Dymanics","Setup MIMI for magnetospheric dynamics observations, INCA imaging, any OPMODE or TLM mode."]
["2009-181T19:24:00","000T08:00:00","2009-06-30","CIRS","SPASS Rider","InstrumentCalibration","DSCAL09","Deep space calibration","CIRS_113IC_DSCAL09181_SP","rider"]
["2009-184T05:04:00","004T22:56:00","2009-07-03","CDA","Non-SPASS","Other","RATE010","Dust survey","Data rate Enter:SApo","Range enter= 8.6042321 Rs exit= 5.6667681 Range altitude= 40140.553 km ... -40577.514"]
["2009-185T06:22:00","001T00:00:00","2009-07-04","VIMS","Non-SPASS","SpacecraftActivity","DECONHIGH","Decontamination","Decontamination - High Power","IR Optics Decontamination at high power (88 Watts). Other instruments can observe during this request."]
["2009-188T02:42:00","001T01:18:00","2009-07-07","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SURVEY Campaign","Part of SURVEY MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2009-189T14:44:03","000T00:48:00","2009-07-08","ISS","SPASS Rider","Titan","HIRES","High resolution image","RCI (Ridealong Context Imaging)","ISS on, max data rate = 182.784 kbps, number of frames and bits/frame are input parameters, data volume = number of frames x bits/frame, average data rate = data volume/duration."]
["2009-189T16:04:03","000T00:40:00","2009-07-08","INMS","Non-SPASS","Titan","TITAN58",null,"Titan Flyby","Titan observation"]
["2009-189T18:29:03","000T00:35:00","2009-07-08","CIRS","SPASS Rider","Titan","HIRES","High resolution image",null,"Cloud monitor"]
["2009-191T02:58:13","000T01:54:47","2009-07-10","INMS","Non-SPASS","Saturn","RINGPLN",null,"Ring Plane Observation","Observe neutral molecules in the equatorial plane"]
["2009-191T19:35:00","000T04:47:00","2009-07-10","CIRS","SPASS Rider","rings(general)","EQXSHADOW",null,"CIRS_114RI_EQXSHADOW003_ISS","rider"]
["2009-192T04:02:00","000T07:35:03","2009-07-11","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SURVEY Campaign","Part of SURVEY MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2009-194T11:07:00","000T08:00:00","2009-07-13","CIRS","SPASS Rider","InstrumentCalibration","DSCAL09","Deep space calibration","CIRS_114IC_DSCAL09194_SP","rider"]
["2009-196T07:39:00","000T09:41:00","2009-07-15","CIRS","SPASS Rider","rings(general)","TMAPN30MP",null,"CIRS_114RI_TMAPN30MP001_SI"]
["2009-197T03:25:00","000T02:00:00","2009-07-16","CAPS","Prime","Saturn","MAGBNDPTG","MAPS magnetosphere boundary campaign","MAPS Survey w/ prime pointing","MAPS Survey w/ prime pointing"]
["2009-199T04:30:00","000T05:00:00","2009-07-18","UVIS","SPASS Rider","rings(general)","POLARIZ",null,"URSTAR"]
["2009-201T02:21:00","001T16:15:00","2009-07-20","CAPS","SPASS Rider","Saturn","MAGBOUND","MAPS magnetosphere boundary campaign","MAPS magnetospheric boundaries Campaign","MAPS magnetospheric boundaries Campaign"]
["2009-203T19:10:00","000T10:50:00","2009-07-22","CIRS","SPASS Rider","rings(general)","SPKMVDFHP",null,"CIRS_115RI_SPKMVDFHP004_ISS","rider"]
["2009-204T22:41:00","000T00:05:00","2009-07-23","INMS","Non-SPASS","Saturn","IEBLOAD","INMS IEB Load","IEB Load","Startup sequence. Load FSW, MRO, Load IEB from SSR's, MRO"]
["2009-205T05:34:03","000T01:00:00","2009-07-24","VIMS","SPASS Rider","Titan","PHOTOMWAC","Photometry map","Stare at Titan","VIMS ridealong with ISS.  Stare at Titan.  Phase = 154 deg. Lat/Lon = 26N/133 deg. Template N."]
["2009-205T13:34:03","000T01:41:00","2009-07-24","CIRS","SPASS Rider","Titan","TITANPTG","Titan observation",null,"Ride along with CAPS."]
["2009-205T16:34:03","000T01:00:00","2009-07-24","MIMI","SPASS Rider","Titan","TITANOUT",null,"MAPS TI Campaign","Part of TI MAPS Campaign.   Investigate micro-scale and near aspects of the Titan interaction by observing during about one hour period around an encounter. With -Y pointed toward Titan, when within 30 minutes of the targeted flyby, optimize secondary axis for corotation flow as close to the S/C -X, +/- Z plane as works with the other constraints on pointing. Also, measure Titan exosphere/magnetosphere interaction by imaging in ENA with INCA (when sun is not in INCA FOV)."]
["2009-206T17:20:00","000T06:00:00","2009-07-25","CIRS","SPASS Rider","rings(general)","EQLBS",null,"CIRS_115RI_EQLBS001_SI"]
["2009-207T17:53:59","000T01:14:00","2009-07-26","CDA","Non-SPASS","Other","RATE320",null,"Data rate","Range enter= 4.0690305 Rs exit= 4.3832191 Range altitude= -19208.708 km ... 19582.940"]
["2009-208T17:20:00","000T04:00:00","2009-07-27","CIRS","SPASS Rider","rings(general)","MNRNGSHAD",null,"CIRS_115RI_MNRNGSHAD003_ISS","rider"]
["2009-209T04:03:00","000T05:02:00","2009-07-28","CIRS","SPASS Rider","rings(general)","MNRNGSHAD",null,"CIRS_115RI_MNRNGSHAD004_ISS","rider"]
["2009-211T01:01:00","000T12:49:00","2009-07-30","CIRS","SPASS Rider","rings(general)","FMOVIEEQX",null,"CIRS_115RI_FMOVIEEQX001_ISS","rider"]
["2009-215T14:00:00","000T02:00:00","2009-08-03","CIRS","SPASS Rider","SpacecraftRAM direction","DEEPSPACE","Deep space calibration","CIRS_115SRI_DEEPSPACE004_CAPS","rider"]
["2009-217T02:20:00","000T13:35:00","2009-08-05","CIRS","SPASS Rider","rings(general)","SPKMVDFHP",null,"CIRS_116RI_SPKMVDFHP002_ISS","rider"]
["2009-219T16:05:00","000T09:00:00","2009-08-07","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2009-221T12:03:53","000T00:48:00","2009-08-09","RADAR","Prime","Titan","T60INSCAT",null,"T60 Inbound Scatterometry"]
["2009-221T12:03:53","000T01:00:00","2009-08-09","CAPS","SPASS Rider","Titan","T60INBND",null,"Inbound 116TI (T60)","Inbound 116TI (T60)"]
["2009-221T18:05:00","000T08:00:00","2009-08-09","CIRS","SPASS Rider","InstrumentCalibration","DSCAL09","Deep space calibration","CIRS_116IC_DSCAL09221_SP","rider"]
["2009-223T06:35:00","000T05:25:00","2009-08-11","ISS","Prime","rings(general)","EQXSHADOW",null,"Equinox shadow","looking for the shadow of vertical features in the rings during the equinox period"]
["2009-223T23:55:00","000T03:05:00","2009-08-11","UVIS","SPASS Rider","rings(general)","POSTEQX",null,"URSPEC"]
["2009-225T08:45:00","000T06:30:00","2009-08-13","CIRS","SPASS Rider","rings(general)","TMAPN20MP",null,"CIRS_116RI_TMAPN20MP001_SI"]
["2009-227T01:05:00","000T06:45:00","2009-08-15","CIRS","SPASS Rider","rings(general)","EQXSHADOW",null,"CIRS_116RI_EQXSHADOW015_ISS","rider"]
["2009-227T09:04:00","000T08:00:00","2009-08-15","CIRS","SPASS Rider","InstrumentCalibration","DSCAL09","Deep space calibration","CIRS_116IC_DSCAL09227_SP","rider"]
["2009-230T15:19:00","000T09:00:00","2009-08-18","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2009-233T00:40:00","000T20:15:00","2009-08-21","ISS","Prime","rings(general)","EQXSHADOW",null,"Equinox shadow","looking for the shadow of vertical features in the rings during the equinox period"]
["2009-234T10:30:00","000T06:35:00","2009-08-22","ISS","Prime","rings(general)","EQXSHADOW",null,"Equinox shadow","looking for the shadow of vertical features in the rings during the equinox period"]
["2009-237T03:51:38","000T03:50:00","2009-08-25","CIRS","Prime","Titan","MIRLMBINT","Mid infrared limb integration",null,"Obtain vertical profiles of temperatures in Titan's stratosphere. The arrays are stepped along the limb at two altitudes at 5 degree latitude intervals."]
["2009-237T12:33:38","000T00:43:00","2009-08-25","RADAR","Prime","Titan","T61INOSAR",null,"T61 Inbound and Outbound SAR"]
["2009-237T14:51:38","001T11:12:22","2009-08-25","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SURVEY Campaign","Part of SURVEY MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2009-239T02:04:00","000T06:51:00","2009-08-27","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG MAPS Survey","Continuous low-rate magnetospheric survey"]
["2009-239T14:00:00","000T01:01:00","2009-08-27","CDA","Non-SPASS","Other","RATE010","Dust survey","Data rate","Range enter= 4.4397676 Rs exit= 5.5292055 Range altitude= -19900.998 km ... 19981.454"]
["2009-240T14:42:00","001T08:35:00","2009-08-28","RPWS","Non-SPASS","Sun","DUSKMSPH",null,"MAPS MB,D Campaign","Part of MB,D MAPS Campaign.  Observe magnetospheric boundaries on dusk flank"]
["2009-241T23:17:00","001T23:25:00","2009-08-29","MIMI","SPASS Rider","Saturn","MAGBOUND","MAPS magnetosphere boundary campaign","MAPS MB/A Campaign","Part of MB/A MAPS Campaign. Set up MIMI for magnetospheric boundaries campaign with corotation pointing. Pointing: -X to corotation, Saturn B in X, Z plane; or spin about Z. Observe dawn-side magnetospheric boundaries at a variety of radial distances."]
["2009-243T16:35:00","000T01:15:00","2009-08-31","ISS","Prime","Titan","M90R3CLD",null,"Titan Monitoring Campaign","Titan Monitoring Campaign, phase 87.8 range 3.2 Mkm"]
["2009-245T00:00:00","000T00:34:00","2009-09-02","CAPS","Non-SPASS","InstrumentCalibration","ELSCAL","CAPS Electron Spectrometer calibration","ELS calibration","ELS calibration"]
["2009-249T21:33:00","000T08:00:00","2009-09-06","CIRS","SPASS Rider","InstrumentCalibration","DSCAL09","Deep space calibration","CIRS_117IC_DSCAL09249_SP","rider"]
["2009-250T20:33:00","000T09:00:00","2009-09-07","RSS","SPASS Rider","Earth","SCE6",null,"Solar Conjunction Experiment (SCE) #6","Characterize the solar corona at 2 frequency bands (X and Ka1), and assess the electron content and possible Faraday rotation, during the solar conjunction period."]
["2009-252T07:50:00","000T12:25:00","2009-09-09","ISS","Prime","rings(general)","SPKMVLFHP",null,"Lit Face High Phase Spoke Movie","Spoke Movie to search for periodicities"]
["2009-254T23:25:00","000T01:15:00","2009-09-11","ISS","Prime","Titan","M90R3CLD",null,"Titan Monitoring Campaign","Titan Monitoring Campaign, phase 85.4 range 2.5 Mkm"]
["2009-255T00:40:00","000T13:00:00","2009-09-12","VIMS","SPASS Rider","rings(general)","SPKMVLFHP",null,"Spoke movie, lit face, high phase","ISS rider"]
["2009-256T23:03:00","005T06:41:00","2009-09-13","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2009-262T13:29:25","000T09:03:35","2009-09-19","INMS","Non-SPASS","Saturn","RINGPLN",null,"Ring Plane Observation","Observe neutral molecules in the equatorial plane"]
["2009-263T14:52:04","000T04:00:00","2009-09-20","MAG","Non-SPASS","Dione","DITAR","Dione targeted flyby","D3 flyby","Monitor magnetic field perturbations and waves to confirm evidence of plasma pickup observed during the sole previous upstream Dione flyby."]
["2009-263T22:00:00","000T04:00:00","2009-09-20","UVIS","SPASS Rider","rings(general)","POSTEQX",null,"URSTAR"]
["2009-265T06:55:00","000T04:15:00","2009-09-22","CIRS","SPASS Rider","rings(general)","PHOTLIT","Ring system photometry","CIRS_118RI_PHOTLIT001_ISS","rider"]
["2009-268T13:18:00","000T09:00:00","2009-09-25","RSS","SPASS Rider","Earth","SCE6",null,"Solar Conjunction Experiment (SCE) #6","Characterize the solar corona at 2 frequency bands (X and Ka1), and assess the electron content and possible Faraday rotation, during the solar conjunction period."]
["2009-270T04:33:00","002T08:30:00","2009-09-27","RPWS","Non-SPASS","Saturn","SWAURORA","Solar wind campaign","MAPS SW2 Campaign","Part of SW2 MAPS Campaign.  Monitor the solar wind while Cassini is well upstream of Saturn's bow shock in coordination with RPWS and Earth based observations of Saturn's aurora"]
["2009-275T05:18:00","000T09:00:00","2009-10-02","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2009-278T04:03:00","001T10:15:00","2009-10-05","MIMI","SPASS Rider","Saturn","SWAURORA","Solar wind campaign","MAPS SWAurora Campaign","Part of AS MAPS Campaign.  Observe the auroral magnetosphere (e.g. the acceleration region) and SKR source regions"]
["2009-279T14:58:00","000T13:25:00","2009-10-06","ISS","SPASS Rider","Sun","SWAURPTG","MAPS aurora campaign","NAC aurora stare","CL1 NAC image per 10 minutes or otherwise according to CAPS plan."]
["2009-282T06:04:00","000T08:00:00","2009-10-09","CIRS","SPASS Rider","InstrumentCalibration","DSCAL09","Deep space calibration","CIRS_119IC_DSCAL09282_SP","rider"]
["2009-283T05:04:00","000T09:00:00","2009-10-10","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2009-284T19:36:25","000T03:00:00","2009-10-11","ISS","SPASS Rider","Titan","FIRNADCMP","Far infrared nadir composition map","RCI (Ridealong Context Imaging)","ISS on, max data rate = 182.784 kbps, number of frames and bits/frame are input parameters, data volume = number of frames x bits/frame, average data rate = data volume/duration."]
["2009-285T06:36:25","000T01:30:00","2009-10-12","RPWS","Non-SPASS","Titan","TIINTRMED","Titan magnetosphere interaction","Titan Interaction - Intermediate","Study the interaction of the magnetosphere with Titan at intermediate distances for evidence of ion pickup, radio emissions, density profiles, and the general wave environment.  Prefer Langmuir probe within 90 degrees of plasma ram."]
["2009-285T12:36:25","000T13:25:35","2009-10-12","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG MAPS Survey","Continuous low-rate magnetospheric survey"]
["2009-286T13:49:00","001T18:28:00","2009-10-13","MIMI","SPASS Rider","Saturn","RNGSAT","Ring / Satellite","MIMI Satellite & Ring Interactions","Part of RS MAPS Campaign. Observe the interaction between the magnetospheric hot ion and electron distributions, rings, and icy satellites. Pointing: Corotation ram in -X, +/-Z half-plane; B field in X, Z plane. Measure properties of a statistically significant number of satellite L shell crossings distributed amoung the satellites and in longitudinal distance from the satellites."]
["2009-286T14:24:00","000T01:05:00","2009-10-13","VIMS","Prime","Saturn","NHEMDYN",null,"North Hemisphere  dynamics mosaic","3x2 regional mosaic of northern hemisphere.  10-minute centers (7 mins for science, 3 for repositioning)"]
["2009-287T01:15:00","000T10:55:54","2009-10-14","MAG","Non-SPASS","co-rotation","RNGSAT","Ring / Satellite","MAG MAPS RS Campaign","Observe Saturn's inner magnetosphere and the interactions between icy satellites, rings and the magnetosphere. Measure properties of a statistically significant number of satellite L-shell crossings distributed among the satellites and in longitudinal distance from the satellites.  Data rate 0 bps, overlaps INTFLD, MITAR & TETAR requests."]
["2009-287T15:10:00","000T00:30:00","2009-10-14","ISS","Prime","Tethys","LOWPHASE","Low phase imaging","Tethys","Tethys"]
["2009-289T14:52:00","000T01:15:00","2009-10-16","UVIS","SPASS Rider","Titan","M90R3CLD",null,"Rider for Titan Monitoring Campaign","UVIS will be riding with the design determined by the prime instrument, ISS"]
["2009-290T09:09:00","000T04:00:00","2009-10-17","ISS","Prime","Saturn","NALGTNG",null,"Lightning search in CL1 in NAC from ~20-30Rs at ph","~15X1 NAC stripe N to S on the dark side repeated 2x in CL1 at each  footprint. 10 min per footprint. Cycled until observation ends."]
["2009-292T08:51:00","000T00:42:00","2009-10-19","ISS","Prime","Mimas","MUTUALEVE","Mutual event satellite transit observation","Mutual Event, transit of Mimas across Rhea","Images of mutual event, transit of Mimas across Rhea for orbit determination purposes. This observation CANNOT take place earlier or later"]
["2009-294T03:44:00","000T13:40:00","2009-10-21","VIMS","SPASS Rider","Saturn","GLOBDYN","Saturn Global dynamics","Global dynamics mosaic 006","Dynamics ridealong with CIRS composition map"]
["2009-296T16:58:59","000T00:00:01","2009-10-23","MP","SPASS Note","Saturn","APOAPSE","Apoapse",null,"Apoapse  Per = 19.0 d, inc = 0.5 deg, r = 42.294 Rs, phase = 110 deg"]
["2009-299T14:59:00","000T05:13:00","2009-10-26","VIMS","SPASS Rider","Saturn","NALGTNG",null,"ISS Lightning Ridealong #3","ISS Lightning  ridealong"]
["2009-301T15:30:00","000T06:55:00","2009-10-28","VIMS","SPASS Rider","Saturn","NALGTNG",null,"ISS Lightning Ridealong #5","ISS Lightning  ridealong"]
["2009-304T03:15:00","000T01:15:00","2009-10-31","CIRS","SPASS Rider","Titan","M90R2CLD",null,"Rider for Titan Monitoring Campaign","Rider to ISS Titan cloud monitor"]
["2009-305T00:05:00","000T02:50:00","2009-11-01","CIRS","Prime","Saturn","NADIROCC","Occultation","NADIROCC egress OR ingress","Helium abundance measurement at the RSS ingress or egress occultation point.  If RSS request deleted, this can be, too."]
["2009-305T14:35:00","000T01:00:00","2009-11-01","RPWS","Non-SPASS","rings(general)","RPXING","Measurements of dust flux, scale height and plasma waves at the magnetic equator during ring plane crossing","RPWS Ring Plane Crossing","Determine the equatorial dust flux and scale height as a function of radial distance.  Obtain high resolution of plasma waves at the magnetic equator."]
["2009-306T06:41:58","000T02:00:00","2009-11-02","CAPS","SPASS Rider","Enceladus","ENCOUNTER","MAPS Campaign","MAPS 120EN Campaign","Part of 120EN MAPS Campaign. Observe interaction between Enceladus and Saturn's magnetosphere"]
["2009-306T08:13:58","000T01:28:00","2009-11-02","UVIS","Prime","Enceladus","ICYMAP","Icy satellite surface map","ICYMAP:  UV of plume occulting Saturn","Image plume with Saturn in the background.  Stare at Saturn, targeted such that Enceladus' plume moves from pixel to pixel as Enceladus moves relative to Saturn from the s/c perspective."]
["2009-306T11:44:00","000T02:20:00","2009-11-02","UVIS","SPASS Rider","Enceladus","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Icy Satellite Longitude / Phase Coverage","Measure satellite albedo in ultraviolet light for a good sampling of longitude and phase space.  Determine phase function to investigate surface microstructure and frost properties, as a function of location."]
["2009-308T12:35:00","000T04:22:00","2009-11-04","RPWS","Non-SPASS","Sun","DUSKMSPH",null,"MAPS MB,D Campaign","Part of MB,D MAPS Campaign.  Observe magnetospheric boundaries on dusk flank"]
["2009-310T15:01:00","000T02:18:00","2009-11-06","CAPS","Prime","Saturn","MAGBNDPTG","MAPS magnetosphere boundary campaign","MAPS Survey w/ prime pointing","MAPS Survey w/ prime pointing"]
["2009-310T21:54:00","000T03:17:00","2009-11-06","VIMS","SPASS Rider","Saturn","NALGTNG",null,"ISS Lightning Ridealong #9","ISS Lightning  ridealong"]
["2009-313T04:26:00","000T01:00:00","2009-11-09","ISS","Prime","Saturn","1X2WPXX",null,"WAC Saturn Photopol 140 Phase","Saturn WAC Photopolarimetry 140 Phase 1X2 mosaic"]
["2009-315T14:22:00","000T08:00:00","2009-11-11","UVIS","Prime","Saturn","MOS120APO",null,null,"As no data will be collected while Cassini is slewing, actual data volume = (9533.9253 bps, from Alain's spreadsheet)x(127.0s per stare)x(125 stares) = 151.35x10^6 bits  Mosaic scan of Saturn magnetosphere, day 4. One 8.0-hr block of time assumed. EUV and FUV low resolution slits on. Note: data to be taken only when slit is stationary.  Slew from WAYPOINT to Saturn center. Align slit with Saturn spin axis. Start data capture, stare 127.0 s, stop data capture. Repeat PATTERN 124 times.  PATTERN: Slew -2.0 mrad about z-axis. Start data capture, stare 127.0 s, stop data capture."]
["2009-317T20:01:00","000T01:15:00","2009-11-13","UVIS","SPASS Rider","Titan","M90R2CLD",null,"Rider for Titan Monitoring Campaign","UVIS will be riding with the design determined by the prime instrument, ISS"]
["2009-319T02:31:00","000T01:15:00","2009-11-15","ISS","Prime","Titan","M90R3CLD",null,"Titan Monitoring Campaign","Titan Monitoring Campaign, phase 87.4 range 2.1 Mkm"]
["2009-320T10:16:00","000T02:40:00","2009-11-16","ISS","Prime","Saturn","NALGTNG",null,"Lightning search in CL1 in NAC from ~20-30Rs","~15X1 NAC stripe N to S on the dark side repeated 2x in CL1 at each footprint. 10 min/footprint.   2x1 WAC dayside. Cycled while observation lasts."]
["2009-321T17:37:00","000T04:00:00","2009-11-17","CIRS","SPASS Rider","InstrumentCalibration","DSCAL09","Deep space calibration","CIRS_121IC_DSCAL09321_SP","rider"]
["2009-323T04:57:00","000T04:40:00","2009-11-19","ISS","Prime","Saturn","NALGTNG",null,"Lightning search in CL1 in NAC from ~20-30Rs","~15X1 NAC stripe N to S on the dark side repeated 2x in CL1 at each footprint. 10 min/footprint.   2x1 WAC dayside. Cycled while observation lasts."]
["2009-324T14:15:00","000T05:09:00","2009-11-20","CIRS","SPASS Rider","Enceladus","RIDER","Instrument rider","CIRS_121EN_RIDER_ISS;","FP1 and FP3 only"]
["2009-325T01:32:50","000T00:30:00","2009-11-21","ISS","Prime","Enceladus","PLMHR",null,"High res plume obs during flyby.","Highest resolution plume observations during flyby."]
["2009-325T05:01:50","000T01:38:00","2009-11-21","VIMS","SPASS Rider","Enceladus","ENCELADUS","Enceladus","Enceladus","multiple 160/640 ms."]
["2009-325T08:10:00","000T02:00:00","2009-11-21","RPWS","Non-SPASS","rings(general)","RPXING","Measurements of dust flux, scale height and plasma waves at the magnetic equator during ring plane crossing","RPWS Ring Plane Crossing","Determine the equatorial dust flux and scale height as a function of radial distance.  Obtain high resolution of plasma waves at the magnetic equator."]
["2009-325T18:15:58","000T07:06:02","2009-11-21","CDA","Non-SPASS","Other","RATE080","Dust survey","Data rate","Range enter= 9.0003448 Rs exit= 15.991357 Range altitude= 3605.0985 km ... 8067.4799"]
["2009-327T04:45:00","000T04:00:00","2009-11-23","UVIS","Prime","Enceladus","ICYATM","Icy satellite system volatile map","ICYATM:  Satellite/System Volatile Map","Map volatiles in system in immediate neighborhood of Enceladus.  Observations will test connection of volatile changes to plume eruptions."]
["2009-328T10:31:00","000T02:00:00","2009-11-24","CAPS","Prime","Saturn","MAGBNDPTG","MAPS magnetosphere boundary campaign","MAPS Survey w/ prime pointing","MAPS Survey w/ prime pointing"]
["2009-330T15:06:00","000T00:42:00","2009-11-26","ISS","Prime","Rhea","MUTUALEVE","Mutual event satellite transit observation","Mutual Event, transit of Rhea across Tethys","Images of mutual event, transit of Rhea across Tethys for orbit determination purposes. This observation CANNOT take place earlier or later"]
["2009-332T15:53:00","002T01:44:00","2009-11-28","MIMI","SPASS Rider","Saturn","MAGBOUND","MAPS magnetosphere boundary campaign","MAPS MB/A Campaign","Part of MB/A MAPS Campaign. Set up MIMI for magnetospheric boundaries campaign with corotation pointing. Pointing: -X to corotation, Saturn B in X, Z plane; or spin about Z. Observe dawn-side magnetospheric boundaries at a variety of radial distances."]
["2009-334T11:33:00","000T01:15:00","2009-11-30","ISS","Prime","Titan","M90R3CLD",null,"Titan Monitoring Campaign","Titan Monitoring Campaign, phase 79.3 range 2.2 Mkm"]
["2009-334T15:18:00","000T05:42:00","2009-11-30","ISS","Prime","Saturn","NALGTNG",null,"Lightning search in CL1 in NAC from ~20-30Rs","~15X1 NAC stripe N to S on the dark side repeated 2x in CL1 at each footprint. 10 min/footprint.   2x1 WAC dayside. Cycled while observation lasts."]
["2009-338T00:00:00","001T01:39:00","2009-12-04","MAG","Non-SPASS","Sun","MAGBOUND","MAPS magnetosphere boundary campaign","MAG MAPS MAGBOUND Campaign","Observe magnetospheric boundaries near noon on highly inclined orbits."]
["2009-339T14:49:00","000T01:00:00","2009-12-05","ISS","Prime","Saturn","1X2WPXX",null,"WAC Saturn Photopol 140 Phase","Saturn WAC Photopolarimetry 140 Phase 1X2 mosaic"]
["2009-341T12:44:00","000T02:00:00","2009-12-07","CAPS","Prime","Saturn","SURVEYPTG","MAPS survey/Prime pointing","MAPS Survey w/ prime pointing","MAPS Survey w/ prime pointing"]
["2009-343T01:44:00","000T04:00:00","2009-12-09","CIRS","SPASS Rider","InstrumentCalibration","DSCAL09","Deep space calibration","CIRS_122IC_DSCAL09343_SP","rider"]
["2009-344T13:13:00","000T19:54:00","2009-12-10","CAPS","SPASS Rider","Saturn","RINGSAT","Ring solar occultation","MAPS rings and satellites Campaign","MAPS rings and satellites Campaign"]
["2009-345T10:10:00","000T02:53:14","2009-12-11","INMS","Non-SPASS","Saturn","SURVEYSEG","Campaign to determine atmospheric and ionospheric thermal structure","Segment Boundary Survey","Part of the MAPS/TOST Campaign. Determine atmospheric and ionospheric thermal structure."]
["2009-345T16:03:14","000T04:00:00","2009-12-11","UVIS","SPASS Rider","Titan","MIRLMBINT","Mid infrared limb integration","UVIS Rider to CIRS MIRLMBINT","UVIS Rider to CIRS Mid IR Limb INT"]
["2009-346T04:48:14","000T05:15:00","2009-12-12","CIRS","SPASS Rider","Titan","GLOBMAPC","Global coverage mapping",null,"Ride along with ISS"]
["2009-347T10:50:00","000T01:10:00","2009-12-13","VIMS","SPASS Rider","Titan","CLOUDMAP","Cloud map","Titan stare","Caboose segment for cloud mapping. Phase=47 deg"]
["2009-349T09:55:00","001T00:00:00","2009-12-15","INMS","Non-SPASS","Saturn","SURVPOTM","MAPS survey","Post OTM Survey","MAPS magnetospheric survey"]
["2009-351T00:55:00","000T09:00:00","2009-12-17","RSS","SPASS Rider","Saturn","OCCORT","Operations Readiness Test to demonstrate DSN and RSSG preparedness to support upcoming occultations","RSS Operational Readiness Test","RSS Operations Readiness Test (ORT), to demonstrate DSN and RSSG preparedness to support the Rev123 Saturn occultation on 2009/359."]
["2009-353T00:41:00","000T09:00:00","2009-12-19","RSS","SPASS Rider","Saturn","OCCORT","Operations Readiness Test to demonstrate DSN and RSSG preparedness to support upcoming occultations","RSS Operational Readiness Test","RSS Operations Readiness Test (ORT), to demonstrate DSN and RSSG preparedness to support the Rev123 Saturn occultation on 2009/359."]
["2009-354T13:01:00","000T11:00:00","2009-12-20","UVIS","Prime","Saturn","MOS122APO",null,null,"Mosaic scan of Saturn magnetosphere.  One 11.0-hr block of time assumed.  EUV and FUV low resolution slits on.  Note:  data to be taken only when slit is stationary.  Slew from WAYPOINT to Saturn center.  Align slit with Saturn spin axis.   Start data capture, stare 129.0 s, stop data capture.  Repeat PATTERN 189times.  PATTERN:  Slew -1.5 mrad about z-axis.  Start data capture, stare 129.0 s, stop data capture."]
["2009-357T16:35:00","000T23:05:00","2009-12-23","CAPS","SPASS Rider","Saturn","DUSKMSPH",null,"Dusk Magnetosphere observations","null"]
["2009-358T15:40:00","002T17:32:00","2009-12-24","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","null"]
["2009-359T16:57:00","000T02:03:00","2009-12-25","INMS","Non-SPASS","Saturn","SURVBOTM","MAPS survey","Post OTM Survey","Post-OTM request to resume science mode after NAV OTM."]
["2009-360T04:58:00","000T02:27:00","2009-12-26","ISS","Prime","Prometheus","PROMPROP",null,"Prometheus close flyby, Propellor observation","Prometheus close flyby, ~56,300 km at CA, 36 deg phase. followed by propellor imaging"]
["2009-360T20:42:00","000T02:00:00","2009-12-26","CIRS","SPASS Rider","rings(general)","PHOTLIT","Ring system photometry","CIRS_RIRI_PHOTLIT001_ISS","rider"]
["2009-361T15:16:59","000T04:00:00","2009-12-27","VIMS","SPASS Rider","Titan","MIRLMBMAP","Mid infrared limb map","Limb mapping","Limb mapping of Titan.  Phase = 136 deg.  Lat/Lon = 04N/17 deg.  Resolution = 89 - 47 km/px. Temp. =  R.  Obtain various cubes for limb mapping."]
["2009-361T23:01:59","000T00:37:00","2009-12-27","ISS","SPASS Rider","Titan","FIRLMBAER","Ring photometry","RCI (Ridealong Context Imaging)","ISS on, max data rate = 182.784 kbps, number of frames and bits/frame are input parameters, data volume = number of frames x bits/frame, average data rate = data volume/duration."]
["2009-362T05:16:59","000T04:00:00","2009-12-28","CIRS","Prime","Titan","MIRLMBINT","Mid infrared limb integration",null,"Obtain vertical profiles of temperatures in Titan's stratosphere. The arrays are stepped along the limb at two altitudes at 5 degree latitude intervals."]
["2009-362T09:16:59","000T03:00:00","2009-12-28","CIRS","Prime","Titan","FIRNADCMP","Far infrared nadir composition map",null,"Obtain information on CO, HCN, CH4. Integrate on disk at airmass 1.5--2.0."]
["2009-363T15:32:00","000T08:00:00","2009-12-29","CIRS","Prime","Titan","COMPMAP","Composition map","Titan Composition","Titan composition"]
["2010-001T13:52:00","000T06:40:00","2010-01-01","VIMS","Prime","Other","PLEIADES","Pleiades","Pleiades","Turn to Pleiades; Time: 30 min  Pleiades: multiple cubes w/64x64 FOV IR @ 640 ms, VIS @ 40000 ms; Time: 6.0 hr 40 min; Volume: 86.5 Mbits; CompRatio: 2.0  Turn to waypoint: 30 min  Primary: -y to Pleiades; Secondary: +z to TBD  Not time critical.  RWA REQUIRED."]
["2010-003T03:49:00","003T04:54:00","2010-01-03","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2010-004T00:43:00","000T08:00:00","2010-01-04","CIRS","SPASS Rider","InstrumentCalibration","DSCAL10",null,"CIRS_124IC_DSCAL10004_SP","rider"]
["2010-007T01:55:00","000T05:00:00","2010-01-07","CIRS","SPASS Rider","rings(general)","EQLBS",null,null,"Priority: M/N~1/2; other opps exist unless otherwise noted."]
["2010-008T22:50:00","000T12:15:00","2010-01-08","VIMS","Prime","rings(general)","FMOVIE","F ring movie","F Ring movie","64x12 frame, hi res mode. 640 msec tau_IR."]
["2010-009T22:29:00","000T17:30:00","2010-01-09","INMS","Non-SPASS","Saturn","SURVPOTM","MAPS survey","Post OTM Survey","Post-OTM request to resume science mode after NAV OTM."]
["2010-011T01:00:00","000T00:16:00","2010-01-11","RPWS","Non-SPASS","Saturn","WHISTLER","RPWS lightning search","Obtain wideband examples of lightning whistlers","Obtain wideband evidence of lightning whistlers.  These would verify the existence of lightning already suspected from Saturn Electrostatic Discharges (SED) and would provide information on the electron density along the field line to the source.  No pointing requirement."]
["2010-012T06:45:00","000T01:29:00","2010-01-12","RPWS","Non-SPASS","Sun","DUSKMSPH",null,"MAPS MB,D Campaign","Part of MB,D MAPS Campaign.  Observe magnetospheric boundaries on dusk flank"]
["2010-012T22:47:36","000T00:23:00","2010-01-12","RADAR","Prime","Titan","T65RASAR",null,"T65 Ride-along SAR with INMS"]
["2010-012T23:10:36","000T00:16:00","2010-01-12","RADAR","Prime","Titan","T65OUTSAR",null,"T65 Outbound SAR for Ontario Lacus"]
["2010-013T17:29:59","001T14:44:01","2010-01-13","MAG","Non-SPASS","Sun","MAGBOUND","MAPS magnetosphere boundary campaign","MAG MAPS MAGBOUND Campaign","Observe magnetospheric boundaries near noon on highly inclined orbits."]
["2010-015T08:14:00","001T02:31:00","2010-01-15","MIMI","SPASS Rider","Saturn","MAGBOUND","MAPS magnetosphere boundary campaign","MAPS MB/A Campaign","Part of MB/A MAPS Campaign. Set up MIMI for magnetospheric boundaries campaign with corotation pointing. Pointing: -X to corotation, Saturn B in X, Z plane; or spin about Z. Observe dawn-side magnetospheric boundaries at a variety of radial distances."]
["2010-016T09:54:00","000T01:05:00","2010-01-16","ISS","Prime","Epimetheus","MUTUALEVE","Mutual event satellite transit observation","Mutual Event, transit of Epimetheus across Janus","Images of mutual event, transit of Epimetheus across Janus for orbit determination purposes. This observation CANNOT take place earlier or later"]
["2010-019T14:05:00","000T08:00:00","2010-01-19","UVIS","Prime","Saturn","MOS124APO",null,null,"Mosaic scan of Saturn magnetosphere, day 4.  One 8.0-hr block of time assumed.  EUV and FUV low resolution slits on.  Note:  data to be taken only when slit is stationary.  Slew from WAYPOINT to Saturn center.  Align slit with Saturn spin axis.  Start data capture, stare 153.0 s, stop data capture.  Repeat PATTERN 105 times.  PATTERN:  Slew +2.5 mrad about z-axis.  Start data capture, stare 153.0 s, stop data capture.  Note:  As no data will be collected while Cassini is slewing, actual data volume = (7913.781 bps, from Alain's spreadsheet)x(153.0s per stare)x(106 stares) = 128.346x10^6 bits"]
["2010-021T22:45:00","000T09:00:00","2010-01-21","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2010-024T00:31:00","000T11:20:00","2010-01-24","VIMS","Prime","rings(general)","EG105PHAS",null,"E/G Ring phase observation","E-G phase observation."]
["2010-024T15:05:00","001T00:05:00","2010-01-24","CAPS","SPASS Rider","Saturn","DUSKMSPH",null,"Dusk Magnetosphere observations","null"]
["2010-026T12:38:30","000T02:05:00","2010-01-26","RSS","SPASS Rider","Enceladus","THERMAL","Thermal stabilization period","RSS 125RI OCC Thermal Stabilization","A period of thermal stabilization is required immediately prior to any radio science experiment and test using Ka-band or S-band."]
["2010-027T09:00:00","000T02:00:00","2010-01-27","CIRS","SPASS Rider","rings(general)","LOWPHASE","Low phase imaging","Rider to VIMS Low Phase","Priority: M/N~1/2; other opps exist unless otherwise noted."]
["2010-027T15:30:00","000T15:06:00","2010-01-27","RPWS","Non-SPASS","Saturn","INSURVEY","Inner magnetosphere survey","RPWS Inner Survey","Setup RPWS for inner magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2010-028T07:16:00","000T13:12:49","2010-01-28","MIMI","SPASS Rider","Saturn","DUSKMSPH",null,"MIMI Magnetospheric Dymanics","Part of Dusk Magnetosphere MAPS Campaign. Set up MIMI for with corotation pointing. Pointing: -X to corotation, Saturn B in X, Z plane; or spin about Z. Observe dusk-side magnetosphere at a variety of radial distances."]
["2010-028T12:28:49","000T01:00:00","2010-01-28","CIRS","SPASS Rider","Titan","PHOTOMWAC","Photometry map",null,"Ride along with ISS."]
["2010-028T23:28:49","000T01:00:00","2010-01-28","CAPS","SPASS Rider","Titan","T66OUTBND",null,"Titan Encounter","null"]
["2010-029T00:28:49","000T07:00:00","2010-01-29","VIMS","SPASS Rider","Titan","EUVFUV","UVIS EUV / FUV imaging","Titan scan.","VIMS ridealong with UVIS for slow scan across Titan.  Phase = 40 deg.  Lat/Lon = 10S/213 deg.  Resolution = 24 km/px.  Obtain cubes while scanning across Titan. Temp. X."]
["2010-030T07:56:00","000T04:04:00","2010-01-30","CIRS","SPASS Rider","Titan","CLOUD",null,"Titan Composition","Titan composition"]
["2010-032T02:25:00","003T19:54:00","2010-02-01","MIMI","SPASS Rider","Saturn","SWAURORA","Solar wind campaign","MAPS SWAurora Campaign","Part of AS MAPS Campaign.  Observe the auroral magnetosphere (e.g. the acceleration region) and SKR source regions"]
["2010-032T07:41:00","000T01:15:00","2010-02-01","UVIS","SPASS Rider","Titan","M60R2CLD",null,"Rider for Titan Monitoring Campaign","UVIS will be riding with the design determined by the prime instrument, ISS"]
["2010-034T16:12:00","000T09:00:00","2010-02-03","UVIS","Prime","Saturn","MOS125APO",null,null,"Mosaic scan of Saturn magnetosphere, day 1.  One 9.0-hr block of time assumed.  EUV and FUV low resolution slits on.  Note:  data to be taken only when slit is stationary.  As no data will be collected while Cassini is slewing, actual data volume = (7761.59303 bps, from Alain's spreadsheet)x(156.0s per stare)x(125 stares) = 151.35x10^6 bits.   Slew from WAYPOINT to Saturn center.  Align slit with Saturn spin axis.  Start data capture, stare 156.0 s, stop data capture.  Repeat PATTERN 124 times.  PATTERN:  Slew +2.0 mrad about z-axis.  Start data capture, stare 156.0 s, stop data capture."]
["2010-038T20:02:00","000T03:00:00","2010-02-07","UVIS","SPASS Rider","Other","OUTERSATS","Icy satellite observaton","ICYLON:  Icy Satellite Longitude / Phase Coverage","Measure satellite albedo in ultraviolet light for a good sampling of longitude and phase space.  Determine phase function to investigate surface microstructure and frost properties, as a function of location."]
["2010-040T22:17:00","000T04:00:00","2010-02-09","CIRS","SPASS Rider","InstrumentCalibration","DSCAL10",null,"CIRS_126IC_DSCAL10040_SP","rider"]
["2010-042T16:00:00","000T05:00:00","2010-02-11","MAG","Non-SPASS","InstrumentCalibration","SCAS","MAG SCAS instrument","MAG/SCAS_Cal","Boom alignment calibration using SCAS.   If moved within scheduling window, KEEP OUTSIDE SCHEDULED MAPS CAMPAIGNS. Note: SCAS operations disturb RSS and RPWS.   If OpMode is not ORS, a unique sequence will be required."]
["2010-044T11:30:00","000T00:45:00","2010-02-13","UVIS","SPASS Rider","Calypso","ICYLON","Icy satellite longitudinal coverage",null,"albedo map"]
["2010-044T17:55:00","000T00:25:00","2010-02-13","VIMS","SPASS Rider","Mimas","GEOLOG","Geologic study","Mimas","640ms, 160ms pairs"]
["2010-044T18:45:00","000T00:25:00","2010-02-13","UVIS","SPASS Rider","Mimas","ICYLON","Icy satellite longitudinal coverage",null,"albedo map"]
["2010-045T21:03:00","000T09:00:00","2010-02-14","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2010-048T06:43:00","000T01:15:00","2010-02-17","UVIS","SPASS Rider","Titan","M60R2CLD",null,"Rider for Titan Monitoring Campaign","UVIS will be riding with the design determined by the prime instrument, ISS"]
["2010-049T13:43:00","000T01:15:00","2010-02-18","ISS","Prime","Titan","M90R3CLD",null,"Titan Monitoring Campaign","Titan Monitoring Campaign, phase 60.4 range 2.3 Mkm"]
["2010-053T11:27:00","001T22:51:00","2010-02-22","RPWS","Non-SPASS","Saturn","SWAURORA","Solar wind campaign","MAPS SW2 Campaign","Part of SW2 MAPS Campaign.  Monitor the solar wind while Cassini is well upstream of Saturn's bow shock in coordination with RPWS and Earth based observations of Saturn's aurora"]
["2010-055T06:48:00","000T00:47:00","2010-02-24","ISS","Prime","Dione","MUTUALEVE","Mutual event satellite transit observation","Mutual Event, transit of Dione across Enceladus","Images of mutual event, transit of Dione across Enceladus for orbit determination purposes. This observation CANNOT take place earlier or later"]
["2010-056T20:00:00","001T23:19:00","2010-02-25","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","Survey","Part of the MAPS/TOST Campaign. Determine atmospheric and ionospheric thermal structure."]
["2010-058T23:59:00","000T03:25:00","2010-02-27","VIMS","Prime","rings(general)","EG130PHAS",null,"E/G Ring phase observation","E-G phase observation. Can be shifted roughly +/- 1 day. SAT segment. Do 3 of 9 EG130 phase at priority 2."]
["2010-060T19:55:00","000T07:04:00","2010-03-01","UVIS","SPASS Rider","Enceladus","ICYPLU","Observe Enceladus plumes","ICYPLU:  Enceladus Plume Observation","Observe Enceladus' plume, usually at very high phase angles"]
["2010-061T12:00:00","000T04:40:36","2010-03-02","RPWS","Non-SPASS","co-rotation","RNGSAT","Ring / Satellite","MAPS RS Campaign","Part of RS MAPS Campaign.  Observe Saturn's inner magnetosphere and the interactions between icy satellites, rings and the magnetosphere. Measure properties of a statistically significant number of satellite L shell crossings distributed amoung the satellites and in longitudinal distance from the satellites."]
["2010-061T18:50:36","000T03:10:00","2010-03-02","VIMS","SPASS Rider","Rhea","RHEA","Rhea","Rhea","multiple 160/640 ms."]
["2010-062T01:53:59","000T08:17:00","2010-03-03","MAG","Non-SPASS","Other","INTFLD","MAG Internal field observation","MAG_Internal_Field_Measurements","This request will yield unique observations of Saturns internal magnetic field over a unique orbit track in latitude and longitude space."]
["2010-062T17:00:00","000T12:00:00","2010-03-03","CIRS","SPASS Rider","InstrumentCalibration","DSCAL10",null,"CIRS_127IC_DSCAL10062_SP","rider"]
["2010-065T10:49:00","000T07:00:56","2010-03-06","RPWS","Non-SPASS","Sun","MAGBOUND","MAPS magnetosphere boundary campaign","MAPS MB,D Campaign","Part of MB,D MAPS Campaign.  Observe magnetospheric boundaries near noon on highly inclined orbits"]
["2010-067T18:24:00","000T00:30:00","2010-03-08","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT CAMPAIGN, 013 TH OBS SET IN REV 12","Turn to first satellite, take 1 NAC (CL1,CL2). Turn to second satellite take 1 NAC (CL1,CL2), repeat for up to 8 satellites if visible"]
["2010-069T20:34:00","000T08:00:00","2010-03-10","CIRS","SPASS Rider","InstrumentCalibration","DSCAL10",null,"CIRS_127IC_DSCAL10069_SP","rider"]
["2010-074T19:04:00","000T05:20:00","2010-03-15","CAPS","Prime","SolarWind","SWAURPTG","MAPS aurora campaign","MAPS Survey w/ prime pointing","null"]
["2010-074T23:05:00","002T09:40:00","2010-03-15","MIMI","SPASS Rider","Saturn","MAGBOUND","MAPS magnetosphere boundary campaign","MAPS MB/A Campaign","Part of MB/A MAPS Campaign. Set up MIMI for magnetospheric boundaries campaign with corotation pointing. Pointing: -X to corotation, Saturn B in X, Z plane; or spin about Z. Observe dawn-side magnetospheric boundaries at a variety of radial distances."]
["2010-077T23:00:00","000T04:00:00","2010-03-18","INMS","Non-SPASS","Titan","TTNTORUS","Titan torus observation","Titan Torus observation","Titan Torus observation"]
["2010-079T20:05:00","000T00:31:00","2010-03-20","VIMS","Prime","Saturn","ALPCMAOCC",null,"alpCMa Saturn occultation","alpCMa atmosphere occultation.  Stellar occ mode, no spectral summing, tau_IR = 40 msec.  Secondary axis for CDA. Latitude 41S."]
["2010-081T05:05:08","002T22:28:52","2010-03-22","INMS","Non-SPASS","Saturn","SURVEYSEG","Campaign to determine atmospheric and ionospheric thermal structure","Segment Boundary Survey","Part of the MAPS/TOST Campaign. Determine atmospheric and ionospheric thermal structure."]
["2010-081T19:15:00","000T00:30:00","2010-03-22","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT CAMPAIGN, 003 TH OBS SET IN REV 12","Turn to first satellite, take 1 NAC (CL1,CL2). Turn to second satellite take 1 NAC (CL1,CL2), repeat for up to 8 satellites if visible"]
["2010-084T19:30:00","007T18:55:00","2010-03-25","CAPS","SPASS Rider","SolarWind","SWAURORA","Solar wind campaign","MAPS Solar Wind/Aurora/SKR","null"]
["2010-086T18:19:00","000T09:00:00","2010-03-27","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2010-087T23:00:00","000T04:00:00","2010-03-28","INMS","Non-SPASS","Saturn","ENGBCKGND",null,"Engineering background observation","Full rate measurement to gather engineering background data"]
["2010-089T18:04:00","000T09:00:00","2010-03-30","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2010-094T06:34:00","000T11:15:00","2010-04-04","MAG","Non-SPASS","Sun","MAGBOUND","MAPS magnetosphere boundary campaign","MAG MAPS MAGBOUND Campaign","Observe magnetospheric boundaries near noon on highly inclined orbits."]
["2010-095T04:39:59","000T10:10:40","2010-04-05","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","Survey","Part of the MAPS/TOST Campaign. Determine atmospheric and ionospheric thermal structure."]
["2010-095T05:50:39","000T01:00:00","2010-04-05","VIMS","SPASS Rider","Titan","PHOTOMWAC","Photometry map","Stare at Titan","VIMS ridealong with ISS.  Stare at Titan.  Phase = 161 deg.  Lat/Lon = 04N/143 deg.  Resolution = 99 km/px.  Obtain 160 and 640 msec cubes for global mapping and cloud monitoring.  Temp. N"]
["2010-095T15:05:39","000T00:30:00","2010-04-05","ISS","SPASS Rider","Titan","FIRLMBT","Far Infrared limb tracking","RCI (Ridealong Context Imaging)","ISS on, max data rate = 182.784 kbps, number of frames and bits/frame are input parameters, data volume = number of frames x bits/frame, average data rate = data volume/duration."]
["2010-095T17:50:39","000T15:34:21","2010-04-05","MIMI","Non-SPASS","Saturn","MAGDYN","MAPS magnetosphere dynamics campaign","MIMI Magnetospheric Dymanics","Setup MIMI for magnetospheric dynamics observations, INCA imaging, any OPMODE or TLM mode."]
["2010-097T01:25:00","000T00:10:00","2010-04-07","ISS","Prime","Dione","PLUMESEAR",null,"Dione plume search","Sit'n'stare on western limb of Dione for 10 min."]
["2010-097T04:53:11","000T00:46:00","2010-04-07","INMS","Non-SPASS","Dione","DIONE","Dione","Dione Flyby","Dione observation"]
["2010-097T08:31:10","000T01:20:00","2010-04-07","ISS","SPASS Rider","Dione","DIONE","Dione","Dione multi color","Sit'n'stare"]
["2010-097T21:30:00","000T02:00:00","2010-04-07","RPWS","Non-SPASS","rings(general)","RPXING","Measurements of dust flux, scale height and plasma waves at the magnetic equator during ring plane crossing","RPWS Ring Plane Crossing","Determine the equatorial dust flux and scale height as a function of radial distance.  Obtain high resolution of plasma waves at the magnetic equator."]
["2010-098T02:04:46","000T17:00:00","2010-04-08","CDA","Non-SPASS","Other","RATE080","Dust survey","Data rate","Range enter= 9.0072932 Rs exit= 15.997996 Range altitude= 716.56776 km ... 3730.0188"]
["2010-099T08:00:00","001T18:19:00","2010-04-09","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","Survey","Part of the MAPS/TOST Campaign. Determine atmospheric and ionospheric thermal structure."]
["2010-102T02:59:00","000T01:15:00","2010-04-12","CIRS","SPASS Rider","Titan","M90R3CLD",null,"Rider for Titan Monitoring Campaign","Rider to ISS Titan cloud monitor"]
["2010-105T03:13:00","000T15:10:00","2010-04-15","CAPS","Prime","SolarWind","SWAURPTG","MAPS aurora campaign","MAPS Survey w/ prime pointing","null"]
["2010-106T12:00:00","001T05:21:00","2010-04-16","INMS","Non-SPASS","Saturn","SURVEYREV",null,"Orbit Boundary Survey","Part of the MAPS/TOST Campaign. Determine atmospheric and ionospheric thermal structure."]
["2010-108T06:33:00","000T09:00:00","2010-04-18","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2010-113T10:58:00","000T04:55:00","2010-04-23","UVIS","Prime","Enceladus","ICYATM","Icy satellite system volatile map","ICYATM:  Satellite/System Volatile Map","Map volatiles in system in immediate neighborhood of Enceladus.  Observations will test connection of volatile changes to plume eruptions."]
["2010-115T01:18:00","001T00:00:00","2010-04-25","INMS","Non-SPASS","Saturn","SURVPOTM","MAPS survey","Post OTM Survey","Post-OTM request to resume science mode after NAV OTM."]
["2010-116T18:14:00","000T13:33:00","2010-04-26","RPWS","Non-SPASS","Saturn","INSURVEY","Inner magnetosphere survey","RPWS Inner Survey","Setup RPWS for inner magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2010-117T13:11:00","000T09:59:17","2010-04-27","CAPS","SPASS Rider","Saturn","TRINGSAT",null,"Rings and Satellites","null"]
["2010-117T14:00:00","000T06:07:00","2010-04-27","VIMS","SPASS Rider","Enceladus","TENCEL",null,"Enceladus","multiple 160/640 ms."]
["2010-118T00:23:46","000T02:00:00","2010-04-28","CDA","SPASS Rider","DustRAM direction","RPX0110",null,"CDA RPXing 2010-118T01:23:46","RPXing at 4.4071604 Rs"]
["2010-118T08:44:00","000T02:16:00","2010-04-28","UVIS","SPASS Rider","Enceladus","TICYLON",null,null,"Map uv albedo"]
["2010-119T02:18:00","000T02:49:00","2010-04-29","ISS","SPASS Rider","Saturn","GLOBDYN","Saturn Global dynamics","WAC global day movie + NAC lightning search","2x2 mosaic made of corners of VIMS 3x3 90-minute mosaics plus a central footprint of night side row of VIMS mosaic. Day side: WAC in MT3, CB3, CB2, MT2, and BL1. Night side: NAC CL1 images at 3 footprints, 13 images per 90 min."]
["2010-120T10:05:00","002T03:25:00","2010-04-30","MAG","Non-SPASS","Sun","MAGBOUND","MAPS magnetosphere boundary campaign","MAG MAPS MAGBOUND Campaign","Observe magnetospheric boundaries near noon on highly inclined orbits."]
["2010-125T01:27:00","000T20:55:00","2010-05-05","CIRS","Prime","Saturn","MIRMAP","Mid infrared map","CIRS_130SA_MIRMAP001_PRIME","Either hemisphere Determine upper troposphere and tropopause temperature with spatial resolution of about two degrees of latitude and longitude  POINTING: -y to Saturn, z to pole"]
["2010-127T19:00:00","000T02:00:00","2010-05-07","INMS","Non-SPASS","Saturn","ENGBCKGND",null,"Engineering background observation","Full rate measurement to gather engineering background data"]
["2010-128T16:16:00","000T08:00:00","2010-05-08","CIRS","SPASS Rider","InstrumentCalibration","DSCAL10",null,"CIRS_131IC_DSCAL10128_SP","rider"]
["2010-131T14:01:00","001T00:00:00","2010-05-11","INMS","Non-SPASS","Saturn","SURVPOTM","MAPS survey","Post OTM Survey","Post-OTM request to resume science mode after NAV OTM."]
["2010-133T06:00:00","000T04:41:36","2010-05-13","CAPS","Non-SPASS","SolarWind","BURST16K","16 kbps burst","Burst of 16kbps data","Burst of 16 kbps data (which gives uncollapsed ELS data). 64 B cycles duration. Data is in addition to 1000 bps from SWSKR."]
["2010-136T15:30:00","000T22:01:00","2010-05-16","INMS","Non-SPASS","Saturn","SURVEYSEQ",null,"Sequence Boundary Survey","Part of the MAPS/TOST Campaign. Determine atmospheric and ionospheric thermal structure."]
["2010-137T15:21:59","000T06:38:01","2010-05-17","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","Survey","Part of the MAPS/TOST Campaign. Determine atmospheric and ionospheric thermal structure."]
["2010-137T23:08:00","000T03:08:00","2010-05-17","VIMS","SPASS Rider","Sun","USUNOCC","Solar occultation","Saturn Solar Occultation","Saturn Solar Occultation Egress."]
["2010-138T05:34:03","000T01:00:00","2010-05-18","MIMI","SPASS Rider","Enceladus","ENCOUNTER","MAPS Campaign","MAPS RS Campaign","Part of RS MAPS Campaign.   Icy moon encounter. Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2010-138T08:31:30","000T00:00:01","2010-05-18","MP","SPASS Note","Saturn","PERIAPSE","Periapse",null,"Periapse R = 3.518 Rs, lat = -0 deg, phase = 81 deg"]
["2010-139T14:24:20","000T03:00:00","2010-05-19","ISS","SPASS Rider","Titan","FIRNADCMP","Far infrared nadir composition map","RCI (Ridealong Context Imaging)","ISS on, max data rate = 182.784 kbps, number of frames and bits/frame are input parameters, data volume = number of frames x bits/frame, average data rate = data volume/duration."]
["2010-140T03:44:20","000T00:40:00","2010-05-20","INMS","Non-SPASS","Titan","TITAN68",null,"Titan Flyby","Titan observation"]
["2010-140T16:24:20","000T04:40:44","2010-05-20","ISS","SPASS Rider","Titan","MIDIRTMAP","Mid infrared thermal map","RCI (Ridealong Context Imaging)","ISS on, max data rate = 182.784 kbps, number of frames and bits/frame are input parameters, data volume = number of frames x bits/frame, average data rate = data volume/duration."]
["2010-141T17:40:00","000T02:10:00","2010-05-21","CAPS","Prime","Saturn","MAGBNDPTG","MAPS magnetosphere boundary campaign","MAPS Survey w/ prime pointing","null"]
["2010-143T13:55:00","000T01:15:00","2010-05-23","ISS","Prime","Titan","M60R2CLD",null,"Titan Monitoring Campaign","Titan Monitoring Campaign, phase 44.9 range 1.7 Mkm"]
["2010-146T08:04:00","000T04:55:00","2010-05-26","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2010-149T04:00:00","000T12:00:00","2010-05-29","CDA","SPASS Rider","DustRAM direction","ISD",null,"CDA ISD","CDA to interstellar dust direction (approx 259, 8)"]
["2010-151T18:00:00","001T10:45:00","2010-05-31","MIMI","SPASS Rider","Saturn","DUSKMSPH",null,"MIMI Magnetospheric Dymanics","Part of Dusk Magnetosphere MAPS Campaign. Set up MIMI for with corotation pointing. Pointing: -X to corotation, Saturn B in X, Z plane; or spin about Z. Observe dusk-side magnetosphere at a variety of radial distances."]
["2010-152T14:44:00","000T08:00:00","2010-06-01","CIRS","SPASS Rider","InstrumentCalibration","DSCAL10",null,"CIRS_132IC_DSCAL10152_SP","rider"]
["2010-153T23:59:00","000T03:16:00","2010-06-02","CIRS","Prime","rings(general)","EQLBN",null,null,"Priority: M/N~1/2; other opps exist unless otherwise noted."]
["2010-155T03:03:44","000T10:16:00","2010-06-04","CDA","Non-SPASS","Other","RATE080","Dust survey","Data rate","Range enter= 12.020940 Rs exit= 15.996924 Range altitude= -39997.456 km ... -18632.255"]
["2010-155T13:19:44","006T18:07:16","2010-06-04","CDA","Non-SPASS","Other","RATE010","Dust survey","Data rate End:SApo","Range enter= 16.008717 Rs exit= 16.001514 Range altitude= -18559.322 km ... -25721.644"]
["2010-156T02:11:27","000T02:15:00","2010-06-05","VIMS","Prime","Titan","REGMAP","Regional mapping","Regional mapping of Titan.","Regional mapping of Titan during C/A.  At C/A, phase = 87 deg.  Lat/Lon = 87N/09 deg.  Resolution = 1.0 km/px.  Obtain mosaics of Ligeia mare (~80N lat, 248W lon). Obtain 4x4 mosaics between 70 and 20 N latitutde (area should cover Selk crater)."]
["2010-157T14:00:00","000T04:48:00","2010-06-06","VIMS","SPASS Rider","Titan","CLOUDMAP","Cloud map","Titan Cloud Monitoring.","Caboose segment.  VIMS ridealong with ISS for cloud monitoring.  Phase = 34 deg.  Lat/Lon = 00S/236 deg.  Resolution = 362 km/px.  Obtain cubes of various integrations for cloud monitoring."]
["2010-159T06:18:00","000T13:50:00","2010-06-08","CDA","Prime","DustRAM direction","ISD",null,"CDA ISD","CDA to interstellar dust direction (approx 259, 8)"]
["2010-159T21:43:00","000T08:00:00","2010-06-08","CIRS","SPASS Rider","InstrumentCalibration","DSCAL10",null,"CIRS_132IC_DSCAL10159_SP","rider"]
["2010-162T22:12:00","001T15:25:00","2010-06-11","CAPS","SPASS Rider","SolarWind","SWAURORA","Solar wind campaign","MAPS Solar Wind/Aurora/SKR","null"]
["2010-165T02:42:00","000T09:00:00","2010-06-14","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2010-169T11:46:00","000T09:00:00","2010-06-18","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2010-170T07:04:00","000T13:36:00","2010-06-19","CAPS","Prime","Saturn","RNGSATPTG","Ring / Satellite","Rings and Satellites","null"]
["2010-171T11:11:00","005T09:59:00","2010-06-20","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2010-171T20:37:43","000T02:45:00","2010-06-20","VIMS","SPASS Rider","Titan","FIRNADMAP","Far infrared nadir composition map","Titan Scan.","VIMS ridealong with CIRS slow scan across Titan.  Phase = 149 deg.  Lat/Lon = 03N/21 deg.  Resolution = 47 km/px.  Temp. T.  Obtain cubes while scanning across Titan."]
["2010-172T01:47:43","000T00:40:00","2010-06-21","INMS","Non-SPASS","Titan","TITAN70",null,"Titan Flyby","Titan observation"]
["2010-172T19:56:00","000T09:00:00","2010-06-21","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2010-175T10:56:00","001T10:14:00","2010-06-24","MIMI","SPASS Rider","Saturn","SWAURORA","Solar wind campaign","MAPS SWAurora Campaign","Part of AS MAPS Campaign.  Observe the auroral magnetosphere (e.g. the acceleration region) and SKR source regions"]
["2010-176T21:10:00","001T08:13:00","2010-06-25","RPWS","Non-SPASS","Saturn","SWAURORA","Solar wind campaign","MAPS SW2 Campaign","Part of SW2 MAPS Campaign.  Monitor the solar wind while Cassini is well upstream of Saturn's bow shock in coordination with RPWS and Earth based observations of Saturn's aurora"]
["2010-176T22:05:00","000T00:33:00","2010-06-25","INMS","Non-SPASS","Saturn","MRO","Instrument memory readout","MRO","Startup sequence. Load FSW, Load IEB from SSR's, MRO"]
["2010-178T15:00:00","000T01:37:00","2010-06-27","INMS","Non-SPASS","Saturn","ENGBCKGND",null,"Engineering background observation","Full rate measurement to gather engineering background data"]
["2010-182T10:40:00","002T17:29:00","2010-07-01","INMS","Non-SPASS","Saturn","SURVBOTM","MAPS survey","Post OTM Survey","Post-OTM request to resume science mode after NAV OTM."]
["2010-183T12:39:00","000T08:00:00","2010-07-02","CIRS","SPASS Rider","InstrumentCalibration","DSCAL10",null,"CIRS_134IC_DSCAL10183_SP","rider"]
["2010-185T18:00:00","000T22:00:00","2010-07-04","RPWS","Non-SPASS","Saturn","CHORUS",null,"RPWS CHORUS Campaign","Part of RPWS Chorus campaign, attempt to get high rate data from within L Shell of 8"]
["2010-186T00:40:00","000T09:00:00","2010-07-05","MAG","Non-SPASS","Other","INTFLD","MAG Internal field observation","MAG_Internal_Field_Measurements","This request will yield unique observations of Saturns internal magnetic field over a unique orbit track in latitude and longitude space."]
["2010-187T08:14:00","000T01:55:00","2010-07-06","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2010-187T23:52:45","000T00:25:30","2010-07-06","INMS","Non-SPASS","Titan","TITAN71",null,"Titan Flyby","Titan observation"]
["2010-188T14:22:45","000T03:35:00","2010-07-07","CIRS","SPASS Rider","Titan","GLOBMAP","Global coverage mapping",null,"Ride along with ISS."]
["2010-190T10:09:00","001T23:44:00","2010-07-09","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2010-191T10:33:00","000T13:40:00","2010-07-10","VIMS","SPASS Rider","Saturn","MIRMAP","Mid infrared map","CIRS MIRMAP ridealong","CIRS Ridealong for full Saturn rotation"]
["2010-196T04:21:00","011T04:45:00","2010-07-15","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","null"]
["2010-197T10:18:00","000T13:00:00","2010-07-16","UVIS","Non-SPASS","Saturn","COMPSIT","Sit and stare at one location to derive composition","UVIS Rider to CIRS Compsit","UVIS Rider to CIRS Compsit"]
["2010-199T12:17:00","000T09:00:00","2010-07-18","CIRS","Prime","Saturn","COMPSIT","Sit and stare at one location to derive composition","CIRS_135SA_COMPSIT002","Measure oxygen compounds (H2O, CO2) in  stratosphere as a function of latitude. POINTING: -Y to Saturn, Z to pole Either hemisphere"]
["2010-203T07:02:00","000T14:00:00","2010-07-22","ISS","Prime","Saturn","NALGTNG",null,"Lightning search in CL1 in NAC from ~20-30Rs","~15X1 NAC stripe N to S on the dark side repeated 2x in CL1 at each footprint. 10 min/footprint 2x2 sum.   Cycled while observation lasts."]
["2010-206T00:20:00","000T02:00:00","2010-07-25","RPWS","Non-SPASS","rings(general)","RPXING","Measurements of dust flux, scale height and plasma waves at the magnetic equator during ring plane crossing","RPWS Ring Plane Crossing","Determine the equatorial dust flux and scale height as a function of radial distance.  Obtain high resolution of plasma waves at the magnetic equator."]
["2010-208T15:00:00","002T05:00:00","2010-07-27","MIMI","SPASS Rider","Saturn","RNGSAT","Ring / Satellite","MIMI Satellite & Ring Interactions","Part of RS MAPS Campaign. Observe the interaction between the magnetospheric hot ion and electron distributions, rings, and icy satellites. Pointing: Corotation ram in -X, +/-Z half-plane; B field in X, Z plane. Measure properties of a statistically significant number of satellite L shell crossings distributed amoung the satellites and in longitudinal distance from the satellites."]
["2010-209T10:51:00","000T08:00:00","2010-07-28","CIRS","SPASS Rider","InstrumentCalibration","DSCAL10",null,"CIRS_135IC_DSCAL10209_SP","rider"]
["2010-211T21:07:00","000T06:45:00","2010-07-30","MAG","Prime","Sun","CALROLL","MAG calibration roll","MAG Calibration Rolls","Roll about axis other than Z for determination of sensor offsets, actual roll axis is not important - selected axis is usually suitable for MAPS.  Preferably calibrations should be made every 15-20 days in areas where field conditions are suitable.  Note: periods of suitable data are defined as follows; 1) More distant than 15 RS from Saturn's axis (to try and get into the more uniform part of the internal+sheet field). 2) Inside the magnetopause (more specifically inside a most compressed model MP). 3) More distant than 3 RS from the current sheet. Using a 'hinged' sheet model which departs from Saturn's equatorial plane at about 15 RS and then follows the anti-solar direction on the nightside. This means that, even though its orbit is equatorial, if the spacecraft is situated far enough away from the planet, it should see the nightside current sheet divert northwards away from it (using Saturn axis tilted 17 deg away from Sun).  Apart from possible injection events, sheet disruptions etc the resultant periods should have a reasonable probability of seeing a 'quiescent' 'lobe-like' or 'disk-like' field. We would prefer as far downtail as possible so the field has more chance of pointing in a single direction over larger length scales."]
["2010-215T09:36:00","000T09:00:00","2010-08-03","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2010-218T02:00:00","000T09:00:00","2010-08-06","CDA","Non-SPASS","DustRAM direction","ISD",null,"CDA ISD","CDA to interstellar dust direction (approx 259, 8)"]
["2010-223T11:55:00","000T04:00:00","2010-08-11","CAPS","Prime","co-rotation","LLACORPTG",null,"MAPS low latitude apoapsis w/ prime pointing","null"]
["2010-225T08:29:00","000T02:00:00","2010-08-13","ISS","Prime","Titan","M30R1CLD",null,"Titan Monitoring Campaign","Titan Monitoring Campaign, requested phase 19.5 requested range 0.7 Mkm"]
["2010-225T12:50:00","000T02:10:00","2010-08-13","ISS","Prime","Enceladus","PLMLRHP",null,"Low res plume obs at high phase","High resolution plume observation at low phase"]
["2010-225T21:29:59","000T03:00:00","2010-08-13","CIRS","SPASS Rider","Enceladus","HIRES","High resolution image","CIRS_136EN HIRES001 SI","One NAC at 21:58:46, exposed for the sunlit crescent, 2x2 binned, 8-bit, lossy compression  One NAC at about 22:06:15, exposed for the sunlit crescent, 2x2 binned, 8-bit, lossy compression  One NAC at 22:29:00, exposed for Saturn shine (1 second exposure recommended: should be adequate SNR for pointing, and will have only ~2 pixels of smear).  Unbinned (1x1), 12-bit, lossless compression"]
["2010-226T02:14:59","000T00:45:00","2010-08-14","UVIS","SPASS Rider","Enceladus","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Map uv albedo"]
["2010-227T22:34:00","000T09:00:00","2010-08-15","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2010-230T07:59:00","000T08:20:00","2010-08-18","CAPS","Prime","Saturn","MAGBNDPTG","MAPS magnetosphere boundary campaign","MAPS MAGBOUND w/ prime pointing","null"]
["2010-233T01:14:00","000T08:00:00","2010-08-21","CIRS","SPASS Rider","Other","CWSTAROBS",null,"CIRS_136OT CW Leo SI","4 clear NACs, at 2010-233T02:54, 2010-233T04:38, 2010-233T06:22, and 2010-233T08:06.  Exposure information:  Spectral class=F,   V magnitude=13.0"]
["2010-236T07:59:00","000T01:30:00","2010-08-24","VIMS","SPASS Rider","Titan","M120R2HZ",null,"Titan Monitoring Campaign","Titan Monitoring Campaign; phase = 117 deg, range = 1.6 Mkm"]
["2010-243T19:25:00","000T17:35:00","2010-08-31","CIRS","SPASS Rider","rings(general)","HPLELR",null,null,"CIRS Rider to ISS High Phase Rings Observation in XD 136/137"]
["2010-245T00:58:00","000T05:54:00","2010-09-02","VIMS","Prime","rings(general)","FMOVIE","F ring movie","F Ring movie","64x12 frame, hi res mode. 640 msec tau_IR. In order to satisfy ISS and CIRS requirements, primary pointing will be to a ring radius-longitude to be determined."]
["2010-245T22:41:00","000T02:00:00","2010-09-02","CDA","Non-SPASS","Other","RATE080","Dust survey","Data rate","Range enter= 8.5933172 Rs exit= 15.990178 Range altitude= -39953.174 km ... 14426.832"]
["2010-246T18:40:00","000T02:13:00","2010-09-03","VIMS","SPASS Rider","rings(general)","BMOVIE","B ring movie","B Ring composition","160 msec exposures interleaved with longer integration time (640 msec)."]
["2010-247T06:33:00","002T00:00:00","2010-09-04","MIMI","SPASS Rider","Saturn","DUSKMSPH",null,"MIMI Magnetospheric Dymanics","Part of Dusk Magnetosphere MAPS Campaign. Set up MIMI for with corotation pointing. Pointing: -X to corotation, Saturn B in X, Z plane; or spin about Z. Observe dusk-side magnetosphere at a variety of radial distances."]
["2010-249T06:38:00","000T00:02:00","2010-09-06","CIRS","Non-SPASS","Other","SEQSETUP","CIRS sequence setup activity","CIRS S63 Sequence Setup","Enforce CIRS science no-data state, load tables (IEBs) from the SSR, set the focal plane assembly set point"]
["2010-252T13:43:00","013T06:37:00","2010-09-09","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG MAPS Survey","Continuous low-rate magnetospheric survey"]
["2010-253T11:43:00","000T05:00:00","2010-09-10","VIMS","Non-SPASS","Saturn","WIND5HR",null,"Wind Observation #5","Ride-along with ISS"]
["2010-256T00:44:00","009T10:54:00","2010-09-13","CDA","Non-SPASS","Other","RATE010","Dust survey","Data rate Enter:SApo","Range enter= 16.002150 Rs exit= 8.6158938 Range altitude= 14399.748 km ... -40035.005"]
["2010-260T05:47:00","004T10:00:00","2010-09-17","INMS","Non-SPASS","Saturn","SURVBOTM","MAPS survey","Post OTM Survey","Post-OTM request to resume science mode after NAV OTM."]
["2010-262T16:27:00","000T13:40:00","2010-09-19","VIMS","Non-SPASS","Saturn","MIRMAP","Mid infrared map","CIRS MIRMAP Ridealong","Ridealong with CIRS"]
["2010-264T15:47:00","000T13:45:00","2010-09-21","INMS","Non-SPASS","Saturn","SURVPOTM","MAPS survey","Post OTM Survey","Post-OTM request to resume science mode after NAV OTM."]
["2010-265T19:16:00","000T01:55:00","2010-09-22","UVIS","SPASS Rider","Enceladus","ICYPLU","Observe Enceladus plumes","ICYPLU:  Enceladus Plume Observation","Observe Enceladus' plume, usually at very high phase angles"]
["2010-266T14:45:00","000T04:52:00","2010-09-23","UVIS","Prime","Saturn","EUVFUV","UVIS EUV / FUV imaging","EUVFUV Imaging of Saturn","One slow scans across Saturn's visible hemisphere to form spectral images"]
["2010-267T17:23:41","000T00:30:00","2010-09-24","CIRS","Prime","Titan","FIRLMBAER","Ring photometry",null,"Limb scanning for aerosols."]
["2010-267T20:53:41","000T06:45:00","2010-09-24","CIRS","SPASS Rider","Titan","EUVFUV","UVIS EUV / FUV imaging",null,"Ride along with UVIS."]
["2010-269T06:17:00","001T22:45:00","2010-09-26","INMS","Non-SPASS","Saturn","SURVEYSEG","Campaign to determine atmospheric and ionospheric thermal structure","Segment Boundary Survey","Part of the MAPS/TOST Campaign. Determine atmospheric and ionospheric thermal structure."]
["2010-270T20:02:00","000T09:00:00","2010-09-27","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2010-276T22:32:00","000T04:00:00","2010-10-03","UVIS","SPASS Rider","Other","OUTERSATS","Icy satellite observaton","ICYLON:  Icy Satellite Longitude / Phase Coverage","Measure satellite albedo in ultraviolet light for a good sampling of longitude and phase space.  Determine phase function to investigate surface microstructure and frost properties, as a function of location."]
["2010-282T05:15:00","001T08:00:00","2010-10-09","UVIS","Prime","Saturn","MOS138APO",null,null,"Mosaic scan of Saturn magnetosphere, second 32.0-hr block of time.    Scan pattern of the UVIS slit boresight is a rectangle with Saturn at the midpoint of the lower edge.  The rectangle extends out to +/- 10 Rs along the east-west direction and from 0 to approx. 2.88 Rs southward.  (The two 32-hr blocks combine to form three east-west swaths stretching from -10 Rs to +10 Rs; one swath lies along the Saturn equator, while the second lies just north and the third lies just south.)   Allowances of 30 minutes for turn to/from waypoint and 20 minutes observation margin have been included at each end of the observation.   EUV and FUV low resolution slits on.   Note:  data to be taken only when slit is stationary.  Slew from WAYPOINT to Saturn center.  Align slit with Saturn spin axis.  Start data capture, stare 275.0 s, stop data capture.  Repeat PATTERN-A 111 times.  Slew +0.064 rad about the x-axis.  Start data capture, stare 275.0 s, stop data capture.  Repeat PATTERN-B 222 times.  Return boresight to Saturn center:  slew -0.064 rad about the x-axis and -0.222222 rad about the z-axis.  PATTERN-A:  Slew -1.5 mrad about z-axis.  Start data capture, stare 275.0 s, stop data capture.  PATTERN-B:  Slew +1.5 mrad about z-axis.  Start data capture, stare 275.0 s, stop data capture.  Note:  As no data will be collected while Cassini is slewing, actual data volume = (4402.94005 bps, from Alain Jouchoux's spreadsheet)x(275.0s per stare)x(335 stares) = 405.6209x10^6 bits."]
["2010-285T05:00:00","000T01:30:00","2010-10-12","ISS","Prime","Titan","M180R2HZ",null,"Titan Monitoring Campaign","Titan Monitoring Campaign, requested phase 152.5 requested range 1.2 Mkm"]
["2010-288T04:02:00","000T09:58:00","2010-10-15","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2010-289T03:20:00","000T03:55:00","2010-10-16","ISS","Prime","Enceladus","PLMSCECL",null,"Rhea","ISS on, max data rate = 182.784 kbps, number of frames and bits/frame are input parameters, data volume = number of frames x bits/frame, average data rate = data volume/duration."]
["2010-289T17:15:00","000T01:30:00","2010-10-16","VIMS","SPASS Rider","Pallene","ICYLON","Icy satellite longitudinal coverage","composition","composition"]
["2010-291T06:00:00","000T08:00:00","2010-10-18","VIMS","SPASS Rider","Saturn","AURSLEW","Saturn aurora","Aurorae UVIS Slew","Ridealong with UVIS slew observations of aurorae"]
["2010-296T18:33:00","000T09:00:00","2010-10-23","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2010-300T21:33:00","001T16:00:00","2010-10-27","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG MAPS Survey","Continuous low-rate magnetospheric survey"]
["2010-302T13:33:00","006T13:30:00","2010-10-29","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2010-309T03:03:00","002T10:01:00","2010-11-05","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG MAPS Survey","Continuous low-rate magnetospheric survey"]
["2010-313T09:00:00","000T03:00:00","2010-11-09","ISS","SPASS Rider","Dione","FP3SECLX",null,"Dione eclipse exit","ISS on, max data rate = 182.784 kbps, number of frames and bits/frame are input parameters, data volume = number of frames x bits/frame, average data rate = data volume/duration."]
["2010-313T18:16:29","000T00:00:01","2010-11-09","MP","SPASS Note","Saturn","PERIAPSE","Periapse",null,"Periapse R = 4.100 Rs, lat = 2 deg, phase = 80 deg"]
["2010-314T20:19:00","000T19:18:01","2010-11-10","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SURVEY Campaign","Part of SURVEY MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2010-315T13:12:01","000T02:40:00","2010-11-11","VIMS","SPASS Rider","Titan","REGMAP","Regional mapping","Regional mapping of Titan.","VIMS ridealong with CIRS during C/A for regional mapping of Titan.  Phase = 154 deg. SSC Lat/Lon = 26.024S/69.435 deg, SS Lat/Lon = 6.921N/231.178 deg.  Alt = 10402.619 km, range = 12977.619 km  Resolution = 5.2 km/px.  Obtain cubes for regional mapping of Titan during C/A."]
["2010-315T22:37:01","000T05:00:00","2010-11-11","VIMS","Prime","Titan","GLOBMAP","Global coverage mapping","Global mapping.","Global mapping of Titan.  Phase = 35 deg. SSC Lat/Lon = 2.339S/205.827 deg.  SS Lat/Lon = 6.926N/240.028 deg. Alt = 176796.8 km range = 179371.8 km.  Resolution = 88 km/px.  Obtain cubes of various exposure times for global mapping of Titan.  Template V."]
["2010-316T10:34:00","000T10:30:00","2010-11-12","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2010-319T02:19:00","000T07:00:00","2010-11-15","ISS","Prime","Other","TARRES",null,"Tarvos","Observation of irregular moon of Saturn."]
["2010-324T01:57:00","004T17:38:00","2010-11-20","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2010-325T14:00:00","000T02:00:00","2010-11-21","RADAR","Prime","Saturn","ENGTEST","Engineering test","Engineering Test of Diagnostic Modes","Engineering test of diagnostic modes on the flight unit."]
["2010-330T22:30:00","000T11:00:00","2010-11-26","VIMS","SPASS Rider","Saturn","AURSTARE","Saturn aurora","Auroral Stare","Auroral Stare ridealong with UVIS"]
["2010-332T19:21:00","000T05:05:00","2010-11-28","ISS","Prime","Hyperion","FLYBY",null,"Hyperion flyby","ORS observation during 290,000 - 380,000 km flyby of Hyperion."]
["2010-333T11:36:00","000T10:58:00","2010-11-29","VIMS","SPASS Rider","Rhea","ICYLON","Icy satellite longitudinal coverage",null,"null"]
["2010-334T10:23:59","000T03:00:00","2010-11-30","RSS","Prime","Enceladus","GRAVITY","RSS gravity science experiment","RSS Enceladus' Gravity Field Experiment","Experiment to determine Enceladus's gravity field, possibly detecting a diapir under the south pole, and infer constraints on its internal structure."]
["2010-335T10:25:00","009T05:50:00","2010-12-01","CDA","Non-SPASS","Other","RATE010","Dust survey","Data rate End:SApo","Range enter= 14.003535 Rs exit= 14.000623 Range altitude= 477.97167 km ... -1131.2580"]
["2010-339T19:30:00","000T01:30:00","2010-12-05","CIRS","SPASS Rider","Titan","M90R3CLD",null,"Rider for Titan Monitoring Campaign","Rider to ISS Titan cloud monitor"]
["2010-344T16:15:00","009T18:08:00","2010-12-10","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SURVEY Campaign","Part of SURVEY MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2010-346T02:00:00","000T12:00:00","2010-12-12","MAG","Prime","Other","MAPSROLL",null,"MAPS Offset Rolls","Offset rolls similar to MAG calrolls. Use in periods where MAPS downlink rolls are removed due to RBOT \"2 out of 3\" rule. Suitable for MAPS science. Unlike MAG calrolls orbital location is not critical. Duration 5hrs or greater preferred (typical roll period approx 53mins).  MAG data at survey rate."]
["2010-352T16:23:00","000T08:00:00","2010-12-18","CIRS","SPASS Rider","InstrumentCalibration","DSCAL10",null,"CIRS_142IC_DSCAL10352_SP","rider"]
["2010-354T15:15:00","000T04:40:00","2010-12-20","ISS","Prime","Enceladus","PLMHPHR","Observe Enceladus' plumes","Enceladus","Enceladus plume PIE"]
["2010-354T22:45:00","000T01:30:00","2010-12-20","CIRS","SPASS Rider","Enceladus","PLMHPHR","Observe Enceladus' plumes","CIRS ISS RIDER","null"]
["2010-355T02:13:40","000T00:54:46","2010-12-21","INMS","Non-SPASS","Enceladus","ENCEL13",null,"Enceladus encounter","Enceladus observation"]
["2010-357T13:30:00","000T07:00:00","2010-12-23","CAPS","Prime","co-rotation","LLACORPTG",null,"MAPS low latitude apoapsis prime pointing","null"]
["2010-357T20:30:00","000T04:00:00","2010-12-23","CAPS","Prime","co-rotation","IONCALPTG",null,"IMS and IBS calibration","null"]
["2010-365T00:55:00","000T09:00:00","2010-12-31","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2011-004T16:55:00","001T06:00:00","2011-01-04","CDA","Prime","DustRAM direction","ISD0023",null,"CDA ISD 2010-365T07:30:00","ISD observation around apoapse 2010-365T07:30:00 44.706183 Rs"]
["2011-009T09:11:00","001T03:39:00","2011-01-09","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG MAPS Survey","Continuous low-rate magnetospheric survey"]
["2011-010T00:11:00","000T09:00:00","2011-01-10","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2011-010T16:53:25","000T10:00:00","2011-01-10","INMS","Non-SPASS","Rhea","R3INBND",null,"Rhea flyby","Rhea observation"]
["2011-012T17:26:00","004T15:16:00","2011-01-12","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","null"]
["2011-014T08:27:00","000T08:00:00","2011-01-14","CIRS","SPASS Rider","InstrumentCalibration","DSCAL11",null,"CIRS_143IC_DSCAL11014_SP","rider"]
["2011-017T08:42:00","003T12:46:00","2011-01-17","CDA","Non-SPASS","Other","RATE010","Dust survey","Data rate End:SApo Enter: S66","Range enter= 14.009241 Rs exit= 14.011157 Range altitude= 1984.8706 km ... 4188.2766"]
["2011-021T07:58:00","000T08:00:00","2011-01-21","CIRS","SPASS Rider","InstrumentCalibration","DSCAL11",null,"CIRS_144IC_DSCAL11021_SP","rider"]
["2011-029T02:59:00","000T02:00:00","2011-01-29","RADAR","Prime","Titan","RADIOMCAL","RADAR distant Titan radiometry calibration","Distant Titan Radiometry Calibration","Obtain distant Titan radiometer science and calibration data."]
["2011-030T16:49:00","000T03:36:00","2011-01-30","UVIS","SPASS Rider","Enceladus","ICYPLU","Observe Enceladus plumes","ICYPLU:  Enceladus Plume Observation","Observe Enceladus' plume, usually at very high phase angles"]
["2011-031T04:00:00","000T01:30:00","2011-01-31","ISS","Prime","Enceladus","PLMHPHR","Observe Enceladus' plumes","Enceladus Plume PIE","Enceladus plume PIE"]
["2011-031T12:00:00","000T01:30:00","2011-01-31","ISS","SPASS Rider","Mimas","MIMAS","Mimas","Mimas flyby","ORS observation, VIMS rider"]
["2011-032T08:29:00","000T03:40:00","2011-02-01","ISS","Prime","Other","L5MIMAS",null,"Mimas L5 satellite search","Satellite search around Mimas L5 Lagrange point."]
["2011-039T07:15:00","000T13:45:00","2011-02-08","CAPS","Prime","co-rotation","LLACORPTG",null,"MAPS low latitude apoapsis prime pointing","null"]
["2011-041T10:06:00","005T10:40:00","2011-02-10","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","Survey","Part of the MAPS/TOST Campaign. Determine atmospheric and ionospheric thermal structure."]
["2011-043T07:00:00","004T04:46:00","2011-02-12","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2011-048T12:31:00","000T08:00:00","2011-02-17","CIRS","SPASS Rider","InstrumentCalibration","DSCAL11",null,"CIRS_145IC_DSCAL11048_SP","rider"]
["2011-049T18:04:11","001T02:26:49","2011-02-18","MIMI","Non-SPASS","co-rotation","SURVEYOV",null,"MAPS SURVEY Campaign Overlay","Overlay:  adding 350 bps  Part of SURVEY MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2011-051T19:21:00","000T11:50:00","2011-02-20","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG MAPS Survey","Continuous low-rate magnetospheric survey"]
["2011-053T07:11:00","000T03:00:00","2011-02-22","ISS","Prime","Other","SIAPHA",null,"Siarnaq","Observation of irregular moon of Saturn."]
["2011-055T02:07:00","000T06:00:00","2011-02-24","CIRS","Prime","Saturn","COMPSIT","Sit and stare at one location to derive composition","Saturn COMPSIT","Measure oxygen compounds (H2O, CO2) in  stratosphere as a function of latitude. POINTING: -Y to Saturn, Z to pole Either hemisphere"]
["2011-056T13:27:00","000T06:00:00","2011-02-25","CIRS","Prime","Saturn","COMPSIT","Sit and stare at one location to derive composition","Saturn COMPSIT","Measure oxygen compounds (H2O, CO2) in  stratosphere as a function of latitude. POINTING: -Y to Saturn, Z to pole Either hemisphere"]
["2011-062T04:17:00","000T09:00:00","2011-03-03","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2011-064T04:17:00","000T09:00:00","2011-03-05","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2011-065T14:27:00","000T06:00:00","2011-03-06","UVIS","Non-SPASS","Saturn","COMPSIT","Sit and stare at one location to derive composition","UVIS Rider to CIRS Compsit","UVIS Rider to CIRS Compsit"]
["2011-067T16:39:00","000T20:00:00","2011-03-08","CDA","SPASS Rider","DustRAM direction","ISD0026",null,"CDA ISD 2011-065T12:39:00","ISD observation around apoapse 2011-065T12:39:00 54.182163 Rs"]
["2011-068T15:13:00","000T05:00:00","2011-03-09","VIMS","SPASS Rider","Saturn","WIND5HR",null,"ISS Winds Ride-along","Wind observations Ride-along with ISS"]
["2011-070T13:28:00","000T01:30:00","2011-03-11","VIMS","SPASS Rider","Titan","M90R3CLD",null,"Titan Monitoring Campaign","Titan Monitoring Campaign; phase = 82 deg, range = 4 Mkm."]
["2011-076T12:58:00","000T16:00:00","2011-03-17","UVIS","Prime","Saturn","EUVFUV","UVIS EUV / FUV imaging","EUVFUV Imaging of Saturn","One slow scans across Saturn's visible hemisphere to form spectral images"]
["2011-079T01:15:00","000T17:15:00","2011-03-20","CDA","Non-SPASS","Other","RATE080B",null,"Data rate","Range enter= 13.995423 Rs exit= 13.992545 Range altitude= 3597.6194 km ... 1243.4029"]
["2011-080T12:45:00","000T04:38:00","2011-03-21","CIRS","Non-SPASS","Saturn","EUVFUV","UVIS EUV / FUV imaging","EUVFUV rider"]
["2011-086T10:03:00","000T08:00:00","2011-03-27","CIRS","SPASS Rider","InstrumentCalibration","DSCAL11",null,"CIRS_146IC_DSCAL11086_SP","rider"]
["2011-091T16:03:00","000T15:00:00","2011-04-01","CAPS","Prime","co-rotation","LLAROLPTG",null,"MAPS low latitude apoapsis w/ prime pointing","null"]
["2011-093T10:51:00","012T21:17:59","2011-04-03","CDA","Non-SPASS","Other","RATE010","Dust survey","Data rate Enter:SApo","Range enter= 14.005239 Rs exit= 14.002102 Range altitude= 1248.5606 km ... 3597.5935"]
["2011-097T07:18:00","000T17:00:00","2011-04-07","VIMS",null,"Saturn","AURSLEW","Saturn aurora","UVIS Auroral Slew Ridealong","Auroral Slew UVIS Ridealong"]
["2011-104T01:33:00","000T04:45:00","2011-04-14","CAPS","Prime","co-rotation","LLACORPTG",null,"MAPS low latitude apoapsis prime pointing","null"]
["2011-105T06:00:00","000T11:23:00","2011-04-15","CIRS","SPASS Rider","Saturn","AURSLEW","Saturn aurora","Saturn polar aurorae","null"]
["2011-108T10:18:00","000T14:42:39","2011-04-18","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG MAPS Survey","Continuous low-rate magnetospheric survey"]
["2011-109T04:00:39","000T02:00:00","2011-04-19","INMS","Non-SPASS","Titan","TITAN75",null,"Titan Flyby","Titan observation"]
["2011-109T14:00:39","000T08:37:21","2011-04-19","CIRS","SPASS Rider","Titan","HDACSTARE",null,null,"Ride along with UVIS."]
["2011-111T02:03:00","000T08:00:00","2011-04-21","CIRS","SPASS Rider","InstrumentCalibration","DSCAL11",null,"CIRS_147IC_DSCAL11111_SP","rider"]
["2011-115T16:58:00","000T00:33:00","2011-04-25","INMS","Non-SPASS","Saturn","MRO","Instrument memory readout","MRO","Startup sequence. Load FSW, Load IEB from SSR's, MRO"]
["2011-119T03:06:00","010T15:40:58","2011-04-29","CDA","Non-SPASS","Other","RATE010","Dust survey","Data rate Enter:SApo","Range enter= 14.001492 Rs exit= 14.011283 Range altitude= 1268.9020 km ... 4042.2535"]
["2011-124T16:00:00","000T23:00:00","2011-05-04","CIRS","Prime","Saturn","MIRMAP","Mid infrared map","Saturn Mid-IR map","Either hemisphere Determine upper troposphere and tropopause temperature with spatial resolution of about two degrees of latitude and longitude  POINTING: -y to Saturn, z to pole"]
["2011-127T06:00:00","000T01:00:00","2011-05-07","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT CAMPAIGN, 007 TH OBS SET IN REV 14","Turn to first satellite, take 1 NAC (CL1,CL2). Turn to second satellite take 1 NAC (CL1,CL2), repeat for up to 10 satellites if visible"]
["2011-128T18:53:45","000T08:00:00","2011-05-08","MAG","Non-SPASS","Titan","MAGTITAN","MAG Titan observation","T76 flyby","T76 is a post-dusk, upstream equatorial flyby at 1862 km altitude, similar to prime mission T34 flyby. During T76 MAG will investigate the structure of Titan's induced magnetosphere along the ram direction while being on the dayside, a geometry which is ideal for  pressure balance studies. The high altitude of periapsis (above the exobase) however limits the study of diffusion of magnetic field within the ionosphere.  We assign grade one priority. Data rate: 1976bps (32vps)."]
["2011-129T06:53:45","001T03:38:15","2011-05-09","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG MAPS Survey","Continuous low-rate magnetospheric survey"]
["2011-130T00:32:00","000T07:00:00","2011-05-10","RPWS","Non-SPASS","Saturn","INSURVEY","Inner magnetosphere survey","RPWS Inner Survey","Setup RPWS for inner magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2011-130T13:11:33","000T23:00:00","2011-05-10","INMS","Non-SPASS","Saturn","RINGPLND",null,"Ring Plane Observation","Observe neutral molecules in the equatorial plane"]
["2011-132T21:13:00","000T11:19:00","2011-05-12","INMS","Non-SPASS","Saturn","SURVEYSEG","Campaign to determine atmospheric and ionospheric thermal structure","Segment Boundary Survey","Part of the MAPS/TOST Campaign. Determine atmospheric and ionospheric thermal structure."]
["2011-136T15:30:00","000T01:30:00","2011-05-16","VIMS","SPASS Rider","Titan","M60R3CLD",null,"Titan Monitoring Campaign","Titan Monitoring Campaign; phase = 56 deg, range = 3.1 Mkm."]
["2011-138T15:30:00","000T01:30:00","2011-05-18","CIRS","SPASS Rider","Titan","M90R3CLD",null,"Rider for Titan Monitoring Campaign","Rider to ISS Titan cloud monitor"]
["2011-146T23:30:00","000T08:00:00","2011-05-26","CIRS","SPASS Rider","InstrumentCalibration","DSCAL11",null,"CIRS_148IC_DSCAL11146_SP","rider"]
["2011-155T08:00:00","000T01:30:00","2011-06-04","CIRS","SPASS Rider","Titan","M90R3CLD",null,"Rider for Titan Monitoring Campaign","Rider to ISS Titan cloud monitor"]
["2011-157T06:44:00","001T13:30:00","2011-06-06","UVIS","SPASS Rider","Iapetus","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Map uv albedo"]
["2011-161T04:00:00","000T12:00:00","2011-06-10","ISS","Prime","Star","CANOPUS1",null,"ISS PSF calibration","Point to bright star Canopus"]
["2011-168T05:57:00","000T09:26:42","2011-06-17","INMS","Non-SPASS","Saturn","SURVPOTM","MAPS survey","Post OTM Survey","Post-OTM request to resume science mode after NAV OTM."]
["2011-169T14:53:42","000T01:30:00","2011-06-18","INMS","Non-SPASS","Saturn","RINGPLND",null,"Ring Plane Observation","Observe neutral molecules in the equatorial plane"]
["2011-170T09:00:00","000T01:00:00","2011-06-19","CDA","Prime","Other","ERING","E ring observation","CDA ERING _06","CDA ERING_06; objective code RC1b"]
["2011-171T17:32:01","000T02:00:00","2011-06-20","MIMI","SPASS Rider","Titan","TITCAOV",null,"MAPS TI Campaign","Part of TI MAPS Campaign.   Investigate micro-scale and near aspects of the Titan interaction by observing during about one hour period around an encounter. With -Y pointed toward Titan, when within 30 minutes of the targeted flyby, optimize secondary axis for corotation flow as close to the S/C -X, +/- Z plane as works with the other constraints on pointing. Also, measure Titan exosphere/magnetosphere interaction by imaging in ENA with INCA (when sun is not in INCA FOV)."]
["2011-172T08:32:01","000T09:44:59","2011-06-21","CIRS","Prime","Titan","MIDIRTMAP","Mid infrared thermal map",null,"Obtain information on the thermal structure of Titan's stratosphere. Slew across disk at 4 microrad/s. Template A2: two or more dwells for ISS, 30 mins duration."]
["2011-173T07:42:00","002T04:00:00","2011-06-22","INMS","Non-SPASS","Saturn","SURVEYSEG","Campaign to determine atmospheric and ionospheric thermal structure","Segment Boundary Survey","Part of the MAPS/TOST Campaign. Determine atmospheric and ionospheric thermal structure."]
["2011-176T11:42:00","000T13:29:00","2011-06-25","ISS",null,"Titan","TEA",null,"RCI (Ridealong Context Imaging)","ISS on, max data rate = 182.784 kbps, number of frames and bits/frame are input parameters, data volume = number of frames x bits/frame, average data rate = data volume/duration."]
["2011-182T03:26:00","000T08:00:00","2011-07-01","CIRS","SPASS Rider","InstrumentCalibration","DSCAL11",null,"CIRS_150IC_DSCAL11182_SP","rider"]
["2011-184T11:53:00","000T00:07:00","2011-07-03","INMS","Non-SPASS","Saturn","RESETLOAD","INMS instrument flight software load","Flight software load","Startup sequence. Load FSW, Load IEBs, MRO"]
["2011-190T10:54:00","003T23:45:00","2011-07-09","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SURVEY Campaign","Part of SURVEY MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane.   SAT_150"]
["2011-190T12:48:11","000T23:00:00","2011-07-09","INMS","Non-SPASS","Saturn","RINGPLND",null,"Ring Plane Observation","Observe neutral molecules in the equatorial plane"]
["2011-192T11:19:00","000T01:30:00","2011-07-11","ISS","Prime","Titan","M60R2CLD",null,"Titan Monitoring Campaign","Titan Monitoring Campaign, requested phase 54.7 requested range 1.8 Mkm"]
["2011-194T11:18:00","000T00:02:00","2011-07-13","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2011-199T01:58:00","000T00:02:00","2011-07-18","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2011-202T12:10:21","000T00:00:01","2011-07-21","MP","SPASS Note","Saturn","APOAPSE","Apoapse",null,"Apoapse  Per = 21.7 d, inc = 0.4 deg, r = 45.664 Rs, phase = 45 deg"]
["2011-205T16:00:00","000T01:30:00","2011-07-24","CIRS","SPASS Rider","Titan","M90R2CLD",null,"Rider for Titan Monitoring Campaign","Rider to ISS Titan cloud monitor"]
["2011-211T03:07:00","008T05:59:00","2011-07-30","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","null"]
["2011-211T03:07:00","008T05:59:00","2011-07-30","MIMI","Non-SPASS","co-rotation","SURVEYOV",null,"MAPS SURVEY Campaign Overlay","Overlay:  adding 250 bps  Part of SURVEY MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane."]
["2011-213T08:12:28","000T00:00:01","2011-08-01","MP","SPASS Note","Saturn","PERIAPSE","Periapse",null,"Periapse R = 4.045 Rs, lat = -0 deg, phase = 135 deg"]
["2011-215T21:01:00","000T09:59:00","2011-08-03","MAG","Prime","Sun","CALROLL","MAG calibration roll","MAG Calibration Rolls","Roll about axis other than Z for determination of sensor offsets, actual roll axis is not important - selected axis is usually suitable for MAPS.  Preferably calibrations should be made every 15-20 days in areas where field conditions are suitable.  Note: periods of suitable data are defined as follows; 1) More distant than 15 RS from Saturn's axis (to try and get into the more uniform part of the internal+sheet field). 2) Inside the magnetopause (more specifically inside a most compressed model MP). 3) More distant than 3 RS from the current sheet. Using a 'hinged' sheet model which departs from Saturn's equatorial plane at about 15 RS and then follows the anti-solar direction on the nightside. This means that, even though its orbit is equatorial, if the spacecraft is situated far enough away from the planet, it should see the nightside current sheet divert northwards away from it (using Saturn axis tilted 17 deg away from Sun).  Apart from possible injection events, sheet disruptions etc the resultant periods should have a reasonable probability of seeing a 'quiescent' 'lobe-like' or 'disk-like' field. We would prefer as far downtail as possible so the field has more chance of pointing in a single direction over larger length scales."]
["2011-219T11:16:00","000T03:00:00","2011-08-07","UVIS","Non-SPASS","Saturn","WIND",null,"UVIS Rider to ISS WIND","UVIS Rider to ISS WIND sit-and-stare"]
["2011-220T04:16:00","000T08:00:00","2011-08-08","UVIS","Non-SPASS","Saturn","COMPSIT","Sit and stare at one location to derive composition","UVIS Rider to CIRS Compsit","UVIS Rider to CIRS Compsit"]
["2011-222T08:40:00","000T05:00:00","2011-08-10","CIRS",null,"Saturn","WIND5HR",null,"low emit COMPSIT near-Equator avoid rings"]
["2011-225T09:30:00","000T06:00:00","2011-08-13","UVIS","Non-SPASS","Saturn","COMPSIT","Sit and stare at one location to derive composition","UVIS Rider to CIRS Compsit","UVIS Rider to CIRS Compsit"]
["2011-226T07:30:00","000T05:00:00","2011-08-14","ISS","Prime","Saturn","WIND5HR",null,"Wind measuring 5-6-5 template + polarimetry, 5-hr","Stare and shoot every 10 min to mosaic in longitude, part of the windspeed template. CB2, (2x2 MT2, MT3,BL1) NAC  Cycled while observation lasts. First 9 minutes is a 13-filter polarmetry block (see the note)"]
["2011-229T15:12:00","000T04:00:00","2011-08-17","ISS","Prime","Saturn","WIND4HR",null,"Wind measuring 4-7-4 template + polarimetry, 4-hr","CHANGED to 3hrs to cut data volumeStare and shoot every 10 min to mosaic in longitude, part of the windspeed template. CB2, (2x2 MT2, MT3,BL1) NAC  Cycled while observation lasts. First 9 minutes is a 13-filter polarmetry block (see the note)"]
["2011-234T02:32:58","000T20:11:00","2011-08-22","CDA","Non-SPASS","Other","RATE080","Dust survey","Data rate","Range enter= 13.990292 Rs exit= 13.998431 Range altitude= 5380.5031 km ... -1234.5231"]
["2011-234T18:44:00","000T05:36:00","2011-08-22","UVIS","Prime","Saturn","EUVFUV","UVIS EUV / FUV imaging","EUVFUV Imaging of Saturn","One slow scans across Saturn's visible hemisphere to form spectral images"]
["2011-235T18:30:00","000T08:30:00","2011-08-23","CDA","Non-SPASS","Other","RATE080A",null,"Data rate","Range enter= 13.990292 Rs exit= 13.998431 Range altitude= 5380.5031 km ... -1234.5231"]
["2011-237T23:49:00","000T08:00:00","2011-08-25","CIRS","SPASS Rider","InstrumentCalibration","DSCAL11",null,"CIRS_152IC_DSCAL11237_SP","rider"]
["2011-240T09:19:00","000T22:00:00","2011-08-28","CDA","Prime","DustRAM direction","ISD0033",null,"CDA ISD","ISD observation around apoapse 2011-246T01:47:00 45.911332 Rs"]
["2011-243T01:03:00","000T13:30:00","2011-08-31","CDA","Prime","DustRAM direction","ISD0033",null,"CDA ISD 2011-246T01:47:00","ISD observation around apoapse 2011-246T01:47:00 45.911332 Rs"]
["2011-249T02:00:00","000T01:30:00","2011-09-06","VIMS","SPASS Rider","Titan","M90R3CLD",null,"Titan Monitoring Campaign","Titan Monitoring Campaign; phase = 22 deg, range = 2.8 Mkm."]
["2011-250T01:45:00","000T01:30:00","2011-09-07","CIRS","SPASS Rider","Titan","M90R3CLD",null,"Rider for Titan Monitoring Campaign","Rider to ISS Titan cloud monitor"]
["2011-250T17:48:00","000T01:00:00","2011-09-07","RSS","Prime","Earth","BORESIGHT","HGA boresight calibration","HGA Boresight Calibration","HGA Boresight Calibration. Pointing=XBAND to Earth + crosshair maneuver.  Telemetry OFF, TWNC ON for 1-hr calibration from 2011-250T17:48:00 to 2011-250T18:48:00.  Required to be tracked by DSS-25 (or DSS-26).  Keep Ka-band ON until EOT at 2011-251T00:48:00.  Playback of telemetry required afterwards for C-Kernel generation."]
["2011-254T00:00:00","000T00:34:00","2011-09-11","INMS","Non-SPASS","Saturn","MRO","Instrument memory readout","MRO","Backup MRO"]
["2011-255T00:50:06","000T01:00:00","2011-09-12","CAPS","SPASS Rider","Titan","T78INBND",null,"Inbound 153TI (T78)","null"]
["2011-255T17:47:00","000T13:00:00","2011-09-12","CIRS","SPASS Rider","InstrumentCalibration","DSCAL11",null,"CIRS_153IC_DSCAL11255_SP","rider"]
["2011-256T18:35:01","000T03:24:59","2011-09-13","CDA","Prime","Other","RINGSHAD",null,"CDA Ring Shadow Crossing1_4Rs","CDA Ring Shadow Crossing @ 4Rs; objective code RC1a"]
["2011-257T01:00:00","000T01:30:00","2011-09-14","UVIS","SPASS Rider","Pallene","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2011-258T02:26:00","000T14:21:00","2011-09-15","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2011-260T00:20:00","000T00:02:00","2011-09-17","VIMS","SPASS Rider","Saturn","STORMW","Saturn storm watch","Storm Watch Ridealong","Stiorm Watch: 32*32 pixels with 80 msec integration"]
["2011-260T10:02:00","002T20:15:00","2011-09-17","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG MAPS Survey","Continuous low-rate magnetospheric survey"]
["2011-262T21:17:00","000T09:00:00","2011-09-19","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2011-265T17:58:00","000T00:02:00","2011-09-22","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2011-265T19:59:00","000T02:00:00","2011-09-22","INMS","Non-SPASS","Saturn","ENGBCKGND",null,"Engineering background observation","Full rate measurement to gather engineering background data"]
["2011-269T08:02:00","000T08:00:00","2011-09-26","CIRS","SPASS Rider","InstrumentCalibration","DSCAL11",null,"CIRS_154IC_DSCAL11269_SP","rider"]
["2011-273T03:00:00","000T08:52:00","2011-09-30","CIRS","SPASS Rider","Saturn","AURSLEW","Saturn aurora","Saturn polar aurorae","null"]
["2011-274T01:52:26","000T10:00:00","2011-10-01","INMS","Non-SPASS","Enceladus","E14INBND",null,"Enceladus flyby","Enceladus observation"]
["2011-274T14:19:26","000T03:40:34","2011-10-01","CIRS","SPASS Rider","Enceladus","FP1SECLX",null,"CIRS_154EN_FP1SECLX001 eclipse support images","Five clear WAC images (at 50 second intervals centered on nominal eclipse exit at 2011-274T14:49:51)  at 2011-274T14:48:11, T14:49:01, T14:49:51, T14:50:41, and T14:51:31.  CLR1-CLR2; 2x2 summation mode."]
["2011-276T02:00:00","000T01:24:00","2011-10-03","RPWS","Non-SPASS","co-rotation","HIRATE","High rate mode","MAPS MB,A Campaign","Part of MB,A MAPS Campaign.  Observe plasma waves on dawn-side magnetospheric boundaries at a variety of radial distances"]
["2011-277T02:30:00","000T12:00:00","2011-10-04","CIRS","Prime","Saturn","COMPSIT","Sit and stare at one location to derive composition","Saturn COMPSIT","Measure oxygen compounds (H2O, CO2) in  stratosphere as a function of latitude. POINTING: -Y to Saturn, Z to pole Either hemisphere"]
["2011-277T19:28:00","000T00:02:00","2011-10-04","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2011-280T06:00:00","000T12:00:00","2011-10-07","UVIS","Prime","Saturn","MOS154APO",null,null,"Mosaic scan of Saturn magnetosphere, day 2. Scan will focus on vicinity of Saturn disk to image oxygen. Overall extent of scan: +/- 2.5 Rs E-W and N-S (one quadrant covered in each of the first four observation periods; fifth period covers Saturn disk).  EUV and FUV low resolution slits on. Note: data to be taken only when slit is stationary. Allowances for 20 minutes of observation margin at start and end, and 30 minutes for turn to waypoint at end, have been made.  Start at WAYPOINT (Saturn center). Align slit with Saturn spin axis. Slew +32 mrad about x axis. Start data capture, stare 755.0 s, stop data capture. Repeat PATTERN 45 times.  PATTERN: Slew -1.5 mrad about z-axis. Start data capture, stare 755.0 s, stop data capture.  Note: As no data will be collected while Cassini is slewing, actual data volume = (1603.71989 bps, from Alain's spreadsheet)x(755.0s per stare)x(46 stares) = 55.6972x10^6 bits. Data rate multiplier includes an extra 1% per Alain because of data packet filling issues."]
["2011-282T06:58:00","000T00:02:00","2011-10-09","VIMS","SPASS Rider","Saturn","STORMW","Saturn storm watch","Storm Watch Ridealong","Stiorm Watch: 32*32 pixels with 80 msec integration"]
["2011-284T05:01:00","006T12:47:00","2011-10-11","INMS","Non-SPASS","Saturn","SURVBOTM","MAPS survey","Post OTM Survey","Post-OTM request to resume science mode after NAV OTM."]
["2011-290T05:46:00","000T09:00:00","2011-10-17","RSS","SPASS Rider","Earth","SCE8",null,"Solar Conjunction Experiment (SCE) #8","Characterize the solar corona at 2 frequency bands (X and Ka1 or X and S, depending on DSN antenna requested by SP), and assess the electron content and possible Faraday rotation, during the solar conjunction period."]
["2011-291T05:46:00","000T09:00:00","2011-10-18","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2011-291T23:50:00","000T02:00:00","2011-10-18","CIRS","SPASS Rider","Titan","CLOUD",null,null,"null"]
["2011-292T08:52:12","000T01:00:00","2011-10-19","MIMI","Non-SPASS","Enceladus","ENCNTROV",null,"MIMI Enceladus 142","BIT_OVERLAY_300"]
["2011-293T15:28:00","000T00:02:00","2011-10-20","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2011-295T07:28:00","000T00:02:00","2011-10-22","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2011-295T14:30:00","000T03:30:00","2011-10-22","CAPS","Prime","co-rotation","IONCALPTG",null,"IMS and IBS calibration","null"]
["2011-300T05:17:00","000T09:00:00","2011-10-27","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2011-303T14:02:00","000T13:30:00","2011-10-30","CIRS","Prime","Titan","TEA",null,"Titan Composition","Titan composition"]
["2011-308T23:00:00","000T11:00:00","2011-11-04","UVIS","Prime","Saturn","AURSLEW","Saturn aurora","Saturn Aurora","Auroral Observations led by UVIS Repeated slews across the auroral oval"]
["2011-309T21:17:00","001T14:08:00","2011-11-05","RPWS","Non-SPASS","Saturn","INSURVEY","Inner magnetosphere survey","RPWS Inner Survey","Setup RPWS for inner magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2011-310T04:51:29","000T00:44:24","2011-11-06","RADAR","Prime","Enceladus","ENCELCA",null,"E16 Inb/outb Imaging Near C/A","SOST E16 PIE."]
["2011-310T11:55:00","001T15:37:00","2011-11-06","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG MAPS Survey","Continuous low-rate magnetospheric survey"]
["2011-312T03:32:00","007T02:41:00","2011-11-08","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SURVEY Campaign","Part of SURVEY MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane.   MAG_156_157"]
["2011-319T06:12:47","000T00:00:01","2011-11-15","MP","SPASS Note","Saturn","APOAPSE","Apoapse",null,"Apoapse  Per = 17.9 d, inc = 0.2 deg, r = 40.424 Rs, phase = 50 deg"]
["2011-322T04:00:00","000T12:00:00","2011-11-18","RPWS","Non-SPASS","co-rotation","HIRATE","High rate mode","RPWS High Rate Campaign","RPWS high rate observations when we have extra bits"]
["2011-326T18:33:00","000T08:00:00","2011-11-22","CIRS","SPASS Rider","InstrumentCalibration","DSCAL11",null,"CIRS_157IC_DSCAL11326_SP","rider"]
["2011-327T03:13:00","000T01:30:00","2011-11-23","ISS","Prime","Titan","M90R3CLD",null,"Titan Monitoring Campaign","Titan Monitoring Campaign, requested phase 86.6 requested range 2.1 Mkm"]
["2011-328T04:13:00","000T03:00:00","2011-11-24","RPWS","Non-SPASS","Saturn","CHORUS",null,"RPWS CHORUS Campaign","Part of RPWS Chorus campaign, attempt to get high rate data from within L Shell of 8"]
["2011-331T04:33:00","000T08:00:00","2011-11-27","CIRS","SPASS Rider","InstrumentCalibration","DSCAL11",null,"CIRS_157IC_DSCAL11331_SP","rider"]
["2011-333T20:00:00","000T16:30:00","2011-11-29","RPWS","Non-SPASS","co-rotation","HIRATE","High rate mode","RPWS High Rate Campaign","RPWS high rate observations when we have extra bits"]
["2011-336T02:04:00","000T23:45:00","2011-12-02","INMS","Non-SPASS","Saturn","SURVPOTMA",null,"Post OTM Survey","Post-OTM request to resume science mode after NAV OTM."]
["2011-340T16:34:00","000T09:00:00","2011-12-06","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2011-342T03:49:00","000T08:00:00","2011-12-08","CIRS","SPASS Rider","InstrumentCalibration","DSCAL11",null,"CIRS_158IC_DSCAL11342_SP","rider"]
["2011-343T03:49:00","000T08:00:00","2011-12-09","CIRS","SPASS Rider","InstrumentCalibration","DSCAL11",null,"CIRS_158IC_DSCAL11343_SP","rider"]
["2011-344T22:36:00","002T06:52:00","2011-12-10","RPWS","Non-SPASS","Saturn","INSURVEY","Inner magnetosphere survey","RPWS Inner Survey","Setup RPWS for inner magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2011-346T04:09:22","000T02:30:00","2011-12-12","CIRS",null,"Enceladus","ENCEL","Enceladus",null,"null"]
["2011-346T08:39:22","000T02:00:00","2011-12-12","RPWS","Non-SPASS","Dione","DICA",null,"RPWS Dione closest approach observations","Make high resolution RPWS observations of the magnetosphere - Dione interaction using WBR, WFR, and LP."]
["2011-347T15:11:24","000T02:45:00","2011-12-13","UVIS","Non-SPASS","Titan","FIRNADMAP","Far infrared nadir composition map","Rider to CIRS","Rider to CIRS."]
["2011-347T21:11:24","000T01:00:00","2011-12-13","MIMI","SPASS Rider","Titan","TITOUTOV",null,"MAPS TI Campaign","Part of TI MAPS Campaign.   Investigate micro-scale and near aspects of the Titan interaction by observing during about one hour period around an encounter. With -Y pointed toward Titan, when within 30 minutes of the targeted flyby, optimize secondary axis for corotation flow as close to the S/C -X, +/- Z plane as works with the other constraints on pointing. Also, measure Titan exosphere/magnetosphere interaction by imaging in ENA with INCA (when sun is not in INCA FOV)."]
["2011-348T10:11:24","000T02:28:36","2011-12-14","VIMS","SPASS Rider","Titan","MIDIRTMAP","Mid infrared thermal map","Titan scan.","VIMS ridealong with CIRS while scanning across Titan.  Phase = 16 deg.  SSC Lat/Lon = 0.603S/212.230 deg, SS Lat/Lon = 12.358N/201.896 deg.  Alt = 278235.240 and range = 280810.240 km.  Resolution = 139 km/px.  Temp. A.  Obtain cubes while scanning across Titan."]
["2011-349T18:15:00","000T03:00:00","2011-12-15","VIMS","SPASS Rider","Titan","CLOUDMAP","Cloud map","Titan Cloud monitoring","VIMS ridealong with ISS for cloud monitoring.  Phase = 14 deg, SSC Lat/Lon = 0.66S/237 deg, SS Lat/Lon = 12N/232 deg.  Alt = 968156 km, range = 970731 km.  Resolution = 484 km/px.  Obtain 160 and 640 ms cubes for cloud mapping during caboose segment."]
["2011-353T03:21:00","000T08:00:00","2011-12-19","CIRS","SPASS Rider","InstrumentCalibration","DSCAL11",null,"CIRS_158IC_DSCAL11353_SP","rider"]
["2011-355T21:44:00","000T00:02:00","2011-12-21","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2011-358T03:00:00","008T21:22:00","2011-12-24","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","Survey","Part of the MAPS/TOST Campaign. Determine atmospheric and ionospheric thermal structure."]
["2011-359T16:36:00","000T08:00:00","2011-12-25","CIRS","SPASS Rider","InstrumentCalibration","DSCAL11",null,"CIRS_159IC_DSCAL11359_SP","rider"]
["2011-361T09:44:00","000T00:02:00","2011-12-27","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2012-002T00:22:00","000T10:51:37","2012-01-02","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG MAPS Survey","Continuous low-rate magnetospheric survey"]
["2012-002T10:13:37","000T02:45:00","2012-01-02","VIMS","SPASS Rider","Titan","FIRNADMAP","Far infrared nadir composition map","Titan scan.","VIMS ridealong with CIRS while scanning across Titan.  Phase = 114 deg, SSC Lat/Lon = 16.662S/158.933 deg, SS Lat/Lon = 12.593N/270.344 deg.  Alt =100963.1 km, range = 103538.1 km.  Resolution = 50 km/px.  Temp. T.  Obtain cubes while scanning across Titan."]
["2012-002T17:28:37","000T02:45:00","2012-01-02","RADAR","Prime","Titan","T80OUTRAD",null,"T80 Outbound Radiometry"]
["2012-004T05:00:00","000T12:00:00","2012-01-04","RPWS","Non-SPASS","Saturn","CHORUS",null,"RPWS CHORUS Campaign","Part of RPWS Chorus campaign, attempt to get high rate data from within L Shell of 8"]
["2012-004T12:45:00","003T11:08:00","2012-01-04","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","null"]
["2012-006T00:48:00","000T08:00:00","2012-01-06","UVIS","SPASS Rider","Other","OUTERSATS","Icy satellite observaton","ICYLON:  Icy Satellite Longitude / Phase Coverage","Measure satellite albedo in ultraviolet light for a good sampling of longitude and phase space.  Determine phase function to investigate surface microstructure and frost properties, as a function of location."]
["2012-009T09:23:00","000T08:00:00","2012-01-09","CIRS","SPASS Rider","InstrumentCalibration","DSCAL12",null,"CIRS_159IC_DSCAL12009_SP","rider"]
["2012-010T11:33:00","000T05:00:00","2012-01-10","UVIS","Non-SPASS","Saturn","WIND5HR",null,"UVIS Rider to ISS WIND","UVIS Rider to ISS WIND sit-and-stare"]
["2012-012T00:39:00","000T09:00:00","2012-01-12","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2012-014T10:17:00","000T00:02:00","2012-01-14","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2012-014T10:19:00","000T01:30:00","2012-01-14","VIMS","SPASS Rider","Titan","M90R3CLD",null,"Titan Monitoring Campaign","Titan Monitoring Campaign; phase = 73 range =2.1 Mkm."]
["2012-017T01:46:00","000T20:00:00","2012-01-17","CDA","SPASS Rider","DustRAM direction","ISD0040",null,"CDA ISD 2012-016T15:46:00","ISD observation around apoapse 2012-016T15:46:00 49.163222 Rs"]
["2012-017T22:35:00","000T02:00:00","2012-01-17","ISS","Prime","Saturn","WIND2HR",null,"Wind measuring 5-6-5 template + polarimetry, 5-hr","Track features for ~2 hours to get the 2-hr time step for winds, mosaic in longitude, part of the windspeed template. CB2, (2x2 MT2, MT3,BL1) NAC  Cycled while observation lasts. First 9 minutes is a 13-filter polarmetry block (see the note)"]
["2012-018T23:50:00","000T01:30:00","2012-01-18","CIRS","SPASS Rider","Titan","M60R3CLD",null,"Rider for Titan Monitoring Campaign","Rider to ISS Titan cloud monitor"]
["2012-021T01:18:00","000T00:02:00","2012-01-21","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2012-023T01:05:00","000T22:00:00","2012-01-23","VIMS","SPASS Rider","Saturn","MIRMAP","Mid infrared map","CIRS MIRMAP Ride-along","MIRMAP ridelong with CIRS"]
["2012-024T22:55:00","000T20:00:00","2012-01-24","CDA","Non-SPASS","Other","DECON","Decontamination","Decon in S72","SSR-Load (6Ext_Mem_Load) planned to be at exactly 2012-024T23:55:00.  One hour apart from the preceeding D/L (SP_160EA_C70METSEQ024_PRIME) having a carryover with 0 MB. Expectations is that a SSR-Ping-Pong disable might not be necessary.  No additional DV necessary"]
["2012-025T21:44:00","000T00:02:00","2012-01-25","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2012-028T17:10:40","000T02:34:00","2012-01-28","INMS","Non-SPASS","Saturn","RINGPLND",null,"Ring Plane Observation","Observe neutral molecules in the equatorial plane"]
["2012-030T11:24:48","000T05:00:00","2012-01-30","VIMS","SPASS Rider","Titan","REGMAP","Regional mapping","Regional mapping of Titan.","VIMS ridealong with ISS during C/A. At C/A, phase = 96.3 deg.  SSC Lat/Lon = 59.98S/104.91 deg, SS Lat/Lon = 12.964N/184.833 deg.  Alt = 31130.2 km, range = 33705.2 km.  Resolution = 15.6 km/px.  Obtain mosaics and cubes for regional mapping."]
["2012-030T17:39:48","000T23:01:12","2012-01-30","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG MAPS Survey","Continuous low-rate magnetospheric survey"]
["2012-031T22:00:00","002T00:00:00","2012-01-31","CDA","SPASS Rider","DustRAM direction","RETROGRAD",null,"CDA Retrograde campaign","Retrograde observation - outbound leg - Apo region"]
["2012-035T00:27:00","000T08:00:00","2012-02-04","CIRS","SPASS Rider","InstrumentCalibration","DSCAL12",null,"CIRS_160IC_DSCAL12034_SP","rider"]
["2012-037T17:52:00","000T01:00:00","2012-02-06","VIMS","SPASS Rider","Saturn","STORMW","Saturn storm watch","Storm Watch Ridealong","Stiorm Watch: 32*32 pixels with 80 msec integration"]
["2012-041T06:28:00","008T08:31:00","2012-02-10","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG MAPS Survey","Continuous low-rate magnetospheric survey"]
["2012-044T22:54:00","000T01:30:00","2012-02-13","VIMS","SPASS Rider","Saturn","STORMW","Saturn storm watch","Storm Watch Ridealong","Stiorm Watch: 32*32 pixels with 80 msec integration"]
["2012-047T09:51:00","000T00:02:00","2012-02-16","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2012-048T07:29:00","001T01:14:17","2012-02-17","INMS","Non-SPASS","Saturn","SURVBOTM","MAPS survey","Post OTM Survey","Post-OTM request to resume science mode after NAV OTM."]
["2012-049T20:43:17","000T02:00:00","2012-02-18","VIMS","SPASS Rider","Titan","FIRNADCMP","Far infrared nadir composition map","Stare at Titan.","VIMS ridealong with CIRS.  Phase = 118 deg.  SSC Lat/Lon = 0.565S/140.626 deg, SS Lat/Lon = 13.199N/258.951 deg.  Alt = 260248.5 km, range =262823.5 km.  Resolution = 130 km/px.  Temp. N.  Obtain cubes of Titan for global mapping."]
["2012-050T07:58:17","000T00:45:00","2012-02-19","VIMS","SPASS Rider","Titan","REGMAP","Regional mapping","Regional mapping.","VIMS ridealong with CIRS during C/A.  At C/A, Phase = 142.6 deg.  SSC Lat/Lon = 9.779N/61.442 deg, SS Lat/Lon = 13.203N/271.164 deg.  Alt = 3803.3 km, range = 6378.3 km.  Resolution = 1.9 km/px.  Obtain mosaics and cubes of Titan during C/A."]
["2012-050T10:58:17","000T02:45:00","2012-02-19","CIRS","Prime","Titan","FIRNADMAP","Far infrared nadir composition map","CIRS_014TI_FIRNADIRMAP_01","Obtain information on surface & tropopause temperatures, and on tropospheric CH4.  Scan  or contiguous steps across disk.  POINTING: -y to Titan, x away from sun.  Z axis generally aligned N/S or E/W, perpendicular to scan or steps."]
["2012-050T23:14:00","000T08:30:00","2012-02-19","CIRS","SPASS Rider","InstrumentCalibration","DSCAL12",null,"CIRS_161IC_DSCAL12050_SP","rider"]
["2012-052T21:54:00","000T10:51:00","2012-02-21","CAPS","Prime","Saturn","EQIMAGPTG",null,"MAPS equatorial inner magnetosphere","null"]
["2012-055T09:07:00","000T00:02:00","2012-02-24","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2012-056T19:48:00","000T00:02:00","2012-02-25","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2012-062T06:15:00","000T08:00:00","2012-03-02","CIRS","SPASS Rider","InstrumentCalibration","DSCAL12",null,"CIRS_162IC_DSCAL12062_SP","rider"]
["2012-067T05:46:00","000T08:00:00","2012-03-07","CIRS","SPASS Rider","InstrumentCalibration","DSCAL12",null,"CIRS_162IC_DSCAL12067_SP","rider"]
["2012-068T20:01:00","000T02:23:08","2012-03-08","INMS","Non-SPASS","Saturn","SURVEYSEG","Campaign to determine atmospheric and ionospheric thermal structure","Segment Boundary Survey","Part of the MAPS/TOST Campaign. Determine atmospheric and ionospheric thermal structure."]
["2012-070T15:00:00","000T01:30:00","2012-03-10","UVIS",null,"Rhea","ICYMAP","Icy satellite surface map","ICYMAP:  UV Surface Map of Rhea, ORS Rider","UV albedo map of Rhea's surface plus limb drifts"]
["2012-071T06:01:00","007T17:54:00","2012-03-11","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2012-072T01:00:00","000T01:00:00","2012-03-12","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT CAMPAIGN, 003 RD OBS SET IN REV 16","Turn to first satellite, take 1 NAC (CL1,CL2). Turn to second satellite take 1 NAC (CL1,CL2), repeat for up to 10 satellites if visible"]
["2012-074T00:39:00","000T00:02:00","2012-03-14","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2012-078T14:58:00","000T00:02:00","2012-03-18","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2012-080T00:30:00","000T01:30:00","2012-03-20","CIRS","SPASS Rider","Titan","M90R2CLD",null,"Rider for Titan Monitoring Campaign","Rider to ISS Titan cloud monitor"]
["2012-083T17:00:00","000T16:00:00","2012-03-23","VIMS","SPASS Rider","Saturn","STORMW","Saturn storm watch","Storm Watch Ridealong","Stiorm Watch: 32*32 pixels with 80 msec integration"]
["2012-084T20:00:00","000T02:00:00","2012-03-24","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT CAMPAIGN, 006 TH OBS SET IN REV 16","Turn to first satellite, take 1 NAC (CL1,CL2). Turn to second satellite take 1 NAC (CL1,CL2), repeat for up to 10 satellites if visible"]
["2012-086T19:27:00","000T01:30:00","2012-03-26","CIRS","SPASS Rider","Titan","M60R2CLD",null,"Rider for Titan Monitoring Campaign","Rider to ISS Titan cloud monitor"]
["2012-087T21:10:00","000T03:40:00","2012-03-27","ISS","Prime","Janus","JANUS","Janus","Janus ORS observation","ORS observation"]
["2012-088T10:00:00","000T02:00:00","2012-03-28","INMS","Non-SPASS","Saturn","INNERMAG","Observing neutral molecules in the inner magnetosphere","Inner Mag Survey","Inner magnetospheric survey"]
["2012-088T22:42:00","000T03:33:00","2012-03-28","VIMS","SPASS Rider","Other","L5RHEA",null,"Rock spectra","ISS NAC to Rocks 160, 640ms IR"]
["2012-089T07:22:00","000T06:40:00","2012-03-29","MAG","Non-SPASS","Other","R1DLROLL","MAG downlink roll calibration","MAG_R1_DLROLL_CAL","Rider on rolling downlink with MAG FGM in range 1. Used for calibration of range 1. Rides on current MAG activities - no additional power or datavolume used."]
["2012-095T04:02:00","000T08:00:00","2012-04-04","CIRS","SPASS Rider","InstrumentCalibration","DSCAL12",null,"CIRS_163IC_DSCAL12095_SP","rider"]
["2012-096T19:17:00","000T16:30:00","2012-04-05","CDA","Non-SPASS","Other","RATE010","Dust survey","Data rate Enter:SApo End: S73","Range enter= 14.006619 Rs exit= 14.000931 Range altitude= 1600.2676 km ... 5554.0959"]
["2012-098T19:47:00","000T05:16:00","2012-04-07","CDA","Prime","DustRAM direction","ISD0044",null,"CDA ISD 2012-096T19:17:00","ISD observation around apoapse 2012-096T19:17:00 40.400826 Rs"]
["2012-101T13:00:00","000T09:00:00","2012-04-10","RPWS","Non-SPASS","co-rotation","HIRATE","High rate mode","RPWS High Rate Campaign","RPWS high rate observations when we have extra bits"]
["2012-102T19:58:00","000T01:00:00","2012-04-11","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT CAMPAIGN, 006 TH OBS SET IN REV 16","Turn to first satellite, take 1 NAC (CL1,CL2). Turn to second satellite take 1 NAC (CL1,CL2), repeat for up to 10 satellites if visible"]
["2012-104T17:33:00","001T15:45:00","2012-04-13","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SURVEY Campaign","Part of SURVEY MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane.   SOST_164_E18 part 1"]
["2012-105T16:01:38","000T04:58:22","2012-04-14","MAG","Non-SPASS","Other","INTFLD","MAG Internal field observation","MAG_Internal_Field_Measurements","This request will yield unique observations of Saturns internal magnetic field over a unique orbit track in latitude and longitude space."]
["2012-106T00:30:00","000T02:00:00","2012-04-15","UVIS","SPASS Rider","Tethys","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2012-106T22:08:00","000T01:30:00","2012-04-15","CIRS","Prime","Rhea","RHEA","Rhea",null,"Old shutter closed request (subsequently changed to Lego table): Shutter closed details: 15.67 cm-1 resolution No Add, FP1 Data, FP3 Data, FP3 Blink, FP4 Data, FP4 Blink. Requested shutter closed time: 2012-106T22:36:10-22:40:10  This is a daytime observation (small dark crescent - phase is <40 deg) with dark sky behind. Rhea is only slightly larger than the FP3/4 FOV and Rhea is smaller than the FP1 fov.  Preliminary Plan: 22:08 - 22:10 Turn  22:10 - 22:36 Global FP3/4 coverage (2 swaths) at 6 mu rad/s [Please schedule the first FP3/4 shutter closed observation to take place during this FP1 stare using table number 355:1] 22:36 - 22:41 FP1 stare, centered on Rhea's center 22:41 - 23:26 2 x Global FP3/4 coverage (2 swaths each) at 6 mu rad/s 23:26 - 23:38 Turn"]
["2012-110T03:18:00","004T11:28:00","2012-04-19","INMS","Non-SPASS","Saturn","SURVBOTM","MAPS survey","Post OTM Survey","Post-OTM request to resume science mode after NAV OTM."]
["2012-111T11:28:00","000T02:00:00","2012-04-20","ISS","Prime","Titan","M90R1CLD",null,"Titan Monitoring Campaign","Titan Monitoring Campaign, requested phase 69.8 requested range 1.1 Mkm"]
["2012-111T13:26:00","000T00:02:00","2012-04-20","VIMS","SPASS Rider","Saturn","STORMW","Saturn storm watch","Storm Watch Ridealong","Storm Watch: 32*32 pixels with 80 msec integration"]
["2012-114T12:41:00","000T00:02:00","2012-04-23","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2012-116T10:32:00","003T23:45:00","2012-04-25","INMS","Non-SPASS","Saturn","SURVBOTM","MAPS survey","Post OTM Survey","Post-OTM request to resume science mode after NAV OTM."]
["2012-119T10:55:00","000T00:02:00","2012-04-28","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2012-122T10:02:00","002T23:45:00","2012-05-01","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SURVEY Campaign","Part of SURVEY MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane.   SOST_165_E19"]
["2012-123T07:31:29","000T04:00:00","2012-05-02","MAG","Non-SPASS","Enceladus","ENTAR","Enceladus","Enceladus targeted flyby","Monitor the interaction of Enceladus with the Saturnian magnetospheric plasma and determine whether it generates an internal magnetic field."]
["2012-123T10:31:29","001T23:15:31","2012-05-02","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","null"]
["2012-124T01:41:00","000T02:00:00","2012-05-03","RPWS","Non-SPASS","rings(general)","RPXING","Measurements of dust flux, scale height and plasma waves at the magnetic equator during ring plane crossing","RPWS Ring Plane Crossing","Determine the equatorial dust flux and scale height as a function of radial distance.  Obtain high resolution of plasma waves at the magnetic equator."]
["2012-127T09:47:00","000T23:45:00","2012-05-06","INMS","Non-SPASS","Saturn","SURVPOTM","MAPS survey","Post OTM Survey","Post-OTM request to resume science mode after NAV OTM."]
["2012-132T09:33:00","000T00:33:00","2012-05-11","INMS","Non-SPASS","Saturn","MRO","Instrument memory readout","MRO","MRO"]
["2012-135T01:01:00","000T08:00:00","2012-05-14","CIRS","SPASS Rider","InstrumentCalibration","DSCAL12",null,"CIRS_166IC_DSCAL12134_SP","rider"]
["2012-136T09:01:00","000T13:30:00","2012-05-15","VIMS",null,"Saturn","AURSTARE","Saturn aurora","UVIS Auroral Stare Ridealong.","Auroral Stare Ridealong"]
["2012-138T08:46:00","000T12:00:00","2012-05-17","ISS",null,"Saturn","AURSTARE","Saturn aurora","NAC aurora stare greyscale","CL1 NAC 4x4 images.  10 Mbits/hr, only half of the time expected to be a stare"]
["2012-140T00:46:00","000T08:00:00","2012-05-19","CIRS","SPASS Rider","InstrumentCalibration","DSCAL12",null,"CIRS_166IC_DSCAL12139_SP","rider"]
["2012-141T06:34:00","000T01:52:00","2012-05-20","UVIS",null,"Methone","ICYLON","Icy satellite longitudinal coverage","ICYLON:  Longitude / Phase Space Coverage","Target to icy satellite.  Measure uv albedo across longitude / phase space.  Opportunities selected by SOST-ORS consortium.  Slit orientation is flexible."]
["2012-142T08:31:00","000T12:39:11","2012-05-21","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG MAPS Survey","Continuous low-rate magnetospheric survey"]
["2012-143T01:05:11","000T00:05:00","2012-05-22","RADAR","Prime","Titan","T83IRASAR",null,"T83 Inbound Ride-along SAR"]
["2012-143T01:28:11","000T00:12:00","2012-05-22","RADAR","Prime","Titan","T83OUTALT",null,"T83 Outbound Altimetry"]
["2012-144T02:01:00","007T05:59:00","2012-05-23","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG MAPS Survey","Continuous low-rate magnetospheric survey"]
["2012-148T08:56:00","000T01:30:00","2012-05-27","VIMS","SPASS Rider","Titan","M60R3CLD",null,"Titan Monitoring Campaign and Stormwatch","Titan Monitoring Campaign and Stormwatch; phase = 32 deg, range =2.5 Mkm."]
["2012-150T08:40:00","000T01:30:00","2012-05-29","CIRS","SPASS Rider","Titan","M60R3CLD",null,"Rider for Titan Monitoring Campaign","Rider to ISS Titan cloud monitor"]
["2012-151T23:00:00","000T09:00:00","2012-05-30","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2012-155T01:00:00","000T13:00:00","2012-06-03","UVIS","Prime","Saturn","AURSLEW","Saturn aurora","Saturn Aurora","Auroral Observations led by UVIS Repeated slews across the auroral oval"]
["2012-156T13:45:00","000T10:55:00","2012-06-04","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG MAPS Survey","Continuous low-rate magnetospheric survey"]
["2012-157T01:50:00","000T01:57:00","2012-06-05","UVIS","Prime","Sun","USUNOCC","Solar occultation","Saturn solar occ","This is an egress solar occ by Saturn.  Egress start time is 2011-157T02:24:55 and the line-of-sight impact parameter reaches the desired end distance of 2 Rs around the observation's end time, 2011-157T03:47:00.    Unfortunately, the observation margin and allowance for waypoint turn at the end cut into the egress.  I have compromised by keeping the observation margin at the requested 20 minutes and shortening the time for the waypoint turn from the usual 30 minutes to 10 minutes.  The final LOS impact parameter then ends up at ~1.6 Rs which is smaller than ideal but better than the 1.36 Rs provided by the 30 minute waypoint turn.  EUV occultation port centered on the Sun.  1) 20 minutes observation margin.  2) Record data from 2012-157T02:10:00 until 2012-157T03:17:00.  3) 20 minutes observation margin and 10 minutes for turn to waypoint.  Note:  Egress start and end times are based on the 091005 kernel.  If the timing allows a later end for data collection, we will gladly shift the start of data collection closer to the start of the actual egress in exchange.  Total data collection time:  000T01:07:00.  Total observation request duration:  000T01:57:00.  bps = 18918.883 bps (from Alain's spreadsheet).  Total data volume = 76.054e+6 bits."]
["2012-157T22:29:00","000T09:00:00","2012-06-05","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2012-158T20:07:21","000T08:00:00","2012-06-06","MAG","Non-SPASS","Titan","MAGTITAN","MAG Titan observation","T84 flyby","T84 is another low altitude (990 km) north polar flyby in the post noon sector of Saturn's magnetosphere. With closest approach slightly in the dayside ionosphere, Cassini will be able to study the diffusion of the external magnetic field at low altitudes and high solar zenith angles. A comparison with T83 will be useful.  We assign grade one priority. Data rate: 1976bps (32vps)."]
["2012-159T09:07:21","000T05:00:00","2012-06-07","CIRS","Prime","Titan","FIRNADCMP","Far infrared nadir composition map",null,"Obtain information on CO, HCN, CH4. Integrate on disk at airmass 1.5--2.0."]
["2012-159T09:07:21","000T05:00:00","2012-06-07","VIMS","SPASS Rider","Titan","FIRNADCMP","Far infrared nadir composition map","Stare at Titan","VIMS ridealong with CIRS while staring at Titan.  Phase = 28.255 deg, SSC Lat/Lon = 13.659S/207.750 deg.  SS Lat/Lon = 14.569N/209.078 deg.  Alt = 178439.8 km, range = 178439.8 km.  Resolution = 88 km/px.  Temp. C.  Obtain cubes of 160 and 640 while staring at Titan."]
["2012-161T20:00:00","000T01:00:00","2012-06-09","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT CAMPAIGN, 009 TH OBS SET IN REV 16","Turn to first satellite, take 1 NAC (CL1,CL2). Turn to second satellite take 1 NAC (CL1,CL2), repeat for up to 10 satellites if visible"]
["2012-163T16:37:00","000T00:02:00","2012-06-11","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2012-167T15:08:00","000T01:00:00","2012-06-15","ISS","Prime","Other","SATELLORB","Satellite orbit campaign","SATELLITE ORBIT CAMPAIGN, 013 TH OBS SET IN REV 16","Turn to first satellite, take 1 NAC (CL1,CL2). Turn to second satellite take 1 NAC (CL1,CL2), repeat for up to 10 satellites if visible"]
["2012-170T23:03:00","000T00:02:00","2012-06-18","CIRS","Non-SPASS","Other","SEQSETUP","CIRS sequence setup activity","CIRS S74 Sequence Setup","Enforce CIRS science no-data state, load tables (IEBs) from the SSR, set the focal plane assembly set point"]
["2012-172T06:28:00","000T08:00:00","2012-06-20","MAG","Prime","Sun","CALROLL","MAG calibration roll","MAG Calibration Rolls","Roll about axis other than Z for determination of sensor offsets, actual roll axis is not important - selected axis is usually suitable for MAPS.  Preferably calibrations should be made every 15-20 days in areas where field conditions are suitable.  Note: periods of suitable data are defined as follows; 1) More distant than 15 RS from Saturn's axis (to try and get into the more uniform part of the internal+sheet field). 2) Inside the magnetopause (more specifically inside a most compressed model MP). 3) More distant than 3 RS from the current sheet. Using a 'hinged' sheet model which departs from Saturn's equatorial plane at about 15 RS and then follows the anti-solar direction on the nightside. This means that, even though its orbit is equatorial, if the spacecraft is situated far enough away from the planet, it should see the nightside current sheet divert northwards away from it (using Saturn axis tilted 17 deg away from Sun).  Apart from possible injection events, sheet disruptions etc the resultant periods should have a reasonable probability of seeing a 'quiescent' 'lobe-like' or 'disk-like' field. We would prefer as far downtail as possible so the field has more chance of pointing in a single direction over larger length scales."]
["2012-177T03:00:00","000T15:40:00","2012-06-25","UVIS","SPASS Rider","rings(general)","FMOVIE","F ring movie",null,"ISS rider"]
["2012-178T21:58:00","000T14:47:00","2012-06-26","CIRS",null,"Titan","LRMONITOR","Long range monitor","long range monitor","Ride along with ISS."]
["2012-180T03:30:00","000T05:21:00","2012-06-28","VIMS","SPASS Rider","rings(general)","DRCLOSE",null,"D-Ring observation","640 msec tau_IR"]
["2012-180T07:26:00","000T01:25:00","2012-06-28","RSS","SPASS Rider","rings(general)","THERMAL","Thermal stabilization period","RSS 168 RI OCC Thermal Stabilization","A thermal stabilization period of 2 hrs and 5 min is required immediately prior to any radio science experiment which uses Ka-band or S-band.  Note that the  observation period of the corresponding science request includes a budgeted 40 min waypoint turn that can be considered as part of the warmup time.  Hence, the total duration of this warmup request is shorter than the required 2 hrs and 5 min by those 40 min (that is, only 1 hr and 25 min).  The duration should be increased back to the original 2 hrs 5 min if a waypoint turn proves unnecessary."]
["2012-180T08:51:00","000T03:55:00","2012-06-28","RSS","Prime","rings(general)","OCC","Occultation","RSS XXM Ring Occ - Ingress","Ingress ring occultation conducted using TBD bands (TBD Op-mode). The op-mode is selected based on power constraints. Observations will commence after a 2 hrs 5 min period of thermal stabilization (in RSS WARMUP op-mode)."]
["2012-180T12:46:00","000T04:19:00","2012-06-28","ISS","Prime","Saturn","LIMBSCAN","Limb scan","Saturn Limb Scan","Sun behind Saturn limb"]
["2012-180T12:46:00","000T04:19:00","2012-06-28","VIMS","SPASS Rider","Saturn","SATLIMB",null,"Saturn Limb in eclipse","Images of Saturn's limb in eclipse. ISS Rider."]
["2012-180T17:23:00","000T02:52:00","2012-06-28","CDA","Prime","rings(general)","VERT59",null,"CDA RPXing 2012-180T19:23:56","RPXing at 5.8881283 Rs, CDA Articulation 90 degrees compatible with INMS"]
["2012-180T17:23:00","000T02:52:00","2012-06-28","CDA","Non-SPASS","Other","RATE080","Dust survey","Data rate","Range enter= 6.6588050 Rs exit= 5.3158804 Range altitude= -39658.170 km ... 39765.492"]
["2012-180T18:22:26","000T00:30:00","2012-06-28","INMS","Non-SPASS","Saturn","RINGPLNA",null,"Ring Plane Observation","Observe neutral molecules in the equatorial plane"]
["2012-180T18:52:26","000T01:30:00","2012-06-28","INMS","SPASS Rider","Saturn","INNERMAG","Observing neutral molecules in the inner magnetosphere","Inner Magnetosphere Observation","Observe neutral molecules in the equatorial plane"]
["2012-180T20:15:00","000T02:30:00","2012-06-28","ISS","Prime","Tethys","TETHYS","Tethys","Tethys ORS observation","ORS observation"]
["2012-180T20:15:00","000T02:30:00","2012-06-28","CIRS",null,"Tethys","TETHYS","Tethys",null,"Could we please have the following tables Marcia? 352:1, 402:1   Scan times from ISS design are confirmed by Todd A (22 Feb 2012) as  FP1 raster scan: 2012-180T20:40:51 -> 21:12:20 at 300 urad/s FP3 scans: 22:09:01 -> 22:29:01 at 7 urad/s  Adjusted tables so shutter closed is taken from  20:15:00->20:16:53 (355) 21:15:00->21:16:53 (402)  FP1 and FP3 only   Shutter closed will be taken at:  20:15:00->20:16:53 21:15:00->21:16:53 22:15:00->22:16:53  Note, please ensure the FP3 scan isn't being taken during the shutter closed periods.  Design Requests:  ~20:45: 20 minutes FP1 full-disk raster scan (timing flexible) ~22:15: 30 minutes for FP3 scan at 6 murad/sec along 90 degree meridian (timing flexible)"]
["2012-180T20:15:00","000T02:30:00","2012-06-28","UVIS",null,"Tethys","ICYMAP","Icy satellite surface map","ICYMAP:  UV Surface Map of Tethys, ORS Rider","UV albedo map of Tethys's surface"]
["2012-180T20:15:00","000T02:30:00","2012-06-28","VIMS","SPASS Rider","Tethys","TETHYS","Tethys","Tethys","follow ISS"]
["2012-180T20:22:26","000T23:00:00","2012-06-28","INMS","Non-SPASS","Saturn","RINGPLNA",null,"Ring Plane Observation","Observe neutral molecules in the equatorial plane"]
["2012-180T21:46:56","012T01:58:04","2012-06-28","CDA","Non-SPASS","Other","RATE010","Dust survey","Data rate End:SApo","Range enter= 5.3099829 Rs exit= 6.6894416 Range altitude= 40304.630 km ... -40522.143"]
["2012-180T22:45:00","000T01:30:00","2012-06-28","UVIS","Prime","Star","URALPCMA",null,"URSTAR"]
["2012-180T22:45:00","000T01:30:00","2012-06-28","CIRS","SPASS Rider","rings(general)","URALPCMA",null,"CIRS_168RI_URALPCMA001_UVIS","rider"]
["2012-180T22:45:00","000T01:30:00","2012-06-28","VIMS","SPASS Rider","Saturn","ALPCMAOCC",null,"Alp CMa Saturn atmosphere occultation","Rider on UVIS_168ST_URALPCMA001_PRIME.  Ring occ portion unusable (begins in B ring)."]
["2012-181T00:15:00","000T03:05:00","2012-06-29","UVIS","Prime","Star","URKAPCMA",null,"URSTAR","This follows a UVIS PRIME AlpCMa observation directly. Should do direct turn without waypoint turn. Turn directly from AlpCMa to KapCMa."]
["2012-181T00:15:00","000T03:05:00","2012-06-29","CIRS","SPASS Rider","rings(general)","URKAPCMA",null,"CIRS_168RI_URKAPCMA001_UVIS","rider"]
["2012-181T00:15:00","000T03:05:00","2012-06-29","ISS","SPASS Rider","Star","URKAPCMA",null,"UVIS occultation rider","UVIS occultation rider"]
["2012-181T00:27:21","000T00:00:01","2012-06-29","MP","SPASS Note","Saturn","PERIAPSE","Periapse",null,"Periapse R = 5.063 Rs, lat = 15 deg, phase = 104 deg"]
["2012-181T03:20:00","000T02:10:00","2012-06-29","VIMS","Prime","rings(general)","COMPLIT",null,"Lit side composition","High-res radial scan across rings.  160 msec IR integration time."]
["2012-181T03:20:00","000T02:10:00","2012-06-29","CIRS","SPASS Rider","rings(general)","COMPLIT",null,"CIRS_168RI_COMPLIT001_VIMS","rider"]
["2012-181T03:20:00","000T02:10:00","2012-06-29","UVIS","SPASS Rider","rings(general)","COMPLIT",null,null,"VIMS rider"]
["2012-181T05:30:00","000T05:47:00","2012-06-29","ISS","Prime","rings(general)","MOONLETCD",null,"Cassini Division moonlet search","Cassini Division moonlet search"]
["2012-181T05:30:00","000T05:47:00","2012-06-29","CIRS","SPASS Rider","rings(general)","MOONLETCD",null,"CIRS_168RI_MOONLETCD001_ISS","rider"]
["2012-181T12:55:00","001T16:46:00","2012-06-29","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","null"]
["2012-181T13:27:00","000T09:00:00","2012-06-29","RSS","SPASS Rider","rings(general)","GSE",null,"Gravity Science Enhancement (GSE)","Rings Occultation onbound GSE (Gravity Science Enhancement)  Additional downlink pass at Ka-band to improve Saturn's gravity field determination, and for improving Cassini's orbit locally for data analysis of rings and atmosphere occultation.  DSS-55 required for X- and Ka-band support."]
["2012-181T13:27:00","000T09:00:00","2012-06-29","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2012-181T14:27:00","000T06:00:00","2012-06-29","CIRS","SPASS Rider","InstrumentCalibration","DSCAL12",null,"CIRS_168IC_DSCAL12181_SP","rider"]
["2012-181T19:22:26","001T01:50:34","2012-06-29","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","Survey","Part of the MAPS/TOST Campaign. Determine atmospheric and ionospheric thermal structure."]
["2012-181T22:57:00","000T01:30:00","2012-06-29","ISS","Prime","Titan","M30R2CLD",null,"Titan Monitoring Campaign","Titan Monitoring Campaign, requested phase 11.6 requested range 2 Mkm"]
["2012-181T22:57:00","000T01:30:00","2012-06-29","CIRS","SPASS Rider","Titan","M30R2CLD",null,"Rider for Titan Monitoring Campaign","Rider to ISS Titan cloud monitor"]
["2012-181T22:57:00","000T01:30:00","2012-06-29","VIMS","SPASS Rider","Titan","M30R2CLD",null,"Titan Monitoring Campaign","Titan Monitoring Campaign; phase = 12 deg, range =1.98 Mkm."]
["2012-182T00:27:00","000T10:30:00","2012-06-30","ISS","Prime","RingB","BMOVIE","B ring movie","B-ring ansa movie","B-ring ansa movie"]
["2012-182T00:27:00","000T10:30:00","2012-06-30","CIRS","SPASS Rider","rings(general)","BMOVIE","B ring movie","CIRS_168RI_BMOVIE001_ISS","rider"]
["2012-182T05:46:00","000T23:55:00","2012-06-30","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2012-182T10:57:00","000T07:34:00","2012-06-30","ISS","Prime","rings(general)","DRLPMOV",null,"D Ring Close-in observation at low phase","D Ring Close-In Observation at low phase"]
["2012-182T20:41:00","000T09:00:00","2012-06-30","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2012-182T21:13:00","000T02:00:00","2012-06-30","INMS","Non-SPASS","Titan","TTNTORUS","Titan torus observation","Titan Torus observation","Titan Torus observation"]
["2012-182T21:41:00","000T08:00:00","2012-06-30","CIRS","SPASS Rider","InstrumentCalibration","DSCAL12",null,"CIRS_168IC_DSCAL12182_SP","rider"]
["2012-182T23:13:00","000T06:28:00","2012-06-30","INMS","Non-SPASS","Saturn","SURVEYSEG","Campaign to determine atmospheric and ionospheric thermal structure","Segment Boundary Survey","Part of the MAPS/TOST Campaign. Determine atmospheric and ionospheric thermal structure."]
["2012-183T05:41:00","004T20:40:00","2012-07-01","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","null"]
["2012-183T05:41:00","009T18:04:00","2012-07-01","INMS","Non-SPASS","Saturn","SURVEYSEG","Campaign to determine atmospheric and ionospheric thermal structure","Segment Boundary Survey","Part of the MAPS/TOST Campaign. Determine atmospheric and ionospheric thermal structure."]
["2012-183T05:41:00","009T07:54:00","2012-07-01","MAG","Non-SPASS","Other","MAPSCAKE",null,"MAPS CAKE","MAPS CAKE observation"]
["2012-183T05:41:00","009T18:04:00","2012-07-01","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SURVEY Campaign","Part of SURVEY MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane.   MAPS_168_169"]
["2012-183T05:41:00","009T18:04:00","2012-07-01","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2012-183T06:19:00","000T00:02:00","2012-07-01","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2012-183T06:21:00","000T12:09:00","2012-07-01","UVIS","Prime","Saturn","AURSLEW","Saturn aurora","Saturn Aurora","Auroral Observations led by UVIS Repeated slews across the auroral oval"]
["2012-183T06:21:00","000T12:09:00","2012-07-01","CIRS","SPASS Rider","Saturn","AURSLEW","Saturn aurora","Saturn polar aurorae","South pole rider FP1 may be off planet. UVIS slews to track auroral oval."]
["2012-183T06:21:00","000T12:09:00","2012-07-01","VIMS",null,"Saturn","AURSLEW","Saturn aurora","UVIS Auroral Slew Ridealong and Stormwatch","Auroral  Slew UVIS Ridealong and Stormwatch  cube"]
["2012-183T07:00:00","000T01:08:00","2012-07-01","CAPS","Non-SPASS","InstrumentCalibration","ELSCAL","CAPS Electron Spectrometer calibration","ELS Calibration","null"]
["2012-183T18:30:00","000T01:30:00","2012-07-01","ISS","Prime","Titan","M60R3CLD",null,"Titan Monitoring Campaign","Titan Monitoring Campaign, requested phase 31.4 requested range 2.6 Mkm"]
["2012-183T18:30:00","000T01:30:00","2012-07-01","CIRS","SPASS Rider","Titan","M60R3CLD",null,"Rider for Titan Monitoring Campaign","Rider to ISS Titan cloud monitor"]
["2012-183T18:30:00","000T01:30:00","2012-07-01","VIMS","SPASS Rider","Titan","M60R3CLD",null,"Titan Monitoring Campaign and Stormwatch","Titan Monitoring Campaign; phase = 31 deg, range =2.58 Mkm. Stiormwatch cube at end"]
["2012-183T20:00:00","000T14:46:00","2012-07-01","UVIS","Prime","Saturn","AURSLEW","Saturn aurora","Saturn Aurora","Auroral Observations led by UVIS Repeated slews across the auroral oval"]
["2012-183T20:00:00","000T14:46:00","2012-07-01","VIMS",null,"Saturn","AURSLEW","Saturn aurora","UVIS Auroral Slew Ridealong and Stormwatch Cube","Auroral  Slew UVIS Ridealong with Stormwatch cube at the end"]
["2012-184T10:44:00","000T00:02:00","2012-07-02","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2012-184T12:56:00","000T09:00:00","2012-07-02","RSS","SPASS Rider","Saturn","OCCORT","Operations Readiness Test to demonstrate DSN and RSSG preparedness to support upcoming occultations","RSS Operational Readiness Test","RSS Operations Readiness Test (ORT), to demonstrate DSN and RSSG preparedness to support the Rev169 Saturn rings and atmospheric occultation on 2012/204. DSS-55 required for X- and Ka-band support."]
["2012-184T13:56:00","000T08:00:00","2012-07-02","CIRS","SPASS Rider","InstrumentCalibration","DSCAL12",null,"CIRS_168IC_DSCAL12184_SP","rider"]
["2012-184T22:36:00","000T01:30:00","2012-07-02","ISS","Prime","Titan","M60R3CLD",null,"Titan Monitoring Campaign","Titan Monitoring Campaign, requested phase 53.8 requested range 3.1 Mkm"]
["2012-184T22:36:00","000T01:30:00","2012-07-02","CIRS","SPASS Rider","Titan","M60R3CLD",null,"Rider for Titan Monitoring Campaign","Rider to ISS Titan cloud monitor"]
["2012-184T22:36:00","000T01:30:00","2012-07-02","VIMS","SPASS Rider","Titan","M60R3CLD",null,"Titan Monitoring Campaign and Stormwatch Cube","Titan Monitoring Campaign; phase = 54 deg, range =3.06 Mkm. Stormwatch cube at end"]
["2012-185T00:06:00","000T01:00:00","2012-07-03","ISS","Prime","rings(general)","PROPRETRG","Ring propeller targetting observation","Propeller retargetting","Reacquire and track orbits of individual known propellers."]
["2012-185T00:06:00","000T01:00:00","2012-07-03","CIRS","SPASS Rider","rings(general)","PROPRETRG","Ring propeller targetting observation","CIRS_168RI_PROPRETRG001_ISS","rider"]
["2012-185T01:04:00","000T00:02:00","2012-07-03","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2012-185T01:04:00","000T00:02:00","2012-07-03","VIMS","SPASS Rider","Saturn","STORMW","Saturn storm watch","Storm Watch Ridealong","Storm Watch: 32*32 pixels with 80 msec integration"]
["2012-185T01:06:00","000T23:25:00","2012-07-03","UVIS","Prime","Saturn","AURSLEW","Saturn aurora","Saturn Aurora","Auroral Observations led by UVIS Repeated slews across the auroral oval"]
["2012-185T01:06:00","000T23:25:00","2012-07-03","VIMS",null,"Saturn","AURSLEW","Saturn aurora","UVIS Auroral Slew Ridealong an Stormwatch cube","Auroral  Slew UVIS Ridealong and Stormwatch Cube"]
["2012-186T03:41:00","000T08:00:00","2012-07-04","CIRS","SPASS Rider","InstrumentCalibration","DSCAL12",null,"CIRS_168IC_DSCAL12186_SP","rider"]
["2012-186T12:21:00","000T01:30:00","2012-07-04","ISS","Prime","Titan","M90R3CLD",null,"Titan Monitoring Campaign","Titan Monitoring Campaign, requested phase 70 requested range 3.2 Mkm"]
["2012-186T12:21:00","000T01:30:00","2012-07-04","CIRS","SPASS Rider","Titan","M90R3CLD",null,"Rider for Titan Monitoring Campaign","Rider to ISS Titan cloud monitor"]
["2012-186T12:21:00","000T01:30:00","2012-07-04","VIMS","SPASS Rider","Titan","M90R3CLD",null,"Titan Monitoring Campaign and Stormwatch Cube","Titan Monitoring Campaign; phase = 70 deg, range =3.17 Mkm. Stormwatch Cube at end"]
["2012-186T13:49:00","000T00:02:00","2012-07-04","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2012-186T13:51:00","001T10:40:00","2012-07-04","UVIS","Prime","Saturn","AURSLEW","Saturn aurora","Saturn Aurora","Auroral Observations led by UVIS Repeated slews across the auroral oval"]
["2012-186T13:51:00","001T10:40:00","2012-07-04","VIMS",null,"Saturn","AURSLEW","Saturn aurora","UVIS Auroral Slew Ridealong and Stormwatch Cube","Auroral  Slew UVIS Ridealong and Stormwatch cube"]
["2012-188T02:21:00","005T14:19:00","2012-07-06","CAPS","SPASS Rider","Saturn","LOWLATAPO",null,"MAPS Low latitude apoapsis","null"]
["2012-188T03:41:00","000T08:00:00","2012-07-06","CIRS","SPASS Rider","InstrumentCalibration","DSCAL12",null,"CIRS_168IC_DSCAL12188_SP","rider"]
["2012-188T12:21:00","000T01:30:00","2012-07-06","ISS","Prime","Titan","M90R3CLD",null,"Titan Monitoring Campaign","Titan Monitoring Campaign, requested phase 85.7 requested range 2.9 Mkm"]
["2012-188T12:21:00","000T01:30:00","2012-07-06","CIRS","SPASS Rider","Titan","M90R3CLD",null,"Rider for Titan Monitoring Campaign","Rider to ISS Titan cloud monitor"]
["2012-188T12:21:00","000T01:30:00","2012-07-06","VIMS","SPASS Rider","Titan","M90R3CLD",null,"Titan Monitoring Campaign and Stormwatch Cube","Titan Monitoring Campaign; phase = 86 deg, range =2.86 Mkm. Ends with Stormwatch Cube"]
["2012-188T13:49:00","000T00:02:00","2012-07-06","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2012-188T13:51:00","001T10:24:00","2012-07-06","UVIS","Prime","Saturn","AURSLEW","Saturn aurora","Saturn Aurora","Auroral Observations led by UVIS Repeated slews across the auroral oval"]
["2012-188T13:51:00","001T10:24:00","2012-07-06","VIMS",null,"Saturn","AURSLEW","Saturn aurora","UVIS Auroral Slew Ridealong and Stomwatch","Auroral  Slew UVIS Ridealong. Ends with Stormwatch Cube"]
["2012-189T23:45:00","000T20:00:00","2012-07-07","CDA","SPASS Rider","DustRAM direction","ISD0049",null,"CDA ISD 2012-192T23:45:00","ISD observation around apoapse 2012-192T23:45:00 48.096044 Rs"]
["2012-190T00:13:00","000T00:02:00","2012-07-08","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2012-190T03:25:00","000T08:00:00","2012-07-08","CIRS","SPASS Rider","InstrumentCalibration","DSCAL12",null,"CIRS_168IC_DSCAL12190_SP","rider"]
["2012-190T12:03:00","000T00:02:00","2012-07-08","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2012-190T12:05:00","001T12:10:00","2012-07-08","UVIS","Prime","Saturn","AURSLEW","Saturn aurora","Saturn Aurora","Auroral Observations led by UVIS Repeated slews across the auroral oval"]
["2012-190T12:05:00","001T12:10:00","2012-07-08","VIMS",null,"Saturn","AURSLEW","Saturn aurora","UVIS Auroral Slew Ridealong and Stormwatch Cube","Auroral  Slew UVIS Ridealong. Ends with Stormwatch cube"]
["2012-191T17:45:00","000T20:00:00","2012-07-09","CDA","SPASS Rider","DustRAM direction","ISD0049",null,"CDA ISD 2012-192T23:45:00","ISD observation around apoapse 2012-192T23:45:00 48.096044 Rs"]
["2012-192T00:13:00","000T00:02:00","2012-07-10","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2012-192T03:25:00","000T08:00:00","2012-07-10","CIRS","SPASS Rider","InstrumentCalibration","DSCAL12",null,"CIRS_168IC_DSCAL12192_SP","rider"]
["2012-192T12:05:00","000T01:30:00","2012-07-10","ISS","Prime","Titan","M90R2CLD",null,"Titan Monitoring Campaign","Titan Monitoring Campaign, requested phase 83.9 requested range 1.8 Mkm"]
["2012-192T12:05:00","000T01:30:00","2012-07-10","CIRS","SPASS Rider","Titan","M90R2CLD",null,"Rider for Titan Monitoring Campaign","Rider to ISS Titan cloud monitor"]
["2012-192T12:05:00","000T01:30:00","2012-07-10","VIMS","SPASS Rider","Titan","M90R2CLD",null,"Titan Monitoring Campaign","Titan Monitoring Campaign; phase = 84 deg, range =1.76 Mkm."]
["2012-192T13:35:00","000T08:00:00","2012-07-10","MAG","Prime","Sun","CALROLL","MAG calibration roll","MAG Calibration Rolls","Roll about axis other than Z for determination of sensor offsets, actual roll axis is not important - selected axis is usually suitable for MAPS.  Preferably calibrations should be made every 15-20 days in areas where field conditions are suitable.  Note: periods of suitable data are defined as follows; 1) More distant than 15 RS from Saturn's axis (to try and get into the more uniform part of the internal+sheet field). 2) Inside the magnetopause (more specifically inside a most compressed model MP). 3) More distant than 3 RS from the current sheet. Using a 'hinged' sheet model which departs from Saturn's equatorial plane at about 15 RS and then follows the anti-solar direction on the nightside. This means that, even though its orbit is equatorial, if the spacecraft is situated far enough away from the planet, it should see the nightside current sheet divert northwards away from it (using Saturn axis tilted 17 deg away from Sun).  Apart from possible injection events, sheet disruptions etc the resultant periods should have a reasonable probability of seeing a 'quiescent' 'lobe-like' or 'disk-like' field. We would prefer as far downtail as possible so the field has more chance of pointing in a single direction over larger length scales."]
["2012-192T21:35:00","000T04:00:00","2012-07-10","CAPS","Prime","co-rotation","IONCALPTG",null,"IMS and IBS calibration","null"]
["2012-192T21:35:00","000T04:00:00","2012-07-10","CAPS","Non-SPASS","co-rotation","IONCALCOM",null,"IMS and IBS Calibration Commanding","This request will be used IONCAL commanding. The times are identical to the IONCAL pointing request"]
["2012-192T21:35:00","011T06:48:00","2012-07-10","MAG","Non-SPASS","Other","MAPSCAKE",null,"MAPS CAKE","MAPS CAKE observation"]
["2012-192T23:45:00","011T15:45:56","2012-07-10","CDA","Non-SPASS","Other","RATE010","Dust survey","Data rate Enter:SApo","Range enter= 5.3099829 Rs exit= 6.6894416 Range altitude= 40304.630 km ... -40522.143"]
["2012-192T23:45:00","000T02:00:00","2012-07-10","INMS","Non-SPASS","Saturn","ENGBCKGND",null,"Engineering background observation","Full rate measurement to gather engineering background data"]
["2012-192T23:45:00","011T04:38:00","2012-07-10","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SURVEY Campaign","Part of SURVEY MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane.   MAPS_168_169"]
["2012-192T23:45:00","010T17:55:00","2012-07-10","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2012-192T23:45:08","000T00:00:01","2012-07-10","MP","SPASS Note","Saturn","APOAPSE","Apoapse",null,"Apoapse  Per = 24.0 d, inc = 21.2 deg, r = 48.049 Rs, phase = 76 deg"]
["2012-193T01:35:00","000T15:05:00","2012-07-11","CAPS","Prime","co-rotation","LLACORPTG",null,"MAPS low latitude apoapsis prime pointing","null"]
["2012-193T01:45:00","010T08:53:00","2012-07-11","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","Survey","Part of the MAPS/TOST Campaign. Determine atmospheric and ionospheric thermal structure."]
["2012-193T09:45:00","000T20:00:00","2012-07-11","CDA","SPASS Rider","DustRAM direction","ISD0049",null,"CDA ISD 2012-192T23:45:00","ISD observation around apoapse 2012-192T23:45:00 48.096044 Rs"]
["2012-193T16:40:00","000T08:00:00","2012-07-11","ISS","Prime","Other","YMIPHA",null,"Ymir","Observation of irregular moon of Saturn."]
["2012-193T16:40:00","000T08:00:00","2012-07-11","UVIS","SPASS Rider","Other","OUTERSATS","Icy satellite observaton","ICYLON:  Icy Satellite Longitude / Phase Coverage","Measure satellite albedo in ultraviolet light for a good sampling of longitude and phase space.  Determine phase function to investigate surface microstructure and frost properties, as a function of location."]
["2012-193T16:40:00","000T12:00:00","2012-07-11","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","null"]
["2012-194T02:10:00","000T09:00:00","2012-07-12","RSS","SPASS Rider","Saturn","OCCORT","Operations Readiness Test to demonstrate DSN and RSSG preparedness to support upcoming occultations","RSS Operational Readiness Test","RSS Operations Readiness Test (ORT), to demonstrate DSN and RSSG preparedness to support the Rev169 Saturn rings and atmospheric occultation on 2012/204. DSS-43 required for X- and S-band support."]
["2012-194T02:10:00","000T09:00:00","2012-07-12","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2012-194T03:10:00","000T06:00:00","2012-07-12","CIRS","SPASS Rider","InstrumentCalibration","DSCAL12",null,"CIRS_169IC_DSCAL12194_SP","rider"]
["2012-194T04:40:00","003T19:20:00","2012-07-12","CAPS","SPASS Rider","Saturn","LOWLATAPO",null,"MAPS Low latitude apoapsis","null"]
["2012-194T11:10:00","000T18:45:00","2012-07-12","CAPS","Prime","co-rotation","LLACORPTG",null,"MAPS low latitude apoapsis prime pointing","null"]
["2012-195T00:00:00","000T01:08:00","2012-07-13","CAPS","Non-SPASS","InstrumentCalibration","ELSCAL","CAPS Electron Spectrometer calibration","ELS Calibration","null"]
["2012-195T03:45:00","000T20:00:00","2012-07-13","CDA","SPASS Rider","DustRAM direction","ISD0049",null,"CDA ISD 2012-192T23:45:00","ISD observation around apoapse 2012-192T23:45:00 48.096044 Rs"]
["2012-195T07:25:00","000T17:15:00","2012-07-13","UVIS","Prime","Saturn","AURSTARE","Saturn aurora","Saturn Aurora","Auroral Observations led by UVIS Mixture of slews for UV imaging and fixed pointings at the auroral oval"]
["2012-195T07:25:00","000T17:15:00","2012-07-13","CIRS","SPASS Rider","Saturn","AURSTARE","Saturn aurora","Saturn polar aurorae"]
["2012-195T07:25:00","000T17:15:00","2012-07-13","ISS",null,"Saturn","AURSTARE","Saturn aurora","NAC aurora stare. For rotation timing","Rider on UVIS PIE. CL1 NAC 4x4 images.  10 Mbits/hr, expected only half of the time to be usable stare"]
["2012-195T07:25:00","000T17:15:00","2012-07-13","VIMS",null,"Saturn","AURSTARE","Saturn aurora","Auroral Stare","Auroral Stare ridealong with UVIS"]
["2012-196T02:10:00","000T09:00:00","2012-07-14","RSS","SPASS Rider","Saturn","OCCORT","Operations Readiness Test to demonstrate DSN and RSSG preparedness to support upcoming occultations","RSS Operational Readiness Test","RSS Operations Readiness Test (ORT), to demonstrate DSN and RSSG preparedness to support the Rev169 Saturn rings and atmospheric occultation on 2012/204. DSS-34 required for X- and Ka-band support."]
["2012-196T02:10:00","000T09:00:00","2012-07-14","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2012-196T03:10:00","000T08:00:00","2012-07-14","CIRS","SPASS Rider","InstrumentCalibration","DSCAL12",null,"CIRS_169IC_DSCAL12196_SP","rider"]
["2012-196T11:10:00","001T11:29:00","2012-07-14","CAPS","Prime","co-rotation","LLACORPTG",null,"MAPS low latitude apoapsis prime pointing","null"]
["2012-197T22:39:00","000T12:00:00","2012-07-15","UVIS","Prime","Saturn","AURSTARE","Saturn aurora","Saturn Aurora","Auroral Observations led by UVIS Mixture of slews for UV imaging and fixed pointings at the auroral oval"]
["2012-197T22:39:00","000T12:00:00","2012-07-15","CIRS","SPASS Rider","Saturn","AURSTARE","Saturn aurora","Saturn polar aurorae"]
["2012-197T22:39:00","000T12:00:00","2012-07-15","ISS",null,"Saturn","AURSTARE","Saturn aurora","NAC aurora stare. For rotation timing","Rider on UVIS PIE. CL1 NAC 4x4 images.  10 Mbits/hr, expected only half of the time to be usable stare"]
["2012-197T22:39:00","000T12:00:00","2012-07-15","VIMS",null,"Saturn","AURSTARE","Saturn aurora","Auroral Stare","Auroral Stare ridealong with UVIS"]
["2012-198T00:00:00","000T10:00:00","2012-07-16","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","null"]
["2012-198T10:00:00","005T18:23:00","2012-07-16","CAPS","SPASS Rider","Saturn","LOWLATAPO",null,"MAPS Low latitude apoapsis","null"]
["2012-198T12:09:00","000T09:00:00","2012-07-16","RSS","SPASS Rider","Saturn","OCCORT","Operations Readiness Test to demonstrate DSN and RSSG preparedness to support upcoming occultations","RSS Operational Readiness Test","RSS Operations Readiness Test (ORT), to demonstrate DSN and RSSG preparedness to support the Rev169 Saturn rings and atmospheric occultation on 2012/204. DSS-63 required for X- and S-band support."]
["2012-198T12:09:00","000T09:00:00","2012-07-16","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2012-198T13:09:00","000T08:00:00","2012-07-16","CIRS","SPASS Rider","InstrumentCalibration","DSCAL12",null,"CIRS_169IC_DSCAL12198_SP","rider"]
["2012-198T21:49:00","000T01:30:00","2012-07-16","ISS","Prime","Titan","M90R3CLD",null,"Titan Monitoring Campaign","Titan Monitoring Campaign, requested phase 71.2 requested range 3 Mkm"]
["2012-198T21:49:00","000T01:30:00","2012-07-16","CIRS","SPASS Rider","Titan","M90R3CLD",null,"Rider for Titan Monitoring Campaign","Rider to ISS Titan cloud monitor"]
["2012-198T21:49:00","000T01:30:00","2012-07-16","VIMS","SPASS Rider","Titan","M90R3CLD",null,"Titan Monitoring Campaign","Titan Monitoring Campaign; phase = 71 deg, range =3.03 Mkm."]
["2012-198T23:19:00","000T13:05:00","2012-07-16","CAPS","Prime","co-rotation","LLACORPTG",null,"MAPS low latitude apoapsis prime pointing","null"]
["2012-199T12:24:00","000T12:00:00","2012-07-17","UVIS","Prime","Saturn","AURSTARE","Saturn aurora","Saturn Aurora","Auroral Observations led by UVIS Mixture of slews for UV imaging and fixed pointings at the auroral oval"]
["2012-199T12:24:00","000T12:00:00","2012-07-17","CIRS","SPASS Rider","Saturn","AURSTARE","Saturn aurora","Saturn polar aurorae"]
["2012-199T12:24:00","000T12:00:00","2012-07-17","ISS",null,"Saturn","AURSTARE","Saturn aurora","NAC aurora stare. For rotation timing","Rider on UVIS PIE. CL1 NAC 4x4 images.  10 Mbits/hr, expected only half of the time to be usable stare"]
["2012-199T12:24:00","000T12:00:00","2012-07-17","VIMS",null,"Saturn","AURSTARE","Saturn aurora","Auroral Stare","Auroral Stare ridealong with UVIS"]
["2012-200T01:54:00","000T09:00:00","2012-07-18","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2012-200T02:54:00","000T08:00:00","2012-07-18","CIRS","SPASS Rider","InstrumentCalibration","DSCAL12",null,"CIRS_169IC_DSCAL12200_SP","rider"]
["2012-200T11:34:00","000T01:30:00","2012-07-18","ISS","Prime","Titan","M90R3CLD",null,"Titan Monitoring Campaign","Titan Monitoring Campaign, requested phase 84.2 requested range 3 Mkm"]
["2012-200T11:34:00","000T01:30:00","2012-07-18","CIRS","SPASS Rider","Titan","M90R3CLD",null,"Rider for Titan Monitoring Campaign","Rider to ISS Titan cloud monitor"]
["2012-200T11:34:00","000T01:30:00","2012-07-18","VIMS","SPASS Rider","Titan","M90R3CLD",null,"Titan Monitoring Campaign","Titan Monitoring Campaign; phase = 84 deg, range =3.04 Mkm."]
["2012-200T13:04:00","000T11:20:00","2012-07-18","CAPS","Prime","co-rotation","LLACORPTG",null,"MAPS low latitude apoapsis prime pointing","null"]
["2012-201T01:54:00","000T09:00:00","2012-07-19","RSS","SPASS Rider","Saturn","OCCORT","Operations Readiness Test to demonstrate DSN and RSSG preparedness to support upcoming occultations","RSS Operational Readiness Test","RSS Operations Readiness Test (ORT), to demonstrate DSN and RSSG preparedness to support the Rev169 Saturn rings and atmospheric occultation on 2012/204. DSS-34 required for X- and Ka-band support."]
["2012-201T01:54:00","000T09:00:00","2012-07-19","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2012-201T02:54:00","000T08:00:00","2012-07-19","CIRS","SPASS Rider","InstrumentCalibration","DSCAL12",null,"CIRS_169IC_DSCAL12201_SP","rider"]
["2012-201T10:54:00","000T13:15:00","2012-07-19","CAPS","Prime","co-rotation","LLACORPTG",null,"MAPS low latitude apoapsis prime pointing","null"]
["2012-202T01:39:00","000T09:00:00","2012-07-20","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2012-202T02:39:00","000T08:00:00","2012-07-20","CIRS","SPASS Rider","InstrumentCalibration","DSCAL12",null,"CIRS_169IC_DSCAL12202_SP","rider"]
["2012-202T10:39:00","000T14:59:00","2012-07-20","CAPS","Prime","co-rotation","LLACORPTG",null,"MAPS low latitude apoapsis prime pointing","null"]
["2012-203T01:38:00","000T09:00:00","2012-07-21","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2012-203T01:43:00","000T04:00:00","2012-07-21","MAG","Non-SPASS","Other","R1DLROLL","MAG downlink roll calibration","MAG_R1_DLROLL_CAL","Rider on rolling downlink with MAG FGM in range 1. Used for calibration of range 1. Rides on current MAG activities - no additional power or datavolume used."]
["2012-203T02:38:00","000T08:00:00","2012-07-21","CIRS","SPASS Rider","InstrumentCalibration","DSCAL12",null,"CIRS_169IC_DSCAL12203_SP","rider"]
["2012-203T10:38:00","000T08:45:00","2012-07-21","CAPS","Prime","co-rotation","LLACORPTG",null,"MAPS low latitude apoapsis prime pointing","null"]
["2012-203T10:38:00","000T07:17:48","2012-07-21","INMS","Non-SPASS","Saturn","SURVPOTM","MAPS survey","Post OTM Survey","Post-OTM request to resume science mode after NAV OTM."]
["2012-203T17:40:00","000T10:43:00","2012-07-21","RPWS","Non-SPASS","Saturn","INSURVEY","Inner magnetosphere survey","RPWS Inner Survey","Setup RPWS for inner magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2012-203T17:55:48","000T10:27:12","2012-07-21","INMS","Non-SPASS","Saturn","SURVEYRPA",null,"Ring Plane Observation","Observe neutral molecules in the equatorial plane"]
["2012-203T19:23:00","000T09:00:00","2012-07-21","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2012-204T04:23:00","001T16:15:00","2012-07-22","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","null"]
["2012-204T04:23:00","000T12:32:48","2012-07-22","INMS","Non-SPASS","Saturn","SURVBOTM","MAPS survey","Post OTM Survey","Post-OTM request to resume science mode after NAV OTM."]
["2012-204T04:23:00","001T16:15:00","2012-07-22","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG MAPS Survey","Continuous low-rate magnetospheric survey"]
["2012-204T04:23:00","001T16:15:00","2012-07-22","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SURVEY Campaign","Part of SURVEY MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane.   RINGS_169"]
["2012-204T04:23:00","001T16:15:00","2012-07-22","RPWS","Non-SPASS","Saturn","INSURVEY","Inner magnetosphere survey","RPWS Inner Survey","Setup RPWS for inner magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2012-204T05:50:00","000T01:25:00","2012-07-22","RSS","SPASS Rider","rings(general)","THERMAL","Thermal stabilization period","RSS 169 RI OCC Thermal Stabilization","A thermal stabilization period of 2 hrs and 5 min is required immediately prior to any radio science experiment which uses Ka-band or S-band.  Note that the  observation period of the corresponding science request includes a budgeted 40 min waypoint turn that can be considered as part of the warmup time.  Hence, the total duration of this warmup request is shorter than the required 2 hrs and 5 min by those 40 min (that is, only 1 hr and 25 min).  The duration should be increased back to the original 2 hrs 5 min if a waypoint turn proves unnecessary."]
["2012-204T07:15:11","000T02:55:48","2012-07-22","RSS","Prime","rings(general)","OCC","Occultation","RSS XXM Ring Occ - Ingress","Ingress ring occultation conducted using TBD bands (TBD Op-mode). The op-mode is selected based on power constraints. Observations will commence after a 2 hrs 5 min period of thermal stabilization (in RSS WARMUP op-mode)."]
["2012-204T10:10:59","000T01:32:00","2012-07-22","RSS","Prime","Saturn","OCCIN","Ingress Occultation","RSS Saturn Ingress Atmospheric Occultation","This is for the RSS occultation of Saturn's ionosphere and atmosphere, to measure vertical profiles of electron density in the ionosphere, and of density, pressure, and temperature in the neutral atmosphere. X, S, and Ka bands will be used. Prior to this point the RFIS bay will have been thermally stabilized (see thermal stabilisation request)."]
["2012-204T12:03:00","000T04:17:00","2012-07-22","VIMS","Prime","rings(general)","HIPHASE","High phase observation","High phase ring observation","High phase ring observation. Custom turn period."]
["2012-204T12:03:00","000T04:17:00","2012-07-22","CIRS","SPASS Rider","rings(general)","HIPHASE","High phase observation","CIRS_169RI_HIPHASE001_VIMS","rider"]
["2012-204T12:03:00","000T04:17:00","2012-07-22","ISS",null,"rings(general)","HIPHASE","High phase observation","Rider on VIMS Hiphase","ISS on, max data rate = 182.784 kbps, number of frames and bits/frame are input parameters, data volume = number of frames x bits/frame, average data rate = data volume/duration."]
["2012-204T15:30:56","000T04:50:00","2012-07-22","CDA","Non-SPASS","Other","RATE080","Dust survey","Data rate","Range enter= 6.6775853 Rs exit= 5.3187880 Range altitude= -39975.865 km ... 39848.025"]
["2012-204T16:25:00","000T03:00:00","2012-07-22","CDA","Prime","rings(general)","VERT59",null,"CDA RPXing 2012-204T17:55:56","RPXing at 5.9032706 Rs, CDA Articulation 90 degrees, compatible with INMS"]
["2012-204T16:30:00","000T03:00:00","2012-07-22","RPWS","Non-SPASS","rings(general)","RPXING","Measurements of dust flux, scale height and plasma waves at the magnetic equator during ring plane crossing","RPWS Ring Plane Crossing","Determine the equatorial dust flux and scale height as a function of radial distance.  Obtain high resolution of plasma waves at the magnetic equator."]
["2012-204T16:55:48","000T00:30:00","2012-07-22","INMS","Non-SPASS","Saturn","RINGPLNA",null,"Ring Plane Observation","Observe neutral molecules in the equatorial plane"]
["2012-204T17:25:48","000T01:30:00","2012-07-22","INMS","SPASS Rider","Saturn","INNERMAG","Observing neutral molecules in the inner magnetosphere","Inner Magnetosphere Observation","Observe neutral molecules in the equatorial plane"]
["2012-204T18:55:48","000T23:00:00","2012-07-22","INMS","Non-SPASS","Saturn","RINGPLNA",null,"Ring Plane Observation","Observe neutral molecules in the equatorial plane"]
["2012-204T19:25:00","000T00:55:00","2012-07-22","CIRS","Prime","rings(general)","NP140L30",null,null,"null"]
["2012-204T19:25:00","000T00:55:00","2012-07-22","CIRS","SPASS Rider","rings(general)","NP140L30",null,"CIRS_169RI_NP140L30001_SI"]
["2012-204T20:20:00","000T01:56:00","2012-07-22","VIMS","Prime","Saturn","ALPCMAOCC",null,"alp Cma atmosphere occultation","alp Cma atmosphere occultation. Stellar occ mode, no spectral summing, tau_IR = 40 msec."]
["2012-204T20:20:00","000T01:56:00","2012-07-22","ISS","SPASS Rider","Saturn","ALPCMAOCC",null,"VIMS occultation rider","VIMS occultation rider"]
["2012-204T20:20:00","000T01:56:00","2012-07-22","UVIS","SPASS Rider","Star","URALPCMA",null,"URSTAR"]
["2012-204T20:20:56","008T23:46:04","2012-07-22","CDA","Non-SPASS","Other","RATE010A",null,"Data rate End:SApo","Range enter= 5.3128487 Rs exit= 7.2761371 Range altitude= 40386.044 km ... -40678.270"]
["2012-204T20:28:00","000T01:48:00","2012-07-22","CIRS","SPASS Rider","rings(general)","URALPCMA",null,"CIRS_169RI_URALPCMA001_UVIS","rider"]
["2012-204T22:16:00","000T03:44:00","2012-07-22","UVIS","Prime","Star","URZETCMA",null,"URSTAR"]
["2012-204T22:16:00","000T03:18:00","2012-07-22","CIRS","SPASS Rider","rings(general)","URZETCMA",null,"CIRS_169RI_URZETCMA001_UVIS","rider"]
["2012-204T22:16:00","000T03:44:00","2012-07-22","ISS","SPASS Rider","Star","URZETCMA",null,"UVIS occultation rider","UVIS occultation rider"]
["2012-204T23:02:34","000T00:00:01","2012-07-22","MP","SPASS Note","Saturn","PERIAPSE","Periapse",null,"Periapse R = 5.062 Rs, lat = 15 deg, phase = 104 deg"]
["2012-205T02:00:00","000T02:00:00","2012-07-23","UVIS","Prime","Dione","ICYEXO","Icy satellite exosphere","ICYEXO:  Icy Satellite Exospheres","Target to alpha Vir to look for volatiles."]
["2012-205T02:00:00","000T02:00:00","2012-07-23","CIRS",null,"Dione","ICYEX",null,null,"FP1, FP3 only  Shutter closed between:  2012-205T02:00:00 -> 02:01:53 2012-205T03:00:00 -> 03:01:53"]
["2012-205T02:00:00","000T02:00:00","2012-07-23","ISS",null,"Dione","ICYEXO","Icy satellite exosphere","Dione","Dione occultation of Alpha Virginis (Spica)"]
["2012-205T02:00:00","000T02:00:00","2012-07-23","VIMS","SPASS Rider","Dione","ICYEX",null,"occultation","follow UVIS occultation"]
["2012-205T04:00:00","000T05:28:00","2012-07-23","ISS","Prime","rings(general)","MOONLETCD",null,"Cassini Division moonlet search","Cassini Division moonlet search"]
["2012-205T04:00:00","000T05:28:00","2012-07-23","CIRS","SPASS Rider","rings(general)","MOONLETCD",null,"CIRS_169RI_MOONLETCD001_ISS","rider"]
["2012-205T11:38:00","000T09:00:00","2012-07-23","RSS","SPASS Rider","rings(general)","GSE",null,"Gravity Science Enhancement (GSE)","Rings Occultation onbound GSE (Gravity Science Enhancement)  Additional downlink pass at Ka-band to improve Saturn's gravity field determination, and for improving Cassini's orbit locally for data analysis of rings and atmosphere occultation.  DSS-55 required for X- and Ka-band support."]
["2012-205T11:38:00","000T09:00:00","2012-07-23","RSS","SPASS Rider","Saturn","OCCORT","Operations Readiness Test to demonstrate DSN and RSSG preparedness to support upcoming occultations","RSS Operational Readiness Test","RSS Operations Readiness Test (ORT), to demonstrate DSN and RSSG preparedness to support the Rev170 Saturn rings occultation on 2012/225. DSS-55 required for X- and Ka-band support."]
["2012-205T11:38:00","000T09:00:00","2012-07-23","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2012-205T12:38:00","000T08:00:00","2012-07-23","CIRS","SPASS Rider","InstrumentCalibration","DSCAL12",null,"CIRS_169IC_DSCAL12205_SP","rider"]
["2012-205T17:55:48","000T02:42:12","2012-07-23","INMS","Non-SPASS","Saturn","SURVEYSEG","Campaign to determine atmospheric and ionospheric thermal structure","Segment Boundary Survey","Part of the MAPS/TOST Campaign. Determine atmospheric and ionospheric thermal structure."]
["2012-205T20:38:00","000T21:25:07","2012-07-23","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","null"]
["2012-205T20:38:00","000T11:25:07","2012-07-23","INMS","Non-SPASS","Saturn","SURVEYSEG","Campaign to determine atmospheric and ionospheric thermal structure","Segment Boundary Survey","Part of the MAPS/TOST Campaign. Determine atmospheric and ionospheric thermal structure."]
["2012-205T20:38:00","000T19:25:07","2012-07-23","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG MAPS Survey","Continuous low-rate magnetospheric survey"]
["2012-205T20:38:00","001T22:00:00","2012-07-23","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SURVEY Campaign","Part of SURVEY MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane.   TOST_169_T85"]
["2012-205T20:38:00","000T07:42:00","2012-07-23","RPWS","Non-SPASS","Saturn","INSURVEY","Inner magnetosphere survey","RPWS Inner Survey","Setup RPWS for inner magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2012-205T21:32:59","000T09:30:08","2012-07-23","CIRS","Prime","Titan","MIDIRTMAP","Mid infrared thermal map",null,"Obtain information on the thermal structure of Titan's stratosphere. Slew across disk at 4 microrad/s."]
["2012-205T21:32:59","000T09:30:08","2012-07-23","ISS","SPASS Rider","Titan","MIDIRTMAP","Mid infrared thermal map","RCI (Ridealong Context Imaging)","ISS on, max data rate = 182.784 kbps, number of frames and bits/frame are input parameters, data volume = number of frames x bits/frame, average data rate = data volume/duration."]
["2012-205T21:32:59","000T09:30:08","2012-07-23","VIMS","SPASS Rider","Titan","FIRNADCMP","Far infrared nadir composition map","Stare at Titan","VIMS ridealong with CIRS while staring at Titan.  Phase = 151.178 deg.  SSC Lat/Lon = 13.653N/356.284 deg, SS Lat/Lon = 15.127N/177.860 deg.  Alt = 461969.7 km, range = 464544.7 km.  Resolution = 230 km/px.  Temp. M4.   Obtain 160 and 640 ms cubes while staring at Titan."]
["2012-206T04:20:00","001T14:18:00","2012-07-24","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2012-206T07:03:07","000T04:00:00","2012-07-24","CIRS","Prime","Titan","FIRNADCMP","Far infrared nadir composition map",null,"Obtain information on CO, HCN, CH4. Integrate on disk at airmass 1.5--2.0."]
["2012-206T07:03:07","000T04:00:00","2012-07-24","ISS","SPASS Rider","Titan","FIRNADCMP","Far infrared nadir composition map","RCI (Ridealong Context Imaging)","ISS on, max data rate = 182.784 kbps, number of frames and bits/frame are input parameters, data volume = number of frames x bits/frame, average data rate = data volume/duration."]
["2012-206T07:03:07","000T04:00:00","2012-07-24","VIMS","SPASS Rider","Titan","FIRNADCMP","Far infrared nadir composition map","Stare at Titan","VIMS ridealong with CIRS while staring at Titan.  Phase = 149.808 deg.  SSC Lat/Lon = 15.051N/6.052 deg, SS Lat/Lon = 15.131N/186.793 deg.  Alt = 256278.3 km, range = 258853.3 km.  Resolution = 128 km/px.  Temp. N1.   Obtain 160 and 640 ms cubes while staring at Titan."]
["2012-206T07:03:07","000T04:00:00","2012-07-24","UVIS","Non-SPASS","Titan","FIRNADCMP","Far infrared nadir composition map","FIRNADCMP rider","Several slow wcans across Titan's visible hemisphere to form spectral images"]
["2012-206T08:03:07","000T11:00:00","2012-07-24","INMS","Non-SPASS","Titan","T85INBND",null,"Titan flyby","Titan observation"]
["2012-206T11:03:07","000T04:00:00","2012-07-24","VIMS","Prime","Titan","MEDRES","Medium resolution global mapping","Global Mapping of Titan","VIMS global mapping of Titan.  Phase = 159.237 deg.  SSC Lat/Lon = 14.628N/10.194 deg, SS Lat/Lon = 15.133N/190.554 deg.  Alt = 175527.2 km, range = 178102.2 km.  Resolution = 88 km/px.  Temp. Q.  Global mapping of Titan at medium resolution.  1 or 2 2x2 mosaics."]
["2012-206T11:03:07","000T04:00:00","2012-07-24","CIRS","SPASS Rider","Titan","MEDRES","Medium resolution global mapping",null,"Ride along with VIMS."]
["2012-206T11:03:07","000T04:00:00","2012-07-24","ISS","SPASS Rider","Titan","MEDRES","Medium resolution global mapping","RCI (Ridealong Context Imaging)","ISS on, max data rate = 182.784 kbps, number of frames and bits/frame are input parameters, data volume = number of frames x bits/frame, average data rate = data volume/duration."]
["2012-206T15:03:07","000T02:30:00","2012-07-24","VIMS","Prime","Titan","REGMAP","Regional mapping","Regional Mapping of Titan","VIMS regional mapping of Titan.  Phase = 148.185 deg.  SSC Lat/Lon = 16.680N/14.492 deg, SS Lat/Lon = 15.135N/194.315 deg.  Alt = 96299.7 km, range = 98874.7 km.  Resolution = 48 km/px.  Temp. Y.  Regional mapping of Titan's terminator area."]
["2012-206T15:03:07","000T02:30:00","2012-07-24","CIRS","SPASS Rider","Titan","REGMAP","Regional mapping",null,"Ride along with VIMS."]
["2012-206T15:03:07","000T02:30:00","2012-07-24","ISS","SPASS Rider","Titan","REGMAP","Regional mapping","RCI (Ridealong Context Imaging)","ISS on, max data rate = 182.784 kbps, number of frames and bits/frame are input parameters, data volume = number of frames x bits/frame, average data rate = data volume/duration."]
["2012-206T16:03:07","000T08:00:00","2012-07-24","MAG","Non-SPASS","Titan","MAGTITAN","MAG Titan observation","T85 flyby","T85 is another low altitude (990 km) north polar flyby in the post noon sector of Saturn's magnetosphere. With closest approach in the dayside ionosphere, Cassini will be able to study the diffusion of the external magnetic field at low altitudes and mid solar zenith angles. A comparison with T83 and T84 will be very useful.  We assign grade one priority. Data rate: 1976bps (32vps)."]
["2012-206T17:33:07","000T01:15:00","2012-07-24","CIRS","Prime","Titan","FIRLMBINT","Vertical limb sounding",null,"Vertical sounding of stratospheric compounds on Titan, including H2O. Integrations at 2 locations on the limb displaced vertically."]
["2012-206T17:33:07","000T01:15:00","2012-07-24","ISS","SPASS Rider","Titan","FIRLMBINT","Vertical limb sounding","RCI (Ridealong Context Imaging)","ISS on, max data rate = 182.784 kbps, number of frames and bits/frame are input parameters, data volume = number of frames x bits/frame, average data rate = data volume/duration."]
["2012-206T17:33:07","000T01:15:00","2012-07-24","VIMS","SPASS Rider","Titan","REGMAP","Regional mapping","Regional Mapping of Titan","VIMS ridealong with CIRS - pb with CIRS having 2 observations in the same slot"]
["2012-206T17:33:07","000T01:15:00","2012-07-24","UVIS","Non-SPASS","Titan","FIRLMBINT","Vertical limb sounding","Rider with CIRS FIRLMBINT","Rider with CIRS MIRLMBINT"]
["2012-206T18:03:07","000T01:00:00","2012-07-24","CAPS","SPASS Rider","Titan","T85INBND",null,"Inbound 169TI (T85)","null"]
["2012-206T18:03:07","000T01:00:00","2012-07-24","MIMI","SPASS Rider","Titan","TITINOV",null,"MAPS TI Campaign","Part of TI MAPS Campaign.   Investigate micro-scale and near aspects of the Titan interaction by observing during about one hour period around an encounter. With -Y pointed toward Titan, when within 30 minutes of the targeted flyby, optimize secondary axis for corotation flow as close to the S/C -X, +/- Z plane as works with the other constraints on pointing. Also, measure Titan exosphere/magnetosphere interaction by imaging in ENA with INCA (when sun is not in INCA FOV)."]
["2012-206T18:03:07","000T01:00:00","2012-07-24","RPWS","Non-SPASS","Titan","TIINTRMED","Titan magnetosphere interaction","Titan Interaction - Intermediate","Study the interaction of the magnetosphere with Titan at intermediate distances for evidence of ion pickup, radio emissions, density profiles, and the general wave environment.  Prefer Langmuir probe within 90 degrees of plasma ram."]
["2012-206T18:48:07","000T00:30:00","2012-07-24","CIRS","Prime","Titan","FIRLMBAER","Ring photometry",null,"Limb scanning for aerosols."]
["2012-206T18:48:07","000T00:30:00","2012-07-24","ISS","SPASS Rider","Titan","FIRLMBAER","Ring photometry","RCI (Ridealong Context Imaging)","ISS on, max data rate = 182.784 kbps, number of frames and bits/frame are input parameters, data volume = number of frames x bits/frame, average data rate = data volume/duration."]
["2012-206T18:48:07","000T00:30:00","2012-07-24","VIMS","SPASS Rider","Titan","REGMAP","Regional mapping","Regional Mapping of Titan","VIMS ridealong with CIRS - Specular reflection on Kivu Lacus at 18:20:08 - pointing on Kivu done by CIRS Phase = 145.606 deg.  SSC Lat/Lon = 19.235N/18.180 deg, SS Lat/Lon = 15.136N/196.190 deg.  Alt = 42244.6 km, range = 44819.6 km.  Resolution = 21 km/px.  Limb observations - atmospheric composition"]
["2012-206T19:03:07","000T02:00:00","2012-07-24","CAPS","SPASS Rider","Titan","T85CLOSE",null,"Closest Approach 169TI (T85)","null"]
["2012-206T19:03:07","000T02:00:00","2012-07-24","MIMI","SPASS Rider","Titan","TITCAOV",null,"MAPS TI Campaign","Part of TI MAPS Campaign.   Investigate micro-scale and near aspects of the Titan interaction by observing during about one hour period around an encounter. With -Y pointed toward Titan, when within 30 minutes of the targeted flyby, optimize secondary axis for corotation flow as close to the S/C -X, +/- Z plane as works with the other constraints on pointing. Also, measure Titan exosphere/magnetosphere interaction by imaging in ENA with INCA (when sun is not in INCA FOV)."]
["2012-206T19:03:07","000T00:55:30","2012-07-24","INMS","Non-SPASS","Titan","TITAN85",null,"Titan Flyby","Titan observation"]
["2012-206T19:03:07","000T02:00:00","2012-07-24","RPWS","Non-SPASS","Titan","TICA","Titan closest approach","Titan closest approach observations","RPWS observations in the immediate vicinity of Titan, including thermal plasma density and temperature measurements with the Langmuir probe, search for lightning and other radio emissions, characterization of plasma wave spectrum, search for evidence of pickup ions.  Langmuir  probe within 90 degrees of spacecraft ram at closest approach, corotational ram outside of +/- 15 minutes."]
["2012-206T19:19:07","000T00:34:00","2012-07-24","CIRS","Prime","Titan","FIRLMBT","Far Infrared limb tracking","CIRS_169TI_FIRLMBT001_PRIME","Vertical temperature sounding of Titan's tropopause & stratosphere. Slow radial scans."]
["2012-206T19:19:07","000T00:34:00","2012-07-24","ISS","SPASS Rider","Titan","FIRLMBT","Far Infrared limb tracking","RCI (Ridealong Context Imaging)","ISS on, max data rate = 182.784 kbps, number of frames and bits/frame are input parameters, data volume = number of frames x bits/frame, average data rate = data volume/duration."]
["2012-206T19:19:07","000T00:34:00","2012-07-24","VIMS","SPASS Rider","Titan","REGMAP","Regional mapping","Regional Mapping of Titan","VIMS ridealong with CIRS for regional mapping of Titan.  Phase = 136.614 deg.  SSC Lat/Lon = 27.954N/23.531 deg, SS Lat/Lon = 15.137N/198.310 deg.  Alt = 12903.2 km, range = 15478.2 km.  Resolution = 6.5 km/px.  Obtain mosaics and cubes of Titan for regional mapping prior to CA."]
["2012-206T19:53:07","000T00:55:00","2012-07-24","VIMS","Prime","Titan","HIRES","High resolution image","Hi-resolution regional Mapping of Titan","VIMS regional mapping of Titan during C/A.  At C/A, phase = 58.260 deg.  SSC Lat/Lon = 61.630N/149.256 deg, SS Lat/Lon = 15.137N/199.016 deg.  Alt = 1012 km, range = 3587 km.  Resolution = 0.51 km/px.  Obtain mosaics of Titan during C/A."]
["2012-206T19:53:07","000T00:55:00","2012-07-24","CIRS","SPASS Rider","Titan","HIRES","High resolution image",null,"Ride along with VIMS."]
["2012-206T19:53:07","000T00:55:00","2012-07-24","ISS","SPASS Rider","Titan","HIRES","High resolution image","RCI (Ridealong Context Imaging)","ISS on, max data rate = 182.784 kbps, number of frames and bits/frame are input parameters, data volume = number of frames x bits/frame, average data rate = data volume/duration."]
["2012-206T19:58:37","000T00:08:40","2012-07-24","INMS","Non-SPASS","Titan","TITAN85",null,"Titan Flyby","Titan observation"]
["2012-206T20:07:17","000T00:55:50","2012-07-24","INMS","Non-SPASS","Titan","TITAN85",null,"Titan Flyby","Titan observation"]
["2012-206T20:48:07","000T00:22:00","2012-07-24","CIRS","SPASS Rider","Titan","TRANS",null,null,"Ride along with ENGR."]
["2012-206T20:48:07","000T00:22:00","2012-07-24","VIMS","SPASS Rider","Titan","TRANS",null,"Hi-resolution  Mapping during transition","VIMS cubes during transitionSsegional mapping of Titan during C/A.  At C/A, phase = ??? deg.  SC Lat/Lon = ??? deg, SS Lat/Lon = 15.N/199. deg.  Alt = 20,000km,.  Resolution =10 km/px."]
["2012-206T21:03:07","000T01:00:00","2012-07-24","CAPS","SPASS Rider","Titan","T85OUTBND",null,"Outbound 169TI (T85)","null"]
["2012-206T21:03:07","000T01:00:00","2012-07-24","MIMI","SPASS Rider","Titan","TITOUTOV",null,"MAPS TI Campaign","Part of TI MAPS Campaign.   Investigate micro-scale and near aspects of the Titan interaction by observing during about one hour period around an encounter. With -Y pointed toward Titan, when within 30 minutes of the targeted flyby, optimize secondary axis for corotation flow as close to the S/C -X, +/- Z plane as works with the other constraints on pointing. Also, measure Titan exosphere/magnetosphere interaction by imaging in ENA with INCA (when sun is not in INCA FOV)."]
["2012-206T21:03:07","000T11:00:00","2012-07-24","INMS","Non-SPASS","Titan","T85OUTBND",null,"Titan flyby","Titan observation"]
["2012-206T21:03:07","000T01:00:00","2012-07-24","RPWS","Non-SPASS","Titan","TIINTRMED","Titan magnetosphere interaction","Titan Interaction - Intermediate","Study the interaction of the magnetosphere with Titan at intermediate distances for evidence of ion pickup, radio emissions, density profiles, and the general wave environment.  Prefer Langmuir probe within 90 degrees of plasma ram."]
["2012-206T21:10:07","000T01:08:00","2012-07-24","VIMS","Prime","Titan","HIRES","High resolution image","Hi-resolution regional Mapping of Titan","VIMS regional mapping of Titan.  Phase = 28.736 deg.  SSC Lat/Lon = 13.581S/199.019 deg, SS Lat/Lon = 15.137N/200.034 deg.  Alt = 19384.6 km, range = 21959.6 km.  Resolution = 9.7 km/px.  Obtain mosaics of Titan for regional mapping."]
["2012-206T21:10:07","000T01:08:00","2012-07-24","CIRS","SPASS Rider","Titan","HIRES","High resolution image",null,"Ride along with VIMS."]
["2012-206T21:10:07","000T01:08:00","2012-07-24","ISS","SPASS Rider","Titan","HIRES","High resolution image","RCI (Ridealong Context Imaging)","ISS on, max data rate = 182.784 kbps, number of frames and bits/frame are input parameters, data volume = number of frames x bits/frame, average data rate = data volume/duration."]
["2012-206T22:03:07","000T20:29:52","2012-07-24","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","null"]
["2012-206T22:18:07","000T02:45:00","2012-07-24","CIRS","Prime","Titan","FIRNADMAP","Far infrared nadir composition map","CIRS_014TI_FIRNADIRMAP_01","Obtain information on surface & tropopause temperatures, and on tropospheric CH4.  Scan  or contiguous steps across disk.  POINTING: -y to Titan, x away from sun.  Z axis generally aligned N/S or E/W, perpendicular to scan or steps."]
["2012-206T22:18:07","000T02:45:00","2012-07-24","ISS","SPASS Rider","Titan","FIRNADMAP","Far infrared nadir composition map","RCI (Ridealong Context Imaging)","ISS on, max data rate = 182.784 kbps, number of frames and bits/frame are input parameters, data volume = number of frames x bits/frame, average data rate = data volume/duration."]
["2012-206T22:18:07","000T02:45:00","2012-07-24","VIMS","SPASS Rider","Titan","FIRNADMAP","Far infrared nadir composition map","Titan Scan.","VIMS ridealong with CIRS while scanning across Titan.  Phase = 33.528 deg.  SSC Lat/Lon = 18.377N/202.052 deg, SS Lat/Lon = 15.138N/201.131 deg.  Alt = 42247.8 km, range = 44822.8 km.  Resolution = 21 km/px.  Temp. E.   Obtain cubes while scanning across Titan."]
["2012-207T00:03:07","001T06:34:53","2012-07-25","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG MAPS Survey","Continuous low-rate magnetospheric survey"]
["2012-207T01:03:07","000T04:00:00","2012-07-25","CIRS","Prime","Titan","MIRLMBMAP","Mid infrared limb map",null,"Obtain vertical profiles of temperatures in Titan's stratosphere. The arrays are stepped along the limb at two altitudes at 5 degree latitude intervals."]
["2012-207T01:03:07","000T04:00:00","2012-07-25","ISS","SPASS Rider","Titan","MIRLMBMAP","Mid infrared limb map","RCI (Ridealong Context Imaging)","ISS on, max data rate = 182.784 kbps, number of frames and bits/frame are input parameters, data volume = number of frames x bits/frame, average data rate = data volume/duration."]
["2012-207T01:03:07","000T04:00:00","2012-07-25","VIMS","SPASS Rider","Titan","MIRLMBMAP","Mid infrared limb map","Limb Mapping","VIMS ridealong with CIRS for limb mapping of Titan.  Phase = 30.037 deg.  SSC Lat/Lon = 20.849N/205.637 deg, SS Lat/Lon = 15.139N/203.717 deg.  Alt = 96270.4 km, range = 98845.4 km.  Resolution = 48 km/px.  Temp. F.   Obtain cubes of Titan's limb."]
["2012-207T05:03:07","000T05:00:00","2012-07-25","VIMS","Prime","Titan","GLOBMAP","Global coverage mapping","Global Mapping of Titan","VIMS global  mapping of Titan.  Phase = 36.872 deg.  SSC Lat/Lon = 21.672S/209.622 deg, SS Lat/Lon = 15.141N/207.477 deg.  Alt = 175115.8 km, range = 177690.8 km.  Resolution = 88 km/px.  Temp. V.  Obtain cubes for global mapping of Titan."]
["2012-207T05:03:07","000T05:00:00","2012-07-25","CIRS","SPASS Rider","Titan","GLOBMAP","Global coverage mapping",null,"Ride along with VIMS."]
["2012-207T05:03:07","000T05:00:00","2012-07-25","ISS",null,"Titan","GLOBMAP","Global coverage mapping","RCI (Ridealong Context Imaging)","ISS on, max data rate = 182.784 kbps, number of frames and bits/frame are input parameters, data volume = number of frames x bits/frame, average data rate = data volume/duration."]
["2012-207T08:03:07","000T22:34:52","2012-07-25","INMS","Non-SPASS","Saturn","SURVEYSEG","Campaign to determine atmospheric and ionospheric thermal structure","Segment Boundary Survey","Part of the MAPS/TOST Campaign. Determine atmospheric and ionospheric thermal structure."]
["2012-207T10:03:07","000T07:39:52","2012-07-25","VIMS","Prime","Titan","GLOBMAP","Global coverage mapping","Global Mapping of  Titan","VIMS global mapping of Titan.  Phase = 37.099 deg.  SSC Lat/Lon = 21.906S/214.149 deg, SS Lat/Lon = 15.143N/212.178 deg.  Alt = 274416.0 km, range = 276991.0 km.  Resolution = 137 km/px.  Temp. B.  Obtain cubes for global mapping of Titan."]
["2012-207T10:03:07","000T07:39:52","2012-07-25","CIRS","SPASS Rider","Titan","GLOBMAP","Global coverage mapping",null,"Ride along with VIMS."]
["2012-207T10:03:07","000T07:39:52","2012-07-25","ISS",null,"Titan","GLOBMAP","Global coverage mapping","RCI (Ridealong Context Imaging)","ISS on, max data rate = 182.784 kbps, number of frames and bits/frame are input parameters, data volume = number of frames x bits/frame, average data rate = data volume/duration."]
["2012-207T18:33:00","000T12:05:00","2012-07-25","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","null"]
["2012-207T18:38:00","000T12:00:00","2012-07-25","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SURVEY Campaign","Part of SURVEY MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane.   TOST_169_T85"]
["2012-207T18:38:00","000T12:00:00","2012-07-25","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2012-207T18:38:00","000T10:00:00","2012-07-25","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2012-207T19:38:00","000T11:00:00","2012-07-25","CIRS","SPASS Rider","InstrumentCalibration","DSCAL12",null,"CIRS_169IC_DSCAL12207_SP","rider"]
["2012-208T04:38:00","000T02:00:00","2012-07-26","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2012-208T06:38:00","017T02:43:00","2012-07-26","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","null"]
["2012-208T06:38:00","002T03:30:00","2012-07-26","INMS","Non-SPASS","Saturn","SURVEYSEG","Campaign to determine atmospheric and ionospheric thermal structure","Segment Boundary Survey","Part of the MAPS/TOST Campaign. Determine atmospheric and ionospheric thermal structure."]
["2012-208T06:38:00","001T03:45:00","2012-07-26","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG MAPS Survey","Continuous low-rate magnetospheric survey"]
["2012-208T06:38:00","007T04:14:00","2012-07-26","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SURVEY Campaign","Part of SURVEY MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane.   XD_169_170"]
["2012-208T06:38:00","005T13:29:00","2012-07-26","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2012-208T06:53:00","000T17:00:00","2012-07-26","UVIS","Prime","Saturn","MOS169APO",null,null,"Mosaic scan of Saturn magnetosphere, day 1. EUV and FUV low resolution slits on.  Allowances have been made for 20 minutes observation margin at start and end, and 30 minutes for turning back to waypoint at the end.  Note: data to be taken only when slit is stationary.  Waypoint is assumed to be Saturn center. Align slit with Saturn spin axis. Initial slews: 0 mrad about x-axis, -0 mrad about z-axis (z = 0 Rs). Start data capture, stare 757.0 s, stop data capture. Repeat PATTERN 70 times.  PATTERN: Slew -1.5 mrad about z-axis. Start data capture, stare 757.0 s, stop data capture.  Note: As no data will be collected while Cassini is slewing, actual data volume = (1599.48284 bps, from Alain's spreadsheet)x(757.0s per stare)x(71 stares) = 85.9674x10^6 bits. Data rate multiplier includes factor of 1.01 for data packet filling."]
["2012-208T08:00:00","002T00:00:00","2012-07-26","CDA","SPASS Rider","DustRAM direction","RETROGR","MAPS retrograde campaign","Retrograde campaign","Retrograde measurement - DV, TLM and power are covered by the background requests (..._RATE..._)"]
["2012-209T01:23:00","000T09:00:00","2012-07-27","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2012-209T02:23:00","000T08:00:00","2012-07-27","CIRS","SPASS Rider","InstrumentCalibration","DSCAL12",null,"CIRS_169IC_DSCAL12209_SP","rider"]
["2012-209T10:23:00","000T08:00:00","2012-07-27","MAG","Prime","Sun","CALROLL","MAG calibration roll","MAG Calibration Rolls","Roll about axis other than Z for determination of sensor offsets, actual roll axis is not important - selected axis is usually suitable for MAPS.  Preferably calibrations should be made every 15-20 days in areas where field conditions are suitable.  Note: periods of suitable data are defined as follows; 1) More distant than 15 RS from Saturn's axis (to try and get into the more uniform part of the internal+sheet field). 2) Inside the magnetopause (more specifically inside a most compressed model MP). 3) More distant than 3 RS from the current sheet. Using a 'hinged' sheet model which departs from Saturn's equatorial plane at about 15 RS and then follows the anti-solar direction on the nightside. This means that, even though its orbit is equatorial, if the spacecraft is situated far enough away from the planet, it should see the nightside current sheet divert northwards away from it (using Saturn axis tilted 17 deg away from Sun).  Apart from possible injection events, sheet disruptions etc the resultant periods should have a reasonable probability of seeing a 'quiescent' 'lobe-like' or 'disk-like' field. We would prefer as far downtail as possible so the field has more chance of pointing in a single direction over larger length scales."]
["2012-209T18:23:00","004T01:44:00","2012-07-27","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG MAPS Survey","Continuous low-rate magnetospheric survey"]
["2012-210T01:08:00","000T09:00:00","2012-07-28","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2012-210T02:08:00","000T08:00:00","2012-07-28","CIRS","SPASS Rider","InstrumentCalibration","DSCAL12",null,"CIRS_169IC_DSCAL12210_SP","rider"]
["2012-210T10:08:00","000T15:00:00","2012-07-28","UVIS","Prime","Saturn","MOS169APO",null,null,"Mosaic scan of Saturn magnetosphere, day 2.  EUV and FUV low resolution slits on.  Allowances have been made for 20 minutes observation margin at start and end, and 30 minutes for turning back to waypoint at the end.  Note:  data to be taken only when slit is stationary.  Waypoint is assumed to be Saturn center.  Align slit with Saturn spin axis.  Initial slews:  0 mrad about x-axis, -83.8 mrad about z-axis (z ~ -3.1 Rs).  Start data capture, stare 765.0 s, stop data capture.  Repeat PATTERN 60 times.  PATTERN:  Slew -1.5 mrad about z-axis.  Start data capture, stare 765.0 s, stop data capture.  Note:  As no data will be collected while Cassini is slewing, actual data volume = (1582.75623 bps, from Alain's spreadsheet)x(765.0s per stare)x(61 stares) = 73.85932x10^6 bits.  Data rate multiplier includes factor of 1.01 for data packet filling."]
["2012-210T10:08:00","000T07:00:00","2012-07-28","ISS","SPASS Rider","InstrumentCalibration","NACDARK","ISS Narrow Angle Camera dark current calibration","ISS NAC dark current calibration","ISS NAC dark current calibration"]
["2012-210T10:08:00","001T00:00:00","2012-07-28","INMS","Non-SPASS","Saturn","SURVPOTM","MAPS survey","Post OTM Survey","Post-OTM request to resume science mode after NAV OTM."]
["2012-210T17:23:00","000T07:00:00","2012-07-28","ISS","SPASS Rider","InstrumentCalibration","WACDARK","ISS Wide Angle Camera dark current calibration","ISS WAC dark current calibration","ISS WAC dark current calibration"]
["2012-211T01:08:00","000T09:00:00","2012-07-29","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2012-211T02:08:00","000T08:00:00","2012-07-29","CIRS","SPASS Rider","InstrumentCalibration","DSCAL12",null,"CIRS_169IC_DSCAL12211_SP","rider"]
["2012-211T10:08:00","001T23:29:00","2012-07-29","UVIS","Prime","Saturn","MOS169APO",null,null,"Mosaic scan of Saturn magnetosphere, day 3.  EUV and FUV low resolution slits on.  Allowances have been made for 20 minutes observation margin at start and end, and 30 minutes for turning back to waypoint at the end.  Note:  data to be taken only when slit is stationary.  Waypoint is assumed to be Saturn center.  Align slit with Saturn spin axis.  Initial slews:  +50 mrad about x-axis, +142.5 mrad about z-axis (z ~ 5.7 Rs).  Start data capture, stare 586.0 s, stop data capture.  Repeat PATTERN 261 times.  PATTERN:  Slew -1.5 mrad about z-axis.  Start data capture, stare 586.0 s, stop data capture.  Note:  As no data will be collected while Cassini is slewing, actual data volume = (2066.22613 bps, from Alain's spreadsheet)x(586.0s per stare)x(262 stares) = 317.23183x10^6 bits.  Data rate multiplier includes factor of 1.01 for data packet filling."]
["2012-211T10:08:00","004T00:44:00","2012-07-29","INMS","Non-SPASS","Saturn","SURVBOTM","MAPS survey","Post OTM Survey","Post-OTM request to resume science mode after NAV OTM."]
["2012-212T10:52:00","000T20:00:00","2012-07-30","CDA","SPASS Rider","DustRAM direction","ISD0050",null,"CDA ISD 2012-215T10:52:00","ISD observation around apoapse 2012-215T10:52:00 43.307727 Rs"]
["2012-213T11:07:00","000T09:00:00","2012-07-31","RSS","SPASS Rider","Saturn","OCCORT","Operations Readiness Test to demonstrate DSN and RSSG preparedness to support upcoming occultations","RSS Operational Readiness Test","RSS Operations Readiness Test (ORT), to demonstrate DSN and RSSG preparedness to support the Rev170 Saturn rings occultation on 2012/225. DSS-55 required for X- and Ka-band support."]
["2012-213T11:07:00","000T09:00:00","2012-07-31","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2012-213T12:07:00","000T08:00:00","2012-07-31","CIRS","SPASS Rider","InstrumentCalibration","DSCAL12",null,"CIRS_169IC_DSCAL12213_SP","rider"]
["2012-213T20:07:00","001T03:15:00","2012-07-31","UVIS","Prime","Saturn","MOS169APO",null,null,"Mosaic scan of Saturn magnetosphere, day 4. EUV and FUV low resolution slits on.  Allowances have been made for 20 minutes observation margin at start and end, and 30 minutes for turning back to waypoint at the end.  Note: data to be taken only when slit is stationary.  Waypoint is assumed to be Saturn center. Align slit with Saturn spin axis. Initial slews: -50 mrad about x-axis, +29.4 mrad about z-axis (z ~ +1.25 Rs). Start data capture, stare 633.5 s, stop data capture. Repeat PATTERN 136 times.  PATTERN: Slew +1.5 mrad about z-axis. Start data capture, stare 633.5 s, stop data capture.  Note: As no data will be collected while Cassini is slewing, actual data volume = (1911.29994 bps, from Alain's spreadsheet)x(633.5 s per stare)x(137 stares) = 165.881x10^6 bits. Data rate multiplier includes factor of 1.01 for data packet filling."]
["2012-213T20:07:00","001T14:45:00","2012-07-31","CDA","Non-SPASS","Other","RATE010B",null,"Data rate End:SApo","Range enter= 5.3128487 Rs exit= 7.2761371 Range altitude= 40386.044 km ... -40678.270"]
["2012-213T20:07:00","012T18:38:00","2012-07-31","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG MAPS Survey","Continuous low-rate magnetospheric survey"]
["2012-213T20:07:00","001T14:45:00","2012-07-31","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2012-214T04:52:00","000T20:00:00","2012-08-01","CDA","SPASS Rider","DustRAM direction","ISD0050",null,"CDA ISD 2012-215T10:52:00","ISD observation around apoapse 2012-215T10:52:00 43.307727 Rs"]
["2012-215T00:52:00","000T09:00:00","2012-08-02","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2012-215T01:52:00","000T08:00:00","2012-08-02","CIRS","SPASS Rider","InstrumentCalibration","DSCAL12",null,"CIRS_169IC_DSCAL12215_SP","rider"]
["2012-215T10:30:00","000T00:02:00","2012-08-02","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2012-215T10:32:00","000T01:30:00","2012-08-02","ISS","Prime","Titan","M90R3CLD",null,"Titan Monitoring Campaign","Titan Monitoring Campaign, requested phase 64 requested range 3.6 Mkm"]
["2012-215T10:32:00","000T01:30:00","2012-08-02","CIRS","SPASS Rider","Titan","M90R3CLD",null,"Rider for Titan Monitoring Campaign","Rider to ISS Titan cloud monitor"]
["2012-215T10:32:00","000T01:30:00","2012-08-02","VIMS","SPASS Rider","Titan","M90R3CLD",null,"Titan Monitoring Campaign and Stormwatch Cube","Titan Monitoring Campaign; phase = 64 deg, range =3.60 Mkm. Saturn Stormwatch at end"]
["2012-215T10:52:00","009T09:08:00","2012-08-02","CDA","Non-SPASS","Other","RATE010A",null,"Data rate Enter:SApo","Range enter= 5.3128487 Rs exit= 7.2761371 Range altitude= 40386.044 km ... -40678.270"]
["2012-215T10:52:00","000T02:00:00","2012-08-02","INMS","Non-SPASS","Saturn","ENGBCKGND",null,"Engineering background observation","Full rate measurement to gather engineering background data"]
["2012-215T10:52:00","009T22:29:00","2012-08-02","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SURVEY Campaign","Part of SURVEY MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane.   XD_169_170"]
["2012-215T10:52:00","007T13:29:00","2012-08-02","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2012-215T10:52:25","000T00:00:01","2012-08-02","MP","SPASS Note","Saturn","APOAPSE","Apoapse",null,"Apoapse  Per = 21.2 d, inc = 32.2 deg, r = 43.265 Rs, phase = 78 deg"]
["2012-215T12:00:00","000T00:02:00","2012-08-02","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2012-215T12:02:00","001T10:25:00","2012-08-02","UVIS","Prime","Saturn","MOS169APO",null,null,"Mosaic scan of Saturn magnetosphere, day 5. EUV and FUV low resolution slits on.  Allowances have been made for 20 minutes observation margin at start and end, and 30 minutes for turning back to waypoint at the end.  Note: data to be taken only when slit is stationary.  Waypoint is assumed to be Saturn center. Align slit with Saturn spin axis. Initial slews: -50 mrad about x-axis, +29.1 mrad about z-axis (z ~ +1.25 Rs). Start data capture, stare 633.0 s, stop data capture. Repeat PATTERN 174 times.  PATTERN: Slew -1.5 mrad about z-axis. Start data capture, stare 633.0 s, stop data capture.  Note: As no data will be collected while Cassini is slewing, actual data volume = (1912.80966 bps, from Alain's spreadsheet)x(633.0s per stare)x(175 stares) = 211.8915x10^6 bits. Data rate multiplier includes factor of 1.01 for data packet filling."]
["2012-215T12:02:00","001T10:25:00","2012-08-02","VIMS","SPASS Rider","Saturn","STORMW","Saturn storm watch","Storm Watch Ridealong","Storm Watch: 32*32 pixels with 80 msec integration during the last two minutes of this observation"]
["2012-215T12:52:00","004T20:44:00","2012-08-02","INMS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","Survey","Part of the MAPS/TOST Campaign. Determine atmospheric and ionospheric thermal structure."]
["2012-215T20:52:00","000T20:00:00","2012-08-02","CDA","SPASS Rider","DustRAM direction","ISD0050",null,"CDA ISD 2012-215T10:52:00","ISD observation around apoapse 2012-215T10:52:00 43.307727 Rs"]
["2012-216T22:25:00","000T00:02:00","2012-08-03","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2012-217T00:37:00","000T09:00:00","2012-08-04","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2012-217T01:37:00","000T08:00:00","2012-08-04","CIRS","SPASS Rider","InstrumentCalibration","DSCAL12",null,"CIRS_170IC_DSCAL12217_SP","rider"]
["2012-217T09:37:00","000T13:30:00","2012-08-04","UVIS","Prime","Saturn","MOS169APO",null,null,"Mosaic scan of Saturn magnetosphere, day 6. EUV and FUV low resolution slits on.  Allowances have been made for 20 minutes observation margin at start and end, and 30 minutes for turning back to waypoint at the end.  Note: data to be taken only when slit is stationary.  Waypoint is assumed to be Saturn center. Align slit with Saturn spin axis. Initial slews: +50 mrad about x-axis, +135.7 mrad about z-axis (z ~ +5.7 Rs). Start data capture, stare 583.0 s, stop data capture. Repeat PATTERN 68 times.  PATTERN: Slew +1.5 mrad about z-axis. Start data capture, stare 583.0 s, stop data capture.  Note: As no data will be collected while Cassini is slewing, actual data volume = (2076.85851 bps, from Alain's spreadsheet)x(583.0s per stare)x(69 stares) = 83.5458x10^6 bits. Data rate multiplier includes factor of 1.01 for data packet filling."]
["2012-217T14:52:00","000T20:00:00","2012-08-04","CDA","SPASS Rider","DustRAM direction","ISD0050",null,"CDA ISD 2012-215T10:52:00","ISD observation around apoapse 2012-215T10:52:00 43.307727 Rs"]
["2012-218T00:37:00","000T09:00:00","2012-08-05","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2012-218T09:37:00","000T13:29:00","2012-08-05","UVIS","Prime","Saturn","MOS169APO",null,null,"Mosaic scan of Saturn magnetosphere, day 7. EUV and FUV low resolution slits on.  Allowances have been made for 20 minutes observation margin at start and end, and 30 minutes for turning back to waypoint at the end.  Note: data to be taken only when slit is stationary.  Waypoint is assumed to be Saturn center. Align slit with Saturn spin axis. Initial slews: 0 mrad about x-axis, +168.8 mrad about z-axis (z ~ +6.75 Rs Rs). Start data capture, stare 766.0 s, stop data capture. Repeat PATTERN 53 times.  PATTERN: Slew +1.5 mrad about z-axis. Start data capture, stare 766.0 s, stop data capture.  Note: As no data will be collected while Cassini is slewing, actual data volume = (1580.68997 bps, from Alain's spreadsheet)x(766.0s per stare)x(54 stares) = 65.3837x10^6 bits. Data rate multiplier includes factor of 1.01 for data packet filling."]
["2012-218T20:36:00","000T13:00:00","2012-08-05","RSS","SPASS Rider","Earth","USOPIM","RSS Ultra stable oscillator / Periodic Instrument Maintenance","RSS USO Characterization plus PIM","RSS USO characterization plus PIM. Pointing=XBAND to Earth. No rolling during 3-hour USO from 2012-221T00:21:00 till 2012-221T03:21:00, to be tracked at DSS-34 in 1-way mode.  Keep Ka-band ON till end of downlink at 2012-221T09:21:00 to satisfy PIM requirement."]
["2012-219T00:36:00","000T09:00:00","2012-08-06","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2012-219T09:36:00","000T15:00:00","2012-08-06","UVIS","Prime","Saturn","MOS169APO",null,null,"Mosaic scan of Saturn magnetosphere, day 8. EUV and FUV low resolution slits on.  Allowances have been made for 20 minutes observation margin at start and end, and 30 minutes for turning back to waypoint at the end.  Note: data to be taken only when slit is stationary.  Waypoint is assumed to be Saturn center. Align slit with Saturn spin axis. Initial slews: 0 mrad about x-axis, -171.1 mrad about z-axis (z ~ -6.5 Rs Rs). Start data capture, stare 762.0 s, stop data capture. Repeat PATTERN 60 times.  PATTERN: Slew -1.5 mrad about z-axis. Start data capture, stare 762.0 s, stop data capture.  Note: As no data will be collected while Cassini is slewing, actual data volume = (1588.98755 bps, from Alain's spreadsheet)x(762.0 s per stare)x(61 stares) = 73.8593x10^6 bits. Data rate multiplier includes factor of 1.01 for data packet filling."]
["2012-220T00:36:00","000T09:00:00","2012-08-07","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2012-220T01:36:00","000T08:00:00","2012-08-07","CIRS","SPASS Rider","InstrumentCalibration","DSCAL12",null,"CIRS_170IC_DSCAL12220_SP","rider"]
["2012-220T09:36:00","000T14:45:00","2012-08-07","UVIS","Prime","Saturn","MOS169APO",null,null,"Mosaic scan of Saturn magnetosphere, day 9. EUV and FUV low resolution slits on.  Allowances have been made for 20 minutes observation margin at start and end, and 30 minutes for turning back to waypoint at the end.  Note: data to be taken only when slit is stationary.  Waypoint is assumed to be Saturn center. Align slit with Saturn spin axis. Initial slews: 0 mrad about x-axis, +103.6 mrad about z-axis (z ~ +3.625 Rs Rs). Start data capture, stare 762.0 s, stop data capture. Repeat PATTERN 59 times.  PATTERN: Slew +1.5 mrad about z-axis. Start data capture, stare 762.0 s, stop data capture.  Note: As no data will be collected while Cassini is slewing, actual data volume = (1588.98755 bps, from Alain's spreadsheet)x(762.0 s per stare)x(60 stares) = 72.6485x10^6 bits. Data rate multiplier includes factor of 1.01 for data packet filling."]
["2012-220T09:36:00","000T23:45:00","2012-08-07","INMS","Non-SPASS","Saturn","SURVPOTM","MAPS survey","Post OTM Survey","Post-OTM request to resume science mode after NAV OTM."]
["2012-221T00:21:00","000T09:00:00","2012-08-08","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2012-221T01:21:00","000T08:00:00","2012-08-08","CIRS","SPASS Rider","InstrumentCalibration","DSCAL12",null,"CIRS_170IC_DSCAL12221_SP","rider"]
["2012-221T09:21:00","003T09:34:40","2012-08-08","INMS","Non-SPASS","Saturn","SURVBOTM","MAPS survey","Post OTM Survey","Post-OTM request to resume science mode after NAV OTM."]
["2012-221T09:58:00","000T00:02:00","2012-08-08","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2012-221T10:00:00","000T18:41:00","2012-08-08","UVIS","Prime","Saturn","MOS169APO",null,null,"Mosaic scan of Saturn magnetosphere, day 10. EUV and FUV low resolution slits on.  Allowances have been made for 20 minutes observation margin at start and end, and 30 minutes for turning back to waypoint at the end.  Note: data to be taken only when slit is stationary.  Waypoint is assumed to be Saturn center. Align slit with Saturn spin axis. Initial slews: 0 mrad about x-axis, +0 mrad about z-axis (z = 0 Rs). Start data capture, stare 762.0 s, stop data capture. Repeat PATTERN 77 times.  PATTERN: Slew +1.5 mrad about z-axis. Start data capture, stare 762.0 s, stop data capture.  Note: As no data will be collected while Cassini is slewing, actual data volume = (1588.98755 bps, from Alain's spreadsheet)x(762.0 s per stare)x(78 stares) = 94.4431x10^6 bits. Data rate multiplier includes factor of 1.01 for data packet filling."]
["2012-221T10:00:00","000T18:41:00","2012-08-08","VIMS","SPASS Rider","Saturn","STORMW","Saturn storm watch","Storm Watch Ridealong","Storm Watch: 32*32 pixels with 80 msec integration during the last two minutes of this observation"]
["2012-221T22:00:00","002T00:00:00","2012-08-08","CDA","SPASS Rider","DustRAM direction","RETROGR","MAPS retrograde campaign","Retrograde campaign","Retrograde measurement - DV, TLM and power are covered by the background requests (..._RATE..._)"]
["2012-222T04:39:00","000T00:02:00","2012-08-09","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2012-222T06:11:00","000T16:00:00","2012-08-09","ISS","Prime","RingF","FMOVIE","F ring movie","Long Low Res F Ring Movie","Low Resolution F Ring Movie"]
["2012-222T06:11:00","000T16:00:00","2012-08-09","CIRS","SPASS Rider","rings(general)","FMOVIE","F ring movie",null,"null"]
["2012-222T06:11:00","000T16:00:00","2012-08-09","VIMS","SPASS Rider","rings(general)","FMOVIE","F ring movie","F Movie","Use 640 or 1000 msec tau_IR"]
["2012-222T22:09:00","000T00:02:00","2012-08-09","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2012-223T00:21:00","001T18:26:00","2012-08-10","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2012-223T00:21:00","000T09:00:00","2012-08-10","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2012-223T01:21:00","000T08:00:00","2012-08-10","CIRS","SPASS Rider","InstrumentCalibration","DSCAL12",null,"CIRS_170IC_DSCAL12223_SP","rider"]
["2012-223T06:09:00","000T03:12:00","2012-08-10","MAG","Non-SPASS","Other","R1DLROLL","MAG downlink roll calibration","MAG_R1_DLROLL_CAL","Rider on rolling downlink with MAG FGM in range 1. Used for calibration of range 1. Rides on current MAG activities - no additional power or datavolume used."]
["2012-223T17:51:00","000T03:00:00","2012-08-10","RADAR","Non-SPASS","Other","WU4RADCAL","RADAR distant Titan radiometry warm up","Distant Titan Radiometry Warm Up","Warmup for calibration and science data collection."]
["2012-223T20:51:00","000T02:00:00","2012-08-10","RADAR","Prime","Titan","RADIOMCAL","RADAR distant Titan radiometry calibration","Distant Titan Radiometry Calibration","Obtain distant Titan radiometer science and calibration data."]
["2012-224T00:21:00","000T09:00:00","2012-08-11","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2012-224T01:21:00","000T08:00:00","2012-08-11","CIRS","SPASS Rider","InstrumentCalibration","DSCAL12",null,"CIRS_170IC_DSCAL12224_SP","rider"]
["2012-224T14:25:00","000T06:25:00","2012-08-11","VIMS","Prime","rings(general)","BETPEGOCC",null,"betPeg Ring Occultation","Ring stellar occultation; integration time = 40msec; Egress occ."]
["2012-224T18:47:00","000T14:34:00","2012-08-11","RPWS","Non-SPASS","Saturn","INSURVEY","Inner magnetosphere survey","RPWS Inner Survey","Setup RPWS for inner magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2012-224T18:55:40","000T14:25:20","2012-08-11","INMS","Non-SPASS","Saturn","SURVEYRPA",null,"Ring Plane Observation","Observe neutral molecules in the equatorial plane"]
["2012-224T20:00:00","000T21:08:56","2012-08-11","CDA","Non-SPASS","Other","RATE010B",null,"Data rate Enter:SApo","Range enter= 5.3128487 Rs exit= 7.2761371 Range altitude= 40386.044 km ... -40678.270"]
["2012-225T00:00:00","000T01:08:00","2012-08-12","CAPS","Non-SPASS","InstrumentCalibration","ELSCAL","CAPS Electron Spectrometer calibration","ELS Calibration","null"]
["2012-225T00:21:00","000T09:00:00","2012-08-12","RSS","SPASS Rider","rings(general)","GSE",null,"Gravity Science Enhancement (GSE)","Rings Occultation inbound GSE (Gravity Science Enhancement)  Additional downlink pass at Ka-band to improve Saturn's gravity field determination, and for improving Cassini's orbit locally for data analysis of rings and atmosphere occultation.  DSS-34 required for X- and Ka-band support."]
["2012-225T00:21:00","000T09:00:00","2012-08-12","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2012-225T01:21:00","000T08:00:00","2012-08-12","CIRS","SPASS Rider","InstrumentCalibration","DSCAL12",null,"CIRS_170IC_DSCAL12225_SP","rider"]
["2012-225T07:56:00","000T01:44:59","2012-08-12","RSS","SPASS Rider","rings(general)","THERMAL","Thermal stabilization period","RSS 170 RI OCC Thermal Stabilization","A thermal stabilization period of 2 hrs and 5 min is required immediately prior to any radio science experiment which uses Ka-band or S-band.  Note that the  observation period of the corresponding science request includes a budgeted 40 min waypoint turn that can be considered as part of the warmup time.  Hence, the total duration of this warmup request is shorter than the required 2 hrs and 5 min by those 40 min (that is, only 1 hr and 25 min).  The duration should be increased back to the original 2 hrs 5 min if a waypoint turn proves unnecessary."]
["2012-225T09:21:00","002T09:59:00","2012-08-12","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","null"]
["2012-225T09:21:00","000T08:54:00","2012-08-12","INMS","Non-SPASS","Saturn","RINGPLNA",null,"Ring Plane Observation","Observe neutral molecules in the equatorial plane"]
["2012-225T09:21:00","002T09:59:00","2012-08-12","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SURVEY Campaign","Part of SURVEY MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane.   RINGS_170"]
["2012-225T09:21:00","001T22:51:00","2012-08-12","RPWS","Non-SPASS","Saturn","INSURVEY","Inner magnetosphere survey","RPWS Inner Survey","Setup RPWS for inner magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2012-225T09:40:59","000T02:35:00","2012-08-12","RSS","Prime","Saturn","OCCOUT","Egress Occultation","RSS Saturn Egress Atmospheric Occultation","This is for the RSS occultation of Saturn's ionosphere and atmosphere, to measure vertical profiles of electron density in the ionosphere, and of density, pressure, and temperature in the neutral atmosphere. X, S, and Ka bands will be used. Prior to this point the RFIS bay will have been thermally stabilized (see thermal stabilisation request)."]
["2012-225T12:15:59","000T03:57:00","2012-08-12","RSS","Prime","rings(general)","OCC","Occultation","RSS XXM Ring Occ - Egress","Ingress ring occultation conducted using TBD bands (TBD Op-mode). The op-mode is selected based on power constraints. Observations will commence after a 2 hrs 5 min period of thermal stabilization (in RSS WARMUP op-mode)."]
["2012-225T16:33:00","000T03:45:00","2012-08-12","CDA","Prime","DustRAM direction","RPX0490",null,"CDA RPXing 2012-225T18:55:56","RPXing at 6.7617841 Rs, CDA articulation 90 degrees, compatible with INMS"]
["2012-225T17:08:56","000T03:32:00","2012-08-12","CDA","Non-SPASS","Other","RATE080","Dust survey","Data rate","Range enter= 7.2658746 Rs exit= 6.3247734 Range altitude= -39928.740 km ... 39270.128"]
["2012-225T18:15:00","000T00:10:00","2012-08-12","INMS","Non-SPASS","Saturn","RINGPLNA",null,"Ring Plane Observation","Observe neutral molecules in the equatorial plane"]
["2012-225T18:25:00","000T01:50:00","2012-08-12","INMS","SPASS Rider","Saturn","INNERMAG","Observing neutral molecules in the inner magnetosphere","Inner Magnetosphere Observation","Observe neutral molecules in the equatorial plane"]
["2012-225T20:15:00","000T22:40:40","2012-08-12","INMS","Non-SPASS","Saturn","RINGPLNA",null,"Ring Plane Observation","Observe neutral molecules in the equatorial plane"]
["2012-225T20:40:56","001T22:39:04","2012-08-12","CDA","Non-SPASS","Other","RATE010A",null,"Data rate End:SApo","Range enter= 6.3174539 Rs exit= 7.2917467 Range altitude= 40017.515 km ... -40501.884"]
["2012-225T20:45:00","000T02:00:00","2012-08-12","UVIS","Prime","Dione","ICYEXO","Icy satellite exosphere","ICYEXO:  Icy Satellite Exospheres","Target to kappa Ori to look for volatiles."]
["2012-225T20:45:00","000T02:00:00","2012-08-12","ISS","SPASS Rider","Dione","ICYEXO","Icy satellite exosphere","Dione","Dione occultation of Kappa Orionis (Saiph)"]
["2012-225T20:45:00","000T02:00:00","2012-08-12","VIMS","SPASS Rider","Dione","ICYEX",null,"occultation","follow UVIS occultation"]
["2012-225T20:45:00","000T02:00:00","2012-08-12","CIRS","Non-SPASS","Dione","ICYEX",null,null,"Shutter closed between:  2012-255T20:45:00 -> 20:46:53 2012-255T21:45:00 -> 21:46:53"]
["2012-225T22:45:00","000T02:00:00","2012-08-12","ISS","Prime","RingF","HIRESFRNG","High resolution F ring image","HIGH RES F RING IMAGING","High resolution imaging of the F ring at ~10RS."]
["2012-225T22:45:00","000T02:00:00","2012-08-12","CIRS","SPASS Rider","rings(general)","HIRESFRNG","High resolution F ring image",null,"null"]
["2012-225T22:45:00","000T02:00:00","2012-08-12","VIMS","SPASS Rider","rings(general)","HIRESFRNG","High resolution F ring image","F-Ring observation","320 msec tau_IR"]
["2012-226T00:00:00","000T22:00:00","2012-08-13","RPWS","Non-SPASS","Saturn","AURXNGOUT","Aurora and Saturn Kilometric Radiation","MAPS AS Campaign","Part of AS MAPS Campaign.  Observe the auroral magnetosphere (e.g. the acceleration region) and SKR source regions"]
["2012-226T00:45:00","000T09:00:00","2012-08-13","ISS","Prime","rings(general)","MOONLETC","C ring moonlet search","C-ring moonlet search","C-ring moonlet search"]
["2012-226T00:45:00","000T09:00:00","2012-08-13","CIRS","SPASS Rider","rings(general)","MOONLETC","C ring moonlet search",null,"null"]
["2012-226T01:31:41","000T00:00:01","2012-08-13","MP","SPASS Note","Saturn","PERIAPSE","Periapse",null,"Periapse R = 5.746 Rs, lat = 24 deg, phase = 103 deg"]
["2012-226T04:00:00","000T04:00:00","2012-08-13","RPWS","Non-SPASS","Saturn","NBANDLOW","Campaign to obtain high resolution WBR data in the narrow band emission source region","RPWS Narrowband Source Region Campaign","Part of RPWS campaign to obtain high resolution WBR data in the narrow band emission source region"]
["2012-226T09:45:00","000T04:30:00","2012-08-13","CIRS","Prime","rings(general)","NP50L30S",null,null,"null"]
["2012-226T14:45:00","001T04:35:00","2012-08-13","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG MAPS Survey","Continuous low-rate magnetospheric survey"]
["2012-226T18:55:40","001T00:24:20","2012-08-13","INMS","Non-SPASS","Saturn","SURVEYSEG","Campaign to determine atmospheric and ionospheric thermal structure","Segment Boundary Survey","Part of the MAPS/TOST Campaign. Determine atmospheric and ionospheric thermal structure."]
["2012-226T19:30:00","000T01:30:00","2012-08-13","UVIS","Prime","Mimas","LOPHASE",null,"ICYLON:  Longitude / Phase space coverage","Map uv albedo as a function of longitude and phase angle"]
["2012-226T19:30:00","000T01:30:00","2012-08-13","ISS","SPASS Rider","Mimas","LOPHASE",null,"Mimas ORS observation","ORS observation"]
["2012-226T19:30:00","000T01:30:00","2012-08-13","VIMS","SPASS Rider","Mimas","LOPHASE",null,"low phase","follow UVIS"]
["2012-226T21:00:00","000T11:10:00","2012-08-13","ISS","Prime","RingF","FMOVIE","F ring movie","Med/High Res F Ring Movie","Med/High Resolution F Ring Movie"]
["2012-226T21:00:00","000T11:10:00","2012-08-13","CIRS","SPASS Rider","rings(general)","FMOVIE","F ring movie",null,"null"]
["2012-226T21:00:00","000T11:10:00","2012-08-13","VIMS","SPASS Rider","RingF","FMOVIE","F ring movie","F Movie","Use 640 or 1000 msec tau_IR"]
["2012-227T08:12:00","009T08:27:00","2012-08-14","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2012-227T10:20:00","000T09:00:00","2012-08-14","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2012-227T11:20:00","000T08:00:00","2012-08-14","CIRS","SPASS Rider","InstrumentCalibration","DSCAL12",null,"CIRS_170IC_DSCAL12227_SP","rider"]
["2012-227T19:20:00","010T06:59:00","2012-08-14","CAPS","Non-SPASS","Saturn","SURVEY","Magnetospheric survey","MAPS Survey","null"]
["2012-227T19:20:00","008T21:19:00","2012-08-14","CDA","Non-SPASS","Other","RATE010B",null,"Data rate End:SApo","Range enter= 6.3174539 Rs exit= 7.2917467 Range altitude= 40017.515 km ... -40501.884"]
["2012-227T19:20:00","000T05:33:00","2012-08-14","INMS","Non-SPASS","Saturn","SURVEYSEG","Campaign to determine atmospheric and ionospheric thermal structure","Segment Boundary Survey","Part of the MAPS/TOST Campaign. Determine atmospheric and ionospheric thermal structure."]
["2012-227T19:20:00","009T11:49:00","2012-08-14","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG MAPS Survey","Continuous low-rate magnetospheric survey"]
["2012-227T19:20:00","008T21:19:00","2012-08-14","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SURVEY Campaign","Part of SURVEY MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane.   SATURN_170_171"]
["2012-227T20:00:00","000T16:00:00","2012-08-14","UVIS","Prime","Saturn","EUVFUV","UVIS EUV / FUV imaging","EUVFUV Imaging of Saturn","One slow scans across Saturn's visible hemisphere to form spectral images"]
["2012-227T20:00:00","000T16:00:00","2012-08-14","CIRS","Non-SPASS","Saturn","EUVFUV","UVIS EUV / FUV imaging","EUVFUV rider"]
["2012-228T00:53:00","000T02:00:00","2012-08-15","INMS","Non-SPASS","Titan","TTNTORUS","Titan torus observation","Titan Torus observation","Titan Torus observation"]
["2012-228T02:53:00","008T13:46:00","2012-08-15","INMS","Non-SPASS","Saturn","SURVEYREV",null,"Survey","Part of the MAPS/TOST Campaign. Determine atmospheric and ionospheric thermal structure."]
["2012-228T12:00:00","000T11:00:00","2012-08-15","CIRS","Prime","Saturn","FIRMAP","Far infrared map","Saturn Far-IR map","Northern hemisphere Determine upper troposphere and tropopause temperature with spatial resolution of about two degrees of latitude and longitude"]
["2012-228T12:00:00","000T11:00:00","2012-08-15","VIMS","SPASS Rider","Saturn","FIRMAP","Far infrared map","CIRS FIRMAP ridealong","CIRS FIRMAP Ridealong"]
["2012-228T22:58:00","000T00:02:00","2012-08-15","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2012-229T17:35:00","000T09:00:00","2012-08-16","RSS","SPASS Rider","Saturn","OCCORT","Operations Readiness Test to demonstrate DSN and RSSG preparedness to support upcoming occultations","RSS Operational Readiness Test","RSS Operations Readiness Test (ORT), to demonstrate DSN and RSSG preparedness to support the Rev171 Saturn atmospheric occultation on 2012/246. DSS-25 required for X- and Ka-band support."]
["2012-229T17:35:00","000T09:00:00","2012-08-16","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2012-229T18:35:00","000T08:00:00","2012-08-16","CIRS","SPASS Rider","InstrumentCalibration","DSCAL12",null,"CIRS_170IC_DSCAL12229_SP","rider"]
["2012-230T03:13:00","000T00:02:00","2012-08-17","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2012-230T03:15:00","000T22:00:00","2012-08-17","CIRS","Prime","Saturn","MIRMAP","Mid infrared map","Saturn Mid-IR map","Either hemisphere Determine upper troposphere and tropopause temperature with spatial resolution of about two degrees of latitude and longitude  POINTING: -y to Saturn, z to pole"]
["2012-230T03:15:00","000T22:00:00","2012-08-17","ISS","SPASS Rider","Saturn","MIRMAP","Mid infrared map","Day WAC","Rider on CIRS to monitor day side clouds in WAC every ~2 hours"]
["2012-230T03:15:00","000T22:00:00","2012-08-17","VIMS","SPASS Rider","Saturn","MIRMAP","Mid infrared map","CIRS MIRMAP ridealong","CIRS MIRMAP  Ridealong"]
["2012-231T01:13:00","000T00:02:00","2012-08-18","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2012-231T17:35:00","000T09:00:00","2012-08-18","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2012-231T18:35:00","000T08:00:00","2012-08-18","CIRS","SPASS Rider","InstrumentCalibration","DSCAL12",null,"CIRS_170IC_DSCAL12231_SP","rider"]
["2012-232T03:13:00","000T00:02:00","2012-08-19","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2012-232T03:15:00","000T01:30:00","2012-08-19","ISS","Prime","Titan","M60R3CLD",null,"Titan Monitoring Campaign","Titan Monitoring Campaign, requested phase 55.8 requested range 3.4 Mkm"]
["2012-232T03:15:00","000T01:30:00","2012-08-19","CIRS","SPASS Rider","Titan","M60R3CLD",null,"Rider for Titan Monitoring Campaign","Rider to ISS Titan cloud monitor"]
["2012-232T03:15:00","000T01:30:00","2012-08-19","VIMS","SPASS Rider","Titan","M60R3CLD",null,"Titan Monitoring Campaign and Stormwatch Cube","Titan Monitoring Campaign; phase = 56 deg, range =3.45 Mkm. Ends with Saturn Stormwatch"]
["2012-232T04:43:00","000T00:02:00","2012-08-19","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2012-232T04:45:00","000T05:00:00","2012-08-19","ISS","Prime","Saturn","WIND5HR",null,"Wind measuring 5-6-5 template + polarimetry, 5-hr","STrack features for ~2 hours to get the 2-hr time step for winds, mosaic in longitude, part of the windspeed template. CB2, (2x2 MT2, MT3,BL1) NAC Cycled while observation lasts. First 9 minutes is a 13-filter polarmetry block (see the note)"]
["2012-232T04:45:00","000T05:00:00","2012-08-19","UVIS","SPASS Rider","Saturn","WIND5HR",null,"UVIS Rider to ISS WIND","UVIS Rider to ISS WIND sit-and-stare"]
["2012-232T04:45:00","000T05:00:00","2012-08-19","VIMS","Non-SPASS","Saturn","WIND5HR",null,"5-hr Wind Observation #1","Ride-along with ISS"]
["2012-232T09:45:00","000T06:00:00","2012-08-19","CIRS","Prime","Saturn","COMPSIT","Sit and stare at one location to derive composition","Saturn COMPSIT","Measure oxygen compounds (H2O, CO2) in  stratosphere as a function of latitude. POINTING: -Y to Saturn, Z to pole Either hemisphere"]
["2012-232T09:45:00","000T06:00:00","2012-08-19","UVIS","SPASS Rider","Saturn","COMPSIT","Sit and stare at one location to derive composition","UVIS Rider to CIRS Compsit","UVIS Rider to CIRS Compsit"]
["2012-232T15:43:00","000T00:02:00","2012-08-19","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2012-232T15:43:00","000T00:02:00","2012-08-19","VIMS","SPASS Rider","Saturn","STORMW","Saturn storm watch","Storm Watch Ridealong","Storm Watch: 32*32 pixels with 80 msec integration"]
["2012-232T15:45:00","000T05:00:00","2012-08-19","ISS","Prime","Saturn","WIND5HR",null,"Wind measuring 5-6-5 template + polarimetry, 5-hr","STrack features for ~2 hours to get the 2-hr time step for winds, mosaic in longitude, part of the windspeed template. CB2, (2x2 MT2, MT3,BL1) NAC Cycled while observation lasts. First 9 minutes is a 13-filter polarmetry block (see the note)"]
["2012-232T15:45:00","000T05:00:00","2012-08-19","UVIS","SPASS Rider","Saturn","WIND5HR",null,"UVIS Rider to ISS WIND","UVIS Rider to ISS WIND sit-and-stare"]
["2012-232T15:45:00","000T05:00:00","2012-08-19","VIMS","Non-SPASS","Saturn","WIND5HR",null,"5-hr Wind Observation #1","Ride-along with ISS"]
["2012-232T20:45:00","000T05:00:00","2012-08-19","ISS","Prime","Saturn","WIND5HR",null,"Wind measuring 5-6-5 template + polarimetry, 5-hr","STrack features for ~2 hours to get the 2-hr time step for winds, mosaic in longitude, part of the windspeed template. CB2, (2x2 MT2, MT3,BL1) NAC Cycled while observation lasts. First 9 minutes is a 13-filter polarmetry block (see the note)"]
["2012-232T20:45:00","000T05:00:00","2012-08-19","UVIS","SPASS Rider","Saturn","WIND5HR",null,"UVIS Rider to ISS WIND","UVIS Rider to ISS WIND sit-and-stare"]
["2012-232T20:45:00","000T05:00:00","2012-08-19","VIMS","Non-SPASS","Saturn","WIND5HR",null,"5-hr Wind Observation #1","Ride-along with ISS"]
["2012-233T01:45:00","000T06:00:00","2012-08-20","CIRS","Prime","Saturn","COMPSIT","Sit and stare at one location to derive composition","Saturn COMPSIT","Measure oxygen compounds (H2O, CO2) in  stratosphere as a function of latitude. POINTING: -Y to Saturn, Z to pole Either hemisphere"]
["2012-233T01:45:00","000T06:00:00","2012-08-20","UVIS","SPASS Rider","Saturn","COMPSIT","Sit and stare at one location to derive composition","UVIS Rider to CIRS Compsit","UVIS Rider to CIRS Compsit"]
["2012-233T07:43:00","000T00:02:00","2012-08-20","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2012-233T07:43:00","000T00:02:00","2012-08-20","VIMS","SPASS Rider","Saturn","STORMW","Saturn storm watch","Storm Watch Ridealong","Storm Watch: 32*32 pixels with 80 msec integration"]
["2012-233T07:45:00","000T05:00:00","2012-08-20","ISS","Prime","Saturn","WIND5HR",null,"Wind measuring 5-6-5 template + polarimetry, 5-hr","STrack features for ~2 hours to get the 2-hr time step for winds, mosaic in longitude, part of the windspeed template. CB2, (2x2 MT2, MT3,BL1) NAC Cycled while observation lasts. First 9 minutes is a 13-filter polarmetry block (see the note)"]
["2012-233T07:45:00","000T05:00:00","2012-08-20","UVIS","SPASS Rider","Saturn","WIND5HR",null,"UVIS Rider to ISS WIND","UVIS Rider to ISS WIND sit-and-stare"]
["2012-233T07:45:00","000T05:00:00","2012-08-20","VIMS","Non-SPASS","Saturn","WIND5HR",null,"5-hr Wind Observation #1","Ride-along with ISS"]
["2012-233T16:38:00","000T20:00:00","2012-08-20","CDA","SPASS Rider","DustRAM direction","ISD0051",null,"CDA ISD 2012-236T16:38:00","ISD observation around apoapse 2012-236T16:38:00 43.355822 Rs"]
["2012-233T17:35:00","000T09:00:00","2012-08-20","RSS","SPASS Rider","Saturn","OCCORT","Operations Readiness Test to demonstrate DSN and RSSG preparedness to support upcoming occultations","RSS Operational Readiness Test","RSS Operations Readiness Test (ORT), to demonstrate DSN and RSSG preparedness to support the Rev171 Saturn atmospheric occultation on 2012/246. DSS-25 required for X- and Ka-band support."]
["2012-233T17:35:00","000T09:00:00","2012-08-20","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2012-233T18:35:00","000T08:00:00","2012-08-20","CIRS","SPASS Rider","InstrumentCalibration","DSCAL12",null,"CIRS_170IC_DSCAL12233_SP","rider"]
["2012-234T03:13:00","000T00:02:00","2012-08-21","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2012-234T03:15:00","000T01:30:00","2012-08-21","ISS","Prime","Titan","M90R3CLD",null,"Titan Monitoring Campaign","Titan Monitoring Campaign, requested phase 75.7 requested range 3.5 Mkm"]
["2012-234T03:15:00","000T01:30:00","2012-08-21","CIRS","SPASS Rider","Titan","M90R3CLD",null,"Rider for Titan Monitoring Campaign","Rider to ISS Titan cloud monitor"]
["2012-234T03:15:00","000T01:30:00","2012-08-21","VIMS","SPASS Rider","Titan","M90R3CLD",null,"Titan Monitoring Campaign and Saturn Stormwatch","Titan Monitoring Campaign; phase = 76 deg, range =3.51 Mkm. Ends with Saturn Stormwatch cube"]
["2012-234T04:43:00","000T00:02:00","2012-08-21","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2012-234T04:45:00","000T16:00:00","2012-08-21","UVIS","Prime","Saturn","EUVFUV","UVIS EUV / FUV imaging","EUVFUV Imaging of Saturn","One slow scans across Saturn's visible hemisphere to form spectral images"]
["2012-234T04:45:00","000T16:00:00","2012-08-21","CIRS","Non-SPASS","Saturn","EUVFUV","UVIS EUV / FUV imaging","EUVFUV rider"]
["2012-234T20:43:00","000T00:02:00","2012-08-21","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2012-234T20:43:00","000T00:02:00","2012-08-21","VIMS","SPASS Rider","Saturn","STORMW","Saturn storm watch","Storm Watch Ridealong","Storm Watch: 32*32 pixels with 80 msec integration"]
["2012-234T20:45:00","000T11:00:00","2012-08-21","CIRS","Prime","Saturn","COMPSIT","Sit and stare at one location to derive composition","Saturn COMPSIT","Measure oxygen compounds (H2O, CO2) in  stratosphere as a function of latitude. POINTING: -Y to Saturn, Z to pole Either hemisphere"]
["2012-234T20:45:00","000T11:00:00","2012-08-21","UVIS","SPASS Rider","Saturn","COMPSIT","Sit and stare at one location to derive composition","UVIS Rider to CIRS Compsit","UVIS Rider to CIRS Compsit"]
["2012-234T20:45:00","000T11:00:00","2012-08-21","VIMS","SPASS Rider","Saturn","COMPSIT","Sit and stare at one location to derive composition","CIRS MIRMAP ridealong","CIRS Ridealong"]
["2012-235T07:43:00","000T00:02:00","2012-08-22","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2012-235T10:38:00","000T20:00:00","2012-08-22","CDA","SPASS Rider","DustRAM direction","ISD0051",null,"CDA ISD 2012-236T16:38:00","ISD observation around apoapse 2012-236T16:38:00 43.355822 Rs"]
["2012-235T17:19:00","000T09:00:00","2012-08-22","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2012-235T18:19:00","000T08:00:00","2012-08-22","CIRS","SPASS Rider","InstrumentCalibration","DSCAL12",null,"CIRS_170IC_DSCAL12235_SP","rider"]
["2012-236T02:57:00","000T00:02:00","2012-08-23","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2012-236T02:59:00","000T05:00:00","2012-08-23","ISS","Prime","Saturn","WIND5HR",null,"Wind measuring 5-6-5 template + polarimetry, 5-hr","STrack features for ~2 hours to get the 2-hr time step for winds, mosaic in longitude, part of the windspeed template. CB2, (2x2 MT2, MT3,BL1) NAC Cycled while observation lasts. First 9 minutes is a 13-filter polarmetry block (see the note)"]
["2012-236T02:59:00","000T05:00:00","2012-08-23","UVIS","SPASS Rider","Saturn","WIND5HR",null,"UVIS Rider to ISS WIND","UVIS Rider to ISS WIND sit-and-stare"]
["2012-236T02:59:00","000T05:00:00","2012-08-23","VIMS","Non-SPASS","Saturn","WIND5HR",null,"5-hr Wind Observation #1","Ride-along with ISS"]
["2012-236T07:59:00","000T06:00:00","2012-08-23","CIRS","Prime","Saturn","COMPSIT","Sit and stare at one location to derive composition","Saturn COMPSIT","Measure oxygen compounds (H2O, CO2) in  stratosphere as a function of latitude. POINTING: -Y to Saturn, Z to pole Either hemisphere"]
["2012-236T07:59:00","000T06:00:00","2012-08-23","UVIS","SPASS Rider","Saturn","COMPSIT","Sit and stare at one location to derive composition","UVIS Rider to CIRS Compsit","UVIS Rider to CIRS Compsit"]
["2012-236T13:57:00","000T00:02:00","2012-08-23","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2012-236T13:57:00","000T00:02:00","2012-08-23","VIMS","SPASS Rider","Saturn","STORMW","Saturn storm watch","Storm Watch Ridealong","Storm Watch: 32*32 pixels with 80 msec integration"]
["2012-236T13:59:00","000T05:00:00","2012-08-23","ISS","Prime","Saturn","WIND5HR",null,"Wind measuring 5-6-5 template + polarimetry, 5-hr","STrack features for ~2 hours to get the 2-hr time step for winds, mosaic in longitude, part of the windspeed template. CB2, (2x2 MT2, MT3,BL1) NAC Cycled while observation lasts. First 9 minutes is a 13-filter polarmetry block (see the note)"]
["2012-236T13:59:00","000T05:00:00","2012-08-23","UVIS","SPASS Rider","Saturn","WIND5HR",null,"UVIS Rider to ISS WIND","UVIS Rider to ISS WIND sit-and-stare"]
["2012-236T13:59:00","000T05:00:00","2012-08-23","VIMS","Non-SPASS","Saturn","WIND5HR",null,"5-hr Wind Observation #1","Ride-along with ISS"]
["2012-236T16:38:50","000T00:00:01","2012-08-23","MP","SPASS Note","Saturn","APOAPSE","Apoapse",null,"Apoapse  Per = 21.3 d, inc = 32.2 deg, r = 43.311 Rs, phase = 77 deg"]
["2012-236T16:39:00","001T01:55:00","2012-08-23","CDA","Non-SPASS","Other","RATE010","Dust survey","Data rate Enter:SApo End: S75","Range enter= 6.3174539 Rs exit= 7.2917467 Range altitude= 40017.515 km ... -40501.884"]
["2012-236T16:39:00","000T02:00:00","2012-08-23","INMS","Non-SPASS","Saturn","ENGBCKGND",null,"Engineering background observation","Full rate measurement to gather engineering background data"]
["2012-236T16:39:00","001T09:40:00","2012-08-23","MIMI","Non-SPASS","co-rotation","SURVEY","Magnetospheric survey","MAPS SURVEY Campaign","Part of SURVEY MAPS Campaign.   Pointing: As closely as possible, keep corotation ram in -X, +/-Z half-plane; B field in X, Z plane.   SATURN_170_171"]
["2012-236T16:39:00","001T09:40:00","2012-08-23","RPWS","Non-SPASS","Saturn","OUTSURVEY","Outer magnetospheric survey","RPWS Outer Survey","Setup RPWS for outer magnetosphere survey observations, attitude N/A, any OPMODE or TLM mode including RPWS."]
["2012-236T18:39:00","001T07:40:00","2012-08-23","INMS","Non-SPASS","Saturn","SURVEYSEQ",null,"Sequence Boundary Survey","Part of the MAPS/TOST Campaign. Determine atmospheric and ionospheric thermal structure."]
["2012-236T18:59:00","000T11:00:00","2012-08-23","CIRS","Prime","Saturn","COMPSIT","Sit and stare at one location to derive composition","Saturn COMPSIT","Measure oxygen compounds (H2O, CO2) in  stratosphere as a function of latitude. POINTING: -Y to Saturn, Z to pole Either hemisphere"]
["2012-236T18:59:00","000T11:00:00","2012-08-23","UVIS","SPASS Rider","Saturn","COMPSIT","Sit and stare at one location to derive composition","UVIS Rider to CIRS Compsit","UVIS Rider to CIRS Compsit"]
["2012-236T18:59:00","000T11:00:00","2012-08-23","VIMS","SPASS Rider","Saturn","COMPSIT","Sit and stare at one location to derive composition","CIRS MIRMAP ridealong and Storm Watch","CIRS Ridealong and Stormwatch"]
["2012-237T02:38:00","000T15:56:00","2012-08-24","CDA","SPASS Rider","DustRAM direction","ISD0051",null,"CDA ISD 2012-236T16:38:00 End: S75","ISD observation around apoapse 2012-236T16:38:00 43.355822 Rs"]
["2012-237T05:57:00","000T00:02:00","2012-08-24","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2012-237T07:09:00","000T08:00:00","2012-08-24","MAG","Prime","Sun","CALROLL","MAG calibration roll","MAG Calibration Rolls","Roll about axis other than Z for determination of sensor offsets, actual roll axis is not important - selected axis is usually suitable for MAPS.  Preferably calibrations should be made every 15-20 days in areas where field conditions are suitable.  Note: periods of suitable data are defined as follows; 1) More distant than 15 RS from Saturn's axis (to try and get into the more uniform part of the internal+sheet field). 2) Inside the magnetopause (more specifically inside a most compressed model MP). 3) More distant than 3 RS from the current sheet. Using a 'hinged' sheet model which departs from Saturn's equatorial plane at about 15 RS and then follows the anti-solar direction on the nightside. This means that, even though its orbit is equatorial, if the spacecraft is situated far enough away from the planet, it should see the nightside current sheet divert northwards away from it (using Saturn axis tilted 17 deg away from Sun).  Apart from possible injection events, sheet disruptions etc the resultant periods should have a reasonable probability of seeing a 'quiescent' 'lobe-like' or 'disk-like' field. We would prefer as far downtail as possible so the field has more chance of pointing in a single direction over larger length scales."]
["2012-237T15:07:00","000T00:02:00","2012-08-24","ISS","SPASS Rider","Saturn","STORMW","Saturn storm watch","SATURN STORM WATCH","rider on the last 2 minutes of the turn back to the NEG_Y to Saturn waypoint. Taking advantage of the 2 minute margin."]
["2012-237T15:07:00","000T00:02:00","2012-08-24","VIMS","SPASS Rider","Saturn","STORMW","Saturn storm watch","Storm Watch Ridealong","Storm Watch: 32*32 pixels with 80 msec integration"]
["2012-237T15:09:00","000T11:10:00","2012-08-24","MAG","Non-SPASS","Other","SURVEY","Magnetospheric survey","MAG MAPS Survey","Continuous low-rate magnetospheric survey"]
["2012-237T17:19:00","000T09:00:00","2012-08-24","RSS","SPASS Rider","Saturn","OCCORT","Operations Readiness Test to demonstrate DSN and RSSG preparedness to support upcoming occultations","RSS Operational Readiness Test","RSS Operations Readiness Test (ORT), to demonstrate DSN and RSSG preparedness to support the Rev171 Saturn atmospheric occultation on 2012/246. DSS-14 and DSS-63 required for X- and S-band support."]
["2012-237T17:19:00","000T09:00:00","2012-08-24","UVIS","Non-SPASS","SolarWind","IPHSURVEY","Interplanetary hydrogen survey","UVIS Interplanetary Hydrogen Survey","UVIS is on collecting data at a low rate continuously.  No special pointing is  required."]
["2012-237T18:19:00","000T08:00:00","2012-08-24","CIRS","SPASS Rider","InstrumentCalibration","DSCAL12",null,"CIRS_171IC_DSCAL12237_SP","rider"]
["2012-237T18:34:00","000T04:04:00","2012-08-24","CDA","SPASS Rider","DustRAM direction","ISD0051",null,"CDA ISD 2012-236T16:38:00 Enter: S75","ISD observation around apoapse 2012-236T16:38:00 43.355822 Rs"]
["2012-237T18:34:00","000T07:45:00","2012-08-24","CDA","Non-SPASS","Other","RATE010A",null,"Data rate Enter:SApo Enter: S75","Range enter= 6.3174539 Rs exit= 7.2917467 Range altitude= 40017.515 km ... -40501.884"]